(kicad_pcb (version 4) (host pcbnew 0.201509101502+6177~30~ubuntu14.04.1-product)
  (general
    (links 186)
    (no_connects 0)
    (area 114.161001 40.5024 175.904246 125.738987)
    (thickness 1.2)
    (drawings 41)
    (tracks 1836)
    (zones 0)
    (modules 66)
    (nets 49)
  )
  (page A4)
  (title_block
    (title "Mysensors Node")
    (date "Wed 10 Jun 2015")
    (rev 1.1)
    (company "Designer: Patrick Fallberg")
    (comment 1 "Copyright (c) 2015 Patrick Fallberg")
    (comment 2 "Licensed under CERN OHL v.1.2")
    (comment 3 "Case: Supebat BOX-2252")
  )
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.381)
    (trace_clearance 0.2032)
    (zone_clearance 0.2032)
    (zone_45_only yes)
    (trace_min 0.381)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.635)
    (via_min_drill 0.381)
    (uvia_size 25.4)
    (uvia_drill 0)
    (uvias_allowed no)
    (uvia_min_size 25.4)
    (uvia_min_drill 0)
    (pcb_text_width 0.16)
    (pcb_text_size 0.8 0.8)
    (mod_edge_width 0.15)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.16)
    (pad_size 1.8 1.8)
    (pad_drill 1.8)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 121.311 50.4806)
    (grid_origin 121.311 50.4806)
    (visible_elements 7FFEEE7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Manufacturing/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(ANT1-Pad1)")
  (net 3 +3V3)
  (net 4 "Net-(C4-Pad1)")
  (net 5 "Net-(C5-Pad1)")
  (net 6 VBAT_SMPL)
  (net 7 "Net-(C9-Pad1)")
  (net 8 "Net-(C9-Pad2)")
  (net 9 +3.3VP)
  (net 10 +BATT)
  (net 11 "Net-(JP4-Pad2)")
  (net 12 MYSX_D10_A4)
  (net 13 "Net-(JP6-Pad2)")
  (net 14 "Net-(JP7-Pad1)")
  (net 15 MYSX_D3_INT)
  (net 16 "Net-(JP8-Pad2)")
  (net 17 RF_INT)
  (net 18 RF24_CSN)
  (net 19 "Net-(JP9-Pad2)")
  (net 20 MYSX_D9_A3)
  (net 21 "Net-(L1-Pad1)")
  (net 22 /MISO)
  (net 23 /SCK)
  (net 24 /MOSI)
  (net 25 RESET)
  (net 26 MYSX_3.3V_EN)
  (net 27 MYSX_D7_SCL)
  (net 28 MYSX_D8_SDA)
  (net 29 FLASH_CSN)
  (net 30 MYSX_D14_CS)
  (net 31 ATSHA_SDA)
  (net 32 RF69_NSS)
  (net 33 RF24_CE)
  (net 34 MYSX_D6_PWM)
  (net 35 MYSX_D5_PWM)
  (net 36 MYSX_D4_INT)
  (net 37 MYSX_D1_DFM)
  (net 38 MYSX_D2_DTM)
  (net 39 MYSX_A1)
  (net 40 MYSX_A2)
  (net 41 "Net-(BT1-Pad3)")
  (net 42 "Net-(U4-Pad1)")
  (net 43 "Net-(U4-Pad3)")
  (net 44 "Net-(U4-Pad4)")
  (net 45 "Net-(U4-Pad5)")
  (net 46 "Net-(U4-Pad6)")
  (net 47 "Net-(U4-Pad7)")
  (net 48 "Net-(U4-Pad16)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.381)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 25.4)
    (uvia_drill 0)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net ATSHA_SDA)
    (add_net FLASH_CSN)
    (add_net MYSX_3.3V_EN)
    (add_net MYSX_A1)
    (add_net MYSX_A2)
    (add_net MYSX_D10_A4)
    (add_net MYSX_D14_CS)
    (add_net MYSX_D1_DFM)
    (add_net MYSX_D2_DTM)
    (add_net MYSX_D3_INT)
    (add_net MYSX_D4_INT)
    (add_net MYSX_D5_PWM)
    (add_net MYSX_D6_PWM)
    (add_net MYSX_D7_SCL)
    (add_net MYSX_D8_SDA)
    (add_net MYSX_D9_A3)
    (add_net "Net-(ANT1-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(JP4-Pad2)")
    (add_net "Net-(JP6-Pad2)")
    (add_net "Net-(JP8-Pad2)")
    (add_net "Net-(JP9-Pad2)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad16)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U4-Pad7)")
    (add_net RESET)
    (add_net RF24_CE)
    (add_net RF24_CSN)
    (add_net RF69_NSS)
    (add_net RF_INT)
    (add_net VBAT_SMPL)
  )
  (net_class Power ""
    (clearance 0.2032)
    (trace_width 0.635)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 25.4)
    (uvia_drill 0)
    (add_net +3.3VP)
    (add_net +3V3)
    (add_net +BATT)
    (add_net GND)
    (add_net "Net-(BT1-Pad3)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(JP7-Pad1)")
  )
  (module mysensors_connectors:TerminalBlock2.54mmx2-kcswalter (layer F.Cu) (tedit 55DB1CFA)
    (at 167.666 108.9006 90)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference BT3 (at 3.556 0 180) (layer F.SilkS))
    (fp_text value Generic (at 0 4.50088 90) (layer F.SilkS) hide)
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 1.27 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(BT1-Pad3)"))
    (model mysensors.3dshapes/w.lain.3dshapes/conn_mpt/mpt_0,5-2-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:dc_socket-kcswalter (layer F.Cu) (tedit 55DA49D9)
    (at 146.584 112.9646)
    (descr "Socket, DC power supply")
    (fp_text reference BT1 (at -5.715 -6.858) (layer F.SilkS))
    (fp_text value "2.5mm jack" (at 0 -8.60044) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 5.30098 -3.50012) (size 1.99898 4.0005) (drill oval 1.00076 2.99974) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -0.24892) (size 4.0005 1.99898) (drill oval 2.99974 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 -6.25094) (size 4.50088 1.99898) (drill oval 3.50012 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(BT1-Pad3)"))
    (model mysensors.3dshapes/w.lain.3dshapes/conn_misc/dc_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen_BIG (layer F.Cu) (tedit 55B8AC77)
    (at 134.519 40.9556)
    (descr "Symbol, OSHW-Logo, Silk Screen, BIG")
    (tags "Symbol, OSHW-Logo, Silk Screen, BIG")
    (fp_text reference OSHW_LOGO (at -0.29972 11.50112) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen_BIG (at 0.29972 32.10052) (layer F.Fab))
  )
  (module mysensors_arduino:pro_mini (layer F.Cu) (tedit 55B551B6)
    (at 130.836 98.1056 270)
    (descr "IC, ARDUINO_PRO_MINI x 0,6\"")
    (tags "DIL ARDUINO PRO MINI")
    (fp_text reference U7 (at -18.161 -0.127 360) (layer F.SilkS))
    (fp_text value ArduinoProMini (at 0 0 270) (layer F.Fab) hide)
    (pad 28 thru_hole oval (at 5.08 -5.08 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 40 MYSX_A2))
    (pad 27 thru_hole oval (at 7.62 -5.08 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 39 MYSX_A1))
    (pad 1 thru_hole oval (at -13.97 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 37 MYSX_D1_DFM))
    (pad 2 thru_hole oval (at -11.43 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 38 MYSX_D2_DTM))
    (pad 3 thru_hole oval (at -8.89 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 25 RESET))
    (pad 4 thru_hole oval (at -6.35 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at -3.81 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(JP8-Pad2)"))
    (pad 6 thru_hole oval (at -1.27 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 36 MYSX_D4_INT))
    (pad 7 thru_hole oval (at 1.27 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 26 MYSX_3.3V_EN))
    (pad 8 thru_hole oval (at 3.81 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 35 MYSX_D5_PWM))
    (pad 9 thru_hole oval (at 6.35 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 34 MYSX_D6_PWM))
    (pad 10 thru_hole oval (at 8.89 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 30 MYSX_D14_CS))
    (pad 11 thru_hole oval (at 11.43 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 29 FLASH_CSN))
    (pad 12 thru_hole oval (at 13.97 7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 33 RF24_CE))
    (pad 13 thru_hole oval (at 13.97 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(JP9-Pad2)"))
    (pad 14 thru_hole oval (at 11.43 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 24 /MOSI))
    (pad 15 thru_hole oval (at 8.89 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 /MISO))
    (pad 16 thru_hole oval (at 6.35 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 23 /SCK))
    (pad 17 thru_hole oval (at 3.81 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 VBAT_SMPL))
    (pad 18 thru_hole oval (at 1.27 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 20 MYSX_D9_A3))
    (pad 19 thru_hole oval (at -1.27 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 12 MYSX_D10_A4))
    (pad 20 thru_hole oval (at -3.81 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 31 ATSHA_SDA))
    (pad 21 thru_hole oval (at -6.35 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 22 thru_hole oval (at -8.89 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 25 RESET))
    (pad 23 thru_hole oval (at -11.43 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 24 thru_hole oval (at -13.97 -7.62 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 25 thru_hole oval (at -2.54 -5.08 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 28 MYSX_D8_SDA))
    (pad 26 thru_hole oval (at -5.08 -5.08 270) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 27 MYSX_D7_SCL))
    (pad 27 thru_hole oval (at 13.97 -5.08 270) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 39 MYSX_A1))
    (pad 28 thru_hole oval (at 13.97 -2.54 270) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 40 MYSX_A2))
    (pad 29 thru_hole oval (at 13.97 0 270) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz -0.15 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.55 0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0 0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.25 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model mysensors.3dshapes/arduino_pro_mini.wrl
      (at (xyz -0.05 0 0.48))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model SMD_Packages.3dshapes/TQFP-32.wrl
      (at (xyz 0.05 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 315))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.3 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 0.3 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0.55 0.1 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0.25 0.2 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz -0.15 0.2 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (at (xyz -0.3 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (at (xyz 0.55 -0.175 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x06.wrl
      (at (xyz -0.65 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz -0.3 -0.05 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0.55 -0.125 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz -0.3 0.05 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (at (xyz -0.35 0.15 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (at (xyz -0.35 -0.15 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz -0.4 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz -0.5 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_connectors:MYSX_1.5 (layer F.Cu) (tedit 55B94E9A)
    (at 146.076 103.1856 90)
    (descr "Through hole pin header")
    (tags "pin header MYSX 1.5")
    (fp_text reference P1 (at 4.572 -0.508 180) (layer F.SilkS))
    (fp_text value MYSX_1.5 (at 1.27 26.162 90) (layer F.Fab) hide)
    (fp_text user "MYSX 1.5" (at 4.572 5.715 180) (layer F.SilkS))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 MYSX_D14_CS))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /SCK))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /MISO))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /MOSI))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 MYSX_D10_A4))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 MYSX_D9_A3))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 MYSX_D8_SDA))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 MYSX_D7_SCL))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 MYSX_D6_PWM))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 MYSX_D5_PWM))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 MYSX_D4_INT))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 MYSX_D3_INT))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(JP7-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 +3.3VP))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 MYSX_D1_DFM))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 MYSX_D2_DTM))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 MYSX_A1))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 MYSX_A2))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x10.wrl
      (at (xyz 0.05 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_handsoldering:SOT-23-5_Handsoldering (layer B.Cu) (tedit 55B559E6)
    (at 157.941 62.5456 180)
    (descr "5-pin SOT23 package handsoldering")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 2.34 3.81 180) (layer B.SilkS))
    (fp_text value TPS61097A (at -0.05 -2.35 180) (layer B.Fab))
    (pad 1 smd rect (at -1.47 0.95 180) (size 1.80086 0.65) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at -1.47 0 180) (size 1.80086 0.65) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.47 -0.95 180) (size 1.80086 0.65) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(JP6-Pad2)"))
    (pad 4 smd rect (at 1.47 -0.95 180) (size 1.80086 0.65) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 5 smd rect (at 1.47 0.95 180) (size 1.80086 0.65) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(L1-Pad1)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 55B55AB5)
    (at 141.631 107.1226 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at -3.556 0 360) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -2.3 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 55B94EAE)
    (at 156.236 52.3856 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP9 (at 2.032 5.08 360) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 RF24_CSN))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(JP9-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 RF69_NSS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 55B5586E)
    (at 133.884 77.0236 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U6 (at 0 3.175 180) (layer B.SilkS))
    (fp_text value AT25DF512C (at 0 -3.5 180) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 29 FLASH_CSN))
    (pad 2 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 22 /MISO))
    (pad 3 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 4 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 24 /MOSI))
    (pad 6 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 23 /SCK))
    (pad 7 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 8 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23_Handsoldering (layer B.Cu) (tedit 55B55A6E)
    (at 132.868 87.9456 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U3 (at 0 3.048 180) (layer B.SilkS))
    (fp_text value ATSHA204A (at 0 -3.81 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.50114 180) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 31 ATSHA_SDA))
    (pad 2 smd rect (at 0.95 -1.50114 180) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 0 1.50114 180) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296Y_3-8Zoll_Angular_ScrewUp (layer F.Cu) (tedit 55B55AAA)
    (at 135.916 115.5046 90)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference RV1 (at 1.397 -2.54 180) (layer F.SilkS))
    (fp_text value 1M (at 0 5.08 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 VBAT_SMPL))
    (pad 3 thru_hole circle (at 0 -5.08 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(JP4-Pad2)"))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296Y_3-8Zoll_Angular_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23_Handsoldering (layer F.Cu) (tedit 55B55B9E)
    (at 148.616 88.0726 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 2.286 0 180) (layer F.SilkS))
    (fp_text value DMP3056L-7 (at 0 3.81 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 90) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 26 MYSX_3.3V_EN))
    (pad 2 smd rect (at 0.95 1.50114 90) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 0 -1.50114 90) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 9 +3.3VP))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23_Handsoldering (layer B.Cu) (tedit 55B55ABC)
    (at 144.237 116.79746 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -0.061 3.07086 180) (layer B.SilkS))
    (fp_text value DMP3056L-7 (at 0 -3.81 180) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.50114 180) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C9-Pad2)"))
    (pad 2 smd rect (at 0.95 -1.50114 180) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 10 +BATT))
    (pad 3 smd rect (at 0 1.50114 180) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(JP4-Pad2)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 55B551E3)
    (at 128.296 75.8806 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -1.905 5.207 360) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /MISO))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 55B5556B)
    (at 158.014 59.8786)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference L1 (at 0 -1.524) (layer B.SilkS))
    (fp_text value 4.7uH (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 55B55B84)
    (at 141.631 100.6456)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP10 (at 0 -2.159) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 MYSX_D9_A3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C9-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 55B94EAC)
    (at 158.776 52.3856 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP8 (at 0 7.62 180) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 MYSX_D3_INT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(JP8-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 RF_INT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 55B55B90)
    (at 141.631 90.4856 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP7 (at -3.175 5.969 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(JP7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +BATT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 55B55B97)
    (at 141.631 84.1356 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP6 (at 0 4.445 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 MYSX_D10_A4))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(JP6-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 55B55BBB)
    (at 144.171 90.4856 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP5 (at -3.048 5.969 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 +3.3VP))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 55B94E98)
    (at 139.98 117.9176 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP4 (at -0.635 4.445 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +BATT))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(JP4-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 55B55C5B)
    (at 141.631 77.1506 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP3 (at -1.905 1.27 360) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +BATT))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 55B5520B)
    (at 154.839 107.5036)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP2 (at 0 -2.286) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +BATT))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C4-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 55B55BB0)
    (at 144.044 94.6766 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at -1.905 1.27 360) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(BT1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +BATT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 55B55A81)
    (at 135.662 88.4536 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C17 (at 3.683 0 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -2.3 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55B55A16)
    (at 134.011 77.5316 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C16 (at 2.159 -2.286 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 55B55A59)
    (at 128.423 60.3866 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C15 (at 3.937 -0.508 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -2.3 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_HandSoldering (layer B.Cu) (tedit 55E61B5F)
    (at 131.598 60.3866 270)
    (descr "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (tags "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (attr smd)
    (fp_text reference C14 (at -4.826 0 360) (layer B.SilkS))
    (fp_text value 4.7uF (at -0.09906 -3.59918 270) (layer B.Fab))
    (fp_text user + (at -4.70154 2.4003 270) (layer B.SilkS) hide)
    (pad 2 smd rect (at 2.12598 0 270) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.12598 0 270) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_HandSoldering (layer B.Cu) (tedit 55E61B25)
    (at 152.84002 105.3446)
    (descr "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (tags "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (attr smd)
    (fp_text reference C13 (at -5.49402 -0.254) (layer B.SilkS))
    (fp_text value 4.7uF (at -0.09906 -3.59918) (layer B.Fab))
    (fp_text user + (at -4.70154 2.4003) (layer B.SilkS) hide)
    (pad 2 smd rect (at 2.12598 0) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.12598 0) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_HandSoldering (layer B.Cu) (tedit 55E61B4F)
    (at 147.092 97.7246)
    (descr "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (tags "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (attr smd)
    (fp_text reference C12 (at 0 -2.54) (layer B.SilkS))
    (fp_text value 4.7uF (at -0.09906 -3.59918) (layer B.Fab))
    (fp_text user + (at -4.70154 2.4003) (layer B.SilkS) hide)
    (pad 2 smd rect (at 2.12598 0) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.12598 0) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 9 +3.3VP))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55B55A0C)
    (at 145.822 76.8966 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at 3.683 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer B.Cu) (tedit 55B55A9B)
    (at 132.741 98.3596 90)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference C8 (at 6.985 0 180) (layer B.SilkS))
    (fp_text value C (at -0.39878 -4.20116 90) (layer B.Fab))
    (pad 1 smd trapezoid (at -2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers B.Cu B.Paste B.Mask)
      (net 6 VBAT_SMPL))
    (pad 2 smd trapezoid (at 2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at -5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 6 VBAT_SMPL))
    (pad 2 thru_hole rect (at 5.00126 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 55B55A7A)
    (at 129.947 87.4376 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at -3.683 0 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -2.3 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 55B55A02)
    (at 157.887 65.3396)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at -3.937 0) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2.3) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 55B559CE)
    (at 163.856 63.1806 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at -3.556 0 360) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2.3 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeA_EIA-3216_HandSoldering (layer B.Cu) (tedit 55E61B2B)
    (at 160.26698 111.5676)
    (descr "Tantal Cap. , Size A, EIA-3216, Hand Soldering,")
    (tags "Tantal Cap. , Size A, EIA-3216, Hand Soldering,")
    (attr smd)
    (fp_text reference C4 (at -2.12598 -1.905) (layer B.SilkS))
    (fp_text value 10uF (at -0.09906 -3.0988) (layer B.Fab))
    (fp_text user + (at -4.59994 1.80086) (layer B.SilkS) hide)
    (pad 2 smd rect (at 1.99898 0) (size 2.99974 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.99898 0) (size 2.99974 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeA_EIA-3216_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeA_EIA-3216_HandSoldering (layer B.Cu) (tedit 55E61B20)
    (at 160.427 106.1066 180)
    (descr "Tantal Cap. , Size A, EIA-3216, Hand Soldering,")
    (tags "Tantal Cap. , Size A, EIA-3216, Hand Soldering,")
    (attr smd)
    (fp_text reference C3 (at -4.953 0 180) (layer B.SilkS))
    (fp_text value 10uF (at -0.09906 -3.0988 180) (layer B.Fab))
    (fp_text user + (at -4.59994 1.80086 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at 1.99898 0 180) (size 2.99974 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.99898 0 180) (size 2.99974 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeA_EIA-3216_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_HandSoldering (layer F.Cu) (tedit 55E61B10)
    (at 149.759 93.5336 90)
    (descr "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (tags "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (attr smd)
    (fp_text reference C2 (at 3.302 1.905 180) (layer F.SilkS))
    (fp_text value 4.7uF (at -0.09906 3.59918 90) (layer F.Fab))
    (fp_text user + (at -4.70154 -2.4003 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.12598 0 90) (size 3.1496 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.12598 0 90) (size 3.1496 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(BT1-Pad3)"))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeC_EIA-6032_HandSoldering (layer B.Cu) (tedit 55B5596D)
    (at 144.298 79.3096 90)
    (descr "Tantal Cap. , Size C, EIA-6032, Hand Soldering,")
    (tags "Tantal Cap. , Size C, EIA-6032, Hand Soldering,")
    (attr smd)
    (fp_text reference C1 (at 5.461 0 180) (layer B.SilkS))
    (fp_text value 47uF (at -0.09906 -3.59918 90) (layer B.Fab))
    (fp_text user + (at -5.75056 2.19964 90) (layer B.SilkS))
    (pad 2 smd rect (at 2.99974 0 90) (size 3.50012 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.99974 0 90) (size 3.50012 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 41 "Net-(BT1-Pad3)"))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeC_EIA-6032_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 55B558B6)
    (at 147.346 53.0206)
    (fp_text reference ANT1 (at -1.016 2.54) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(ANT1-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 55B94EAA)
    (at 125.711 54.5806)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference HOLE1 (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module w_logo:Logo_silk_polarity_center_5x1.4mm (layer F.Cu) (tedit 0)
    (at 140.869 109.4086 270)
    (descr "Polarity logo, positive center, 5x1.4mm")
    (fp_text reference PLUG_SPEC (at -0.9 0.6 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 1 0.6 270) (layer F.SilkS) hide)
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 55B94EA2)
    (at 167.411 54.5806)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (clearance 0.1)
    (fp_text reference HOLE2 (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 55B94E93)
    (at 167.411 116.3806)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference HOLE4 (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 55B94E95)
    (at 125.711 116.3806)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference HOLE3 (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 55B55A65)
    (at 128.677 82.9926 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C18 (at 0 1.651 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -2.3 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:DFN-6-1EP_3x3mm_Pitch0.95mm (layer B.Cu) (tedit 55B55A75)
    (at 126.645 86.1676)
    (descr "DFN6 3*3 MM, 0.95 PITCH; CASE 506AH-01 (see ON Semiconductor 506AH.PDF)")
    (tags "DFN 0.95")
    (clearance 0.1)
    (attr smd)
    (fp_text reference U8 (at 0 2.413) (layer B.SilkS))
    (fp_text value Si7021 (at 0 -2.575) (layer B.Fab))
    (pad 1 smd rect (at -1.34 0.95) (size 0.63 0.45) (layers B.Cu B.Paste B.Mask)
      (net 28 MYSX_D8_SDA))
    (pad 2 smd rect (at -1.34 0) (size 0.63 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.34 -0.95) (size 0.63 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at 1.34 -0.95) (size 0.63 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.34 0) (size 0.63 0.45) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 6 smd rect (at 1.34 0.95) (size 0.63 0.45) (layers B.Cu B.Paste B.Mask)
      (net 27 MYSX_D7_SCL))
    (pad 7 smd rect (at 0.425 -0.65) (size 0.85 1.3) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at 0.425 0.65) (size 0.85 1.3) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at -0.425 -0.65) (size 0.85 1.3) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at -0.425 0.65) (size 0.85 1.3) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_3x3mm_Pitch0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 55B55AC3)
    (at 147.473 117.2026 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -2.714 0 360) (layer B.SilkS))
    (fp_text value 10K (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C9-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 +BATT))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 55B55A68)
    (at 134.646 82.7386 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 1.524 180) (layer B.SilkS))
    (fp_text value 56K (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 31 ATSHA_SDA))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55B55BA7)
    (at 146.838 92.8986 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -2.794 0 360) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 MYSX_3.3V_EN))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55B55A27)
    (at 136.297 76.7696 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 3.048 0 360) (layer F.SilkS))
    (fp_text value 56K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 FLASH_CSN))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 55B559D3)
    (at 161.697 61.7366 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -2.747 0 360) (layer B.SilkS))
    (fp_text value 150K (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(JP6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 55B55A8F)
    (at 130.074 96.9626 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -3.302 0 360) (layer B.SilkS))
    (fp_text value 10K (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 27 MYSX_D7_SCL))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 55B55A8A)
    (at 127.28 96.9626 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -3.302 0 360) (layer B.SilkS))
    (fp_text value 10K (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 28 MYSX_D8_SDA))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 55B55AA1)
    (at 129.312 108.5196)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -1.524) (layer B.SilkS))
    (fp_text value 56K (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 30 MYSX_D14_CS))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 55B559DA)
    (at 154.204 61.7836 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 2.667 -0.635 180) (layer B.SilkS))
    (fp_text value 56K (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(JP9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_HandSoldering (layer F.Cu) (tedit 55E61B00)
    (at 148.87 77.4046 270)
    (descr "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (tags "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (attr smd)
    (fp_text reference C10 (at -4.826 0 360) (layer F.SilkS))
    (fp_text value 4.7uF (at -0.09906 3.59918 270) (layer F.Fab))
    (fp_text user + (at -4.70154 -2.4003 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.12598 0 270) (size 3.1496 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.12598 0 270) (size 3.1496 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 55BA35E8)
    (at 170.46 66.3556)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 7.112) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 55B94EA4)
    (at 170.46 58.2276)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -2.159) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 +3.3VP))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 +3.3VP))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 +3.3VP))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_connectors:s2b-ph-kl-kcswalter (layer F.Cu) (tedit 55DA4997)
    (at 160.681 108.9006)
    (descr "JST PH series connector, S2B-PH-KL")
    (fp_text reference BT2 (at 0 -2.159) (layer F.SilkS))
    (fp_text value JST (at 0 7.80034) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.00076 0) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(BT1-Pad3)"))
    (pad 2 thru_hole oval (at 1.00076 0) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model mysensors.3dshapes/w.lain.3dshapes/conn_jst-ph/s2b-ph-kl.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:keystone_3009-kcswalter (layer B.Cu) (tedit 55D79A19)
    (at 158.903 85.1516 270)
    (descr "Keystone type 3009 coin cell retainer")
    (fp_text reference BT5 (at -13.589 5.969 360) (layer B.SilkS))
    (fp_text value 24.5mm (at 0 -10.8 270) (layer B.SilkS))
    (pad 1 thru_hole circle (at -12.7 0 270) (size 3 3) (drill 1.9) (layers *.Cu *.Mask B.SilkS)
      (net 41 "Net-(BT1-Pad3)"))
    (pad 1 thru_hole circle (at 12.7 0 270) (size 3 3) (drill 1.9) (layers *.Cu *.Mask B.SilkS)
      (net 41 "Net-(BT1-Pad3)"))
    (pad 2 smd rect (at 0 0 270) (size 8 8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model mysensors.3dshapes/w.lain.3dshapes/battery_holders/keystone_3009.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_obscurities:d-pak-kcswalter (layer B.Cu) (tedit 55DB55AA)
    (at 155.6645 116.9651 90)
    (descr D-pak)
    (fp_text reference U1 (at 2.6035 7.5565 180) (layer B.SilkS))
    (fp_text value LD1117DT33TR (at 0 -5.9944 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.30124 -3.1242 90) (size 1.6002 3.2004) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 2.30124 -3.1242 90) (size 1.6002 3.2004) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0 3.1242 90) (size 6.49986 7.00024) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model mysensors.3dshapes/w.lain.3dshapes/smd_trans/d-pak.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_radios:RFM69HW_SMD_ThroughHole_Handsoldering (layer F.Cu) (tedit 55DEED2C)
    (at 129.566 70.8006 90)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U4 (at 0 -1.778 180) (layer F.SilkS))
    (fp_text value RFM69HW (at 8.382 7.112 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U4-Pad1)"))
    (pad 2 smd rect (at -1.4 2 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 RF_INT))
    (pad 3 smd rect (at -1.4 4 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U4-Pad3)"))
    (pad 4 smd rect (at -1.4 6 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U4-Pad4)"))
    (pad 5 smd rect (at -1.4 8 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U4-Pad5)"))
    (pad 6 smd rect (at -1.4 10 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U4-Pad6)"))
    (pad 7 smd rect (at -1.4 12 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U4-Pad7)"))
    (pad 8 smd rect (at -1.4 14 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 9 smd rect (at 18.3 14 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 18.3 12 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(ANT1-Pad1)"))
    (pad 11 smd rect (at 18.3 10 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 18.3 8 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 /SCK))
    (pad 13 smd rect (at 18.3 6 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 /MISO))
    (pad 14 smd rect (at 18.3 4 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 /MOSI))
    (pad 15 smd rect (at 18.3 2 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 32 RF69_NSS))
    (pad 16 smd rect (at 18.3 0 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U4-Pad16)"))
    (pad 1 thru_hole rect (at -0.1 0 90) (size 2 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U4-Pad1)"))
    (pad 2 thru_hole circle (at -0.1 2 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 RF_INT))
    (pad 3 thru_hole circle (at -0.1 4 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U4-Pad3)"))
    (pad 4 thru_hole circle (at -0.1 6 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(U4-Pad4)"))
    (pad 5 thru_hole circle (at -0.1 8 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(U4-Pad5)"))
    (pad 6 thru_hole circle (at -0.1 10 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(U4-Pad6)"))
    (pad 7 thru_hole circle (at -0.1 12 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(U4-Pad7)"))
    (pad 8 thru_hole circle (at -0.1 14 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 9 thru_hole circle (at 17 14 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at 17 12 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(ANT1-Pad1)"))
    (pad 11 thru_hole circle (at 17 10 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole circle (at 17 8 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /SCK))
    (pad 13 thru_hole circle (at 17 6 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 /MISO))
    (pad 14 thru_hole circle (at 17 4 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 /MOSI))
    (pad 15 thru_hole circle (at 17 2 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 RF69_NSS))
    (pad 16 thru_hole circle (at 17 0 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(U4-Pad16)"))
    (model mysensors.3dshapes/rfm69hw.wrl
      (at (xyz 0.333 -0.275 0.345))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals_Oscillators_SMD.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0.332 -0.08 0.375))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_strip_2mm_8.wrl
      (at (xyz -0.004 -0.276 0.31))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_strip_2mm_8.wrl
      (at (xyz 0.669 -0.276 0.31))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_socket_2mm_8.wrl
      (at (xyz -0.004 -0.276 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_socket_2mm_8.wrl
      (at (xyz 0.669 -0.276 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.205 -0.445 0.375))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_radios:NRF24L01 (layer F.Cu) (tedit 5587F36C)
    (at 121.692 56.7036 90)
    (descr NRF24L01)
    (tags "nRF 24 NRF24L01 NRF24L01+")
    (fp_text reference U5 (at 0.508 1.397 180) (layer F.SilkS))
    (fp_text value NRF24L01 (at -8.382 7.112 90) (layer F.Fab) hide)
    (pad 7 thru_hole oval (at -9.144 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /MISO))
    (pad 8 thru_hole oval (at -9.144 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 RF_INT))
    (pad 5 thru_hole oval (at -6.604 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /SCK))
    (pad 6 thru_hole oval (at -6.604 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 /MOSI))
    (pad 3 thru_hole oval (at -4.064 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 RF24_CE))
    (pad 4 thru_hole oval (at -4.064 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 RF24_CSN))
    (pad 1 thru_hole rect (at -1.524 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at -1.524 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0.442))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model mysensors.3dshapes/nrf24l01.wrl
      (at (xyz -0.3 -0.5669999999999999 0.475))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz -0.22 -0.51 0.509))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_hc-49s.wrl
      (at (xyz -0.5 -0.475 0.51))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SC-70-6 (layer F.Cu) (tedit 55E61776)
    (at 157.9378 62.43384 270)
    (descr SC-70-6,)
    (tags SC-70-6,)
    (attr smd)
    (fp_text reference U9 (at -1.66624 0.06604 360) (layer F.SilkS))
    (fp_text value TPS61221 (at 0.04064 4.191 270) (layer F.Fab))
    (pad 1 smd rect (at -0.65024 0.94996 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0 0.94996 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 3 smd rect (at 0.65024 0.94996 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65024 -0.94996 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 5 smd rect (at 0 -0.94996 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(L1-Pad1)"))
    (pad 6 smd rect (at -0.65024 -0.94996 270) (size 0.39878 0.7493) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(JP6-Pad2)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:CR123_holder (layer F.Cu) (tedit 55F480B1)
    (at 159.792 57.1106)
    (descr "CR123 battery holder")
    (tags "Battery holder, CR123")
    (fp_text reference BT4 (at -10.414 -1.423) (layer F.SilkS))
    (fp_text value CR123 (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(BT1-Pad3)"))
    (pad 2 thru_hole circle (at 0 37.82) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 8.1 0) (size 1.8 1.8) (drill 1.8) (layers *.Cu Dwgs.User)
      (solder_mask_margin 0.1) (solder_paste_margin 0.1) (clearance 0.1))
    (model mysensors.3dshapes/cr123_holder.wrl
      (at (xyz 0 -0.746 0.28))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 -1.49 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 168.811 117.4806) (end 171.811 117.4806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 124.311 117.4806) (end 124.311 120.4806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 168.811 53.4806) (end 168.811 50.4806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 124.311 53.4806) (end 121.311 53.4806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text GND (at 170.46 75.1186 90) (layer F.SilkS))
  (gr_text +3.3VP (at 170.46 53.4016 90) (layer F.SilkS))
  (gr_text "LP503562 battery pack bottom-layer keepout area\nAvoid components of >2 mm height" (at 161.951 55.5606 90) (layer Cmts.User))
  (dimension 70 (width 0.3) (layer Dwgs.User)
    (gr_text "70.000 mm" (at 120.811 85.4806 270) (layer Dwgs.User))
    (feature1 (pts (xy 121.311 120.4806) (xy 120.811 120.4806)))
    (feature2 (pts (xy 121.311 50.4806) (xy 120.811 50.4806)))
    (crossbar (pts (xy 120.811 50.4806) (xy 120.811 120.4806)))
    (arrow1a (pts (xy 120.811 120.4806) (xy 120.224579 119.354096)))
    (arrow1b (pts (xy 120.811 120.4806) (xy 121.397421 119.354096)))
    (arrow2a (pts (xy 120.811 50.4806) (xy 120.224579 51.607104)))
    (arrow2b (pts (xy 120.811 50.4806) (xy 121.397421 51.607104)))
  )
  (dimension 50.5 (width 0.3) (layer Dwgs.User)
    (gr_text "50.500 mm" (at 146.561 49.9806) (layer Dwgs.User))
    (feature1 (pts (xy 121.311 50.4806) (xy 121.311 49.9806)))
    (feature2 (pts (xy 171.811 50.4806) (xy 171.811 49.9806)))
    (crossbar (pts (xy 171.811 49.9806) (xy 121.311 49.9806)))
    (arrow1a (pts (xy 121.311 49.9806) (xy 122.437504 49.394179)))
    (arrow1b (pts (xy 121.311 49.9806) (xy 122.437504 50.567021)))
    (arrow2a (pts (xy 171.811 49.9806) (xy 170.684496 49.394179)))
    (arrow2b (pts (xy 171.811 49.9806) (xy 170.684496 50.567021)))
  )
  (gr_line (start 121.311 117.4806) (end 121.311 53.4806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 168.811 120.4806) (end 124.311 120.4806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.811 53.4806) (end 171.811 117.4806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.311 50.4806) (end 168.811 50.4806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "MySensorsNode\nRev. 1.1\nLicensed under CERN OHL v.1.2" (at 151.283 118.0446) (layer F.SilkS))
  (gr_text PF (at 163.178469 117.178557) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.508)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 171.811 120.4806) (xy 121.311 120.4806) (xy 121.311 50.4806) (xy 171.811 50.4806)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2032))
    (min_thickness 0.508)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 121.311 120.4806) (xy 121.311 50.4806) (xy 171.811 50.4806) (xy 171.811 120.4806)
      )
    )
  )
)
