(kicad_pcb (version 4) (host pcbnew 0.201509101502+6177~30~ubuntu14.04.1-product)
  (general
    (links 186)
    (no_connects 0)
    (area 80.161001 49.4806 167.066729 150.1516)
    (thickness 1.2)
    (drawings 40)
    (tracks 1841)
    (zones 0)
    (modules 66)
    (nets 49)
  )
  (page A4)
  (title_block
    (title "Mysensors Node")
    (date "Wed 10 Jun 2015")
    (rev 1.1)
    (company "Designer: Patrick Fallberg")
    (comment 1 "Copyright (c) 2015 Patrick Fallberg")
    (comment 2 "Licensed under CERN OHL v.1.2")
    (comment 3 "Case: Supebat LE-BOX-0028")
  )
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.381)
    (trace_clearance 0.2032)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.381)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.635)
    (via_min_drill 0.381)
    (uvia_size 25.4)
    (uvia_drill 0)
    (uvias_allowed no)
    (uvia_min_size 25.4)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 87.811 51.9806)
    (grid_origin 87.811 51.9806)
    (visible_elements 7FFEFE7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Manufacturing/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(ANT1-Pad1)")
  (net 3 "Net-(BT1-Pad3)")
  (net 4 +3V3)
  (net 5 "Net-(C4-Pad1)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 VBAT_SMPL)
  (net 8 "Net-(C9-Pad1)")
  (net 9 "Net-(C9-Pad2)")
  (net 10 +3.3VP)
  (net 11 +BATT)
  (net 12 "Net-(JP4-Pad2)")
  (net 13 MYSX_D10_A4)
  (net 14 "Net-(JP6-Pad2)")
  (net 15 "Net-(JP7-Pad1)")
  (net 16 MYSX_D3_INT)
  (net 17 "Net-(JP8-Pad2)")
  (net 18 RF_INT)
  (net 19 RF24_CSN)
  (net 20 "Net-(JP9-Pad2)")
  (net 21 RF69_NSS)
  (net 22 MYSX_D9_A3)
  (net 23 "Net-(L1-Pad1)")
  (net 24 MYSX_D14_CS)
  (net 25 /SCK)
  (net 26 /MISO)
  (net 27 /MOSI)
  (net 28 MYSX_D8_SDA)
  (net 29 MYSX_D7_SCL)
  (net 30 MYSX_D6_PWM)
  (net 31 MYSX_D5_PWM)
  (net 32 MYSX_D4_INT)
  (net 33 MYSX_D1_DFM)
  (net 34 MYSX_D2_DTM)
  (net 35 MYSX_A1)
  (net 36 MYSX_A2)
  (net 37 RESET)
  (net 38 MYSX_3.3V_EN)
  (net 39 FLASH_CSN)
  (net 40 ATSHA_SDA)
  (net 41 "Net-(U4-Pad1)")
  (net 42 "Net-(U4-Pad3)")
  (net 43 "Net-(U4-Pad4)")
  (net 44 "Net-(U4-Pad5)")
  (net 45 "Net-(U4-Pad6)")
  (net 46 "Net-(U4-Pad7)")
  (net 47 "Net-(U4-Pad16)")
  (net 48 RF24_CE)
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.381)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 25.4)
    (uvia_drill 0)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net ATSHA_SDA)
    (add_net FLASH_CSN)
    (add_net MYSX_3.3V_EN)
    (add_net MYSX_A1)
    (add_net MYSX_A2)
    (add_net MYSX_D10_A4)
    (add_net MYSX_D14_CS)
    (add_net MYSX_D1_DFM)
    (add_net MYSX_D2_DTM)
    (add_net MYSX_D3_INT)
    (add_net MYSX_D4_INT)
    (add_net MYSX_D5_PWM)
    (add_net MYSX_D6_PWM)
    (add_net MYSX_D7_SCL)
    (add_net MYSX_D8_SDA)
    (add_net MYSX_D9_A3)
    (add_net "Net-(ANT1-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(JP4-Pad2)")
    (add_net "Net-(JP6-Pad2)")
    (add_net "Net-(JP8-Pad2)")
    (add_net "Net-(JP9-Pad2)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad16)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U4-Pad7)")
    (add_net RESET)
    (add_net RF24_CE)
    (add_net RF24_CSN)
    (add_net RF69_NSS)
    (add_net RF_INT)
    (add_net VBAT_SMPL)
  )
  (net_class Power ""
    (clearance 0.2032)
    (trace_width 0.635)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 25.4)
    (uvia_drill 0)
    (add_net +3.3VP)
    (add_net +3V3)
    (add_net +BATT)
    (add_net GND)
    (add_net "Net-(BT1-Pad3)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(JP7-Pad1)")
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55E36F7C)
    (at 158.1944 88.4804 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -2.8194 0 360) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 38 MYSX_3.3V_EN))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 55E36C61)
    (at 155.502 75.2216 180)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U6 (at 0 3.175 180) (layer F.SilkS))
    (fp_text value AT25DF512C (at 0 3.5 180) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 FLASH_CSN))
    (pad 2 smd rect (at -2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /MISO))
    (pad 3 smd rect (at -2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 4 smd rect (at -2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 2.7 1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /MOSI))
    (pad 6 smd rect (at 2.7 0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /SCK))
    (pad 7 smd rect (at 2.7 -0.635 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 8 smd rect (at 2.7 -1.905 180) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen_BIG (layer F.Cu) (tedit 55E0825F)
    (at 145.977 95.1606)
    (descr "Symbol, OSHW-Logo, Silk Screen, BIG")
    (tags "Symbol, OSHW-Logo, Silk Screen, BIG")
    (fp_text reference OPHW_LOGO (at -0.29972 11.50112) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen_BIG (at 0.29972 32.10052) (layer F.Fab))
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 55E2354C)
    (at 93.699197 61.395853)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference HOLE1 (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 1.00076 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 55E23550)
    (at 93.699197 138.585853)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference HOLE3 (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 1.00076 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 55E23548)
    (at 157.859197 61.395853)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference HOLE2 (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 1.00076 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module Mounting_Holes:MountingHole_3mm locked (layer F.Cu) (tedit 55E23553)
    (at 157.859197 138.575853)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference HOLE4 (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 1.00076 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module w_logo:Logo_silk_polarity_center_5x1.4mm (layer F.Cu) (tedit 55A6CB85)
    (at 125.911 131.9906)
    (descr "Polarity logo, positive center, 5x1.4mm")
    (fp_text reference PLUG_SPEC (at -0.9 0.6) (layer F.SilkS) hide)
    (fp_text value LOGO (at 1 0.6) (layer F.SilkS) hide)
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 55E3468B)
    (at 160.201 103.4156)
    (fp_text reference ANT1 (at -3.556 0) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(ANT1-Pad1)"))
  )
  (module mysensors_connectors:dc_socket-kcswalter locked (layer F.Cu) (tedit 55E40FF0)
    (at 125.784 140.49452)
    (descr "Socket, DC power supply")
    (fp_text reference BT1 (at -3.683 -8.24992) (layer F.SilkS))
    (fp_text value "2.5mm jack" (at 0 -8.60044) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 5.30098 -3.50012) (size 1.99898 4.0005) (drill oval 1.00076 2.99974) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -0.24892) (size 4.0005 1.99898) (drill oval 2.99974 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 -6.25094) (size 4.50088 1.99898) (drill oval 3.50012 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(BT1-Pad3)"))
    (model mysensors.3dshapes/w.lain.3dshapes/conn_misc/dc_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:s2b-ph-kl-kcswalter (layer F.Cu) (tedit 55E40FF4)
    (at 116.02024 137.0706)
    (descr "JST PH series connector, S2B-PH-KL")
    (fp_text reference BT2 (at 0 -1.905) (layer F.SilkS))
    (fp_text value JST (at 0 7.80034) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.00076 0) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(BT1-Pad3)"))
    (pad 2 thru_hole oval (at 1.00076 0) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model mysensors.3dshapes/w.lain.3dshapes/conn_jst-ph/s2b-ph-kl.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:TerminalBlock2.54mmx2-kcswalter (layer F.Cu) (tedit 55E325E0)
    (at 108.131 139.6106)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference BT3 (at 1.27 -3.81) (layer F.SilkS))
    (fp_text value Generic (at 0 4.50088) (layer F.SilkS) hide)
    (pad 2 thru_hole oval (at -1.27 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 1.27 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(BT1-Pad3)"))
    (model mysensors.3dshapes/w.lain.3dshapes/conn_mpt/mpt_0,5-2-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:keystone_3009-kcswalter locked (layer F.Cu) (tedit 55E325FC)
    (at 100.638 122.5926 270)
    (descr "Keystone type 3009 coin cell retainer")
    (fp_text reference BT5 (at -12.954 10.541 360) (layer F.SilkS))
    (fp_text value 24.5mm (at 0 10.8 270) (layer F.SilkS))
    (pad 1 thru_hole circle (at -12.7 0 270) (size 3 3) (drill 1.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(BT1-Pad3)"))
    (pad 1 thru_hole circle (at 12.7 0 270) (size 3 3) (drill 1.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(BT1-Pad3)"))
    (pad 2 smd rect (at 0 0 270) (size 8 8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model mysensors.3dshapes/w.lain.3dshapes/battery_holders/keystone_3009.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeC_EIA-6032_HandSoldering (layer F.Cu) (tedit 55E61A96)
    (at 109.401 104.0506 270)
    (descr "Tantal Cap. , Size C, EIA-6032, Hand Soldering,")
    (tags "Tantal Cap. , Size C, EIA-6032, Hand Soldering,")
    (attr smd)
    (fp_text reference C1 (at -5.842 0 360) (layer F.SilkS))
    (fp_text value 47uF (at -0.09906 3.59918 270) (layer F.Fab))
    (fp_text user + (at -5.75056 -2.19964 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.99974 0 270) (size 3.50012 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.99974 0 270) (size 3.50012 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BT1-Pad3)"))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeC_EIA-6032_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_HandSoldering (layer F.Cu) (tedit 55E61A90)
    (at 113.465 104.14458 270)
    (descr "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (tags "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (attr smd)
    (fp_text reference C2 (at -4.91998 0 360) (layer F.SilkS))
    (fp_text value 4.7uF (at -0.09906 3.59918 270) (layer F.Fab))
    (fp_text user + (at -4.70154 -2.4003 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.12598 0 270) (size 3.1496 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.12598 0 270) (size 3.1496 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BT1-Pad3)"))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeA_EIA-3216_HandSoldering (layer F.Cu) (tedit 55E61A7C)
    (at 133.023 142.6586 90)
    (descr "Tantal Cap. , Size A, EIA-3216, Hand Soldering,")
    (tags "Tantal Cap. , Size A, EIA-3216, Hand Soldering,")
    (attr smd)
    (fp_text reference C3 (at 4.318 0 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.09906 3.0988 90) (layer F.Fab))
    (fp_text user + (at -4.59994 -1.80086 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.99898 0 90) (size 2.99974 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.99898 0 90) (size 2.99974 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeA_EIA-3216_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeA_EIA-3216_HandSoldering (layer F.Cu) (tedit 55E61A71)
    (at 143.691 142.69162 90)
    (descr "Tantal Cap. , Size A, EIA-3216, Hand Soldering,")
    (tags "Tantal Cap. , Size A, EIA-3216, Hand Soldering,")
    (attr smd)
    (fp_text reference C4 (at 4.22402 0 180) (layer F.SilkS))
    (fp_text value 10uF (at -0.09906 3.0988 90) (layer F.Fab))
    (fp_text user + (at -4.59994 -1.80086 90) (layer F.SilkS) hide)
    (pad 2 smd rect (at 1.99898 0 90) (size 2.99974 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.99898 0 90) (size 2.99974 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeA_EIA-3216_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55E326C5)
    (at 146.993 143.6746 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at -3.81 0 360) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55E326D0)
    (at 154.6638 143.6746 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55E35800)
    (at 154.359 85.0006 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 55E34A0F)
    (at 140.135 101.0026 270)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference C8 (at -6.858 0 360) (layer F.SilkS))
    (fp_text value C (at -0.39878 4.20116 270) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.413 0 270) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 7 VBAT_SMPL))
    (pad 2 smd trapezoid (at 2.413 0 90) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at -5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 7 VBAT_SMPL))
    (pad 2 thru_hole rect (at 5.00126 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55E34A66)
    (at 137.341 101.2566 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at -3.81 0 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_HandSoldering (layer F.Cu) (tedit 55E61A76)
    (at 158.169 133.0066 180)
    (descr "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (tags "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (attr smd)
    (fp_text reference C10 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 4.7uF (at -0.09906 3.59918 180) (layer F.Fab))
    (fp_text user + (at -4.70154 -2.4003 180) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.12598 0 180) (size 3.1496 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.12598 0 180) (size 3.1496 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55E3271F)
    (at 159.185 130.2126)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at -4.445 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_HandSoldering (layer F.Cu) (tedit 55E61AA0)
    (at 137.595 63.9186 270)
    (descr "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (tags "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (attr smd)
    (fp_text reference C12 (at 4.445 0 360) (layer F.SilkS))
    (fp_text value 4.7uF (at -0.09906 3.59918 270) (layer F.Fab))
    (fp_text user + (at -4.70154 -2.4003 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.12598 0 270) (size 3.1496 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.12598 0 270) (size 3.1496 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 10 +3.3VP))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_HandSoldering (layer F.Cu) (tedit 55E61A9E)
    (at 133.023 63.9186 270)
    (descr "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (tags "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (attr smd)
    (fp_text reference C13 (at 4.445 0 360) (layer F.SilkS))
    (fp_text value 4.7uF (at -0.09906 3.59918 270) (layer F.Fab))
    (fp_text user + (at -4.70154 -2.4003 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.12598 0 270) (size 3.1496 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.12598 0 270) (size 3.1496 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_HandSoldering (layer F.Cu) (tedit 55E61A8D)
    (at 125.911 106.5906)
    (descr "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (tags "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (attr smd)
    (fp_text reference C14 (at 0 -2.54) (layer F.SilkS))
    (fp_text value 4.7uF (at -0.09906 3.59918) (layer F.Fab))
    (fp_text user + (at -4.70154 -2.4003) (layer F.SilkS) hide)
    (pad 2 smd rect (at 2.12598 0) (size 3.1496 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.12598 0) (size 3.1496 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55E349D2)
    (at 118.323 106.5906)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C15 (at -0.032 -1.905) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55E36CA4)
    (at 153.851 79.2856 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C16 (at 2.032 -1.778 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55E357F7)
    (at 148.517 92.7476 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C17 (at 3.81 0 360) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55E36950)
    (at 101.781 58.9656)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C18 (at 0 -1.905) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 locked (layer F.Cu) (tedit 55E321D7)
    (at 111.941 95.1606 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(BT1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 +BATT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 locked (layer F.Cu) (tedit 55E321DA)
    (at 111.941 92.6206 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP2 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 +BATT))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C4-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 locked (layer F.Cu) (tedit 55E321DE)
    (at 111.941 90.0806 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP3 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 +BATT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 locked (layer F.Cu) (tedit 55E321E1)
    (at 111.941 87.5406 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP4 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 +BATT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(JP4-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 locked (layer F.Cu) (tedit 55E321E4)
    (at 111.941 85.0006 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP5 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +3.3VP))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 locked (layer F.Cu) (tedit 55E321E8)
    (at 111.941 82.4606 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP6 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 MYSX_D10_A4))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(JP6-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 locked (layer F.Cu) (tedit 55E321EB)
    (at 111.941 79.9206 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP7 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(JP7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 +BATT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 locked (layer F.Cu) (tedit 55E321F4)
    (at 111.941 77.3806 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP8 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 MYSX_D3_INT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(JP8-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 RF_INT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 locked (layer F.Cu) (tedit 55E321F8)
    (at 111.941 74.8406 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP9 (at 0 -2.794 180) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 RF24_CSN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(JP9-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 RF69_NSS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 locked (layer F.Cu) (tedit 55E321EF)
    (at 111.941 72.3006 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP10 (at 0 -3.048 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 MYSX_D9_A3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C9-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 55E326BC)
    (at 150.803 141.8966 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference L1 (at 0 1.524 180) (layer F.SilkS))
    (fp_text value 4.7uH (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:MYSX_1.5 locked (layer F.Cu) (tedit 55E37656)
    (at 137.341 54.5206 270)
    (descr "Through hole pin header")
    (tags "pin header MYSX 1.5")
    (fp_text reference P1 (at 0 -2.413 360) (layer F.SilkS))
    (fp_text value MYSX_1.5 (at 1.27 26.162 270) (layer F.Fab))
    (fp_text user 1.5 (at 2.54 -3.302 270) (layer Cmts.User) hide)
    (pad 20 thru_hole oval (at 2.54 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 MYSX_D14_CS))
    (pad 19 thru_hole oval (at 0 22.86 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /SCK))
    (pad 18 thru_hole oval (at 2.54 20.32 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /MISO))
    (pad 17 thru_hole oval (at 0 20.32 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /MOSI))
    (pad 16 thru_hole oval (at 2.54 17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 MYSX_D10_A4))
    (pad 15 thru_hole oval (at 0 17.78 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 MYSX_D9_A3))
    (pad 14 thru_hole oval (at 2.54 15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 MYSX_D8_SDA))
    (pad 13 thru_hole oval (at 0 15.24 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 MYSX_D7_SCL))
    (pad 12 thru_hole oval (at 2.54 12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 MYSX_D6_PWM))
    (pad 11 thru_hole oval (at 0 12.7 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 MYSX_D5_PWM))
    (pad 10 thru_hole oval (at 2.54 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 MYSX_D4_INT))
    (pad 9 thru_hole oval (at 0 10.16 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 MYSX_D3_INT))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(JP7-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +3.3VP))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 MYSX_D1_DFM))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 MYSX_D2_DTM))
    (pad 7 thru_hole oval (at 0 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 MYSX_A1))
    (pad 8 thru_hole oval (at 2.54 7.62 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 MYSX_A2))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x10.wrl
      (at (xyz 0.05 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 55E3F8A9)
    (at 150.041 57.0606 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /MISO))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 55E41067)
    (at 142.421 54.5206)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 6.985) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +3.3VP))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +3.3VP))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +3.3VP))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 55E4106C)
    (at 144.961 54.5206)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 6.985) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23_Handsoldering (layer F.Cu) (tedit 55E34A15)
    (at 133.277 101.7646)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -3.302 180) (layer F.SilkS))
    (fp_text value DMP3056L-7 (at 0 3.81) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C9-Pad2)"))
    (pad 2 smd rect (at 0.95 1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 11 +BATT))
    (pad 3 smd rect (at 0 -1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(JP4-Pad2)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23_Handsoldering (layer F.Cu) (tedit 55E36F72)
    (at 147.628 62.6486 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 2.1844 0 180) (layer F.SilkS))
    (fp_text value DMP3056L-7 (at 0 3.81 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 90) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 38 MYSX_3.3V_EN))
    (pad 2 smd rect (at 0.95 1.50114 90) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 3 smd rect (at 0 -1.50114 90) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 10 +3.3VP))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55E32705)
    (at 148.263 138.3406 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.524 180) (layer F.SilkS))
    (fp_text value 150K (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(JP6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55E34A18)
    (at 134.039 106.5906)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.524) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C9-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 +BATT))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55E37695)
    (at 104.9814 63.3344 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -2.8448 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 MYSX_D7_SCL))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55E37699)
    (at 103.051 63.3344 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -2.8194 0 180) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 MYSX_D8_SDA))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55E36C9F)
    (at 158.296 80.5556 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 3.048 0 360) (layer F.SilkS))
    (fp_text value 56K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 39 FLASH_CSN))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55E41055)
    (at 114.5064 61.0992 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 2.8194 0.0254 360) (layer F.SilkS))
    (fp_text value 56K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 MYSX_D14_CS))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55E36B72)
    (at 115.2646 69.2272)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0.0038 -1.4478 180) (layer F.SilkS))
    (fp_text value 56K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(JP9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55E35808)
    (at 152.327 89.5726)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 3.048 0) (layer F.SilkS))
    (fp_text value 56K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 ATSHA_SDA))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296Y_3-8Zoll_Angular_ScrewUp (layer F.Cu) (tedit 55E349F1)
    (at 128.451 99.4786 90)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference RV1 (at 1.397 -2.413 180) (layer F.SilkS))
    (fp_text value 1M (at 0 5.08 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 VBAT_SMPL))
    (pad 3 thru_hole circle (at 0 -5.08 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(JP4-Pad2)"))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296Y_3-8Zoll_Angular_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_obscurities:d-pak-kcswalter (layer F.Cu) (tedit 55E32692)
    (at 137.976 142.7348)
    (descr D-pak)
    (fp_text reference U1 (at 0 -7.3152) (layer F.SilkS))
    (fp_text value LD1117DT33TR (at 0 5.9944) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.30124 3.1242) (size 1.6002 3.2004) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 2.30124 3.1242) (size 1.6002 3.2004) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0 -3.1242) (size 6.49986 7.00024) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (model mysensors.3dshapes/w.lain.3dshapes/smd_trans/d-pak.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_handsoldering:SOT-23-5_Handsoldering (layer F.Cu) (tedit 55E326AA)
    (at 150.803 145.5796)
    (descr "5-pin SOT23 package handsoldering")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 0 -2.032) (layer F.SilkS))
    (fp_text value TPS61097A (at -0.05 2.35) (layer F.Fab))
    (pad 1 smd rect (at -1.47 -0.95) (size 1.80086 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at -1.47 0) (size 1.80086 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.47 0.95) (size 1.80086 0.65) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(JP6-Pad2)"))
    (pad 4 smd rect (at 1.47 0.95) (size 1.80086 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 5 smd rect (at 1.47 -0.95) (size 1.80086 0.65) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(L1-Pad1)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23_Handsoldering (layer F.Cu) (tedit 55E35816)
    (at 151.499 85.78546)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U3 (at 0 -3.048) (layer F.SilkS))
    (fp_text value ATSHA204A (at 0 3.81) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 40 ATSHA_SDA))
    (pad 2 smd rect (at 0.95 1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 3 smd rect (at 0 -1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_radios:RFM69HW_SMD_ThroughHole_Handsoldering locked (layer F.Cu) (tedit 55DEED2C)
    (at 148.137 125.6406 90)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U4 (at -4.445 -0.001 180) (layer F.SilkS))
    (fp_text value RFM69HW (at 8.382 7.112 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U4-Pad1)"))
    (pad 2 smd rect (at -1.4 2 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 RF_INT))
    (pad 3 smd rect (at -1.4 4 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U4-Pad3)"))
    (pad 4 smd rect (at -1.4 6 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U4-Pad4)"))
    (pad 5 smd rect (at -1.4 8 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U4-Pad5)"))
    (pad 6 smd rect (at -1.4 10 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U4-Pad6)"))
    (pad 7 smd rect (at -1.4 12 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U4-Pad7)"))
    (pad 8 smd rect (at -1.4 14 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 9 smd rect (at 18.3 14 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 18.3 12 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(ANT1-Pad1)"))
    (pad 11 smd rect (at 18.3 10 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 18.3 8 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 /SCK))
    (pad 13 smd rect (at 18.3 6 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 /MISO))
    (pad 14 smd rect (at 18.3 4 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 27 /MOSI))
    (pad 15 smd rect (at 18.3 2 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 RF69_NSS))
    (pad 16 smd rect (at 18.3 0 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U4-Pad16)"))
    (pad 1 thru_hole rect (at -0.1 0 90) (size 2 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(U4-Pad1)"))
    (pad 2 thru_hole circle (at -0.1 2 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 RF_INT))
    (pad 3 thru_hole circle (at -0.1 4 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U4-Pad3)"))
    (pad 4 thru_hole circle (at -0.1 6 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U4-Pad4)"))
    (pad 5 thru_hole circle (at -0.1 8 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(U4-Pad5)"))
    (pad 6 thru_hole circle (at -0.1 10 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(U4-Pad6)"))
    (pad 7 thru_hole circle (at -0.1 12 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(U4-Pad7)"))
    (pad 8 thru_hole circle (at -0.1 14 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 9 thru_hole circle (at 17 14 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at 17 12 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(ANT1-Pad1)"))
    (pad 11 thru_hole circle (at 17 10 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole circle (at 17 8 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /SCK))
    (pad 13 thru_hole circle (at 17 6 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /MISO))
    (pad 14 thru_hole circle (at 17 4 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /MOSI))
    (pad 15 thru_hole circle (at 17 2 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 RF69_NSS))
    (pad 16 thru_hole circle (at 17 0 90) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(U4-Pad16)"))
    (model mysensors.3dshapes/rfm69hw.wrl
      (at (xyz 0.333 -0.275 0.345))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals_Oscillators_SMD.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0.332 -0.08 0.375))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_strip_2mm_8.wrl
      (at (xyz -0.004 -0.276 0.31))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_strip_2mm_8.wrl
      (at (xyz 0.669 -0.276 0.31))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_socket_2mm_8.wrl
      (at (xyz -0.004 -0.276 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_socket_2mm_8.wrl
      (at (xyz 0.669 -0.276 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.205 -0.445 0.375))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_radios:NRF24L01 locked (layer F.Cu) (tedit 55E34990)
    (at 115.497 108.8766 90)
    (descr NRF24L01)
    (tags "nRF 24 NRF24L01 NRF24L01+")
    (fp_text reference U5 (at -1.524 -1.016 180) (layer F.SilkS))
    (fp_text value NRF24L01 (at -8.382 7.112 90) (layer F.Fab) hide)
    (pad 7 thru_hole oval (at -9.144 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 /MISO))
    (pad 8 thru_hole oval (at -9.144 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 RF_INT))
    (pad 5 thru_hole oval (at -6.604 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 /SCK))
    (pad 6 thru_hole oval (at -6.604 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 /MOSI))
    (pad 3 thru_hole oval (at -4.064 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 RF24_CE))
    (pad 4 thru_hole oval (at -4.064 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 RF24_CSN))
    (pad 1 thru_hole rect (at -1.524 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at -1.524 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0.442))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model mysensors.3dshapes/nrf24l01.wrl
      (at (xyz -0.3 -0.5669999999999999 0.475))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz -0.22 -0.51 0.509))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_hc-49s.wrl
      (at (xyz -0.5 -0.475 0.51))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_arduino:pro_mini (layer F.Cu) (tedit 55A3E6CB)
    (at 153.343 83.3496 90)
    (descr "IC, ARDUINO_PRO_MINI x 0,6\"")
    (tags "DIL ARDUINO PRO MINI")
    (fp_text reference U7 (at 16.129 -8.382 180) (layer F.SilkS))
    (fp_text value ArduinoProMini (at 0 0 90) (layer F.Fab) hide)
    (pad 28 thru_hole oval (at 5.08 -5.08 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 36 MYSX_A2))
    (pad 27 thru_hole oval (at 7.62 -5.08 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 35 MYSX_A1))
    (pad 1 thru_hole oval (at -13.97 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 33 MYSX_D1_DFM))
    (pad 2 thru_hole oval (at -11.43 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 34 MYSX_D2_DTM))
    (pad 3 thru_hole oval (at -8.89 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 37 RESET))
    (pad 4 thru_hole oval (at -6.35 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole oval (at -3.81 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(JP8-Pad2)"))
    (pad 6 thru_hole oval (at -1.27 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 32 MYSX_D4_INT))
    (pad 7 thru_hole oval (at 1.27 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 38 MYSX_3.3V_EN))
    (pad 8 thru_hole oval (at 3.81 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 31 MYSX_D5_PWM))
    (pad 9 thru_hole oval (at 6.35 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 30 MYSX_D6_PWM))
    (pad 10 thru_hole oval (at 8.89 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 24 MYSX_D14_CS))
    (pad 11 thru_hole oval (at 11.43 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 39 FLASH_CSN))
    (pad 12 thru_hole oval (at 13.97 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 48 RF24_CE))
    (pad 13 thru_hole oval (at 13.97 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(JP9-Pad2)"))
    (pad 14 thru_hole oval (at 11.43 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 27 /MOSI))
    (pad 15 thru_hole oval (at 8.89 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 26 /MISO))
    (pad 16 thru_hole oval (at 6.35 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 25 /SCK))
    (pad 17 thru_hole oval (at 3.81 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 VBAT_SMPL))
    (pad 18 thru_hole oval (at 1.27 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 MYSX_D9_A3))
    (pad 19 thru_hole oval (at -1.27 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 13 MYSX_D10_A4))
    (pad 20 thru_hole oval (at -3.81 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 40 ATSHA_SDA))
    (pad 21 thru_hole oval (at -6.35 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (pad 22 thru_hole oval (at -8.89 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 37 RESET))
    (pad 23 thru_hole oval (at -11.43 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 24 thru_hole oval (at -13.97 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 25 thru_hole oval (at -2.54 -5.08 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 28 MYSX_D8_SDA))
    (pad 26 thru_hole oval (at -5.08 -5.08 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 29 MYSX_D7_SCL))
    (pad 27 thru_hole oval (at 13.97 -5.08 90) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 35 MYSX_A1))
    (pad 28 thru_hole oval (at 13.97 -2.54 90) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 36 MYSX_A2))
    (pad 29 thru_hole oval (at 13.97 0 90) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz -0.15 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.55 0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0 0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.25 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model mysensors.3dshapes/arduino_pro_mini.wrl
      (at (xyz -0.05 0 0.48))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model SMD_Packages.3dshapes/TQFP-32.wrl
      (at (xyz 0.05 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 315))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.3 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 0.3 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0.55 0.1 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0.25 0.2 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz -0.15 0.2 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (at (xyz -0.3 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (at (xyz 0.55 -0.175 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x06.wrl
      (at (xyz -0.65 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz -0.3 -0.05 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0.55 -0.125 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz -0.3 0.05 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (at (xyz -0.35 0.15 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (at (xyz -0.35 -0.15 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz -0.4 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz -0.5 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_DFN_QFN:DFN-6-1EP_3x3mm_Pitch0.95mm (layer F.Cu) (tedit 55E36954)
    (at 99.861 62.5656 90)
    (descr "DFN6 3*3 MM, 0.95 PITCH; CASE 506AH-01 (see ON Semiconductor 506AH.PDF)")
    (tags "DFN 0.95")
    (clearance 0.1)
    (attr smd)
    (fp_text reference U8 (at 0 -2.575 180) (layer F.SilkS))
    (fp_text value Si7021 (at 0 2.575 90) (layer F.Fab))
    (pad 1 smd rect (at -1.34 -0.95 90) (size 0.63 0.45) (layers F.Cu F.Paste F.Mask)
      (net 28 MYSX_D8_SDA))
    (pad 2 smd rect (at -1.34 0 90) (size 0.63 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.34 0.95 90) (size 0.63 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.34 0.95 90) (size 0.63 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at 1.34 0 90) (size 0.63 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 6 smd rect (at 1.34 -0.95 90) (size 0.63 0.45) (layers F.Cu F.Paste F.Mask)
      (net 29 MYSX_D7_SCL))
    (pad 7 smd rect (at 0.425 0.65 90) (size 0.85 1.3) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at 0.425 -0.65 90) (size 0.85 1.3) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at -0.425 0.65 90) (size 0.85 1.3) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at -0.425 -0.65 90) (size 0.85 1.3) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_3x3mm_Pitch0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SC-70-6 (layer B.Cu) (tedit 55E61881)
    (at 150.803 145.5796 90)
    (descr SC-70-6,)
    (tags SC-70-6,)
    (attr smd)
    (fp_text reference U9 (at 0.01016 3.05054 90) (layer B.SilkS))
    (fp_text value TPS61221 (at 0.04064 -4.191 90) (layer B.Fab))
    (pad 1 smd rect (at -0.65024 -0.94996 90) (size 0.39878 0.7493) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0 -0.94996 90) (size 0.39878 0.7493) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 3 smd rect (at 0.65024 -0.94996 90) (size 0.39878 0.7493) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65024 0.94996 90) (size 0.39878 0.7493) (layers B.Cu B.Paste B.Mask)
      (net 4 +3V3))
    (pad 5 smd rect (at 0 0.94996 90) (size 0.39878 0.7493) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(L1-Pad1)"))
    (pad 6 smd rect (at -0.65024 0.94996 90) (size 0.39878 0.7493) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(JP6-Pad2)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:CR123_holder (layer F.Cu) (tedit 55F2FFA5)
    (at 97.971 67.8206)
    (descr "CR123 battery holder")
    (tags "Battery holder, CR123")
    (fp_text reference BT4 (at 0 -3.5) (layer F.SilkS))
    (fp_text value CR123 (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(BT1-Pad3)"))
    (pad 2 thru_hole circle (at 0 37.82) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad "" np_thru_hole circle (at 8.1 0) (size 1.98 1.98) (drill 1.98) (layers *.Cu Dwgs.User))
    (model mysensors.3dshapes/cr123_holder.wrl
      (at (xyz 0 -0.746 0.28))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 -1.49 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "MYSX +3.3VP control bypass" (at 127.435 85.0006) (layer F.SilkS))
  (gr_text "MYSX 1.5" (at 109.02 55.5366) (layer F.SilkS))
  (gr_text "Low-power Vbat sample enable" (at 128.451 72.3006) (layer F.SilkS))
  (gr_text "SPI SS (1-2: RF24, 2-3: RF69)" (at 128.705 74.8406) (layer F.SilkS))
  (gr_text "INT0 source (1-2: MYSX, 2-3: RF)" (at 129.467 77.3806) (layer F.SilkS))
  (gr_text "MYSX Vraw measurement tap" (at 127.435 79.9206) (layer F.SilkS))
  (gr_text "3.3V regulator bypass enable" (at 127.689 82.4606) (layer F.SilkS))
  (gr_text "Vbat sample bypass" (at 124.895 87.5406) (layer F.SilkS))
  (gr_text "3.3V regulator bypass" (at 125.403 90.0806) (layer F.SilkS))
  (gr_text "3.3V regulator (1-2: step-up, 2-3: LDO)" (at 131.499 92.6206) (layer F.SilkS))
  (gr_text "Vbat measurement tap" (at 125.657 95.4146) (layer F.SilkS))
  (gr_arc (start 90.779197 54.985253) (end 87.779197 54.985253) (angle 89.9) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 160.779197 54.985253) (end 160.779197 51.985253) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 160.779197 144.985253) (end 163.779197 144.985253) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 90.779197 144.985253) (end 90.779197 147.985253) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 76 (width 0.3) (layer Dwgs.User)
    (gr_text "76.000 mm" (at 125.811 50.9806) (layer Dwgs.User))
    (feature1 (pts (xy 163.811 51.9806) (xy 163.811 50.9806)))
    (feature2 (pts (xy 87.811 51.9806) (xy 87.811 50.9806)))
    (crossbar (pts (xy 87.811 50.9806) (xy 163.811 50.9806)))
    (arrow1a (pts (xy 163.811 50.9806) (xy 162.684496 51.567021)))
    (arrow1b (pts (xy 163.811 50.9806) (xy 162.684496 50.394179)))
    (arrow2a (pts (xy 87.811 50.9806) (xy 88.937504 51.567021)))
    (arrow2b (pts (xy 87.811 50.9806) (xy 88.937504 50.394179)))
  )
  (dimension 96 (width 0.3) (layer Dwgs.User)
    (gr_text "96.000 mm" (at 86.811 99.9806 270) (layer Dwgs.User))
    (feature1 (pts (xy 87.811 147.9806) (xy 86.811 147.9806)))
    (feature2 (pts (xy 87.811 51.9806) (xy 86.811 51.9806)))
    (crossbar (pts (xy 86.811 51.9806) (xy 86.811 147.9806)))
    (arrow1a (pts (xy 86.811 147.9806) (xy 86.224579 146.854096)))
    (arrow1b (pts (xy 86.811 147.9806) (xy 87.397421 146.854096)))
    (arrow2a (pts (xy 86.811 51.9806) (xy 86.224579 53.107104)))
    (arrow2b (pts (xy 86.811 51.9806) (xy 87.397421 53.107104)))
  )
  (gr_line (start 87.779197 54.985253) (end 87.779197 144.985253) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 163.779197 54.985253) (end 163.779197 144.985253) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.779197 51.985253) (end 160.779197 51.985253) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 90.779197 147.985253) (end 160.779197 147.985253) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "MySensorsNode\nRev. 1.1\nLicensed under CERN OHL v.1.2" (at 90.097 145.7066) (layer F.SilkS))
  (gr_text PF (at 102.299 144.6566) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.508)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 163.779197 147.985853) (xy 87.779197 147.985853) (xy 87.779197 51.985853) (xy 163.779197 51.985853) (xy 163.779197 147.985853)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.508)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 87.779197 147.985853) (xy 87.779197 51.985853) (xy 163.779197 51.985853) (xy 163.779197 147.985853)
      )
    )
  )
)
