(kicad_pcb (version 4) (host pcbnew 0.201509101502+6177~30~ubuntu14.04.1-product)
  (general
    (links 181)
    (no_connects 0)
    (area 128.621001 70.8806 190.768246 125.35946)
    (thickness 1.2)
    (drawings 21)
    (tracks 1399)
    (zones 0)
    (modules 61)
    (nets 49)
  )
  (page A4)
  (title_block
    (title "Mysensors Node")
    (date "Wed 10 Jun 2015")
    (rev 1.1)
    (company "Designer: Patrick Fallberg")
    (comment 1 "Copyright (c) 2015 Patrick Fallberg")
    (comment 2 "Licensed under CERN OHL v.1.2")
  )
  (layers
    (0 F.Cu jumper)
    (31 B.Cu mixed)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.381)
    (trace_clearance 0.2032)
    (zone_clearance 0.254)
    (zone_45_only yes)
    (trace_min 0.381)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.635)
    (via_drill 0.381)
    (via_min_size 0.635)
    (via_min_drill 0.381)
    (uvia_size 25.4)
    (uvia_drill 0)
    (uvias_allowed no)
    (uvia_min_size 25.4)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.16)
    (pad_size 1.7272 1.7272)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 136.271 73.3806)
    (grid_origin 136.271 73.3806)
    (visible_elements 7FFEEE7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Manufacturing/))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 +BATT)
  (net 4 +3.3VP)
  (net 5 "Net-(C5-Pad1)")
  (net 6 RESET)
  (net 7 FLASH_CSN)
  (net 8 /MOSI)
  (net 9 /MISO)
  (net 10 /SCK)
  (net 11 VBAT_SMPL)
  (net 12 RF_INT)
  (net 13 "Net-(L1-Pad1)")
  (net 14 RF24_CE)
  (net 15 RF24_CSN)
  (net 16 RF69_NSS)
  (net 17 "Net-(ANT1-Pad1)")
  (net 18 "Net-(JP6-Pad2)")
  (net 19 "Net-(BT1-Pad3)")
  (net 20 "Net-(C4-Pad1)")
  (net 21 "Net-(C9-Pad1)")
  (net 22 "Net-(C9-Pad2)")
  (net 23 "Net-(JP4-Pad2)")
  (net 24 MYSX_D10_A4)
  (net 25 "Net-(JP7-Pad1)")
  (net 26 MYSX_D3_INT)
  (net 27 "Net-(JP8-Pad2)")
  (net 28 "Net-(JP9-Pad2)")
  (net 29 MYSX_D9_A3)
  (net 30 MYSX_D14_CS)
  (net 31 MYSX_D8_SDA)
  (net 32 MYSX_D7_SCL)
  (net 33 MYSX_D6_PWM)
  (net 34 MYSX_D5_PWM)
  (net 35 MYSX_D4_INT)
  (net 36 MYSX_D1_DFM)
  (net 37 MYSX_D2_DTM)
  (net 38 MYSX_A1)
  (net 39 MYSX_A2)
  (net 40 MYSX_3.3V_EN)
  (net 41 ATSHA_SDA)
  (net 42 "Net-(U4-Pad1)")
  (net 43 "Net-(U4-Pad3)")
  (net 44 "Net-(U4-Pad4)")
  (net 45 "Net-(U4-Pad5)")
  (net 46 "Net-(U4-Pad6)")
  (net 47 "Net-(U4-Pad7)")
  (net 48 "Net-(U4-Pad16)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.381)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 25.4)
    (uvia_drill 0)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net ATSHA_SDA)
    (add_net FLASH_CSN)
    (add_net MYSX_3.3V_EN)
    (add_net MYSX_A1)
    (add_net MYSX_A2)
    (add_net MYSX_D10_A4)
    (add_net MYSX_D14_CS)
    (add_net MYSX_D1_DFM)
    (add_net MYSX_D2_DTM)
    (add_net MYSX_D3_INT)
    (add_net MYSX_D4_INT)
    (add_net MYSX_D5_PWM)
    (add_net MYSX_D6_PWM)
    (add_net MYSX_D7_SCL)
    (add_net MYSX_D8_SDA)
    (add_net MYSX_D9_A3)
    (add_net "Net-(ANT1-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(JP4-Pad2)")
    (add_net "Net-(JP6-Pad2)")
    (add_net "Net-(JP8-Pad2)")
    (add_net "Net-(JP9-Pad2)")
    (add_net "Net-(L1-Pad1)")
    (add_net "Net-(U4-Pad1)")
    (add_net "Net-(U4-Pad16)")
    (add_net "Net-(U4-Pad3)")
    (add_net "Net-(U4-Pad4)")
    (add_net "Net-(U4-Pad5)")
    (add_net "Net-(U4-Pad6)")
    (add_net "Net-(U4-Pad7)")
    (add_net RESET)
    (add_net RF24_CE)
    (add_net RF24_CSN)
    (add_net RF69_NSS)
    (add_net RF_INT)
    (add_net VBAT_SMPL)
  )
  (net_class Power ""
    (clearance 0.2032)
    (trace_width 0.635)
    (via_dia 0.635)
    (via_drill 0.381)
    (uvia_dia 25.4)
    (uvia_drill 0)
    (add_net +3.3VP)
    (add_net +3V3)
    (add_net +BATT)
    (add_net GND)
    (add_net "Net-(BT1-Pad3)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(JP7-Pad1)")
  )
  (module mysensors_obscurities:d-pak-kcswalter (layer B.Cu) (tedit 55DF9502)
    (at 177.292 105.2576 270)
    (descr D-pak)
    (fp_text reference U1 (at -3.937 0 360) (layer B.SilkS))
    (fp_text value LD1117DT33TR (at 0 -5.9944 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -2.30124 -3.1242 270) (size 1.6002 3.2004) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 2.30124 -3.1242 270) (size 1.6002 3.2004) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C4-Pad1)"))
    (pad 2 smd rect (at 0 3.1242 270) (size 6.49986 7.00024) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model mysensors.3dshapes/w.lain.3dshapes/smd_trans/d-pak.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_arduino:pro_mini (layer F.Cu) (tedit 55DF962E)
    (at 152.781 83.5406 180)
    (descr "IC, ARDUINO_PRO_MINI x 0,6\"")
    (tags "DIL ARDUINO PRO MINI")
    (fp_text reference U7 (at -18.542 8.636 180) (layer F.SilkS))
    (fp_text value ArduinoProMini (at 0 0 180) (layer F.Fab) hide)
    (pad 28 thru_hole oval (at 5.08 -5.08 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 39 MYSX_A2))
    (pad 27 thru_hole oval (at 7.62 -5.08 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 38 MYSX_A1))
    (pad 1 thru_hole oval (at -13.97 7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 36 MYSX_D1_DFM))
    (pad 2 thru_hole oval (at -11.43 7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 37 MYSX_D2_DTM))
    (pad 3 thru_hole oval (at -8.89 7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 RESET))
    (pad 4 thru_hole oval (at -6.35 7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at -3.81 7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(JP8-Pad2)"))
    (pad 6 thru_hole oval (at -1.27 7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 35 MYSX_D4_INT))
    (pad 7 thru_hole oval (at 1.27 7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 40 MYSX_3.3V_EN))
    (pad 8 thru_hole oval (at 3.81 7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 34 MYSX_D5_PWM))
    (pad 9 thru_hole oval (at 6.35 7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 33 MYSX_D6_PWM))
    (pad 10 thru_hole oval (at 8.89 7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 30 MYSX_D14_CS))
    (pad 11 thru_hole oval (at 11.43 7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 FLASH_CSN))
    (pad 12 thru_hole oval (at 13.97 7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 RF24_CE))
    (pad 13 thru_hole oval (at 13.97 -7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(JP9-Pad2)"))
    (pad 14 thru_hole oval (at 11.43 -7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 8 /MOSI))
    (pad 15 thru_hole oval (at 8.89 -7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 9 /MISO))
    (pad 16 thru_hole oval (at 6.35 -7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SCK))
    (pad 17 thru_hole oval (at 3.81 -7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 11 VBAT_SMPL))
    (pad 18 thru_hole oval (at 1.27 -7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 29 MYSX_D9_A3))
    (pad 19 thru_hole oval (at -1.27 -7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 24 MYSX_D10_A4))
    (pad 20 thru_hole oval (at -3.81 -7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 41 ATSHA_SDA))
    (pad 21 thru_hole oval (at -6.35 -7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 22 thru_hole oval (at -8.89 -7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 RESET))
    (pad 23 thru_hole oval (at -11.43 -7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 24 thru_hole oval (at -13.97 -7.62 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
    (pad 25 thru_hole oval (at -2.54 -5.08 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 31 MYSX_D8_SDA))
    (pad 26 thru_hole oval (at -5.08 -5.08 180) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 32 MYSX_D7_SCL))
    (pad 27 thru_hole oval (at 13.97 -5.08 180) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 38 MYSX_A1))
    (pad 28 thru_hole oval (at 13.97 -2.54 180) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 39 MYSX_A2))
    (pad 29 thru_hole oval (at 13.97 0 180) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz -0.15 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.55 0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0 0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.25 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model mysensors.3dshapes/arduino_pro_mini.wrl
      (at (xyz -0.05 0 0.48))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model SMD_Packages.3dshapes/TQFP-32.wrl
      (at (xyz 0.05 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 315))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.3 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 0.3 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0.55 0.1 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0.25 0.2 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz -0.15 0.2 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (at (xyz -0.3 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (at (xyz 0.55 -0.175 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x06.wrl
      (at (xyz -0.65 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz -0.3 -0.05 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0.55 -0.125 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz -0.3 0.05 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (at (xyz -0.35 0.15 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (at (xyz -0.35 -0.15 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz -0.4 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz -0.5 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_connectors:MYSX_1.5 (layer F.Cu) (tedit 55DF95CA)
    (at 183.515 99.0346 180)
    (descr "Through hole pin header")
    (tags "pin header MYSX 1.5")
    (fp_text reference P1 (at -1.905 0.508 180) (layer F.SilkS))
    (fp_text value MYSX_1.5 (at 1.27 26.162 180) (layer F.Fab))
    (fp_text user 1.5 (at 2.54 -3.302 180) (layer Cmts.User))
    (pad 20 thru_hole oval (at 2.54 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 MYSX_D14_CS))
    (pad 19 thru_hole oval (at 0 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SCK))
    (pad 18 thru_hole oval (at 2.54 20.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /MISO))
    (pad 17 thru_hole oval (at 0 20.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /MOSI))
    (pad 16 thru_hole oval (at 2.54 17.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 MYSX_D10_A4))
    (pad 15 thru_hole oval (at 0 17.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 MYSX_D9_A3))
    (pad 14 thru_hole oval (at 2.54 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 MYSX_D8_SDA))
    (pad 13 thru_hole oval (at 0 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 MYSX_D7_SCL))
    (pad 12 thru_hole oval (at 2.54 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 MYSX_D6_PWM))
    (pad 11 thru_hole oval (at 0 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 MYSX_D5_PWM))
    (pad 10 thru_hole oval (at 2.54 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 MYSX_D4_INT))
    (pad 9 thru_hole oval (at 0 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 MYSX_D3_INT))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(JP7-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3.3VP))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 MYSX_D1_DFM))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 MYSX_D2_DTM))
    (pad 7 thru_hole oval (at 0 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 MYSX_A1))
    (pad 8 thru_hole oval (at 2.54 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 MYSX_A2))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x10.wrl
      (at (xyz 0.05 -0.45 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Potentiometers:Potentiometer_Bourns_3296Y_3-8Zoll_Angular_ScrewUp (layer F.Cu) (tedit 55DF9425)
    (at 160.7566 98.9838 90)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference RV1 (at -0.8128 -8.6106 180) (layer F.SilkS))
    (fp_text value 1M (at 0 5.08 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 -2.54 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 VBAT_SMPL))
    (pad 3 thru_hole circle (at 0 -5.08 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(JP4-Pad2)"))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296Y_3-8Zoll_Angular_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 55DF9629)
    (at 172.085 80.3656)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP8 (at 0 -2.159) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 MYSX_D3_INT))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(JP8-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 RF_INT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Symbols:Symbol_OSHW-Logo_SilkScreen (layer F.Cu) (tedit 55DC501A)
    (at 149.733 114.0206)
    (descr "Symbol, OSHW-Logo, Silk Screen,")
    (tags "Symbol, OSHW-Logo, Silk Screen,")
    (fp_text reference OSHW_LOGO (at 0.09906 -4.38912) (layer F.SilkS) hide)
    (fp_text value Symbol_OSHW-Logo_SilkScreen (at 0.30988 6.56082) (layer F.Fab))
  )
  (module Housings_DFN_QFN:DFN-6-1EP_3x3mm_Pitch0.95mm (layer B.Cu) (tedit 55DF9949)
    (at 157.2895 83.9851)
    (descr "DFN6 3*3 MM, 0.95 PITCH; CASE 506AH-01 (see ON Semiconductor 506AH.PDF)")
    (tags "DFN 0.95")
    (clearance 0.1)
    (attr smd)
    (fp_text reference U8 (at -0.0635 -2.2225) (layer B.SilkS))
    (fp_text value Si7021 (at 0 -2.575) (layer B.Fab))
    (pad 1 smd rect (at -1.34 0.95) (size 0.63 0.45) (layers B.Cu B.Paste B.Mask)
      (net 31 MYSX_D8_SDA))
    (pad 2 smd rect (at -1.34 0) (size 0.63 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.34 -0.95) (size 0.63 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at 1.34 -0.95) (size 0.63 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.34 0) (size 0.63 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 6 smd rect (at 1.34 0.95) (size 0.63 0.45) (layers B.Cu B.Paste B.Mask)
      (net 32 MYSX_D7_SCL))
    (pad 7 smd rect (at 0.425 -0.65) (size 0.85 1.3) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at 0.425 0.65) (size 0.85 1.3) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at -0.425 -0.65) (size 0.85 1.3) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at -0.425 0.65) (size 0.85 1.3) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_3x3mm_Pitch0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 55DF995C)
    (at 144.653 84.3661)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U6 (at 0 -3.2385) (layer F.SilkS))
    (fp_text value AT25DF512C (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 FLASH_CSN))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /MISO))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /MOSI))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /SCK))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23_Handsoldering (layer F.Cu) (tedit 55DF9930)
    (at 158.115 82.67446)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U3 (at -1.524 -1.29286) (layer F.SilkS))
    (fp_text value ATSHA204A (at 0 3.81) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 41 ATSHA_SDA))
    (pad 2 smd rect (at 0.95 1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at 0 -1.50114) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_handsoldering:SOT-23-5_Handsoldering (layer F.Cu) (tedit 55DF9686)
    (at 179.1462 105.5116 180)
    (descr "5-pin SOT23 package handsoldering")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U2 (at 2.032 0 180) (layer F.SilkS))
    (fp_text value TPS61097A (at -0.05 2.35 180) (layer F.Fab))
    (pad 1 smd rect (at -1.47 -0.95 180) (size 1.80086 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at -1.47 0 180) (size 1.80086 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.47 0.95 180) (size 1.80086 0.65) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(JP6-Pad2)"))
    (pad 4 smd rect (at 1.47 0.95 180) (size 1.80086 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at 1.47 -0.95 180) (size 1.80086 0.65) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(L1-Pad1)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55DF993F)
    (at 158.496 86.2076)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at -3.048 0) (layer F.SilkS))
    (fp_text value 56K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 41 ATSHA_SDA))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55DF95B8)
    (at 175.1965 106.2736 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -2.794 0.0635 360) (layer F.SilkS))
    (fp_text value 56K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(JP9-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55DF9929)
    (at 152.4 82.9056 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at -2.794 0 360) (layer F.SilkS))
    (fp_text value 56K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 30 MYSX_D14_CS))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 55DF9971)
    (at 141.859 84.3026 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -2.921 0 360) (layer B.SilkS))
    (fp_text value 56K (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 FLASH_CSN))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55DF9912)
    (at 151.892 88.6206 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 1.524 180) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 MYSX_D8_SDA))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55DF9920)
    (at 163.449 86.8426)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 3.048 0) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 MYSX_D7_SCL))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55DF95F2)
    (at 168.91 88.8746 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -2.794 0 360) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 40 MYSX_3.3V_EN))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55DF9457)
    (at 163.195 106.4006)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -0.127 -1.524) (layer F.SilkS))
    (fp_text value 10K (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C9-Pad2)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 55DF9645)
    (at 182.753 106.172 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 2.794 0.127 180) (layer F.SilkS))
    (fp_text value 150K (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(JP6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23_Handsoldering (layer F.Cu) (tedit 55DF95ED)
    (at 172.466 88.4936 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -1.143 -1.524 360) (layer F.SilkS))
    (fp_text value DMP3056L-7 (at 0 3.81 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 40 MYSX_3.3V_EN))
    (pad 2 smd rect (at 0.95 1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at 0 -1.50114 270) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 +3.3VP))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SOT-23_Handsoldering (layer B.Cu) (tedit 55DF94F6)
    (at 161.671 102.9716 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -2.159 0 360) (layer B.SilkS))
    (fp_text value DMP3056L-7 (at 0 -3.81 270) (layer B.Fab))
    (pad 1 smd rect (at -0.95 -1.50114 270) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(C9-Pad2)"))
    (pad 2 smd rect (at 0.95 -1.50114 270) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 3 +BATT))
    (pad 3 smd rect (at 0 1.50114 270) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(JP4-Pad2)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 55DF959A)
    (at 161.671 116.5606)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -2.159 5.969) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 55DF9461)
    (at 161.671 108.9406)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -1.27 -2.159) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3.3VP))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3.3VP))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3.3VP))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 55DF95DB)
    (at 169.926 94.3356 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -2.159 -1.27 360) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /MISO))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 55DF9661)
    (at 179.07 107.9246)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference L1 (at 2.667 0) (layer F.SilkS))
    (fp_text value 4.7uH (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(L1-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 55DF943C)
    (at 156.591 93.7006 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP10 (at 0.508 -3.175 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 MYSX_D9_A3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(C9-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 55DF9414)
    (at 138.811 95.2246)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP9 (at 0 -2.159) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 RF24_CSN))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(JP9-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 RF69_NSS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 55DF95D2)
    (at 176.911 98.7806 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP7 (at -1.905 1.27 360) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(JP7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +BATT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 55DF9626)
    (at 176.53 81.0006)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP6 (at 0 -2.159) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 MYSX_D10_A4))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(JP6-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 55DF95E3)
    (at 176.911 92.5576 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP5 (at -1.905 1.27 360) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3.3VP))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 55DF94B9)
    (at 165.481 103.8606 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP4 (at 0.254 4.445 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +BATT))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(JP4-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 55DF944F)
    (at 168.021 100.0506 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP3 (at -0.762 5.08 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +BATT))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 55DF9588)
    (at 175.641 109.8296 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP2 (at 0.381 7.62 180) (layer F.SilkS))
    (fp_text value JUMPER3 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +BATT))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(C4-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 55DF94C6)
    (at 168.021 106.4006 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at -2.413 1.27 180) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(BT1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +BATT))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 55DF9936)
    (at 162.274 84.1756)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C18 (at 4.35 0) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -2.3) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55DF9919)
    (at 161.925 89.0016)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C17 (at 4.318 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 55DF996B)
    (at 147.447 83.5406 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C16 (at 3.683 -0.635 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -2.3 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 55DF9A12)
    (at 153.67 96.3676 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C15 (at -3.556 0 360) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -2.3 270) (layer B.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_HandSoldering (layer B.Cu) (tedit 55E615CB)
    (at 151.638 101.5492)
    (descr "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (tags "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (attr smd)
    (fp_text reference C14 (at -5.461 0.0254) (layer B.SilkS))
    (fp_text value 4.7uF (at -0.09906 -3.59918) (layer B.Fab))
    (fp_text user + (at -4.70154 2.4003) (layer B.SilkS) hide)
    (pad 2 smd rect (at 2.12598 0) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.12598 0) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_HandSoldering (layer B.Cu) (tedit 55E61631)
    (at 175.133 89.3826 180)
    (descr "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (tags "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (attr smd)
    (fp_text reference C13 (at -2.794 2.54 180) (layer B.SilkS))
    (fp_text value 4.7uF (at -0.09906 -3.59918 180) (layer B.Fab))
    (fp_text user + (at -4.70154 2.4003 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at 2.12598 0 180) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.12598 0 180) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_HandSoldering (layer B.Cu) (tedit 55E6162D)
    (at 175.514 95.7326 180)
    (descr "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (tags "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (attr smd)
    (fp_text reference C12 (at -3.556 1.651 180) (layer B.SilkS))
    (fp_text value 4.7uF (at -0.09906 -3.59918 180) (layer B.Fab))
    (fp_text user + (at -4.70154 2.4003 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at 2.12598 0 180) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.12598 0 180) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 4 +3.3VP))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer B.Cu) (tedit 55DF93ED)
    (at 144.145 117.0686 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C11 (at -4.445 0 180) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -2.3 180) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_HandSoldering (layer B.Cu) (tedit 55DF93E7)
    (at 145.161 120.1166)
    (descr "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (tags "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (attr smd)
    (fp_text reference C10 (at 5.08 0) (layer B.SilkS))
    (fp_text value 4.7uF (at -0.09906 -3.59918) (layer B.Fab))
    (fp_text user + (at -4.70154 2.4003) (layer B.SilkS))
    (pad 2 smd rect (at 2.12598 0) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.12598 0) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55DF942A)
    (at 160.401 97.0026)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C9 (at -4.064 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C9-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_Universal:Resistor_SMD+THTuniversal_0805to1206_RM10_HandSoldering (layer F.Cu) (tedit 55DF9958)
    (at 144.018 78.9686 180)
    (descr "Resistor, SMD and THT, universal, 0805 to 1206,RM10,  Hand soldering,")
    (tags "Resistor, SMD and THT, universal, 0805 to 1206, RM10, Hand soldering,")
    (fp_text reference C8 (at -6.985 0 180) (layer F.SilkS))
    (fp_text value C (at -0.39878 4.20116 180) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.413 0 180) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 11 VBAT_SMPL))
    (pad 2 smd trapezoid (at 2.413 0) (size 3.50012 1.99898) (rect_delta 0.39878 0 ) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at -5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 11 VBAT_SMPL))
    (pad 2 thru_hole rect (at 5.00126 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55DF9924)
    (at 162.941 83.9216)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C7 (at 4.064 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55DF95C0)
    (at 178.943 102.7176)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C6 (at 0 -1.651) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 55DF964F)
    (at 185.039 104.8766 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at -3.683 -0.127 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeA_EIA-3216_HandSoldering (layer B.Cu) (tedit 55DF98AD)
    (at 184.404 105.5116 90)
    (descr "Tantal Cap. , Size A, EIA-3216, Hand Soldering,")
    (tags "Tantal Cap. , Size A, EIA-3216, Hand Soldering,")
    (attr smd)
    (fp_text reference C4 (at -4.826 0 180) (layer B.SilkS))
    (fp_text value 10uF (at -0.09906 -3.0988 90) (layer B.Fab))
    (fp_text user + (at -4.572 -1.2192 90) (layer B.SilkS))
    (pad 2 smd rect (at 1.99898 0 90) (size 2.99974 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.99898 0 90) (size 2.99974 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(C4-Pad1)"))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeA_EIA-3216_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeA_EIA-3216_HandSoldering (layer B.Cu) (tedit 55E615DB)
    (at 182.372 100.9396)
    (descr "Tantal Cap. , Size A, EIA-3216, Hand Soldering,")
    (tags "Tantal Cap. , Size A, EIA-3216, Hand Soldering,")
    (attr smd)
    (fp_text reference C3 (at -3.175 -1.778) (layer B.SilkS))
    (fp_text value 10uF (at -0.09906 -3.0988) (layer B.Fab))
    (fp_text user + (at -4.59994 1.80086) (layer B.SilkS) hide)
    (pad 2 smd rect (at 1.99898 0) (size 2.99974 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.99898 0) (size 2.99974 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeA_EIA-3216_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeB_EIA-3528_HandSoldering (layer B.Cu) (tedit 55E615B2)
    (at 167.894 112.4966 180)
    (descr "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (tags "Tantal Cap. , Size B, EIA-3528, Hand Soldering,")
    (attr smd)
    (fp_text reference C2 (at -3.302 2.54 180) (layer B.SilkS))
    (fp_text value 4.7uF (at -0.09906 -3.59918 180) (layer B.Fab))
    (fp_text user + (at -4.70154 2.4003 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at 2.12598 0 180) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.12598 0 180) (size 3.1496 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(BT1-Pad3)"))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeC_EIA-6032_HandSoldering (layer B.Cu) (tedit 55E615C1)
    (at 168.529 118.4656 180)
    (descr "Tantal Cap. , Size C, EIA-6032, Hand Soldering,")
    (tags "Tantal Cap. , Size C, EIA-6032, Hand Soldering,")
    (attr smd)
    (fp_text reference C1 (at -3.937 2.286 180) (layer B.SilkS))
    (fp_text value 47uF (at -0.09906 -3.59918 180) (layer B.Fab))
    (fp_text user + (at -5.75056 2.286 180) (layer B.SilkS) hide)
    (pad 2 smd rect (at 2.99974 0 180) (size 3.50012 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.99974 0 180) (size 3.50012 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(BT1-Pad3)"))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeC_EIA-6032_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module mysensors_connectors:TerminalBlock2.54mmx2-kcswalter (layer F.Cu) (tedit 55DF9584)
    (at 182.753 114.0206 90)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference BT3 (at 3.429 0.508 180) (layer F.SilkS))
    (fp_text value Generic (at 0 4.50088 90) (layer F.SilkS) hide)
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 1 thru_hole rect (at 1.27 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(BT1-Pad3)"))
    (model mysensors.3dshapes/w.lain.3dshapes/conn_mpt/mpt_0,5-2-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:s2b-ph-kl-kcswalter (layer F.Cu) (tedit 55DF9996)
    (at 176.2125 116.1161)
    (descr "JST PH series connector, S2B-PH-KL")
    (fp_text reference BT2 (at -0.0635 -1.7145) (layer F.SilkS))
    (fp_text value JST (at 0 7.80034) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.00076 0) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(BT1-Pad3)"))
    (pad 2 thru_hole oval (at 1.00076 0) (size 1.19888 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model mysensors.3dshapes/w.lain.3dshapes/conn_jst-ph/s2b-ph-kl.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:dc_socket-kcswalter (layer F.Cu) (tedit 55DF999A)
    (at 167.9575 115.7351)
    (descr "Socket, DC power supply")
    (fp_text reference BT1 (at -2.7305 -8.0645) (layer F.SilkS))
    (fp_text value "2.5mm jack" (at 0 -8.60044) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 5.30098 -3.50012) (size 1.99898 4.0005) (drill oval 1.00076 2.99974) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 -0.24892) (size 4.0005 1.99898) (drill oval 2.99974 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 -6.25094) (size 4.50088 1.99898) (drill oval 3.50012 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(BT1-Pad3)"))
    (model mysensors.3dshapes/w.lain.3dshapes/conn_misc/dc_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_1-2mmDrill (layer F.Cu) (tedit 55DF93DC)
    (at 154.686 120.1166)
    (fp_text reference ANT1 (at 3.556 0) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -1.905 3.175) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.50012 3.50012) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(ANT1-Pad1)"))
  )
  (module w_logo:Logo_silk_polarity_center_5x1.4mm (layer F.Cu) (tedit 0)
    (at 171.958 107.4166)
    (descr "Polarity logo, positive center, 5x1.4mm")
    (fp_text reference PLUG_SPEC (at -0.9 0.6) (layer F.SilkS) hide)
    (fp_text value LOGO (at 1 0.6) (layer F.SilkS) hide)
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 55DF152F)
    (at 182.275 119.38)
    (descr "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3mm, No Annular, Kein Restring,")
    (fp_text reference HOLE1 (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 1.00076 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers))
  )
  (module mysensors_radios:NRF24L01 (layer F.Cu) (tedit 5587F36C)
    (at 153.035 93.7006)
    (descr NRF24L01)
    (tags "nRF 24 NRF24L01 NRF24L01+")
    (fp_text reference U5 (at -5.334 -0.381) (layer F.SilkS))
    (fp_text value NRF24L01 (at -8.382 7.112) (layer F.Fab) hide)
    (pad 7 thru_hole oval (at -9.144 1.524) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /MISO))
    (pad 8 thru_hole oval (at -9.144 4.064) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 RF_INT))
    (pad 5 thru_hole oval (at -6.604 1.524) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SCK))
    (pad 6 thru_hole oval (at -6.604 4.064) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /MOSI))
    (pad 3 thru_hole oval (at -4.064 1.524) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 RF24_CE))
    (pad 4 thru_hole oval (at -4.064 4.064) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 RF24_CSN))
    (pad 1 thru_hole rect (at -1.524 1.524) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at -1.524 4.064) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0.442))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model mysensors.3dshapes/nrf24l01.wrl
      (at (xyz -0.3 -0.5669999999999999 0.475))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz -0.22 -0.51 0.509))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_hc-49s.wrl
      (at (xyz -0.5 -0.475 0.51))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_radios:RFM69HW_SMD_ThroughHole_Handsoldering (layer F.Cu) (tedit 55DEED2C)
    (at 139.827 104.1146)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U4 (at 0 -1.651) (layer F.SilkS))
    (fp_text value RFM69HW (at 8.382 7.112) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U4-Pad1)"))
    (pad 2 smd rect (at -1.4 2) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 RF_INT))
    (pad 3 smd rect (at -1.4 4) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U4-Pad3)"))
    (pad 4 smd rect (at -1.4 6) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U4-Pad4)"))
    (pad 5 smd rect (at -1.4 8) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(U4-Pad5)"))
    (pad 6 smd rect (at -1.4 10) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(U4-Pad6)"))
    (pad 7 smd rect (at -1.4 12) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(U4-Pad7)"))
    (pad 8 smd rect (at -1.4 14) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 9 smd rect (at 18.3 14) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 18.3 12) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(ANT1-Pad1)"))
    (pad 11 smd rect (at 18.3 10) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 18.3 8) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 /SCK))
    (pad 13 smd rect (at 18.3 6) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 /MISO))
    (pad 14 smd rect (at 18.3 4) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 /MOSI))
    (pad 15 smd rect (at 18.3 2) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 RF69_NSS))
    (pad 16 smd rect (at 18.3 0) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(U4-Pad16)"))
    (pad 1 thru_hole rect (at -0.1 0) (size 2 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(U4-Pad1)"))
    (pad 2 thru_hole circle (at -0.1 2) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 RF_INT))
    (pad 3 thru_hole circle (at -0.1 4) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U4-Pad3)"))
    (pad 4 thru_hole circle (at -0.1 6) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(U4-Pad4)"))
    (pad 5 thru_hole circle (at -0.1 8) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(U4-Pad5)"))
    (pad 6 thru_hole circle (at -0.1 10) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(U4-Pad6)"))
    (pad 7 thru_hole circle (at -0.1 12) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(U4-Pad7)"))
    (pad 8 thru_hole circle (at -0.1 14) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 9 thru_hole circle (at 17 14) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole circle (at 17 12) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(ANT1-Pad1)"))
    (pad 11 thru_hole circle (at 17 10) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole circle (at 17 8) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /SCK))
    (pad 13 thru_hole circle (at 17 6) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /MISO))
    (pad 14 thru_hole circle (at 17 4) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /MOSI))
    (pad 15 thru_hole circle (at 17 2) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 RF69_NSS))
    (pad 16 thru_hole circle (at 17 0) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(U4-Pad16)"))
    (model mysensors.3dshapes/rfm69hw.wrl
      (at (xyz 0.333 -0.275 0.345))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals_Oscillators_SMD.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0.332 -0.08 0.375))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_strip_2mm_8.wrl
      (at (xyz -0.004 -0.276 0.31))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_strip_2mm_8.wrl
      (at (xyz 0.669 -0.276 0.31))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_socket_2mm_8.wrl
      (at (xyz -0.004 -0.276 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_socket_2mm_8.wrl
      (at (xyz 0.669 -0.276 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.205 -0.445 0.375))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOT-23_SOT-143_TSOT-6:SC-70-6 (layer B.Cu) (tedit 55E5EB0C)
    (at 181.483 105.4354 270)
    (descr SC-70-6,)
    (tags SC-70-6,)
    (attr smd)
    (fp_text reference U9 (at -1.9558 -0.889 360) (layer B.SilkS))
    (fp_text value TPS61221 (at 0.04064 -4.191 270) (layer B.Fab))
    (pad 1 smd rect (at -0.65024 -0.94996 270) (size 0.39878 0.7493) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0 -0.94996 270) (size 0.39878 0.7493) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at 0.65024 -0.94996 270) (size 0.39878 0.7493) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 0.65024 0.94996 270) (size 0.39878 0.7493) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at 0 0.94996 270) (size 0.39878 0.7493) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(L1-Pad1)"))
    (pad 6 smd rect (at -0.65024 0.94996 270) (size 0.39878 0.7493) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(JP6-Pad2)"))
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "MYSX 1.5" (at 181.864 74.2696) (layer F.SilkS))
  (gr_arc (start 183.271 120.3806) (end 186.271 120.3806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139.271 120.3806) (end 139.271 123.3806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 183.271 76.3806) (end 183.271 73.3806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139.271 76.3806) (end 136.271 76.3806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 50 (width 0.3) (layer Dwgs.User)
    (gr_text "50.000 mm" (at 135.271 98.3806 270) (layer Dwgs.User))
    (feature1 (pts (xy 136.271 123.3806) (xy 135.271 123.3806)))
    (feature2 (pts (xy 136.271 73.3806) (xy 135.271 73.3806)))
    (crossbar (pts (xy 135.271 73.3806) (xy 135.271 123.3806)))
    (arrow1a (pts (xy 135.271 123.3806) (xy 134.684579 122.254096)))
    (arrow1b (pts (xy 135.271 123.3806) (xy 135.857421 122.254096)))
    (arrow2a (pts (xy 135.271 73.3806) (xy 134.684579 74.507104)))
    (arrow2b (pts (xy 135.271 73.3806) (xy 135.857421 74.507104)))
  )
  (dimension 50 (width 0.3) (layer Dwgs.User)
    (gr_text "50.000 mm" (at 161.271 72.3806) (layer Dwgs.User))
    (feature1 (pts (xy 186.271 73.3806) (xy 186.271 72.3806)))
    (feature2 (pts (xy 136.271 73.3806) (xy 136.271 72.3806)))
    (crossbar (pts (xy 136.271 72.3806) (xy 186.271 72.3806)))
    (arrow1a (pts (xy 186.271 72.3806) (xy 185.144496 72.967021)))
    (arrow1b (pts (xy 186.271 72.3806) (xy 185.144496 71.794179)))
    (arrow2a (pts (xy 136.271 72.3806) (xy 137.397504 72.967021)))
    (arrow2b (pts (xy 136.271 72.3806) (xy 137.397504 71.794179)))
  )
  (gr_text "MySensorsNode\nRev. 1.1\nLicensed under CERN OHL v.1.2" (at 137.541 121.0056) (layer F.SilkS))
  (gr_text PF (at 149.654 120.1486) (layer F.SilkS))
  (gr_line (start 136.275 120.38) (end 136.275 76.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.275 123.38) (end 139.275 123.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.275 76.38) (end 186.275 120.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.275 73.38) (end 183.275 73.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.508)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 186.271 123.3806) (xy 136.271 123.3806) (xy 136.271 73.3806) (xy 158.496 73.3806) (xy 186.271 73.3806)
        (xy 186.271 123.3806)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.508)
    (fill yes (mode segment) (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.635))
    (polygon
      (pts
        (xy 186.271 123.3806) (xy 136.271 123.3806) (xy 136.271 73.3806) (xy 186.271 73.3806)
      )
    )
  )
)
