(kicad_pcb (version 4) (host pcbnew 4.0.0-rc2-stable)
  (general
    (links 34)
    (no_connects 0)
    (area 104.541668 113.885 170.201001 141.900001)
    (thickness 1.6)
    (drawings 44)
    (tracks 164)
    (zones 0)
    (modules 15)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.15)
    (pcb_text_size 0.7 0.7)
    (mod_edge_width 0.15)
    (mod_text_size 0.7 0.7)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 /RESET)
  (net 4 /DTR)
  (net 5 "Net-(C3-Pad1)")
  (net 6 /RX)
  (net 7 /TX)
  (net 8 "Net-(IC1-Pad4)")
  (net 9 "Net-(IC1-Pad5)")
  (net 10 "Net-(IC1-Pad6)")
  (net 11 "Net-(IC1-Pad9)")
  (net 12 "Net-(IC1-Pad10)")
  (net 13 "Net-(IC1-Pad11)")
  (net 14 "Net-(IC1-Pad12)")
  (net 15 "Net-(IC1-Pad13)")
  (net 16 "Net-(IC1-Pad14)")
  (net 17 /D9/CE)
  (net 18 /D10/SS)
  (net 19 /D11/MOSI)
  (net 20 /D12/MISO)
  (net 21 /D13/SCK)
  (net 22 "Net-(IC1-Pad23)")
  (net 23 "Net-(IC1-Pad24)")
  (net 24 "Net-(IC1-Pad25)")
  (net 25 "Net-(IC1-Pad26)")
  (net 26 "Net-(IC1-Pad27)")
  (net 27 "Net-(IC1-Pad28)")
  (net 28 "Net-(P4-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /D10/SS)
    (add_net /D11/MOSI)
    (add_net /D12/MISO)
    (add_net /D13/SCK)
    (add_net /D9/CE)
    (add_net /DTR)
    (add_net /RESET)
    (add_net /RX)
    (add_net /TX)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(P4-Pad8)")
  )
  (net_class PWR_1 ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class PWR_2 ""
    (clearance 0.2)
    (trace_width 0.7)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 56632AFE)
    (at 163.83 130.81 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 2.49 1.33 360) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 56632AA5)
    (at 161.29 118.11)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0.01 -2.51) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /D9/CE))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D10/SS))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D13/SCK))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D11/MOSI))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D12/MISO))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P4-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 56632B7F)
    (at 168.91 118.11 270)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C4 (at -2.31 0.11 360) (layer F.SilkS) hide)
    (fp_text value "" (at 1.25 3.8 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 56632AC4)
    (at 168.91 128.27 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1 180) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D12/MISO))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D13/SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D11/MOSI))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistor_Horizontal_RM5mm (layer F.Cu) (tedit 564CEB49)
    (at 129.286 124.46)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R1 (at 0 0) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.302 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 3.302 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 /RESET))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 56632B7A)
    (at 166.37 118.11 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C5 (at -2.21 0.07 360) (layer F.SilkS) hide)
    (fp_text value "" (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 56632A88)
    (at 123.19 130.81 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P12 (at -2.79 5.51 180) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_DIP:DIP-28_W7.62mm (layer F.Cu) (tedit 56632A06)
    (at 124.46 128.27 90)
    (descr "28-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference IC1 (at 5.77 -0.46 180) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -3.72 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 /RESET))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /RX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /TX))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(IC1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(IC1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(IC1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(IC1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(IC1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(IC1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(IC1-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(IC1-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(IC1-Pad14)"))
    (pad 15 thru_hole oval (at 7.62 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 /D9/CE))
    (pad 16 thru_hole oval (at 7.62 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D10/SS))
    (pad 17 thru_hole oval (at 7.62 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D11/MOSI))
    (pad 18 thru_hole oval (at 7.62 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D12/MISO))
    (pad 19 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D13/SCK))
    (pad 20 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 21 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad1)"))
    (pad 22 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 23 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(IC1-Pad23)"))
    (pad 24 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(IC1-Pad24)"))
    (pad 25 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(IC1-Pad25)"))
    (pad 26 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(IC1-Pad26)"))
    (pad 27 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(IC1-Pad27)"))
    (pad 28 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(IC1-Pad28)"))
    (model Housings_DIP.3dshapes/DIP-28_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 56632A74)
    (at 123.19 118.11 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P11 (at 2.51 5.51 180) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 56632A40)
    (at 120.65 118.11)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0.05 -2.41) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /RX))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /TX))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /DTR))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2_P5 (layer F.Cu) (tedit 564CEBFB)
    (at 151.13 124.46)
    (descr "Film Capacitor Length 7 x Width 2mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 2.54 0) (layer F.SilkS))
    (fp_text value "" (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W2_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2_P5 (layer F.Cu) (tedit 564CEBEE)
    (at 143.51 124.46)
    (descr "Film Capacitor Length 7 x Width 2mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 2.54 0) (layer F.SilkS))
    (fp_text value "" (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W2_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2_P5 (layer F.Cu) (tedit 564CEB55)
    (at 134.62 124.46)
    (descr "Film Capacitor Length 7 x Width 2mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 2.5 0) (layer F.SilkS))
    (fp_text value "" (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 /RESET))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /DTR))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W2_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module egna_footprint:egen_Single_pad (layer F.Cu) (tedit 564A53C7)
    (at 166.37 130.81)
    (fp_text reference "" (at 0 3.556) (layer F.SilkS))
    (fp_text value "" (at 0 -3.556) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  )
  (module egna_footprint:egen_Single_pad (layer F.Cu) (tedit 564A53B4)
    (at 168.91 130.81)
    (fp_text reference "" (at 0 3.556) (layer F.SilkS))
    (fp_text value "" (at 0 -3.556) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  )
  (dimension 50.6 (width 0.15) (layer Dwgs.User)
    (gr_text "50,600 mm" (at 144.7 141.25) (layer Dwgs.User))
    (feature1 (pts (xy 170 132.1) (xy 170 141.9)))
    (feature2 (pts (xy 119.4 132.1) (xy 119.4 141.9)))
    (crossbar (pts (xy 119.4 140.6) (xy 170 140.6)))
    (arrow1a (pts (xy 170 140.6) (xy 168.873496 141.186421)))
    (arrow1b (pts (xy 170 140.6) (xy 168.873496 140.013579)))
    (arrow2a (pts (xy 119.4 140.6) (xy 120.526504 141.186421)))
    (arrow2b (pts (xy 119.4 140.6) (xy 120.526504 140.013579)))
  )
  (dimension 15.2 (width 0.15) (layer Dwgs.User)
    (gr_text "15,200 mm" (at 107.650001 124.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 119.4 132.1) (xy 107.000001 132.1)))
    (feature2 (pts (xy 119.4 116.9) (xy 107.000001 116.9)))
    (crossbar (pts (xy 108.300001 116.9) (xy 108.300001 132.1)))
    (arrow1a (pts (xy 108.300001 132.1) (xy 107.71358 130.973496)))
    (arrow1b (pts (xy 108.300001 132.1) (xy 108.886422 130.973496)))
    (arrow2a (pts (xy 108.300001 116.9) (xy 107.71358 118.026504)))
    (arrow2b (pts (xy 108.300001 116.9) (xy 108.886422 118.026504)))
  )
  (gr_line (start 170 132.1) (end 170 132) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.4 132.1) (end 170 132.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.4 132) (end 119.4 132.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170 116.9) (end 170 117) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.4 116.9) (end 170 116.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.4 117) (end 119.4 116.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.4 132) (end 119.4 117) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 170 117) (end 170 132) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text A5 (at 124.46 122.428 90) (layer B.SilkS))
  (gr_text GND (at 165.1 123.19 90) (layer B.SilkS))
  (gr_text VCC (at 165.1 128.27 90) (layer B.SilkS))
  (gr_text VCC (at 163.83 128.778 90) (layer B.SilkS))
  (gr_text GND (at 161.29 128.778 90) (layer B.SilkS))
  (gr_text D9 (at 157.48 122.428 90) (layer B.SilkS))
  (gr_text D10 (at 154.94 122.682 90) (layer B.SilkS))
  (gr_text D8 (at 157.48 126.492 90) (layer B.SilkS))
  (gr_text D7 (at 154.94 126.492 90) (layer B.SilkS))
  (gr_text D6 (at 152.4 126.492 90) (layer B.SilkS))
  (gr_text D5 (at 149.86 126.492 90) (layer B.SilkS))
  (gr_text X2 (at 147.32 126.492 90) (layer B.SilkS))
  (gr_text X1 (at 144.78 126.492 90) (layer B.SilkS))
  (gr_text D2 (at 132.08 126.492 90) (layer B.SilkS))
  (gr_text D3 (at 134.62 126.492 90) (layer B.SilkS))
  (gr_text D4 (at 137.16 126.492 90) (layer B.SilkS))
  (gr_text D11 (at 152.4 122.682 90) (layer B.SilkS))
  (gr_text D12 (at 149.86 122.682 90) (layer B.SilkS))
  (gr_text D13 (at 147.574 122.682 90) (layer B.SilkS))
  (gr_text AREF (at 142.1 122.9 90) (layer B.SilkS))
  (gr_text A4 (at 127 122.428 90) (layer B.SilkS))
  (gr_text A3 (at 129.54 122.428 90) (layer B.SilkS))
  (gr_text A2 (at 132.08 122.428 90) (layer B.SilkS))
  (gr_text A1 (at 134.62 122.428 90) (layer B.SilkS))
  (gr_text A0 (at 137.16 122.428 90) (layer B.SilkS))
  (gr_text VCC (at 144.9 122.7 90) (layer B.SilkS))
  (gr_text GND (at 139.7 122.682 90) (layer B.SilkS))
  (gr_text GND (at 142.24 126.492 90) (layer B.SilkS))
  (gr_text VCC (at 139.7 126.492 90) (layer B.SilkS))
  (gr_text TX (at 129.54 126.492 90) (layer B.SilkS))
  (gr_text RX (at 127 126.492 90) (layer B.SilkS))
  (gr_text RST (at 124.46 126.238 90) (layer B.SilkS))
  (gr_text VCC (at 122.174 123.19 90) (layer B.SilkS))
  (gr_text GND (at 122.174 120.65 90) (layer B.SilkS))
)
