(kicad_pcb (version 4) (host pcbnew 4.0.0-rc2-stable)
  (general
    (links 172)
    (no_connects 62)
    (area 180.137668 93.851 249.885 157.256001)
    (thickness 1.6)
    (drawings 108)
    (tracks 492)
    (zones 0)
    (modules 213)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.15)
    (pcb_text_size 0.7 0.7)
    (mod_edge_width 0.15)
    (mod_text_size 0.7 0.7)
    (mod_text_width 0.15)
    (pad_size 0.5 0.5)
    (pad_drill 0.5)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 195.58 146.05)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 /RESET)
  (net 4 /DTR)
  (net 5 "Net-(C3-Pad1)")
  (net 6 /RX)
  (net 7 /TX)
  (net 8 "Net-(IC1-Pad4)")
  (net 9 "Net-(IC1-Pad5)")
  (net 10 "Net-(IC1-Pad6)")
  (net 11 "Net-(IC1-Pad9)")
  (net 12 "Net-(IC1-Pad10)")
  (net 13 "Net-(IC1-Pad11)")
  (net 14 "Net-(IC1-Pad12)")
  (net 15 "Net-(IC1-Pad13)")
  (net 16 "Net-(IC1-Pad14)")
  (net 17 /D9/CE)
  (net 18 /D10/SS)
  (net 19 /D11/MOSI)
  (net 20 /D12/MISO)
  (net 21 /D13/SCK)
  (net 22 "Net-(IC1-Pad23)")
  (net 23 "Net-(IC1-Pad24)")
  (net 24 "Net-(IC1-Pad25)")
  (net 25 "Net-(IC1-Pad26)")
  (net 26 "Net-(IC1-Pad27)")
  (net 27 "Net-(IC1-Pad28)")
  (net 28 "Net-(P4-Pad8)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /D10/SS)
    (add_net /D11/MOSI)
    (add_net /D12/MISO)
    (add_net /D13/SCK)
    (add_net /D9/CE)
    (add_net /DTR)
    (add_net /RESET)
    (add_net /RX)
    (add_net /TX)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(P4-Pad8)")
  )
  (net_class PWR_1 ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class PWR_2 ""
    (clearance 0.2)
    (trace_width 0.7)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 245.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 244.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 244.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 243.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 243.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 242.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 241.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 241.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 240.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 240.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 239.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 238.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 238.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 237.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 237.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 236.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 235.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 235.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 234.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 234.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 233.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 232.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 232.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 231.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 231.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 230.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 229.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 229.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 228.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 228.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 227.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 226.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 226.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 225.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 225.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 224.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 223.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 223.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 222.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 222.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 221.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 220.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 220.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 219.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 219.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 218.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 217.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 217.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 216.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 216.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 215.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 214.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 214.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 213.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 213.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 212.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 211.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 211.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 210.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 210.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 209.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 208.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 208.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 207.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 207.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 206.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 205.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 205.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 204.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 204.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 203.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 202.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 202.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 201.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 201.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 200.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 199.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 199.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 198.742 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 198.142 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 197.542 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 196.942 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 196.342 114.554)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 245.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 244.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 244.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 243.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 243.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 242.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 241.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 241.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 240.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 240.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 239.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 238.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 238.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 237.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 237.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 236.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 235.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 235.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 234.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 234.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 233.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 232.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 232.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 231.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 231.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 230.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 229.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 229.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 228.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 228.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 227.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 226.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 226.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 225.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 225.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 224.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 223.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 223.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 222.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 222.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 221.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 220.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 220.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 219.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 219.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 218.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 217.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 217.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 216.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 216.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 215.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 214.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 214.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 213.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 213.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 212.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 211.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 211.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 210.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 210.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 209.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 208.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 208.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 207.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 207.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 206.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 205.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 205.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 204.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 204.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 203.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 202.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 202.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 201.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 201.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 200.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 199.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 199.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 198.742 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 198.142 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 197.542 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 196.942 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 564A4DE0)
    (at 199.39 132.08 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 564E530D)
    (at 237.49 132.08)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /D9/CE))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D10/SS))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D13/SCK))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D11/MOSI))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D12/MISO))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P4-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 564E5340)
    (at 240.03 128.778 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 564E530D)
    (at 237.49 116.078)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /D9/CE))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D10/SS))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D13/SCK))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D11/MOSI))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D12/MISO))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P4-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 564E5287)
    (at 245.11 116.078 270)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference "" (at 1.25 -3.8 270) (layer F.SilkS))
    (fp_text value "" (at 1.25 3.8 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 564E526F)
    (at 245.11 126.238 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D12/MISO))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D13/SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D11/MOSI))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistor_Horizontal_RM5mm (layer F.Cu) (tedit 564CEB49)
    (at 205.486 122.428)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R1 (at 0 0) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.302 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 3.302 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 /RESET))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 564A502C)
    (at 242.57 116.078 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference "" (at 1.25 -2.5 270) (layer F.SilkS))
    (fp_text value "" (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 564A4E4C)
    (at 199.39 128.778 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_DIP:DIP-28_W7.62mm (layer F.Cu) (tedit 564A4E1F)
    (at 200.66 126.238 90)
    (descr "28-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference "" (at 0 -5.22 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.72 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 /RESET))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /RX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /TX))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(IC1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(IC1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(IC1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(IC1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(IC1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(IC1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(IC1-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(IC1-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(IC1-Pad14)"))
    (pad 15 thru_hole oval (at 7.62 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 /D9/CE))
    (pad 16 thru_hole oval (at 7.62 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D10/SS))
    (pad 17 thru_hole oval (at 7.62 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D11/MOSI))
    (pad 18 thru_hole oval (at 7.62 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D12/MISO))
    (pad 19 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D13/SCK))
    (pad 20 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 21 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad1)"))
    (pad 22 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 23 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(IC1-Pad23)"))
    (pad 24 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(IC1-Pad24)"))
    (pad 25 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(IC1-Pad25)"))
    (pad 26 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(IC1-Pad26)"))
    (pad 27 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(IC1-Pad27)"))
    (pad 28 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(IC1-Pad28)"))
    (model Housings_DIP.3dshapes/DIP-28_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 564A4DE0)
    (at 199.39 116.078 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 564A4DAD)
    (at 196.85 116.078)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /RX))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /TX))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /DTR))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2_P5 (layer F.Cu) (tedit 564CEBFB)
    (at 227.33 122.428)
    (descr "Film Capacitor Length 7 x Width 2mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 2.54 0) (layer F.SilkS))
    (fp_text value "" (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W2_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2_P5 (layer F.Cu) (tedit 564CEBEE)
    (at 219.71 122.428)
    (descr "Film Capacitor Length 7 x Width 2mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 2.54 0) (layer F.SilkS))
    (fp_text value "" (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W2_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2_P5 (layer F.Cu) (tedit 564CEB55)
    (at 210.82 122.428)
    (descr "Film Capacitor Length 7 x Width 2mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 2.5 0) (layer F.SilkS))
    (fp_text value "" (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 /RESET))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /DTR))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W2_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module egna_footprint:egen_Single_pad (layer F.Cu) (tedit 564A53C7)
    (at 242.57 128.778)
    (fp_text reference "" (at 0 3.556) (layer F.SilkS))
    (fp_text value "" (at 0 -3.556) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  )
  (module egna_footprint:egen_Single_pad (layer F.Cu) (tedit 564A53B4)
    (at 245.11 128.778)
    (fp_text reference "" (at 0 3.556) (layer F.SilkS))
    (fp_text value "" (at 0 -3.556) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 564E5340)
    (at 240.03 144.78 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 564E530D)
    (at 237.49 132.08)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /D9/CE))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D10/SS))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D13/SCK))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D11/MOSI))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D12/MISO))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P4-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 564E5287)
    (at 245.11 132.08 270)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference "" (at 1.25 -3.8 270) (layer F.SilkS))
    (fp_text value "" (at 1.25 3.8 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 564E526F)
    (at 245.11 142.24 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D12/MISO))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D13/SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D11/MOSI))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistor_Horizontal_RM5mm (layer F.Cu) (tedit 564CEB49)
    (at 205.486 138.43)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R1 (at 0 0) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.302 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 3.302 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 /RESET))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 564A502C)
    (at 242.57 132.08 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference "" (at 1.25 -2.5 270) (layer F.SilkS))
    (fp_text value "" (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 564A4E4C)
    (at 199.39 144.78 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_DIP:DIP-28_W7.62mm (layer F.Cu) (tedit 564A4E1F)
    (at 200.66 142.24 90)
    (descr "28-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference "" (at 0 -5.22 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.72 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 /RESET))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /RX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /TX))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(IC1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(IC1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(IC1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(IC1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(IC1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(IC1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(IC1-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(IC1-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(IC1-Pad14)"))
    (pad 15 thru_hole oval (at 7.62 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 /D9/CE))
    (pad 16 thru_hole oval (at 7.62 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D10/SS))
    (pad 17 thru_hole oval (at 7.62 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D11/MOSI))
    (pad 18 thru_hole oval (at 7.62 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D12/MISO))
    (pad 19 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D13/SCK))
    (pad 20 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 21 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad1)"))
    (pad 22 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 23 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(IC1-Pad23)"))
    (pad 24 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(IC1-Pad24)"))
    (pad 25 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(IC1-Pad25)"))
    (pad 26 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(IC1-Pad26)"))
    (pad 27 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(IC1-Pad27)"))
    (pad 28 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(IC1-Pad28)"))
    (model Housings_DIP.3dshapes/DIP-28_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 564A4DE0)
    (at 199.39 132.08 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 564A4DAD)
    (at 196.85 132.08)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /RX))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /TX))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /DTR))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2_P5 (layer F.Cu) (tedit 564CEBFB)
    (at 227.33 138.43)
    (descr "Film Capacitor Length 7 x Width 2mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 2.54 0) (layer F.SilkS))
    (fp_text value "" (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W2_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2_P5 (layer F.Cu) (tedit 564CEBEE)
    (at 219.71 138.43)
    (descr "Film Capacitor Length 7 x Width 2mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 2.54 0) (layer F.SilkS))
    (fp_text value "" (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W2_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2_P5 (layer F.Cu) (tedit 564CEB55)
    (at 210.82 138.43)
    (descr "Film Capacitor Length 7 x Width 2mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 2.5 0) (layer F.SilkS))
    (fp_text value "" (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 /RESET))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /DTR))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W2_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module egna_footprint:egen_Single_pad (layer F.Cu) (tedit 564A53C7)
    (at 242.57 144.78)
    (fp_text reference "" (at 0 3.556) (layer F.SilkS))
    (fp_text value "" (at 0 -3.556) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  )
  (module egna_footprint:egen_Single_pad (layer F.Cu) (tedit 564A53B4)
    (at 245.11 144.78)
    (fp_text reference "" (at 0 3.556) (layer F.SilkS))
    (fp_text value "" (at 0 -3.556) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 564E5340)
    (at 240.03 112.776 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x04 (layer F.Cu) (tedit 564E530D)
    (at 237.49 100.076)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /D9/CE))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D10/SS))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D13/SCK))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D11/MOSI))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D12/MISO))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(P4-Pad8)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz 0.05 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 564E5287)
    (at 245.11 100.076 270)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference "" (at 1.25 -3.8 270) (layer F.SilkS))
    (fp_text value "" (at 1.25 3.8 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 564E526F)
    (at 245.11 110.236 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 180) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D12/MISO))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D13/SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D11/MOSI))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 /RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistor_Horizontal_RM5mm (layer F.Cu) (tedit 564CEB49)
    (at 205.486 106.426)
    (descr "Resistor, Axial,  RM 10mm, 1/3W,")
    (tags "Resistor, Axial, RM 10mm, 1/3W,")
    (fp_text reference R1 (at 0 0) (layer F.SilkS))
    (fp_text value "" (at 0 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at -3.302 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 3.302 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 /RESET))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 564A502C)
    (at 242.57 100.076 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference "" (at 1.25 -2.5 270) (layer F.SilkS))
    (fp_text value "" (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 564A4E4C)
    (at 199.39 112.776 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_DIP:DIP-28_W7.62mm (layer F.Cu) (tedit 564A4E1F)
    (at 200.66 110.236 90)
    (descr "28-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference "" (at 0 -5.22 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.72 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 /RESET))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 /RX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /TX))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(IC1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(IC1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(IC1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(IC1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(IC1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(IC1-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(IC1-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(IC1-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(IC1-Pad14)"))
    (pad 15 thru_hole oval (at 7.62 33.02 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 /D9/CE))
    (pad 16 thru_hole oval (at 7.62 30.48 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 /D10/SS))
    (pad 17 thru_hole oval (at 7.62 27.94 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D11/MOSI))
    (pad 18 thru_hole oval (at 7.62 25.4 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 20 /D12/MISO))
    (pad 19 thru_hole oval (at 7.62 22.86 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 21 /D13/SCK))
    (pad 20 thru_hole oval (at 7.62 20.32 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 21 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad1)"))
    (pad 22 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 23 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(IC1-Pad23)"))
    (pad 24 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(IC1-Pad24)"))
    (pad 25 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(IC1-Pad25)"))
    (pad 26 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(IC1-Pad26)"))
    (pad 27 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(IC1-Pad27)"))
    (pad 28 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(IC1-Pad28)"))
    (model Housings_DIP.3dshapes/DIP-28_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x15 (layer F.Cu) (tedit 564A4DE0)
    (at 199.39 100.076 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x15.wrl
      (at (xyz 0 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 564A4DAD)
    (at 196.85 100.076)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference "" (at 0 -5.1) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /RX))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /TX))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /DTR))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2_P5 (layer F.Cu) (tedit 564CEBFB)
    (at 227.33 106.426)
    (descr "Film Capacitor Length 7 x Width 2mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 2.54 0) (layer F.SilkS))
    (fp_text value "" (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W2_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2_P5 (layer F.Cu) (tedit 564CEBEE)
    (at 219.71 106.426)
    (descr "Film Capacitor Length 7 x Width 2mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C3 (at 2.54 0) (layer F.SilkS))
    (fp_text value "" (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W2_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L7_W2_P5 (layer F.Cu) (tedit 564CEB55)
    (at 210.82 106.426)
    (descr "Film Capacitor Length 7 x Width 2mm, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 2.5 0) (layer F.SilkS))
    (fp_text value "" (at 2.5 2.5) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 /RESET))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /DTR))
    (model Capacitors_ThroughHole.3dshapes/C_Rect_L7_W2_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module egna_footprint:egen_Single_pad (layer F.Cu) (tedit 564A53C7)
    (at 242.57 112.776)
    (fp_text reference "" (at 0 3.556) (layer F.SilkS))
    (fp_text value "" (at 0 -3.556) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  )
  (module egna_footprint:egen_Single_pad (layer F.Cu) (tedit 564A53B4)
    (at 245.11 112.776)
    (fp_text reference "" (at 0 3.556) (layer F.SilkS))
    (fp_text value "" (at 0 -3.556) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS))
  )
  (module panelizing_holes:MountingHole_2-5mm (layer F.Cu) (tedit 564F2191)
    (at 196.342 130.556)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -3.50012) (layer F.SilkS))
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.5) (layers *.Cu))
  )
  (dimension 47.244 (width 0.15) (layer Dwgs.User)
    (gr_text "47,244 mm" (at 183.246001 122.428 270) (layer Dwgs.User))
    (feature1 (pts (xy 195.58 146.05) (xy 182.596001 146.05)))
    (feature2 (pts (xy 195.58 98.806) (xy 182.596001 98.806)))
    (crossbar (pts (xy 183.896001 98.806) (xy 183.896001 146.05)))
    (arrow1a (pts (xy 183.896001 146.05) (xy 183.30958 144.923496)))
    (arrow1b (pts (xy 183.896001 146.05) (xy 184.482422 144.923496)))
    (arrow2a (pts (xy 183.896001 98.806) (xy 183.30958 99.932504)))
    (arrow2b (pts (xy 183.896001 98.806) (xy 184.482422 99.932504)))
  )
  (dimension 50.546 (width 0.15) (layer Dwgs.User)
    (gr_text "50,546 mm" (at 220.853 156.606) (layer Dwgs.User))
    (feature1 (pts (xy 246.126 146.05) (xy 246.126 157.256)))
    (feature2 (pts (xy 195.58 146.05) (xy 195.58 157.256)))
    (crossbar (pts (xy 195.58 155.956) (xy 246.126 155.956)))
    (arrow1a (pts (xy 246.126 155.956) (xy 244.999496 156.542421)))
    (arrow1b (pts (xy 246.126 155.956) (xy 244.999496 155.369579)))
    (arrow2a (pts (xy 195.58 155.956) (xy 196.706504 156.542421)))
    (arrow2b (pts (xy 195.58 155.956) (xy 196.706504 155.369579)))
  )
  (gr_line (start 246.126 146.05) (end 195.58 146.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 246.126 98.806) (end 246.126 146.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 195.58 98.806) (end 246.126 98.806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 195.58 146.05) (end 195.58 98.806) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text A5 (at 200.66 120.396 90) (layer B.SilkS))
  (gr_text GND (at 241.3 121.158 90) (layer B.SilkS))
  (gr_text VCC (at 241.3 126.238 90) (layer B.SilkS))
  (gr_text VCC (at 240.03 126.746 90) (layer B.SilkS))
  (gr_text GND (at 237.49 126.746 90) (layer B.SilkS))
  (gr_text D9 (at 233.68 120.396 90) (layer B.SilkS))
  (gr_text D10 (at 231.14 120.65 90) (layer B.SilkS))
  (gr_text D8 (at 233.68 124.46 90) (layer B.SilkS))
  (gr_text D7 (at 231.14 124.46 90) (layer B.SilkS))
  (gr_text D6 (at 228.6 124.46 90) (layer B.SilkS))
  (gr_text D5 (at 226.06 124.46 90) (layer B.SilkS))
  (gr_text X2 (at 223.52 124.46 90) (layer B.SilkS))
  (gr_text X1 (at 220.98 124.46 90) (layer B.SilkS))
  (gr_text D2 (at 208.28 124.46 90) (layer B.SilkS))
  (gr_text D3 (at 210.82 124.46 90) (layer B.SilkS))
  (gr_text D4 (at 213.36 124.46 90) (layer B.SilkS))
  (gr_text D11 (at 228.6 120.65 90) (layer B.SilkS))
  (gr_text D12 (at 226.06 120.65 90) (layer B.SilkS))
  (gr_text D13 (at 223.774 120.65 90) (layer B.SilkS))
  (gr_text AREF (at 218.3 120.868 90) (layer B.SilkS))
  (gr_text A4 (at 203.2 120.396 90) (layer B.SilkS))
  (gr_text A3 (at 205.74 120.396 90) (layer B.SilkS))
  (gr_text A2 (at 208.28 120.396 90) (layer B.SilkS))
  (gr_text A1 (at 210.82 120.396 90) (layer B.SilkS))
  (gr_text A0 (at 213.36 120.396 90) (layer B.SilkS))
  (gr_text VCC (at 220.98 120.65 90) (layer B.SilkS))
  (gr_text GND (at 215.9 120.65 90) (layer B.SilkS))
  (gr_text GND (at 218.44 124.46 90) (layer B.SilkS))
  (gr_text VCC (at 215.9 124.46 90) (layer B.SilkS))
  (gr_text TX (at 205.74 124.46 90) (layer B.SilkS))
  (gr_text RX (at 203.2 124.46 90) (layer B.SilkS))
  (gr_text RST (at 200.66 124.206 90) (layer B.SilkS))
  (gr_text VCC (at 198.374 121.158 90) (layer B.SilkS))
  (gr_text GND (at 198.374 118.618 90) (layer B.SilkS))
  (gr_text A5 (at 200.66 136.398 90) (layer B.SilkS))
  (gr_text GND (at 241.3 137.16 90) (layer B.SilkS))
  (gr_text VCC (at 241.3 142.24 90) (layer B.SilkS))
  (gr_text VCC (at 240.03 142.748 90) (layer B.SilkS))
  (gr_text GND (at 237.49 142.748 90) (layer B.SilkS))
  (gr_text D9 (at 233.68 136.398 90) (layer B.SilkS))
  (gr_text D10 (at 231.14 136.652 90) (layer B.SilkS))
  (gr_text D8 (at 233.68 140.462 90) (layer B.SilkS))
  (gr_text D7 (at 231.14 140.462 90) (layer B.SilkS))
  (gr_text D6 (at 228.6 140.462 90) (layer B.SilkS))
  (gr_text D5 (at 226.06 140.462 90) (layer B.SilkS))
  (gr_text X2 (at 223.52 140.462 90) (layer B.SilkS))
  (gr_text X1 (at 220.98 140.462 90) (layer B.SilkS))
  (gr_text D2 (at 208.28 140.462 90) (layer B.SilkS))
  (gr_text D3 (at 210.82 140.462 90) (layer B.SilkS))
  (gr_text D4 (at 213.36 140.462 90) (layer B.SilkS))
  (gr_text D11 (at 228.6 136.652 90) (layer B.SilkS))
  (gr_text D12 (at 226.06 136.652 90) (layer B.SilkS))
  (gr_text D13 (at 223.774 136.652 90) (layer B.SilkS))
  (gr_text AREF (at 218.3 136.87 90) (layer B.SilkS))
  (gr_text A4 (at 203.2 136.398 90) (layer B.SilkS))
  (gr_text A3 (at 205.74 136.398 90) (layer B.SilkS))
  (gr_text A2 (at 208.28 136.398 90) (layer B.SilkS))
  (gr_text A1 (at 210.82 136.398 90) (layer B.SilkS))
  (gr_text A0 (at 213.36 136.398 90) (layer B.SilkS))
  (gr_text VCC (at 220.98 136.652 90) (layer B.SilkS))
  (gr_text GND (at 215.9 136.652 90) (layer B.SilkS))
  (gr_text GND (at 218.44 140.462 90) (layer B.SilkS))
  (gr_text VCC (at 215.9 140.462 90) (layer B.SilkS))
  (gr_text TX (at 205.74 140.462 90) (layer B.SilkS))
  (gr_text RX (at 203.2 140.462 90) (layer B.SilkS))
  (gr_text RST (at 200.66 140.208 90) (layer B.SilkS))
  (gr_text VCC (at 198.374 137.16 90) (layer B.SilkS))
  (gr_text GND (at 198.374 134.62 90) (layer B.SilkS))
  (gr_text A5 (at 200.66 104.394 90) (layer B.SilkS))
  (gr_text GND (at 241.3 105.156 90) (layer B.SilkS))
  (gr_text VCC (at 241.3 110.236 90) (layer B.SilkS))
  (gr_text VCC (at 240.03 110.744 90) (layer B.SilkS))
  (gr_text GND (at 237.49 110.744 90) (layer B.SilkS))
  (gr_text D9 (at 233.68 104.394 90) (layer B.SilkS))
  (gr_text D10 (at 231.14 104.648 90) (layer B.SilkS))
  (gr_text D8 (at 233.68 108.458 90) (layer B.SilkS))
  (gr_text D7 (at 231.14 108.458 90) (layer B.SilkS))
  (gr_text D6 (at 228.6 108.458 90) (layer B.SilkS))
  (gr_text D5 (at 226.06 108.458 90) (layer B.SilkS))
  (gr_text X2 (at 223.52 108.458 90) (layer B.SilkS))
  (gr_text X1 (at 220.98 108.458 90) (layer B.SilkS))
  (gr_text D2 (at 208.28 108.458 90) (layer B.SilkS))
  (gr_text D3 (at 210.82 108.458 90) (layer B.SilkS))
  (gr_text D4 (at 213.36 108.458 90) (layer B.SilkS))
  (gr_text D11 (at 228.6 104.648 90) (layer B.SilkS))
  (gr_text D12 (at 226.06 104.648 90) (layer B.SilkS))
  (gr_text D13 (at 223.774 104.648 90) (layer B.SilkS))
  (gr_text AREF (at 218.3 104.866 90) (layer B.SilkS))
  (gr_text A4 (at 203.2 104.394 90) (layer B.SilkS))
  (gr_text A3 (at 205.74 104.394 90) (layer B.SilkS))
  (gr_text A2 (at 208.28 104.394 90) (layer B.SilkS))
  (gr_text A1 (at 210.82 104.394 90) (layer B.SilkS))
  (gr_text A0 (at 213.36 104.394 90) (layer B.SilkS))
  (gr_text VCC (at 220.98 104.648 90) (layer B.SilkS))
  (gr_text GND (at 215.9 104.648 90) (layer B.SilkS))
  (gr_text GND (at 218.44 108.458 90) (layer B.SilkS))
  (gr_text VCC (at 215.9 108.458 90) (layer B.SilkS))
  (gr_text TX (at 205.74 108.458 90) (layer B.SilkS))
  (gr_text RX (at 203.2 108.458 90) (layer B.SilkS))
  (gr_text RST (at 200.66 108.204 90) (layer B.SilkS))
  (gr_text VCC (at 198.374 105.156 90) (layer B.SilkS))
  (gr_text GND (at 198.374 102.616 90) (layer B.SilkS))
)
