(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 95)
    (no_connects 0)
    (area 20.472136 40.2913 101.006901 75.781601)
    (thickness 1.6)
    (drawings 14)
    (tracks 513)
    (zones 0)
    (modules 39)
    (nets 35)
  )
  (page A4)
  (title_block
    (title "Water meter")
    (date 2016-03-02)
    (rev 0.10)
    (company "MySensors Boards")
    (comment 1 "R. Bisschops")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.5 2)
    (pad_drill 3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 23.46 75.7)
    (grid_origin 23.46 75.7)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../../Nodes/Watermeter/Fabrication/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(CONN1-Pad2)")
  (net 3 RESET)
  (net 4 MISO)
  (net 5 SCK)
  (net 6 MOSI)
  (net 7 SEC-SDA)
  (net 8 D3)
  (net 9 FLASH-CSN)
  (net 10 RAD_CSN)
  (net 11 RAD_IRQ)
  (net 12 RAD_CE)
  (net 13 "Net-(C1-Pad1)")
  (net 14 A0)
  (net 15 "Net-(D2-Pad1)")
  (net 16 "Net-(D3-Pad1)")
  (net 17 "Net-(R4-Pad2)")
  (net 18 "Net-(R6-Pad2)")
  (net 19 +3.3V)
  (net 20 VCC)
  (net 21 TMP_SCL)
  (net 22 TMP_SDA)
  (net 23 "Net-(REF1-Pad18)")
  (net 24 "Net-(REF1-Pad19)")
  (net 25 "Net-(REF1-Pad24)")
  (net 26 "Net-(REF1-Pad34)")
  (net 27 "Net-(REF1-Pad33)")
  (net 28 "Net-(REF1-Pad1)")
  (net 29 "Net-(REF1-Pad2)")
  (net 30 "Net-(REF1-Pad7)")
  (net 31 "Net-(REF1-Pad8)")
  (net 32 "Net-(REF1-Pad9)")
  (net 33 "Net-(REF1-Pad10)")
  (net 34 "Net-(U6-Pad1)")
  (net_class Default "Dit is de standaard class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3V)
    (add_net A0)
    (add_net D3)
    (add_net FLASH-CSN)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(REF1-Pad1)")
    (add_net "Net-(REF1-Pad10)")
    (add_net "Net-(REF1-Pad18)")
    (add_net "Net-(REF1-Pad19)")
    (add_net "Net-(REF1-Pad2)")
    (add_net "Net-(REF1-Pad24)")
    (add_net "Net-(REF1-Pad33)")
    (add_net "Net-(REF1-Pad34)")
    (add_net "Net-(REF1-Pad7)")
    (add_net "Net-(REF1-Pad8)")
    (add_net "Net-(REF1-Pad9)")
    (add_net "Net-(U6-Pad1)")
    (add_net RAD_CE)
    (add_net RAD_CSN)
    (add_net RAD_IRQ)
    (add_net RESET)
    (add_net SCK)
    (add_net SEC-SDA)
    (add_net TMP_SCL)
    (add_net TMP_SDA)
    (add_net VCC)
  )
  (net_class Power ""
    (clearance 0.3)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(CONN1-Pad2)")
  )
  (module MySensors:NRF24L01_STD (layer F.Cu) (tedit 56D1CF93)
    (at 76.1619 57.0484 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference REF2 (at 10.0584 2.1463 360) (layer F.SilkS))
    (fp_text value NRF24L01 (at 3.683 -3.429 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 +3.3V))
    (pad 1 thru_hole rect (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 RAD_CSN))
    (pad 3 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 RAD_CE))
    (pad 6 thru_hole oval (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 MOSI))
    (pad 5 thru_hole oval (at 5.08 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 SCK))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 RAD_IRQ))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 MISO))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz 0.15 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 56CDFBC1)
    (at 41.07436 58.39216)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -0.56 1.73) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 56F90A8C)
    (at 41.07436 54.70216)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 1.44564 1.56784) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 20 VCC))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 56CDFBB5)
    (at 33.7566 64.77 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -1.05216 -1.62224 360) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 19 +3.3V))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 56CDFA03)
    (at 55.0164 51.3969 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -0.07796 1.60474 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 56CDFA07)
    (at 60.0456 50.17008 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 0.21792 -1.87124 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 569A6D23)
    (at 79.33 56.55 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at -2.667 0.381 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 +3.3V))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 56CDF9F3)
    (at 56.642 62.9285 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0.08764 1.57634 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 56F90979)
    (at 80.44436 44.05216 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at -1.52216 -1.85564 360) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 56F9099C)
    (at 69.23436 52.02216 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at -2.36784 0.35564 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 A0))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 56D1CF97)
    (at 67.0179 67.8561)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 3.16646 -2.14394) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 MISO))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 VCC))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 SCK))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 MOSI))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 RESET))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 569A6F00)
    (at 40.92436 52.65216)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.143 -1.6383) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56CDF9F8)
    (at 55.1942 57.1246)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0.24016 1.77756) (layer F.SilkS))
    (fp_text value 56K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 SEC-SDA))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56CDF9EA)
    (at 51.46436 62.95216 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0.89 -1.7 360) (layer F.SilkS))
    (fp_text value 56K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 FLASH-CSN))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56F90961)
    (at 81.61 53.66 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.11 -1.58 360) (layer F.SilkS))
    (fp_text value 180 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56F90A54)
    (at 81.61 51.62 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -1.07 1.56 360) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 A0))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56F9098C)
    (at 69.25056 44.07408 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -1.38408 1.73056 540) (layer F.SilkS))
    (fp_text value 10K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 D3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 569B9D6F)
    (at 77.1525 43.0784 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -1.01854 -1.60528 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 D3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer B.Cu) (tedit 569A6EFC)
    (at 32.23436 56.16216 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 4.5212 1.7399 540) (layer B.SilkS))
    (fp_text value AP1117D50 (at 0 -0.762 270) (layer B.Fab))
    (pad 4 smd rect (at 0 3.302 270) (size 3.6576 2.032) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0 -3.302 270) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 20 VCC))
    (pad 3 smd rect (at 2.286 -3.302 270) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -2.286 -3.302 270) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer B.Cu) (tedit 569A6F1E)
    (at 39.4843 65.7987 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at -4.5085 -1.9304 180) (layer B.SilkS))
    (fp_text value AP1117D33 (at 0 -0.762 90) (layer B.Fab))
    (pad 4 smd rect (at 0 3.302 90) (size 3.6576 2.032) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0 -3.302 90) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 19 +3.3V))
    (pad 3 smd rect (at 2.286 -3.302 90) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 20 VCC))
    (pad 1 smd rect (at -2.286 -3.302 90) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 56CDFA00)
    (at 55.2958 54.2544 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U3 (at -1.23776 -2.04144 180) (layer F.SilkS))
    (fp_text value ATSHA240A (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 7 SEC-SDA))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 568D5E99)
    (at 55.4482 67.0306 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U4 (at 3.4671 1.4097 360) (layer F.SilkS))
    (fp_text value AT25DF512C (at 0 1.27 270) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 5 SCK))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 6 MOSI))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 4 MISO))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 9 FLASH-CSN))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 569B71A0)
    (at 75.46848 45.59808 270)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U6 (at -3.3782 2.3368 360) (layer F.SilkS))
    (fp_text value LM393 (at 0 1.27 270) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 7 smd rect (at -0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 8 D3))
    (pad 6 smd rect (at 0.635 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R6-Pad2)"))
    (pad 5 smd rect (at 1.905 -3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 14 A0))
    (pad 4 smd rect (at 1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -0.635 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.905 3.175 270) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U6-Pad1)"))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_5x5.3 (layer F.Cu) (tedit 569B9BDC)
    (at 42.55262 68.76034 270)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.3")
    (attr smd)
    (fp_text reference C6 (at 3.6957 0.7112 360) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81 270) (layer F.Fab))
    (pad 1 smd rect (at 2.19964 0 270) (size 2.99974 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 19 +3.3V))
    (pad 2 smd rect (at -2.19964 0 270) (size 2.99974 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/c_elec_5x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_5x5.3 (layer F.Cu) (tedit 56CDEBA9)
    (at 41.60266 53.95214 180)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.3")
    (attr smd)
    (fp_text reference C3 (at 3.5883 -2.68002 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 2.19964 0 180) (size 2.99974 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 2 smd rect (at -2.19964 0 180) (size 2.99974 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/c_elec_5x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_5x5.3 (layer F.Cu) (tedit 569B9BD4)
    (at 68.1482 59.1439 90)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.3")
    (attr smd)
    (fp_text reference C9 (at -3.7719 -2.2606 180) (layer F.SilkS))
    (fp_text value 4u7 (at 0 3.81 90) (layer F.Fab))
    (pad 1 smd rect (at 2.19964 0 90) (size 2.99974 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 19 +3.3V))
    (pad 2 smd rect (at -2.19964 0 90) (size 2.99974 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/c_elec_5x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.3 (layer F.Cu) (tedit 56CDEB9F)
    (at 40.6908 60.8457 180)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.3")
    (attr smd)
    (fp_text reference C2 (at 1.95644 -4.13646 180) (layer F.SilkS))
    (fp_text value 47uF (at 0 4.445 180) (layer F.Fab))
    (pad 1 smd rect (at 2.75082 0 180) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -2.75082 0 180) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MySensors:Potentiometer_Custom_Inline_ScrewUp (layer F.Cu) (tedit 56F90954)
    (at 86.5632 45.5168 180)
    (descr "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (tags "3296, 3/8, Square, Trimpot, Trimming, Potentiometer, Bourns")
    (fp_text reference R6 (at -1.7868 -8.4032 180) (layer F.SilkS))
    (fp_text value 10K (at 1.524 3.4671 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 -2.54 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(R6-Pad2)"))
    (pad 3 thru_hole circle (at 0 -5.08 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 20 VCC))
    (model Potentiometers.3dshapes/Potentiometer_Bourns_3296W_3-8Zoll_Inline_ScrewUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MySensors:TCRT5000 (layer B.Cu) (tedit 56D1D1BC)
    (at 71.9201 50.4317)
    (fp_text reference U5 (at -1.28778 5.1689) (layer B.SilkS))
    (fp_text value TCRT5000 (at 6.35 -2.54) (layer B.Fab))
    (pad 1 thru_hole circle (at 5.5 2.54) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 17 "Net-(R4-Pad2)"))
    (pad 2 thru_hole circle (at 5.5 0) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at 0 2.54) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 14 A0))
    (pad 4 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
  )
  (module Mounting_Holes:MountingHole_2-7mm (layer F.Cu) (tedit 56D1E3EC)
    (at 55.1815 45.5168)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers))
  )
  (module Mounting_Holes:MountingHole_2-7mm (layer F.Cu) (tedit 56D1E291)
    (at 29.0576 62.7761)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers))
  )
  (module Mounting_Holes:MountingHole_2-7mm (layer F.Cu) (tedit 56D1E2AB)
    (at 84.5439 58.1025)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_2-5mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56D6A859)
    (at 79.35 62.2 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -2.72 -0.03 180) (layer F.SilkS))
    (fp_text value 56K (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 +3.3V))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 RAD_CSN))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MySensors:SI7021 (layer F.Cu) (tedit 56D1D08D)
    (at 66.60896 45.69968 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference U7 (at 9.84248 0.4446 360) (layer F.SilkS))
    (fp_text value SI7021 (at 3.81 -2.54 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 +3.3V))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 TMP_SCL))
    (pad 4 thru_hole oval (at 7.62 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 TMP_SDA))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MySensors:LED_1206 (layer F.Cu) (tedit 56F9096E)
    (at 82.7024 46.0375 270)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D3 (at 2.3825 2.1324 360) (layer F.SilkS))
    (fp_text value PULSE (at 0 2 270) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D3-Pad1)"))
    (model F:/KiCad/modules/packages3d/led_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MySensors:LED_1206 (layer F.Cu) (tedit 569B9BEC)
    (at 42.3291 47.9552 90)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D2 (at -1.8923 2.3749 180) (layer F.SilkS))
    (fp_text value PWR (at 0 2 90) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 20 VCC))
    (pad 1 smd rect (at -1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D2-Pad1)"))
    (model F:/KiCad/modules/packages3d/led_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MySensors:Arduino_Pro_Mini_non_FTDI (layer F.Cu) (tedit 56D1E3E3)
    (at 47.3583 73.66)
    (fp_text reference REF1 (at 0.58606 -30.96784) (layer F.SilkS))
    (fp_text value "Arduino_Mini_Pro 5V" (at 7.62 -16.51 90) (layer F.Fab))
    (pad 13 thru_hole circle (at 15.24 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 RAD_CSN))
    (pad 14 thru_hole circle (at 15.24 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 MOSI))
    (pad 15 thru_hole circle (at 15.24 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 MISO))
    (pad 16 thru_hole circle (at 15.24 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 SCK))
    (pad 17 thru_hole circle (at 15.24 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 A0))
    (pad 18 thru_hole circle (at 15.24 -12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(REF1-Pad18)"))
    (pad 19 thru_hole circle (at 15.24 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(REF1-Pad19)"))
    (pad 20 thru_hole circle (at 15.24 -17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 SEC-SDA))
    (pad 21 thru_hole circle (at 15.24 -20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 VCC))
    (pad 22 thru_hole circle (at 15.24 -22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 RESET))
    (pad 23 thru_hole circle (at 15.24 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 24 thru_hole circle (at 15.24 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(REF1-Pad24)"))
    (pad 34 thru_hole circle (at 12.7 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(REF1-Pad34)"))
    (pad 33 thru_hole circle (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(REF1-Pad33)"))
    (pad 35 thru_hole circle (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 -27.94) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(REF1-Pad1)"))
    (pad 2 thru_hole circle (at 0 -25.4) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(REF1-Pad2)"))
    (pad 3 thru_hole circle (at 0 -22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 RESET))
    (pad 4 thru_hole circle (at 0 -20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0 -17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 RAD_IRQ))
    (pad 6 thru_hole circle (at 0 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 D3))
    (pad 7 thru_hole circle (at 0 -12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(REF1-Pad7)"))
    (pad 8 thru_hole circle (at 0 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(REF1-Pad8)"))
    (pad 9 thru_hole circle (at 0 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(REF1-Pad9)"))
    (pad 10 thru_hole circle (at 0 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(REF1-Pad10)"))
    (pad 11 thru_hole circle (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 FLASH-CSN))
    (pad 12 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 RAD_CE))
    (pad 32 thru_hole circle (at 12.7 -19.05) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 TMP_SCL))
    (pad 31 thru_hole circle (at 12.7 -16.51) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 TMP_SDA))
    (model F:/KiCad/modules/packages3d/arduino_pro_mini.wrl
      (at (xyz 0.3 0.6 0.31))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 -90))
    )
    (model F:/KiCad/modules/packages3d/pin_socket_12.wrl
      (at (xyz 0.6 0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
    (model F:/KiCad/modules/packages3d/pin_socket_12.wrl
      (at (xyz 0 0.55 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module MySensors:DO-214AC (layer F.Cu) (tedit 56F909E4)
    (at 33.22 55.13)
    (descr "Jedec DO-214AB diode package. Designed according to Fairchild SS32 datasheet.")
    (tags "DO-214AC diode")
    (attr smd)
    (fp_text reference D1 (at -2.71 2.48 180) (layer F.SilkS))
    (fp_text value "1N4007 M7" (at 0 4.6) (layer F.Fab))
    (pad 2 smd rect (at 2.1 0) (size 2.4 2.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(CONN1-Pad2)"))
    (pad 1 smd rect (at -2.1 0) (size 2.4 2.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C1-Pad1)"))
    (model F:/KiCad/modules/packages3d/do214ac.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MySensors:Socket_Jack_5.5-2.1MM (layer F.Cu) (tedit 56F90B21)
    (at 37.64 50.57 90)
    (fp_text reference CONN1 (at -0.94 -7.92 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -0.5 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 4.5 0.2 90) (size 4.5 2) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 2 "Net-(CONN1-Pad2)"))
    (pad 1 thru_hole oval (at 4.5 -6.1 90) (size 4.5 2) (drill oval 3 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at -0.1 -2.8 90) (size 2 4.5) (drill oval 0.8 3) (layers *.Cu *.Mask))
    (model F:/KiCad/modules/packages3d/dc_socket.wrl
      (at (xyz 0.18 0.254 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text "© " (at 32.89 67.75 90) (layer F.SilkS))
  (gr_line (start 23.4531 75.7066) (end 23.4531 40.8921) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 23.4531 75.7066) (end 89.7969 75.7066) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 89.7969 75.7066) (end 89.7969 40.8921) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 23.4531 40.8921) (end 89.7969 40.8921) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text "R. Bisschops" (at 32.99 62.56 90) (layer F.SilkS))
  (gr_text "Licensed\nunder CERN \nOHL v.1.2" (at 35.26 67.39 90) (layer F.SilkS))
  (gr_text Mysensors-Watermeter-Rev.1.0 (at 24.38 51.55 90) (layer B.Cu))
  (gr_text Mysensors-Watermeter-Rev.1.0 (at 24.38 51.55 90) (layer F.Cu))
  (target plus (at 28.45436 70.70216) (size 5) (width 0.15) (layer Edge.Cuts))
  (target plus (at 84.10436 70.72216) (size 5) (width 0.15) (layer Edge.Cuts))
  (target plus (at 28.45436 70.70216) (size 5) (width 0.15) (layer Edge.Cuts))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.83 56.63) (xy 89.7917 40.8867) (xy 88.6741 40.8867) (xy 74.031 40.8867) (xy 73.6119 40.8867)
        (xy 23.4342 40.8613) (xy 23.41 62.73) (xy 42.37 75.73) (xy 73.43 75.7)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73.36 75.77) (xy 89.8 56.66) (xy 89.7917 40.8867) (xy 88.2677 40.8867) (xy 73.7135 40.8867)
        (xy 73.5992 40.8867) (xy 23.4469 40.874) (xy 23.41 62.73) (xy 42.33 75.69) (xy 71.39 75.7)
      )
    )
  )
)
