(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 87)
    (no_connects 0)
    (area 79.949999 109.949999 165.050001 166.050001)
    (thickness 1.6)
    (drawings 14)
    (tracks 444)
    (zones 0)
    (modules 35)
    (nets 76)
  )
  (page A4)
  (title_block
    (title "MySensors Gateway")
    (date 2016-03-02)
    (rev 0.7)
    (company "MySensors Boards")
    (comment 1 "R. Bisschops")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 80 166)
    (grid_origin 80 166)
    (visible_elements 7FFEFF7F)
    (pcbplotparams
      (layerselection 0x080f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gateway))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 RAD-TX)
  (net 4 RAD-RX)
  (net 5 RAD-ERR)
  (net 6 ETH-NSS)
  (net 7 RAD-CSN)
  (net 8 RAD-CE)
  (net 9 SEC-SDA)
  (net 10 ETH-SCK)
  (net 11 +3.3V)
  (net 12 MISO)
  (net 13 SCK)
  (net 14 MOSI)
  (net 15 RESET)
  (net 16 FLASH_CSN)
  (net 17 ETH-MISO)
  (net 18 ETH-MOSI)
  (net 19 "Net-(D2-Pad1)")
  (net 20 "Net-(D3-Pad1)")
  (net 21 "Net-(D4-Pad1)")
  (net 22 "Net-(D5-Pad1)")
  (net 23 "Net-(JP2-Pad5)")
  (net 24 "Net-(JP2-Pad7)")
  (net 25 "Net-(JP2-Pad8)")
  (net 26 "Net-(JP2-Pad15)")
  (net 27 "Net-(JP2-Pad16)")
  (net 28 "Net-(JP2-Pad17)")
  (net 29 "Net-(JP2-Pad18)")
  (net 30 "Net-(REF1-Pad2)")
  (net 31 "Net-(REF1-Pad1)")
  (net 32 "Net-(REF1-Pad30)")
  (net 33 "Net-(REF1-Pad26)")
  (net 34 "Net-(REF1-Pad25)")
  (net 35 "Net-(REF1-Pad24)")
  (net 36 "Net-(REF1-Pad23)")
  (net 37 "Net-(REF1-Pad18)")
  (net 38 "Net-(REF1-Pad17)")
  (net 39 "Net-(REF1-Pad6)")
  (net 40 "Net-(JP2-Pad3)")
  (net 41 "Net-(JP2-Pad10)")
  (net 42 "Net-(JP2-Pad11)")
  (net 43 "Net-(JP2-Pad12)")
  (net 44 "Net-(JP2-Pad13)")
  (net 45 IRQ)
  (net 46 "Net-(JP3-Pad1)")
  (net 47 "Net-(REF3-Pad202)")
  (net 48 "Net-(REF3-Pad218)")
  (net 49 "Net-(REF3-Pad216)")
  (net 50 "Net-(REF3-Pad214)")
  (net 51 "Net-(REF3-Pad212)")
  (net 52 "Net-(REF3-Pad206)")
  (net 53 "Net-(REF3-Pad208)")
  (net 54 "Net-(REF3-Pad207)")
  (net 55 "Net-(REF3-Pad205)")
  (net 56 "Net-(REF3-Pad211)")
  (net 57 "Net-(REF3-Pad213)")
  (net 58 "Net-(REF3-Pad215)")
  (net 59 "Net-(REF3-Pad217)")
  (net 60 "Net-(REF3-Pad119)")
  (net 61 "Net-(REF3-Pad117)")
  (net 62 "Net-(REF3-Pad115)")
  (net 63 "Net-(REF3-Pad113)")
  (net 64 "Net-(REF3-Pad103)")
  (net 65 "Net-(REF3-Pad105)")
  (net 66 "Net-(REF3-Pad107)")
  (net 67 "Net-(REF3-Pad110)")
  (net 68 "Net-(REF3-Pad109)")
  (net 69 "Net-(REF3-Pad108)")
  (net 70 "Net-(REF3-Pad106)")
  (net 71 "Net-(REF3-Pad104)")
  (net 72 "Net-(REF3-Pad114)")
  (net 73 "Net-(REF3-Pad116)")
  (net 74 "Net-(REF3-Pad118)")
  (net 75 "Net-(REF3-Pad120)")
  (net_class Default "Dit is de standaard class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3.3V)
    (add_net ETH-MISO)
    (add_net ETH-MOSI)
    (add_net ETH-NSS)
    (add_net ETH-SCK)
    (add_net FLASH_CSN)
    (add_net GND)
    (add_net IRQ)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(JP2-Pad10)")
    (add_net "Net-(JP2-Pad11)")
    (add_net "Net-(JP2-Pad12)")
    (add_net "Net-(JP2-Pad13)")
    (add_net "Net-(JP2-Pad15)")
    (add_net "Net-(JP2-Pad16)")
    (add_net "Net-(JP2-Pad17)")
    (add_net "Net-(JP2-Pad18)")
    (add_net "Net-(JP2-Pad3)")
    (add_net "Net-(JP2-Pad5)")
    (add_net "Net-(JP2-Pad7)")
    (add_net "Net-(JP2-Pad8)")
    (add_net "Net-(JP3-Pad1)")
    (add_net "Net-(REF1-Pad1)")
    (add_net "Net-(REF1-Pad17)")
    (add_net "Net-(REF1-Pad18)")
    (add_net "Net-(REF1-Pad2)")
    (add_net "Net-(REF1-Pad23)")
    (add_net "Net-(REF1-Pad24)")
    (add_net "Net-(REF1-Pad25)")
    (add_net "Net-(REF1-Pad26)")
    (add_net "Net-(REF1-Pad30)")
    (add_net "Net-(REF1-Pad6)")
    (add_net "Net-(REF3-Pad103)")
    (add_net "Net-(REF3-Pad104)")
    (add_net "Net-(REF3-Pad105)")
    (add_net "Net-(REF3-Pad106)")
    (add_net "Net-(REF3-Pad107)")
    (add_net "Net-(REF3-Pad108)")
    (add_net "Net-(REF3-Pad109)")
    (add_net "Net-(REF3-Pad110)")
    (add_net "Net-(REF3-Pad113)")
    (add_net "Net-(REF3-Pad114)")
    (add_net "Net-(REF3-Pad115)")
    (add_net "Net-(REF3-Pad116)")
    (add_net "Net-(REF3-Pad117)")
    (add_net "Net-(REF3-Pad118)")
    (add_net "Net-(REF3-Pad119)")
    (add_net "Net-(REF3-Pad120)")
    (add_net "Net-(REF3-Pad202)")
    (add_net "Net-(REF3-Pad205)")
    (add_net "Net-(REF3-Pad206)")
    (add_net "Net-(REF3-Pad207)")
    (add_net "Net-(REF3-Pad208)")
    (add_net "Net-(REF3-Pad211)")
    (add_net "Net-(REF3-Pad212)")
    (add_net "Net-(REF3-Pad213)")
    (add_net "Net-(REF3-Pad214)")
    (add_net "Net-(REF3-Pad215)")
    (add_net "Net-(REF3-Pad216)")
    (add_net "Net-(REF3-Pad217)")
    (add_net "Net-(REF3-Pad218)")
    (add_net RAD-CE)
    (add_net RAD-CSN)
    (add_net RAD-ERR)
    (add_net RAD-RX)
    (add_net RAD-TX)
    (add_net RESET)
    (add_net SCK)
    (add_net SEC-SDA)
    (add_net VCC)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 56D6E085)
    (at 126.10592 115.05184 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -1.11816 1.54408 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.9 90) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 11 +3.3V))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56C9D75D)
    (at 98.44278 134.13486)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.4351 -1.83896 270) (layer F.SilkS))
    (fp_text value 56K (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 SEC-SDA))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56C9D6AA)
    (at 89.59596 154.57932 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 1.21412 1.6129 450) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 RAD-TX))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56C9D6A6)
    (at 89.59596 149.79904 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1.21666 1.58496 450) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 RAD-RX))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56C9D6AF)
    (at 89.59596 145.17624 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 1.22936 1.55702 450) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 RAD-ERR))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56C9D6BE)
    (at 89.07 127.46 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 1.1938 1.52146 450) (layer F.SilkS))
    (fp_text value 1K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56C9D783)
    (at 103.28148 152.7048)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -1.41224 1.74752 270) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 FLASH_CSN))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 56D6E091)
    (at 127.16 118.3)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.82 0.22 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_5x5.3 (layer F.Cu) (tedit 56D6DFBD)
    (at 119.62 115.15 270)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.3")
    (attr smd)
    (fp_text reference C6 (at 3.94814 2.21908 450) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.81 270) (layer F.Fab))
    (pad 1 smd rect (at 2.19964 0 270) (size 2.99974 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 11 +3.3V))
    (pad 2 smd rect (at -2.19964 0 270) (size 2.99974 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/c_elec_5x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 56C9D767)
    (at 97.34296 137.63244 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 2.9337 0.16764 450) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 56C9D753)
    (at 105.11028 134.3914 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -1.08966 -1.5367 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_5x5.3 (layer F.Cu) (tedit 56C9D72C)
    (at 131.81584 114.32032 180)
    (descr "SMT capacitor, aluminium electrolytic, 5x5.3")
    (attr smd)
    (fp_text reference C9 (at 4.71678 -2.16154 270) (layer F.SilkS))
    (fp_text value 4uF7 (at 0 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at 2.19964 0 180) (size 2.99974 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 11 +3.3V))
    (pad 2 smd rect (at -2.19964 0 180) (size 2.99974 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/c_elec_5x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 56C9D73B)
    (at 128.68656 118.5672 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 2.59334 -0.28956 450) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 +3.3V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 56C9D789)
    (at 98.57232 152.72004 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 1.28524 -2.26314 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer B.Cu) (tedit 56C9E220)
    (at 120.03024 116.00688 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at -3.91668 -5.50926 450) (layer B.SilkS))
    (fp_text value AP1117D33 (at 0 -0.762 270) (layer B.Fab))
    (pad 4 smd rect (at 0 3.302 270) (size 3.6576 2.032) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0 -3.302 270) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 11 +3.3V))
    (pad 3 smd rect (at 2.286 -3.302 270) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -2.286 -3.302 270) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 56C9D76E)
    (at 100.52812 138.24712 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U3 (at -2.34696 -0.81026 270) (layer F.SilkS))
    (fp_text value ATSHA240A (at 0 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 9 SEC-SDA))
    (pad 2 smd rect (at 0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 3 smd rect (at 0 -1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer F.Cu) (tedit 56C9D77B)
    (at 101.19868 148.52904 90)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U4 (at 3.60426 -1.70434 270) (layer F.SilkS))
    (fp_text value AT25DF512C (at 0 1.27 90) (layer F.Fab))
    (pad 8 smd rect (at -1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 7 smd rect (at -0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 6 smd rect (at 0.635 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 13 SCK))
    (pad 5 smd rect (at 1.905 -3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 14 MOSI))
    (pad 4 smd rect (at 1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at 0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at -0.635 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 12 MISO))
    (pad 1 smd rect (at -1.905 3.175 90) (size 0.508 1.143) (layers F.Cu F.Paste F.Mask)
      (net 16 FLASH_CSN))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 56C9D6E3)
    (at 85.32622 153.48204 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D2 (at 1.97358 -2.35204 270) (layer F.SilkS))
    (fp_text value TX (at 0 2 180) (layer F.Fab))
    (pad 2 smd rect (at 2.16662 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 56C9D6DE)
    (at 85.29828 148.7043 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D3 (at 1.92532 -2.29362 450) (layer F.SilkS))
    (fp_text value RX (at 0 2 180) (layer F.Fab))
    (pad 2 smd rect (at 2.13614 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D3-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 56C9D6D8)
    (at 85.24748 144.07388 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D4 (at 1.87452 -2.25044 270) (layer F.SilkS))
    (fp_text value ERR (at 0 2 180) (layer F.Fab))
    (pad 2 smd rect (at 2.08534 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D4-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 56C9D6C5)
    (at 84.582 127.90932 180)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D5 (at 1.79578 -2.26314 270) (layer F.SilkS))
    (fp_text value PWR (at 0 2 180) (layer F.Fab))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(D5-Pad1)"))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module MySensors:NRF24L01_PA_LNA (layer F.Cu) (tedit 56D6DFAB)
    (at 127.83 122.15 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference REF2 (at 9.42 5.2 270) (layer F.SilkS))
    (fp_text value NRF24L01 (at 3.683 -3.429 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 +3.3V))
    (pad 1 thru_hole rect (at 0 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 RAD-CSN))
    (pad 3 thru_hole oval (at 2.54 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 RAD-CE))
    (pad 6 thru_hole oval (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 MOSI))
    (pad 5 thru_hole oval (at 5.08 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 SCK))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(JP3-Pad1)"))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 MISO))
    (pad 9 thru_hole circle (at -2.554 -34.6 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole circle (at 9.696 -34.6 270) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz 0.15 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Mounting_Holes:MountingHole_2-7mm (layer F.Cu) (tedit 56D31FC0)
    (at 141.5 113.5)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers))
  )
  (module Mounting_Holes:MountingHole_2-7mm (layer F.Cu) (tedit 56D31FB9)
    (at 83.5 113.5)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers))
  )
  (module Mounting_Holes:MountingHole_2-7mm (layer F.Cu) (tedit 56D31FD1)
    (at 141.5 162.5)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers))
  )
  (module Mounting_Holes:MountingHole_2-7mm (layer F.Cu) (tedit 56D31FC9)
    (at 83.5 162.5)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.0005) (layer F.SilkS) hide)
    (fp_text value MountingHole_3mm (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 56D6DFB0)
    (at 131.86 123.25 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 1.22 -1.72 270) (layer F.SilkS))
    (fp_text value 56K (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 +3.3V))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 RAD-CSN))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MySensors:Arduino_Nano (layer F.Cu) (tedit 56C9D799)
    (at 128.97104 145.51152 180)
    (descr "Through hole socket strip")
    (tags Arduino_Nano)
    (fp_text reference REF1 (at 38.33368 -17.76984 450) (layer F.SilkS))
    (fp_text value Arduino_Nano (at 28.523 -0.635 270) (layer F.Fab))
    (pad 15 thru_hole oval (at 35.56 -17.78 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 ETH-MISO))
    (pad 14 thru_hole oval (at 35.56 -15.24 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 ETH-MOSI))
    (pad 13 thru_hole oval (at 35.56 -12.7 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 ETH-NSS))
    (pad 12 thru_hole oval (at 35.56 -10.16 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 RAD-TX))
    (pad 11 thru_hole oval (at 35.56 -7.62 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 RAD-RX))
    (pad 10 thru_hole oval (at 35.56 -5.08 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 RAD-ERR))
    (pad 9 thru_hole oval (at 35.56 -2.54 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 RAD-CSN))
    (pad 8 thru_hole oval (at 35.56 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 RAD-CE))
    (pad 7 thru_hole oval (at 35.56 2.54 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 FLASH_CSN))
    (pad 6 thru_hole oval (at 35.56 5.08 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(REF1-Pad6)"))
    (pad 5 thru_hole oval (at 35.56 7.62 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 IRQ))
    (pad 4 thru_hole oval (at 35.56 10.16 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 35.56 12.7 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 RESET))
    (pad 2 thru_hole oval (at 35.56 15.24 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(REF1-Pad2)"))
    (pad 1 thru_hole rect (at 35.56 17.78 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(REF1-Pad1)"))
    (pad 30 thru_hole oval (at 20.32 17.78 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(REF1-Pad30)"))
    (pad 29 thru_hole oval (at 20.32 15.24 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 28 thru_hole oval (at 20.32 12.7 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 RESET))
    (pad 27 thru_hole oval (at 20.32 10.16 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 26 thru_hole oval (at 20.32 7.62 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(REF1-Pad26)"))
    (pad 25 thru_hole oval (at 20.32 5.08 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(REF1-Pad25)"))
    (pad 24 thru_hole oval (at 20.32 2.54 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(REF1-Pad24)"))
    (pad 23 thru_hole oval (at 20.32 0 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(REF1-Pad23)"))
    (pad 22 thru_hole oval (at 20.32 -2.54 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 SEC-SDA))
    (pad 21 thru_hole oval (at 20.32 -5.08 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 MISO))
    (pad 20 thru_hole oval (at 20.32 -7.62 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 MOSI))
    (pad 19 thru_hole oval (at 20.32 -10.16 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 SCK))
    (pad 18 thru_hole oval (at 20.32 -12.7 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(REF1-Pad18)"))
    (pad 17 thru_hole oval (at 20.32 -15.24 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(REF1-Pad17)"))
    (pad 16 thru_hole oval (at 20.32 -17.78 270) (size 1.7272 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 ETH-SCK))
  )
  (module MySensors:Socket_Strip_Straight_2x09_mirrored (layer F.Cu) (tedit 56D6E0AF)
    (at 88.5444 114.9477)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference JP2 (at -0.0344 2.6023) (layer F.SilkS))
    (fp_text value CONN_02x9 (at 2.54 -5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 +3.3V))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "Net-(JP2-Pad3)"))
    (pad 4 thru_hole oval (at 2.54 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 5 thru_hole oval (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 "Net-(JP2-Pad5)"))
    (pad 6 thru_hole oval (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 "Net-(JP2-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 "Net-(JP2-Pad8)"))
    (pad 9 thru_hole oval (at 10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 "Net-(JP2-Pad10)"))
    (pad 11 thru_hole oval (at 12.7 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 "Net-(JP2-Pad11)"))
    (pad 12 thru_hole oval (at 12.7 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 "Net-(JP2-Pad12)"))
    (pad 13 thru_hole oval (at 15.24 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 44 "Net-(JP2-Pad13)"))
    (pad 14 thru_hole oval (at 15.24 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 17.78 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 "Net-(JP2-Pad15)"))
    (pad 16 thru_hole oval (at 17.78 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 "Net-(JP2-Pad16)"))
    (pad 17 thru_hole oval (at 20.32 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 "Net-(JP2-Pad17)"))
    (pad 18 thru_hole oval (at 20.32 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 "Net-(JP2-Pad18)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x09.wrl
      (at (xyz 0.4 0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_FSMSM (layer F.Cu) (tedit 555C8B1B)
    (at 85.41 135.87 270)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SW1 (at 0.01011 -2.60022 270) (layer F.SilkS))
    (fp_text value SW_PUSH (at 0.01011 -0.00022 270) (layer F.Fab))
    (pad 1 smd rect (at -4.60243 -0.00232 270) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 4.60243 0.00232 270) (size 2.18 1.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(REF1-Pad6)"))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 88.39 121.46 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:c_elec_6.3x5.3 (layer F.Cu) (tedit 55725E31)
    (at 95.33 120.51 180)
    (descr "SMT capacitor, aluminium electrolytic, 6.3x5.3")
    (attr smd)
    (fp_text reference C1 (at 0 -4.445 180) (layer F.SilkS))
    (fp_text value 47uF (at 0 4.445 180) (layer F.Fab))
    (pad 1 smd rect (at 2.75082 0 180) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 2 smd rect (at -2.75082 0 180) (size 3.59918 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/c_elec_6.3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MySensors:Jumper_1x2 (layer F.Cu) (tedit 56D81A25)
    (at 118 131.96 180)
    (fp_text reference JP3 (at 1.11 -2.72 270) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 -2.15 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.9 0 180) (size 1.5 2) (layers F.Cu F.Paste F.Mask)
      (net 45 IRQ))
    (pad 1 smd rect (at -0.9 0 180) (size 1.5 2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(JP3-Pad1)"))
  )
  (module MySensors:WIZ811MJ (layer F.Cu) (tedit 56D70ED8)
    (at 112.37 134.33 270)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference REF3 (at 1.74 1.14 450) (layer F.SilkS))
    (fp_text value WIZ811MJ (at 12.59 -19.57 270) (layer F.Fab))
    (pad 202 thru_hole oval (at 23.73 -31.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(REF3-Pad202)"))
    (pad 102 thru_hole oval (at 3.81 -31.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 ETH-MISO))
    (pad "" np_thru_hole circle (at 21 -4 180) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
    (pad 220 thru_hole oval (at 23.73 -9 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 218 thru_hole oval (at 23.73 -11.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(REF3-Pad218)"))
    (pad 216 thru_hole oval (at 23.73 -14.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(REF3-Pad216)"))
    (pad 214 thru_hole oval (at 23.73 -16.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(REF3-Pad214)"))
    (pad 212 thru_hole oval (at 23.73 -19.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(REF3-Pad212)"))
    (pad 204 thru_hole oval (at 23.73 -29.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 ETH-NSS))
    (pad 206 thru_hole oval (at 23.73 -26.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(REF3-Pad206)"))
    (pad 208 thru_hole oval (at 23.73 -24.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(REF3-Pad208)"))
    (pad 209 thru_hole oval (at 21.19 -21.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 210 thru_hole oval (at 23.73 -21.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 207 thru_hole oval (at 21.19 -24.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(REF3-Pad207)"))
    (pad 205 thru_hole oval (at 21.19 -26.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(REF3-Pad205)"))
    (pad 203 thru_hole oval (at 21.19 -29.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 ETH-SCK))
    (pad 201 thru_hole rect (at 21.19 -31.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 +3.3V))
    (pad 211 thru_hole oval (at 21.19 -19.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(REF3-Pad211)"))
    (pad 213 thru_hole oval (at 21.19 -16.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(REF3-Pad213)"))
    (pad 215 thru_hole oval (at 21.19 -14.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(REF3-Pad215)"))
    (pad 217 thru_hole oval (at 21.19 -11.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(REF3-Pad217)"))
    (pad 219 thru_hole oval (at 21.19 -9 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 119 thru_hole oval (at 1.27 -9 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(REF3-Pad119)"))
    (pad 117 thru_hole oval (at 1.27 -11.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(REF3-Pad117)"))
    (pad 115 thru_hole oval (at 1.27 -14.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(REF3-Pad115)"))
    (pad 113 thru_hole oval (at 1.27 -16.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(REF3-Pad113)"))
    (pad 111 thru_hole oval (at 1.27 -19.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 101 thru_hole rect (at 1.27 -31.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 ETH-MOSI))
    (pad 103 thru_hole oval (at 1.27 -29.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(REF3-Pad103)"))
    (pad 105 thru_hole oval (at 1.27 -26.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(REF3-Pad105)"))
    (pad 107 thru_hole oval (at 1.27 -24.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(REF3-Pad107)"))
    (pad 110 thru_hole oval (at 3.81 -21.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(REF3-Pad110)"))
    (pad 109 thru_hole oval (at 1.27 -21.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(REF3-Pad109)"))
    (pad 108 thru_hole oval (at 3.81 -24.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(REF3-Pad108)"))
    (pad 106 thru_hole oval (at 3.81 -26.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(REF3-Pad106)"))
    (pad 104 thru_hole oval (at 3.81 -29.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(REF3-Pad104)"))
    (pad 112 thru_hole oval (at 3.81 -19.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 +3.3V))
    (pad 114 thru_hole oval (at 3.81 -16.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(REF3-Pad114)"))
    (pad 116 thru_hole oval (at 3.81 -14.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(REF3-Pad116)"))
    (pad 118 thru_hole oval (at 3.81 -11.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(REF3-Pad118)"))
    (pad 120 thru_hole oval (at 3.81 -9 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(REF3-Pad120)"))
    (pad "" np_thru_hole circle (at 4 -4 180) (size 3 3) (drill 3) (layers *.Cu *.Mask F.SilkS))
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 54EA0A4B)
    (at 114.52 125.16 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference JP1 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 MISO))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 MOSI))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text IRQ (at 119.21 135.71 90) (layer F.SilkS))
  (gr_text "© R. Bisschops" (at 152.9 114.9) (layer F.SilkS))
  (gr_text "Licensed under \nCERN OHL v.1.2" (at 154.76 116.23) (layer F.SilkS))
  (gr_line (start 80 166) (end 165 166) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165 110) (end 165 166) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80 110) (end 80 166) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80 110) (end 165 110) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text TX (at 81.36128 153.61412 90) (layer F.SilkS))
  (gr_text RX (at 81.36128 148.6408 90) (layer F.SilkS))
  (gr_text ERR (at 81.36128 143.94688 90) (layer F.SilkS))
  (gr_text PWR (at 81.36128 127.88138 90) (layer F.SilkS))
  (gr_text INCLUSION (at 81.38 135.71 90) (layer F.SilkS))
  (gr_text "MySensors Gateway Rev. 0.8" (at 155.11 112.68) (layer B.Cu))
  (gr_text "MySensors Gateway Rev. 0.8" (at 155.11 112.68) (layer F.Cu))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.95776 110.02772) (xy 164.95776 166.01948) (xy 79.96428 166.01948) (xy 80.020104 110.02772) (xy 164.95776 110.02772)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 79.99222 110.02772) (xy 80.02016 109.97184) (xy 80.020104 110.02772) (xy 79.99222 110.02772)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.02016 109.97184) (xy 165.00348 110.00232) (xy 165.01364 166.01948) (xy 79.96428 166.01948) (xy 80.02016 109.97184)
      )
    )
  )
)
