(kicad_pcb (version 4) (host pcbnew 4.0.0-rc2-stable)
  (general
    (links 97)
    (no_connects 1)
    (area 72.824999 97.124999 112.975001 145.275001)
    (thickness 1.6)
    (drawings 75)
    (tracks 558)
    (zones 0)
    (modules 50)
    (nets 47)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.21)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.21)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 4.064 4.064)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 72.9 145.2)
    (grid_origin 30 142)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /DTR)
  (net 2 /RESET)
  (net 3 +12V)
  (net 4 GND)
  (net 5 /X1)
  (net 6 /X2)
  (net 7 VCC)
  (net 8 /A0)
  (net 9 "Net-(C11-Pad1)")
  (net 10 "Net-(D1-Pad1)")
  (net 11 "Net-(D1-Pad2)")
  (net 12 /12V_relay)
  (net 13 "Net-(D3-Pad1)")
  (net 14 "Net-(D3-Pad2)")
  (net 15 "Net-(D4-Pad1)")
  (net 16 "Net-(D4-Pad2)")
  (net 17 "Net-(F1-Pad2)")
  (net 18 "Net-(F1-Pad1)")
  (net 19 /D3)
  (net 20 "Net-(IC1-Pad2)")
  (net 21 "Net-(IC1-Pad9)")
  (net 22 /D6)
  (net 23 /D7)
  (net 24 /D8)
  (net 25 "/D9(CE)")
  (net 26 "/D10(SS)")
  (net 27 "/D11(MOSI)")
  (net 28 "/D12(MISO)")
  (net 29 "/D13(SCK)")
  (net 30 "Net-(IC1-Pad19)")
  (net 31 "Net-(IC1-Pad22)")
  (net 32 /A1)
  (net 33 /A2)
  (net 34 "Net-(IC1-Pad26)")
  (net 35 "Net-(IC1-Pad27)")
  (net 36 "Net-(IC1-Pad28)")
  (net 37 /RX)
  (net 38 /TX)
  (net 39 "Net-(IC1-Pad32)")
  (net 40 "Net-(P1-Pad1)")
  (net 41 "Net-(P3-Pad1)")
  (net 42 "Net-(P6-Pad8)")
  (net 43 "Net-(Q1-Pad2)")
  (net 44 "Net-(Q2-Pad2)")
  (net 45 "Net-(Q3-Pad2)")
  (net 46 "Net-(F2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(F2-Pad1)")
  )
  (net_class 12V ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net /12V_relay)
  )
  (net_class 230V ""
    (clearance 2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class LinePower ""
    (clearance 2)
    (trace_width 4)
    (via_dia 2)
    (via_drill 1)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (net_class Vcc ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net VCC)
  )
  (net_class gnd ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
  )
  (net_class signal ""
    (clearance 0.2)
    (trace_width 0.21)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net "/D10(SS)")
    (add_net "/D11(MOSI)")
    (add_net "/D12(MISO)")
    (add_net "/D13(SCK)")
    (add_net /D3)
    (add_net /D6)
    (add_net /D7)
    (add_net /D8)
    (add_net "/D9(CE)")
    (add_net /DTR)
    (add_net /RESET)
    (add_net /RX)
    (add_net /TX)
    (add_net /X1)
    (add_net /X2)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad32)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P6-Pad8)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q3-Pad2)")
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 565E2189)
    (at 88.3 98.6 270)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at -0.5 3.2 360) (layer F.SilkS))
    (fp_text value "" (at 1.25 3.8 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +12V))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D8_L11.5_P3.5 (layer F.Cu) (tedit 565E20E5)
    (at 89.7 110.3)
    (descr "Radial Electrolytic Capacitor Diameter 8mm x Length 11.5mm, Pitch 3.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C7 (at 1.7 -0.1) (layer F.SilkS))
    (fp_text value "" (at 1.75 5.3) (layer F.Fab))
    (pad 2 thru_hole circle (at 3.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 VCC))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D8_L11.5_P3.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Varistors:RV_Disc_D12_W3.9_P7.5 (layer F.Cu) (tedit 56578E27)
    (at 86.6 144 180)
    (tags "varistor SIOV")
    (fp_text reference VR1 (at 3.8 1.5 180) (layer F.SilkS))
    (fp_text value VR (at 3.6 -0.3 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(F2-Pad1)"))
    (pad 2 thru_hole circle (at 7.7 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P3-Pad1)"))
  )
  (module Relays_ThroughHole:Relay_SANYOU_SRD_Series_Form_C (layer F.Cu) (tedit 565CC18D)
    (at 105.082 122.593 270)
    (descr "relay, Sanyou SRD series Form C")
    (fp_text reference RELAY1 (at 9.3 5.1 270) (layer F.SilkS))
    (fp_text value "" (at 8.1 -3.2 270) (layer F.Fab))
    (pad 4 thru_hole circle (at 1.95 6.05) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /12V_relay))
    (pad 1 thru_hole circle (at 14.15 6.05) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 18 "Net-(F1-Pad1)"))
    (pad 5 thru_hole circle (at 1.95 -5.95) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(D1-Pad1)"))
    (pad 3 thru_hole circle (at 0 0) (size 2.3 2.3) (drill 1.3) (layers *.Cu *.Mask)
      (net 40 "Net-(P1-Pad1)"))
    (model Relays_ThroughHole.3dshapes/Relay_SANYOU_SRD_Series_Form_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 565E2295)
    (at 108.89 100.81 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference SW1 (at -2.01 2.81 360) (layer F.SilkS))
    (fp_text value "" (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.397 1.397) (drill 0.8198) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole circle (at 0 1.84 180) (size 1.397 1.397) (drill 0.8198) (layers *.Cu *.Mask F.SilkS)
      (net 19 /D3))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_radios:NRF24L01 (layer F.Cu) (tedit 565E2267)
    (at 112.829 112.433 270)
    (descr NRF24L01)
    (tags "nRF 24 NRF24L01 NRF24L01+")
    (fp_text reference P6 (at -1.016 -1.016 270) (layer F.SilkS) hide)
    (fp_text value "" (at -8.382 7.112 270) (layer F.Fab) hide)
    (pad 7 thru_hole oval (at -9.144 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 "/D12(MISO)"))
    (pad 8 thru_hole oval (at -9.144 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(P6-Pad8)"))
    (pad 5 thru_hole oval (at -6.604 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "/D13(SCK)"))
    (pad 6 thru_hole oval (at -6.604 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 "/D11(MOSI)"))
    (pad 3 thru_hole oval (at -4.064 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "/D9(CE)"))
    (pad 4 thru_hole oval (at -4.064 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 "/D10(SS)"))
    (pad 1 thru_hole rect (at -1.524 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole oval (at -1.524 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 VCC))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0.442))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model mysensors.3dshapes/nrf24l01.wrl
      (at (xyz -0.3 -0.5669999999999999 0.475))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz -0.22 -0.51 0.509))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_hc-49s.wrl
      (at (xyz -0.5 -0.475 0.51))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer B.Cu) (tedit 565E2358)
    (at 98.01 120.45 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D1 (at -0.65 -2.31 90) (layer B.SilkS))
    (fp_text value LED (at 1.3 2.9 90) (layer B.Fab))
    (fp_text user K (at -1.55 -0.61 90) (layer B.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 10 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.7 1.7) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 11 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wire_Connections_Bridges:WireConnection_0.80mmDrill_ThinPad (layer F.Cu) (tedit 565E2522)
    (at 110.4 120.4)
    (descr "WireConnection with thin pad and 0.8mm drill")
    (fp_text reference JMP1 (at 4.8514 0.2032) (layer F.SilkS) hide)
    (fp_text value "" (at 5.08 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.8001) (layers *.Cu *.Mask F.SilkS))
  )
  (module Crystals:Crystal_Round_Vertical_2mm (layer F.Cu) (tedit 565E1F10)
    (at 105.63 100.04)
    (descr "Crystal, Quarz, Rundgehaeuse, round, NC26LF, vertical, stehend, Uhrenquarz, Diam. 2mm,")
    (tags "Crystal, Quarz, Rundgehaeuse, round, NC26LF, vertical, stehend, Uhrenquarz, Diam. 2mm,")
    (fp_text reference Y1 (at 0.97 -1.54) (layer F.SilkS))
    (fp_text value "" (at 0 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at -0.7493 0) (size 1.00076 1.00076) (drill 0.59944) (layers *.Cu *.Mask F.SilkS)
      (net 5 /X1))
    (pad 2 thru_hole circle (at 0.7493 0) (size 1.00076 1.00076) (drill 0.59944) (layers *.Cu *.Mask F.SilkS)
      (net 6 /X2))
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 565E227B)
    (at 109.2 119.5)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 2.9 1) (layer F.SilkS))
    (fp_text value "" (at 6.527 -0.291) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 90) (size 1.00076 1.00076) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(Q1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.00076 1.00076) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.00076 1.00076) (drill 0.6) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(D1-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D6_P5 (layer F.Cu) (tedit 565E225D)
    (at 102.4 117.6)
    (descr "Capacitor 6mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference F3 (at 2.4 -1.1) (layer F.SilkS))
    (fp_text value "" (at 2.5 3.5) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 +12V))
    (pad 2 thru_hole circle (at 5 0) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 12 /12V_relay))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01 (layer F.Cu) (tedit 565E229A)
    (at 111.29 100.73)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference P7 (at 3.8 -0.2) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /RESET))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D6_P5 (layer B.Cu) (tedit 565E2376)
    (at 90.9 133.5 90)
    (descr "Capacitor 6mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference F2 (at 2.7 0 90) (layer B.SilkS))
    (fp_text value "" (at 2.6 -1.5 90) (layer B.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 46 "Net-(F2-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask B.SilkS)
      (net 17 "Net-(F1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.098425 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_SemiClosed_Casing10x25mm (layer F.Cu) (tedit 565E2585)
    (at 92.2 131.9 270)
    (descr "Fuseholder, 5x20, Semi closed, horizontal, Casing 10x25mm,")
    (tags "Fuseholder, 5x20, Semi closed, horizontal, Casing 10x25mm, Sicherungshalter, halbgeschlossen,")
    (fp_text reference F1 (at 7.6 -1.2 270) (layer F.SilkS))
    (fp_text value 0.1A (at 0.1 1.2 270) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 11.00074 0 180) (size 2.49936 4.0005) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(F1-Pad2)"))
    (pad 1 thru_hole oval (at -11.00074 0 180) (size 2.49936 4.0005) (drill 1.50114) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(F1-Pad1)"))
  )
  (module YS-12V400-B (layer F.Cu) (tedit 565E258C)
    (at 80.444 138.341 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference U1 (at -1.759 1.256 180) (layer F.SilkS))
    (fp_text value HX-12V400X (at 18.7 1.6 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(F2-Pad1)"))
    (pad 1 thru_hole circle (at -0.1 -5.2 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(F2-Pad1)"))
    (pad 3 thru_hole oval (at 37.598 0.002 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +12V))
    (pad 4 thru_hole oval (at 37.598 5.068 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(F2-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_2x02.wrl
      (at (xyz 0.05 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 565E2598)
    (at 99.2 111.21 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D3 (at 3.3 -1.99 180) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9 180) (layer F.Fab) hide)
    (fp_text user K (at -0.5 -1.79 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 565E20D7)
    (at 89.1 115.5 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D4 (at 3.4 2 180) (layer F.SilkS))
    (fp_text value "" (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -0.7 2 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(D4-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer B.Cu) (tedit 565E230B)
    (at 100.637 104.051 270)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at -0.051 0.037 360) (layer B.SilkS))
    (fp_text value "" (at 0 -6.05 270) (layer B.Fab))
    (pad 1 smd rect (at -4.25 2.8 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 19 /D3))
    (pad 2 smd rect (at -4.25 2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -4.25 1.2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 4 smd rect (at -4.25 0.4 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (pad 5 smd rect (at -4.25 -0.4 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 6 smd rect (at -4.25 -1.2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (pad 7 smd rect (at -4.25 -2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 /X1))
    (pad 8 smd rect (at -4.25 -2.8 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 6 /X2))
    (pad 9 smd rect (at -2.8 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(IC1-Pad9)"))
    (pad 10 smd rect (at -2 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 22 /D6))
    (pad 11 smd rect (at -1.2 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 23 /D7))
    (pad 12 smd rect (at -0.4 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 24 /D8))
    (pad 13 smd rect (at 0.4 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 25 "/D9(CE)"))
    (pad 14 smd rect (at 1.2 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 26 "/D10(SS)"))
    (pad 15 smd rect (at 2 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 27 "/D11(MOSI)"))
    (pad 16 smd rect (at 2.8 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 28 "/D12(MISO)"))
    (pad 17 smd rect (at 4.25 -2.8 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 29 "/D13(SCK)"))
    (pad 18 smd rect (at 4.25 -2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (pad 19 smd rect (at 4.25 -1.2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.25 -0.4 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C11-Pad1)"))
    (pad 21 smd rect (at 4.25 0.4 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (pad 22 smd rect (at 4.25 1.2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.25 2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /A0))
    (pad 24 smd rect (at 4.25 2.8 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 32 /A1))
    (pad 25 smd rect (at 2.8 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 33 /A2))
    (pad 26 smd rect (at 2 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 34 "Net-(IC1-Pad26)"))
    (pad 27 smd rect (at 1.2 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(IC1-Pad27)"))
    (pad 28 smd rect (at 0.4 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(IC1-Pad28)"))
    (pad 29 smd rect (at -0.4 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 /RESET))
    (pad 30 smd rect (at -1.2 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 37 /RX))
    (pad 31 smd rect (at -2 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 38 /TX))
    (pad 32 smd rect (at -2.8 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 39 "Net-(IC1-Pad32)"))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:1pin (layer F.Cu) (tedit 565E25C1)
    (at 108.003 142.659)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P1 (at 0 -3.048) (layer F.SilkS))
    (fp_text value AC_out (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 2.2) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(P1-Pad1)"))
  )
  (module Connect:1pin (layer F.Cu) (tedit 565E25BB)
    (at 100.3 142.6)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P2 (at 0 -3.048) (layer F.SilkS))
    (fp_text value AC_in (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 2.2) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(F1-Pad1)"))
  )
  (module Connect:1pin (layer F.Cu) (tedit 565E25B3)
    (at 76 142.8)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference P3 (at -2.1 -2.6) (layer F.SilkS))
    (fp_text value AC_in (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.064 4.064) (drill 2.2) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(P3-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 565E226C)
    (at 98.605 115.1 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -0.2 15.495 90) (layer F.SilkS) hide)
    (fp_text value "" (at 0 -3.1 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 VCC))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /RX))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /TX))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /DTR))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Discret:R1 (layer F.Cu) (tedit 565E221F)
    (at 102.8 112.3)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference TH1 (at 3.4 0.2) (layer F.SilkS))
    (fp_text value "" (at -1.143 2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.27 0) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /A1))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R1 (layer B.Cu) (tedit 565E2321)
    (at 95.6 115.8 60)
    (descr "Resistance verticale")
    (tags R)
    (fp_text reference TH2 (at 0.399038 -2.308846 60) (layer B.SilkS))
    (fp_text value "" (at -1.143 -2.54 60) (layer B.Fab))
    (pad 1 thru_hole circle (at -1.27 0 60) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask B.SilkS)
      (net 4 GND))
    (pad 2 thru_hole circle (at 1.27 0 60) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask B.SilkS)
      (net 33 /A2))
    (model Discret.3dshapes/R1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ab2_sot:AB2_SOT223 (layer F.Cu) (tedit 565E1E3B)
    (at 92.9 101.3 180)
    (fp_text reference U2 (at 0 -0.1 180) (layer F.SilkS))
    (fp_text value "" (at -0.069 -0.062 180) (layer F.SilkS))
    (pad 2 smd rect (at 0 -2.9 180) (size 3.25 2.15) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 1 smd rect (at -2.3 2.9 180) (size 0.95 2.15) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0 2.9 180) (size 0.95 2.15) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 3 smd rect (at 2.3 2.9 180) (size 0.95 2.15) (layers F.Cu F.Paste F.Mask)
      (net 3 +12V))
    (model ab2_sot/AB2_SOT223.x3d
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 565E21C3)
    (at 105.1 106.3 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.1 -0.4 180) (layer F.SilkS))
    (fp_text value "" (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /DTR))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /RESET))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 565A2FE9)
    (at 92.6 101.1)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 1.9) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 +12V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 565E1EE4)
    (at 102.5 99.8 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -1.9 0.3 360) (layer F.SilkS))
    (fp_text value "" (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 /X1))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 565E1EF9)
    (at 103.7 99.8 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -1.9 -0.7 360) (layer F.SilkS))
    (fp_text value "" (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 /X2))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 565E2315)
    (at 94.02 98.91)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -2.52 -0.61) (layer B.SilkS))
    (fp_text value "" (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 565E1E91)
    (at 100.2 100.3)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 0.3 1.3) (layer F.SilkS))
    (fp_text value "" (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 565E21B7)
    (at 102 108.1 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at 1.8 -0.2 180) (layer F.SilkS))
    (fp_text value "" (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /A0))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 565E1F7B)
    (at 103.2 108.1 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at -2.4 0.2 90) (layer F.SilkS))
    (fp_text value "" (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 565E1ECF)
    (at 99.8 104.4)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -1.3 -2.1) (layer F.SilkS))
    (fp_text value "" (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(Q2-Pad2)"))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 565E210D)
    (at 93.6 106.97)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -1.5 -1.37) (layer F.SilkS))
    (fp_text value "" (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(Q3-Pad2)"))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565E1E7C)
    (at 96.34 103.62)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0.06 1.28) (layer F.SilkS))
    (fp_text value "" (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 /RESET))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565E2254)
    (at 104.1 118.2 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -1 -1.6 180) (layer F.SilkS))
    (fp_text value "" (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /12V_relay))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565E212C)
    (at 97.83 108.19 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -0.59 -1.47 270) (layer F.SilkS))
    (fp_text value "" (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 /A1))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565E213A)
    (at 96.5 107.47 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -0.97 1.2 270) (layer F.SilkS))
    (fp_text value "" (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 /A2))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565E1EA9)
    (at 105 103.3)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -1.9 0.1) (layer F.SilkS))
    (fp_text value "" (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(Q2-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /D7))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565E21DA)
    (at 100.7 108.2 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 1.9 -0.1 270) (layer F.SilkS))
    (fp_text value "" (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /A0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565E2248)
    (at 105.8 118.1 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -1 1.5 180) (layer F.SilkS))
    (fp_text value "" (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /12V_relay))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /A0))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565E1F56)
    (at 105 104.7)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -2.4 0 180) (layer F.SilkS))
    (fp_text value "" (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(Q3-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /D8))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565E20F0)
    (at 89.7 108.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 2.4 0.5) (layer F.SilkS))
    (fp_text value "" (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +12V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565E1E99)
    (at 98.7 99.1 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 1.2 180) (layer F.SilkS))
    (fp_text value "" (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 /D3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565E20FC)
    (at 89.7 106.7)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at -0.3 -1.4) (layer F.SilkS))
    (fp_text value "" (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 +12V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:MiniMELF_Standard (layer B.Cu) (tedit 565E2347)
    (at 100.1 119.6 90)
    (descr "Diode Mini-MELF Standard")
    (tags "Diode Mini-MELF Standard")
    (attr smd)
    (fp_text reference D2 (at 0 1.95 90) (layer B.SilkS))
    (fp_text value "" (at 0 -3.81 90) (layer B.Fab))
    (fp_text user K (at -3.2 0.2 90) (layer B.SilkS))
    (fp_text user A (at 1.8 -1.95 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 12 /12V_relay))
    (pad 2 smd rect (at 1.75006 0 90) (size 1.30048 1.69926) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D1-Pad1)"))
    (model Diodes_SMD.3dshapes/MiniMELF_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2-5mm (layer F.Cu) (tedit 565E20BE)
    (at 92.9 114.2)
    (descr "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,5mm, No Annular, Kein Restring,")
    (fp_text reference H1 (at 0.1 -0.1) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565E1F1E)
    (at 105.02 108.22 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -0.02 -1.48 270) (layer F.SilkS))
    (fp_text value "" (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 /D6))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(Q1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 565E223D)
    (at 111.2 117.1 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.1 -0.1 180) (layer F.SilkS))
    (fp_text value "" (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(Q1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 112.9 143.7) (end 112.9 144.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 112.9 143.7) (end 111.9 143.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.9 142.7) (end 112.9 122.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 72.9 142.7) (end 72.9 137.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 72.9 145.2) (end 72.9 144.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.9 99.9) (end 112.9 121.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.9 98.5) (end 112.9 97.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.9 145.2) (end 112.9 144.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 104 138.8) (end 103.1 138.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 104 138.8) (end 104 137.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.8 119.5) (end 93.7 119.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.8 125.4) (end 93.8 119.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95 125.4) (end 95 118.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 94.4 125.4) (end 94.4 126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 94.4 125.4) (end 95 125.4) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 96.6 138.8) (end 96.6 137.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 96.6 138.8) (end 95.7 138.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 112.9 99.2) (end 112.9 99.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 112.9 99.2) (end 112.2 99.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 72.9 143.7) (end 72.9 142.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 72.9 143.7) (end 73.9 143.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.8 121.7) (end 102.2 121.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 101.8 122.8) (end 101.8 121.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 102.5 122.8) (end 102.5 123.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 102.5 122.8) (end 103.2 122.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107 122.9) (end 107 122.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 105.1 122.8) (end 105.1 120.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 105.1 122.8) (end 103.2 122.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 108.1 121.2) (end 112.9 121.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.8 133.9) (end 87.4 133.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.8 118.6) (end 87.8 133.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.9 118.6) (end 87.8 118.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.7 119.4) (end 92.9 118.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 93.3 116.9) (end 95 118.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 92.8 116.9) (end 93.3 116.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.8 116.9) (end 92.8 116.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.8 111.3) (end 87.8 116.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 72.9 145.2) (end 95.7 145.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 106.8 119.9) (end 108.1 121.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.6 119.9) (end 106.8 119.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 102.2 121.3) (end 103.6 119.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.9 122.9) (end 107 122.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.8 102.2) (end 79.3 102.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.8 111.3) (end 87.8 102.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.3 97.2) (end 112.9 97.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.9 145.2) (end 112.9 145.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.9 138.8) (end 104.9 145.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.1 145.2) (end 103.1 138.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.5 145.2) (end 103.1 145.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 97.5 138.8) (end 97.5 145.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.7 145.2) (end 95.7 138.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.4 137.1) (end 72.9 137.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.4 137.2) (end 76.4 137.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 76.4 140.1) (end 76.4 137.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.2 140.1) (end 76.4 140.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.2 137.8) (end 79.2 140.1) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.8 137.2) (end 79.2 137.8) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 83.3 137.2) (end 79.8 137.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.1 138) (end 83.3 137.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.1 140.2) (end 84.1 138) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.4 140.2) (end 84.1 140.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 87.4 133.9) (end 87.4 140.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 79.3 97.2) (end 79.3 102.2) (angle 90) (layer Edge.Cuts) (width 0.15))
)
