(kicad_pcb (version 20170123) (host pcbnew no-vcs-found-7664~57~ubuntu16.10.1)
  (general
    (links 20)
    (no_connects 0)
    (area 133.24144 100.4094 157.6038 126.958301)
    (thickness 1.6)
    (drawings 4)
    (tracks 63)
    (zones 0)
    (modules 12)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Manufacturing/))
  )
  (net 0 "")
  (net 1 "Net-(P1-Pad14)")
  (net 2 "Net-(P1-Pad13)")
  (net 3 "Net-(P1-Pad12)")
  (net 4 "Net-(P1-Pad11)")
  (net 5 "Net-(P1-Pad9)")
  (net 6 "Net-(P1-Pad2)")
  (net 7 "Net-(P1-Pad3)")
  (net 8 "Net-(P1-Pad5)")
  (net 9 "Net-(P1-Pad6)")
  (net 10 "Net-(P1-Pad7)")
  (net 11 "Net-(P1-Pad8)")
  (net 12 +12V)
  (net 13 GND)
  (net 14 "Net-(P3-Pad2)")
  (net 15 "Net-(P4-Pad2)")
  (net 16 "Net-(P1-Pad10)")
  (net 17 "Net-(Q1-Pad1)")
  (net 18 "Net-(Q2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P1-Pad10)")
    (add_net "Net-(P1-Pad11)")
    (add_net "Net-(P1-Pad12)")
    (add_net "Net-(P1-Pad13)")
    (add_net "Net-(P1-Pad14)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad5)")
    (add_net "Net-(P1-Pad6)")
    (add_net "Net-(P1-Pad7)")
    (add_net "Net-(P1-Pad8)")
    (add_net "Net-(P1-Pad9)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net GND)
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P4-Pad2)")
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58A81B69)
    (at 139.3698 117.9703)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 100k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(P1-Pad11)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 151.2316 117.9957 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 100k (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad12)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 145.4912 117.9703)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value C (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 +12V))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 151.2189 115.7351)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 27 (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P1-Pad12)"))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 139.3698 115.7224 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -2.1 180) (layer F.SilkS))
    (fp_text value 27 (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(P1-Pad11)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 145.4912 115.697)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -2.1) (layer F.SilkS))
    (fp_text value CP (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 12 +12V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 54E9291B)
    (at 139.7127 112.8776 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 -3.81 90) (layer F.SilkS))
    (fp_text value IRLML2502 (at 0 3.81 90) (layer F.Fab))
    (pad 3 smd rect (at 0 -1.50114 90) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P4-Pad2)"))
    (pad 2 smd rect (at 0.95 1.50114 90) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 1 smd rect (at -0.95 1.50114 90) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Q2-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:MYSX_2.3 (layer F.Cu) (tedit 57D06A80)
    (at 137.8331 124.1933 90)
    (descr "Through hole pin header")
    (tags "pin header MYSX 2.3")
    (fp_text reference P1 (at 0 -3.302 90) (layer F.SilkS))
    (fp_text value MYSX_2.4 (at 1.27 18.542 90) (layer F.SilkS))
    (fp_text user 2.3 (at 2.54 -3.302 90) (layer Cmts.User))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P1-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P1-Pad6)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P1-Pad5)"))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(P1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 +12V))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(P1-Pad9)"))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P1-Pad10)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(P1-Pad11)"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(P1-Pad12)"))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(P1-Pad13)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(P1-Pad14)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x07.wrl
      (at (xyz 0.05 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_connectors:TerminalBlock2.54mmx2-kcswalter (layer F.Cu) (tedit 5585791A)
    (at 139.1158 108.1405 90)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P4 (at 0 -4.50088 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 4.50088 90) (layer F.SilkS) hide)
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P4-Pad2)"))
    (pad 1 thru_hole rect (at 1.27 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 12 +12V))
    (model mysensors.3dshapes/w.lain.3dshapes/conn_mpt/mpt_0,5-2-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:TerminalBlock2.54mmx2-kcswalter (layer F.Cu) (tedit 5585791A)
    (at 145.288 106.8705 180)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P2 (at 0 -4.50088 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 4.50088 180) (layer F.SilkS) hide)
    (pad 2 thru_hole oval (at -1.27 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 1 thru_hole rect (at 1.27 0 180) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 12 +12V))
    (model mysensors.3dshapes/w.lain.3dshapes/conn_mpt/mpt_0,5-2-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:TerminalBlock2.54mmx2-kcswalter (layer F.Cu) (tedit 5585791A)
    (at 151.4856 108.1278 90)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference P3 (at 0 -4.50088 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 4.50088 90) (layer F.SilkS) hide)
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P3-Pad2)"))
    (pad 1 thru_hole rect (at 1.27 0 90) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 12 +12V))
    (model mysensors.3dshapes/w.lain.3dshapes/conn_mpt/mpt_0,5-2-2,54.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 54E9291B)
    (at 149.6949 112.9538 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -3.81 90) (layer F.SilkS))
    (fp_text value IRLML2502 (at 0 3.81 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 90) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 1.50114 90) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 13 GND))
    (pad 3 smd rect (at 0 -1.50114 90) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P3-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 154.5082 104.8258) (end 136.017 104.8258) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.017 104.8258) (end 136.017 125.9205) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154.5082 125.9205) (end 154.5082 104.8258) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 136.017 125.9205) (end 154.5082 125.9205) (layer Edge.Cuts) (width 0.15))
  (zone (net 13) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.0551 104.8639) (xy 154.686 104.8639) (xy 154.6098 125.7173) (xy 136.144 126.111)
      )
    )
  )
  (zone (net 12) (net_name +12V) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.017 110.9345) (xy 154.5082 110.9345) (xy 154.4701 104.8512) (xy 136.0297 104.902)
      )
    )
  )
)
