(kicad_pcb (version 4) (host pcbnew 4.0.2-4+6225~38~ubuntu14.04.1-stable)
  (general
    (links 30)
    (no_connects 3)
    (area 160.054999 106.108999 225.076101 184.366001)
    (thickness 1.6)
    (drawings 19)
    (tracks 199)
    (zones 0)
    (modules 9)
    (nets 24)
  )
  (page A4)
  (title_block
    (title Arduino_pro_mini_nrf24L01+_interposer)
    (company Ohotbar)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (user_trace_width 0.4)
    (trace_clearance 0.3)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.25)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.2 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 224.536 134.366)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x210c0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory plot/))
  )
  (net 0 "")
  (net 1 "Net-(IC1-Pad1)")
  (net 2 "Net-(IC1-Pad2)")
  (net 3 "Net-(IC1-Pad3)")
  (net 4 "Net-(IC1-Pad8)")
  (net 5 "Net-(IC1-Pad9)")
  (net 6 "Net-(IC1-Pad10)")
  (net 7 "Net-(IC1-Pad11)")
  (net 8 "Net-(IC1-Pad18)")
  (net 9 "Net-(IC1-Pad19)")
  (net 10 "Net-(IC1-Pad20)")
  (net 11 "Net-(IC1-Pad22)")
  (net 12 "Net-(IC1-Pad24)")
  (net 13 GND)
  (net 14 +3V3)
  (net 15 A0)
  (net 16 INT0)
  (net 17 INT1)
  (net 18 CE)
  (net 19 CSN/CS)
  (net 20 MOSI)
  (net 21 MISO)
  (net 22 SCK)
  (net 23 DS18B20)
  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net A0)
    (add_net CE)
    (add_net CSN/CS)
    (add_net DS18B20)
    (add_net GND)
    (add_net INT0)
    (add_net INT1)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad18)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
    (add_net SCK)
  )
  (net_class DIY_etch ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 1.2)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module mysensors_arduino:pro_mini (layer F.Cu) (tedit 56C8A26C)
    (at 209.4611 125.3236)
    (descr "IC, ARDUINO_PRO_MINI x 0,6\"")
    (tags "DIL ARDUINO PRO MINI")
    (fp_text reference IC1 (at -4.2291 2.9464) (layer F.SilkS))
    (fp_text value ArduinoProMini (at -0.6731 4.7244) (layer F.Fab))
    (pad 1 thru_hole oval (at -13.97 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole oval (at -11.43 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(IC1-Pad2)"))
    (pad 3 thru_hole oval (at -8.89 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole oval (at -6.35 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 5 thru_hole oval (at -3.81 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 16 INT0))
    (pad 6 thru_hole oval (at -1.27 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 17 INT1))
    (pad 7 thru_hole oval (at 1.27 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 23 DS18B20))
    (pad 8 thru_hole oval (at 3.81 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(IC1-Pad8)"))
    (pad 9 thru_hole oval (at 6.35 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(IC1-Pad9)"))
    (pad 10 thru_hole oval (at 8.89 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(IC1-Pad10)"))
    (pad 11 thru_hole oval (at 11.43 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(IC1-Pad11)"))
    (pad 12 thru_hole oval (at 13.97 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 18 CE))
    (pad 13 thru_hole oval (at 13.97 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 19 CSN/CS))
    (pad 14 thru_hole oval (at 11.43 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 20 MOSI))
    (pad 15 thru_hole oval (at 8.89 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 21 MISO))
    (pad 16 thru_hole oval (at 6.35 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 SCK))
    (pad 17 thru_hole oval (at 3.81 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 A0))
    (pad 18 thru_hole oval (at 1.27 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(IC1-Pad18)"))
    (pad 19 thru_hole oval (at -1.27 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(IC1-Pad19)"))
    (pad 20 thru_hole oval (at -3.81 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(IC1-Pad20)"))
    (pad 21 thru_hole oval (at -6.35 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 +3V3))
    (pad 22 thru_hole oval (at -8.89 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(IC1-Pad22)"))
    (pad 23 thru_hole oval (at -11.43 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 24 thru_hole oval (at -13.97 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(IC1-Pad24)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz -0.15 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.55 0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0 0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.25 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model mysensors.3dshapes/arduino_pro_mini.wrl
      (at (xyz -0.05 0 0.48))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model SMD_Packages.3dshapes/TQFP-32.wrl
      (at (xyz 0.05 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 315))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.3 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 0.3 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0.55 0.1 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0.25 0.2 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz -0.15 0.2 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (at (xyz -0.3 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (at (xyz 0.55 -0.175 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x06.wrl
      (at (xyz -0.65 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz -0.3 -0.05 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0.55 -0.125 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz -0.3 0.05 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (at (xyz -0.35 0.15 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (at (xyz -0.35 -0.15 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Housings_SOT-23_SOT-143_TSOT-6.3dshapes/SOT-23-5.wrl
      (at (xyz -0.4 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz -0.5 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_radios:NRF24L01 (layer F.Cu) (tedit 56C77769)
    (at 189.23 132.08 270)
    (descr NRF24L01)
    (tags "nRF 24 NRF24L01 NRF24L01+")
    (fp_text reference U1 (at -0.508 -1.016 270) (layer F.SilkS))
    (fp_text value NRF24L01 (at -4.572 -1.016 270) (layer F.Fab))
    (pad 7 thru_hole oval (at -9.144 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 MISO))
    (pad 8 thru_hole oval (at -9.144 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 INT0))
    (pad 5 thru_hole oval (at -6.604 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 SCK))
    (pad 6 thru_hole oval (at -6.604 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 MOSI))
    (pad 3 thru_hole oval (at -4.064 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 CE))
    (pad 4 thru_hole oval (at -4.064 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 CSN/CS))
    (pad 1 thru_hole rect (at -1.524 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 2 thru_hole oval (at -1.524 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0.442))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model mysensors.3dshapes/nrf24l01.wrl
      (at (xyz -0.3 -0.5669999999999999 0.475))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz -0.22 -0.51 0.509))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_hc-49s.wrl
      (at (xyz -0.5 -0.475 0.51))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x06 (layer F.Cu) (tedit 56C8A500)
    (at 179.07 131.572 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -2.54 -0.762 270) (layer F.SilkS))
    (fp_text value CONN_01X06 (at -2.54 2.794 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 INT1))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 INT0))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Rect_L4_W2.5_P2.5 (layer F.Cu) (tedit 56C77045)
    (at 199.39 120.65 270)
    (descr "Film Capacitor Length 4mm x Width 2.5mm, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 2.032 3.81 270) (layer F.SilkS))
    (fp_text value 0,1uF (at 1.016 2.286 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 15 A0))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56C9B638)
    (at 213.36 123.952 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R1 (at 7.493 0.762 180) (layer F.SilkS))
    (fp_text value 1M (at 3.683 0.508 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 A0))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 13 GND))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56C9B647)
    (at 203.2 120.904)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R2 (at 2.54 0) (layer F.SilkS))
    (fp_text value 470k (at 6.604 0.254) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 14 +3V3))
    (pad 2 thru_hole circle (at 10.16 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 15 A0))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x03 (layer F.Cu) (tedit 56C9B977)
    (at 185.166 119.634 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1 90) (layer F.SilkS))
    (fp_text value DS18B20 (at -0.254 -2.794 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 DS18B20))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 DS18B20))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 +3V3))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 +3V3))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x01 (layer F.Cu) (tedit 56C8A4F6)
    (at 193.294 120.65 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0 -5.1 270) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 8.128 0 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(IC1-Pad24)"))
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM10mm (layer F.Cu) (tedit 56C9B642)
    (at 217.297 127 180)
    (descr "Resistor, Axial,  RM 10mm, 1/3W")
    (tags "Resistor Axial RM 10mm 1/3W")
    (fp_text reference R3 (at 4.318 -0.127 180) (layer F.SilkS))
    (fp_text value 4k7 (at 7.239 -0.127 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 14 +3V3))
    (pad 2 thru_hole circle (at 10.16 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 23 DS18B20))
    (model Resistors_ThroughHole.3dshapes/Resistor_Horizontal_RM10mm.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text RAW (at 193.294 123.19 270) (layer F.Fab))
  (gr_text 1 (at 176.276 125.984 270) (layer F.Fab))
  (gr_text GND (at 177.038 122.428 270) (layer F.Fab))
  (gr_text GND (at 176.784 117.348 270) (layer F.Fab))
  (gr_text GND (at 176.784 127.254 270) (layer F.Fab))
  (gr_text Vcc (at 176.276 130.81 270) (layer F.Fab))
  (gr_text 0 (at 176.276 120.904 270) (layer F.Fab))
  (gr_text ohotbar (at 220.345 130.302 90) (layer F.Cu))
  (gr_text @gmail.com (at 222.25 132.08 90) (layer F.Cu))
  (gr_text Ver02 (at 220.726 125.476 90) (layer B.Cu))
  (gr_text interposer (at 222.758 125.222 90) (layer B.Cu))
  (gr_line (start 175.006 115.824) (end 175.006 134.62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text 1 (at 181.61 126.111 90) (layer B.Cu))
  (gr_text 0 (at 181.61 122.174 90) (layer B.Cu))
  (gr_text GND (at 184.15 129.032) (layer B.Cu))
  (gr_text Vcc (at 183.896 130.81) (layer B.Cu))
  (gr_line (start 175 115.824) (end 224.536 115.824) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 224.536 134.62) (end 175 134.62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 224.536 115.824) (end 224.536 134.62) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 13) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 224.536 115.824) (xy 224.536 134.367388) (xy 224.79 134.366) (xy 224.536 134.62) (xy 224.282086 134.621302)
        (xy 224.282 134.621388) (xy 224.282001 134.621303) (xy 175.006 134.874) (xy 175.006 115.57) (xy 224.536 115.824)
      )
    )
  )
  (zone (net 14) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 224.79 184.366) (xy 165.862 183.858) (xy 165.862 165.57) (xy 224.79 165.57) (xy 224.79 184.366)
      )
    )
  )
  (zone (net 14) (net_name +3V3) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 224.536 134.62) (xy 175.006 134.62) (xy 175.006 115.824) (xy 224.536 115.824) (xy 224.536 134.62)
      )
    )
  )
)
