(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 47)
    (no_connects 0)
    (area 104.924999 69.924999 155.075001 100.075001)
    (thickness 1.6)
    (drawings 44)
    (tracks 196)
    (zones 0)
    (modules 18)
    (nets 33)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 105 70)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory GerberExport/))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 +12V)
  (net 4 MISO)
  (net 5 SCK)
  (net 6 MOSI)
  (net 7 RST)
  (net 8 "Net-(P1-Pad2)")
  (net 9 "Net-(P1-Pad3)")
  (net 10 "Net-(P1-Pad4)")
  (net 11 "Net-(P1-Pad5)")
  (net 12 R)
  (net 13 G)
  (net 14 B)
  (net 15 W)
  (net 16 "Net-(U1-Pad8)")
  (net 17 CE)
  (net 18 CSN)
  (net 19 "Net-(IC1-Pad28)")
  (net 20 "Net-(IC1-Pad27)")
  (net 21 "Net-(IC1-Pad1)")
  (net 22 "Net-(IC1-Pad2)")
  (net 23 "Net-(IC1-Pad5)")
  (net 24 "Net-(IC1-Pad10)")
  (net 25 "Net-(IC1-Pad11)")
  (net 26 "Net-(IC1-Pad17)")
  (net 27 "Net-(IC1-Pad18)")
  (net 28 "Net-(IC1-Pad19)")
  (net 29 "Net-(IC1-Pad20)")
  (net 30 "Net-(IC1-Pad24)")
  (net 31 "Net-(IC1-Pad25)")
  (net 32 "Net-(IC1-Pad26)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net B)
    (add_net CE)
    (add_net CSN)
    (add_net G)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad17)")
    (add_net "Net-(IC1-Pad18)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad24)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad5)")
    (add_net "Net-(U1-Pad8)")
    (add_net R)
    (add_net RST)
    (add_net SCK)
    (add_net W)
  )
  (net_class "12V power" ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(P1-Pad5)")
  )
  (module mysensors_arduino:pro_mini (layer F.Cu) (tedit 55A3E6CB)
    (at 121.92 80.01)
    (descr "IC, ARDUINO_PRO_MINI x 0,6\"")
    (tags "DIL ARDUINO PRO MINI")
    (fp_text reference IC1 (at -13.97 10.16) (layer F.SilkS))
    (fp_text value ArduinoProMini (at 0 0) (layer F.Fab) hide)
    (pad 28 thru_hole oval (at 5.08 -5.08) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(IC1-Pad28)"))
    (pad 27 thru_hole oval (at 7.62 -5.08) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(IC1-Pad27)"))
    (pad 1 thru_hole oval (at -13.97 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole oval (at -11.43 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(IC1-Pad2)"))
    (pad 3 thru_hole oval (at -8.89 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 RST))
    (pad 4 thru_hole oval (at -6.35 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at -3.81 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(IC1-Pad5)"))
    (pad 6 thru_hole oval (at -1.27 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 12 R))
    (pad 7 thru_hole oval (at 1.27 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 17 CE))
    (pad 8 thru_hole oval (at 3.81 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 13 G))
    (pad 9 thru_hole oval (at 6.35 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 B))
    (pad 10 thru_hole oval (at 8.89 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(IC1-Pad10)"))
    (pad 11 thru_hole oval (at 11.43 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(IC1-Pad11)"))
    (pad 12 thru_hole oval (at 13.97 7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 W))
    (pad 13 thru_hole oval (at 13.97 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 18 CSN))
    (pad 14 thru_hole oval (at 11.43 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 MOSI))
    (pad 15 thru_hole oval (at 8.89 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 MISO))
    (pad 16 thru_hole oval (at 6.35 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 SCK))
    (pad 17 thru_hole oval (at 3.81 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(IC1-Pad17)"))
    (pad 18 thru_hole oval (at 1.27 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(IC1-Pad18)"))
    (pad 19 thru_hole oval (at -1.27 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(IC1-Pad19)"))
    (pad 20 thru_hole oval (at -3.81 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(IC1-Pad20)"))
    (pad 21 thru_hole oval (at -6.35 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 22 thru_hole oval (at -8.89 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 RST))
    (pad 23 thru_hole oval (at -11.43 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 24 thru_hole oval (at -13.97 -7.62) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(IC1-Pad24)"))
    (pad 25 thru_hole oval (at -2.54 -5.08) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(IC1-Pad25)"))
    (pad 26 thru_hole oval (at -5.08 -5.08) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(IC1-Pad26)"))
    (pad 27 thru_hole oval (at 13.97 -5.08) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(IC1-Pad27)"))
    (pad 28 thru_hole oval (at 13.97 -2.54) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(IC1-Pad28)"))
    (pad 29 thru_hole oval (at 13.97 0) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz -0.15 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.55 0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0 0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.25 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_arduino.3dshapes/arduino_pro_mini.wrl
      (at (xyz -0.05 0 0.48))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model SMD_Packages.3dshapes/TQFP-32.wrl
      (at (xyz 0.05 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 315))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.3 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 0.3 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0.55 0.1 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0.25 0.2 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz -0.15 0.2 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (at (xyz -0.3 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (at (xyz 0.55 -0.175 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x06.wrl
      (at (xyz -0.65 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz -0.3 -0.05 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0.55 -0.125 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz -0.3 0.05 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (at (xyz -0.35 0.15 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (at (xyz -0.35 -0.15 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz -0.4 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz -0.5 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_radios:NRF24L01 (layer F.Cu) (tedit 56F47B69)
    (at 143.51 85.09 270)
    (descr NRF24L01)
    (tags "nRF 24 NRF24L01 NRF24L01+")
    (fp_text reference U1 (at -1.016 -1.016 270) (layer F.SilkS) hide)
    (fp_text value NRF24L01 (at -8.382 7.112 270) (layer F.Fab) hide)
    (pad 7 thru_hole oval (at -9.144 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 MISO))
    (pad 8 thru_hole oval (at -9.144 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U1-Pad8)"))
    (pad 5 thru_hole oval (at -6.604 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 SCK))
    (pad 6 thru_hole oval (at -6.604 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 MOSI))
    (pad 3 thru_hole oval (at -4.064 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 CE))
    (pad 4 thru_hole oval (at -4.064 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 CSN))
    (pad 1 thru_hole rect (at -1.524 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 2 thru_hole oval (at -1.524 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0.442))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model mysensors.3dshapes/nrf24l01.wrl
      (at (xyz -0.3 -0.5669999999999999 0.475))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz -0.22 -0.51 0.509))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_hc-49s.wrl
      (at (xyz -0.5 -0.475 0.51))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeC_EIA-6032_HandSoldering (layer B.Cu) (tedit 56FE9A94)
    (at 149.352 86.614 180)
    (descr "Tantal Cap. , Size C, EIA-6032, Hand Soldering,")
    (tags "Tantal Cap. , Size C, EIA-6032, Hand Soldering,")
    (attr smd)
    (fp_text reference C2 (at -0.20066 3.29946 180) (layer B.SilkS) hide)
    (fp_text value 22uF (at 0.102 0.114 270) (layer B.Fab))
    (fp_text user + (at -4.048 2.214 180) (layer B.SilkS))
    (pad 2 smd rect (at 2.99974 0 180) (size 3.50012 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.99974 0 180) (size 3.50012 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeC_EIA-6032_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2.5 (layer F.Cu) (tedit 56F47BA6)
    (at 139.7 88.265)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 11mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 -3.8) (layer F.SilkS) hide)
    (fp_text value CP (at 1.25 3.8) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.5.wrl
      (at (xyz 0.049213 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connect:bornier5 (layer F.Cu) (tedit 56F47B35)
    (at 123.5 95)
    (descr "Bornier d'alimentation 4 pins")
    (tags DEV)
    (fp_text reference P1 (at 0 -5.08) (layer F.SilkS) hide)
    (fp_text value "RGBW Strip" (at -0.5 6.5) (layer F.Fab) hide)
    (pad 2 thru_hole circle (at -5.08 0) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 0 0) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(P1-Pad3)"))
    (pad 1 thru_hole rect (at -10.16 0) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 3 +12V))
    (pad 4 thru_hole circle (at 5.08 0) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P1-Pad4)"))
    (pad 5 thru_hole circle (at 10.16 0) (size 3.81 3.81) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(P1-Pad5)"))
    (model Connect.3dshapes/bornier5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 56F47BA0)
    (at 142 95)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P2 (at 1.25 -2.75) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at -0.5 6.5) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at -2.54 0) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 3 +12V))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 56F47AD9)
    (at 120.65 82.55)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 3.81) (layer B.SilkS) hide)
    (fp_text value IRLML2502 (at 0 -3.81) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.95 -1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 12 R))
    (pad 2 smd rect (at 0.95 -1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(P1-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 56F47AE0)
    (at 124.46 82.55)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0 3.81) (layer B.SilkS) hide)
    (fp_text value IRLML2502 (at 0 -3.81) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.95 -1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 13 G))
    (pad 2 smd rect (at 0.95 -1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(P1-Pad3)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 56F47AE6)
    (at 128.27 82.55)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 0 3.81) (layer B.SilkS) hide)
    (fp_text value IRLML2502 (at 0 -3.81) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.95 -1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 14 B))
    (pad 2 smd rect (at 0.95 -1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(P1-Pad4)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 56F47B44)
    (at 107.95 81.28 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 2.3 90) (layer B.SilkS) hide)
    (fp_text value R (at 0 -2.3 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 12 R))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 56F47B4E)
    (at 114.3 81.28 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 2.3 90) (layer B.SilkS) hide)
    (fp_text value R (at 0 -2.3 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 13 G))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 56F47B48)
    (at 111.125 81.28 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 2.3 90) (layer B.SilkS) hide)
    (fp_text value R (at 0 -2.3 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 14 B))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer B.Cu) (tedit 56F47B54)
    (at 117.475 81.28 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at 0 2.3 90) (layer B.SilkS) hide)
    (fp_text value R (at 0 -2.3 90) (layer B.Fab) hide)
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 15 W))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer B.Cu) (tedit 56F47B1A)
    (at 150 94)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 0 0.762) (layer B.SilkS) hide)
    (fp_text value AMS1117 (at 0 -0.762) (layer B.Fab) hide)
    (pad 4 smd rect (at 0 3.302) (size 3.6576 2.032) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0 -3.302) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at 2.286 -3.302) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 3 +12V))
    (pad 1 smd rect (at -2.286 -3.302) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 56F47AEB)
    (at 132.08 82.55)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 0 3.81) (layer B.SilkS) hide)
    (fp_text value IRLML2502 (at 0 -3.81) (layer B.Fab) hide)
    (pad 1 smd rect (at -0.95 -1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 15 W))
    (pad 2 smd rect (at 0.95 -1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 0 1.50114) (size 0.8001 1.80086) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(P1-Pad5)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 56F47B2E)
    (at 147.5 77.5)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference CON1 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value AVR-ISP-6 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 MISO))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 SCK))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 MOSI))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 RST))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_ISO7380 (layer F.Cu) (tedit 56F47B39)
    (at 108 94)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO7380")
    (tags "mounting hole 2.7mm no annular m2.5 iso7380")
    (fp_text reference REF** (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_ISO7380 (at -9.5 7.5) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5_ISO7380 (layer F.Cu) (tedit 56F47B2A)
    (at 149 73)
    (descr "Mounting Hole 2.7mm, no annular, M2.5, ISO7380")
    (tags "mounting hole 2.7mm no annular m2.5 iso7380")
    (fp_text reference REF** (at 0 -3.25) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5_ISO7380 (at 6 -5.5) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text MySensors (at 112 78.8) (layer F.SilkS))
  (gr_text - (at 145 84.6) (layer B.SilkS))
  (gr_text 12V (at 142.2 96.8) (layer F.SilkS))
  (gr_text V1.3 (at 150.8 95.4) (layer F.SilkS))
  (gr_text "RGBW Controller" (at 122.4 82.4) (layer F.SilkS))
  (gr_text - (at 144 89.25) (layer F.SilkS))
  (gr_text + (at 113.25 99.25) (layer F.SilkS))
  (gr_text R (at 118.25 99.25) (layer F.SilkS))
  (gr_text G (at 123.25 99.25) (layer F.SilkS))
  (gr_text B (at 128.5 99.25) (layer F.SilkS))
  (gr_text W (at 133.75 99.25) (layer F.SilkS))
  (gr_text + (at 139.5 99.25) (layer F.SilkS))
  (gr_text - (at 144.5 99.25) (layer F.SilkS))
  (dimension 5.08 (width 0.3) (layer Dwgs.User)
    (gr_text "5,000 mm" (at 148.336 62.992) (layer Dwgs.User))
    (feature1 (pts (xy 151.384 72.644) (xy 151.384 64.864)))
    (feature2 (pts (xy 146.304 72.644) (xy 146.304 64.864)))
    (crossbar (pts (xy 146.304 67.564) (xy 151.384 67.564)))
    (arrow1a (pts (xy 151.384 67.564) (xy 150.257496 68.150421)))
    (arrow1b (pts (xy 151.384 67.564) (xy 150.257496 66.977579)))
    (arrow2a (pts (xy 146.304 67.564) (xy 147.430504 68.150421)))
    (arrow2b (pts (xy 146.304 67.564) (xy 147.430504 66.977579)))
  )
  (dimension 4 (width 0.3) (layer Dwgs.User)
    (gr_text "4,000 mm" (at 93.98 97.536 90) (layer Dwgs.User))
    (feature1 (pts (xy 102 96) (xy 96.3 96)))
    (feature2 (pts (xy 102 100) (xy 96.3 100)))
    (crossbar (pts (xy 99 100) (xy 99 96)))
    (arrow1a (pts (xy 99 96) (xy 99.586421 97.126504)))
    (arrow1b (pts (xy 99 96) (xy 98.413579 97.126504)))
    (arrow2a (pts (xy 99 100) (xy 99.586421 98.873496)))
    (arrow2b (pts (xy 99 100) (xy 98.413579 98.873496)))
  )
  (dimension 50 (width 0.3) (layer Dwgs.User)
    (gr_text "50,000 mm" (at 130 106.35) (layer Dwgs.User))
    (feature1 (pts (xy 155 102) (xy 155 107.7)))
    (feature2 (pts (xy 105 102) (xy 105 107.7)))
    (crossbar (pts (xy 105 105) (xy 155 105)))
    (arrow1a (pts (xy 155 105) (xy 153.873496 105.586421)))
    (arrow1b (pts (xy 155 105) (xy 153.873496 104.413579)))
    (arrow2a (pts (xy 105 105) (xy 106.126504 105.586421)))
    (arrow2b (pts (xy 105 105) (xy 106.126504 104.413579)))
  )
  (dimension 30 (width 0.3) (layer Dwgs.User)
    (gr_text "30,000 mm" (at 161.35 85 270) (layer Dwgs.User))
    (feature1 (pts (xy 157 100) (xy 162.7 100)))
    (feature2 (pts (xy 157 70) (xy 162.7 70)))
    (crossbar (pts (xy 160 70) (xy 160 100)))
    (arrow1a (pts (xy 160 100) (xy 159.413579 98.873496)))
    (arrow1b (pts (xy 160 100) (xy 160.586421 98.873496)))
    (arrow2a (pts (xy 160 70) (xy 159.413579 71.126504)))
    (arrow2b (pts (xy 160 70) (xy 160.586421 71.126504)))
  )
  (gr_arc (start 150 95) (end 155 95) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 150 75) (end 150 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 110 95) (end 110 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 109.5 74.5) (end 105 74.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105 95) (end 105 74.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155 95) (end 155 75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110 100) (end 150 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.5 70) (end 150 70) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 4))
    (polygon
      (pts
        (xy 155 70) (xy 155 100) (xy 105 100) (xy 105 70)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 4))
    (polygon
      (pts
        (xy 155 100) (xy 105 100) (xy 105 70) (xy 155 70) (xy 155 100)
      )
    )
  )
)
