(kicad_pcb (version 4) (host pcbnew 4.1.0-alpha+201606291451+6956~45~ubuntu14.04.1-product)
  (general
    (links 38)
    (no_connects 1)
    (area 213.331667 98.8125 241.328334 114.6825)
    (thickness 1.6)
    (drawings 20)
    (tracks 197)
    (zones 0)
    (modules 17)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1)
    (user_trace_width 0.1)
    (user_trace_width 0.2)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.7)
    (via_drill 0.5)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.7 0.7)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 225.815 102.355)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 /Button)
  (net 3 "Net-(C2-Pad1)")
  (net 4 /Vout)
  (net 5 "Net-(D1-Pad2)")
  (net 6 GND)
  (net 7 /Vin)
  (net 8 "Net-(LED2-Pad2)")
  (net 9 "Net-(LED1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.7)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /Button)
    (add_net /Vin)
    (add_net /Vout)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(LED2-Pad2)")
  )
  (module KiCad/Resistors_SMD.pretty:R_0603_HandSoldering (layer F.Cu) (tedit 575ABB37)
    (at 233.485 109.935 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -0.18 1.2 90) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vout))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(LED2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Resistors_SMD.pretty:R_0603_HandSoldering (layer F.Cu) (tedit 575AB7D2)
    (at 222.225 111.155 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -0.03 -1.33 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /Vin))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(LED1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Resistors_SMD.pretty:R_0603_HandSoldering (layer F.Cu) (tedit 575AB7D5)
    (at 226.43 111.15 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -0.015 -1.345 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vout))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Resistors_SMD.pretty:R_0603_HandSoldering (layer F.Cu) (tedit 575AB863)
    (at 221.075 107.895 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.83 0.97 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /Vin))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 /Button))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Resistors_SMD.pretty:R_0603_HandSoldering (layer F.Cu) (tedit 575AB856)
    (at 223.015 107.885 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -1.62 1.07 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /Vin))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Resistors_SMD.pretty:R_0603_HandSoldering (layer F.Cu) (tedit 575AB891)
    (at 233.365 105.515 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -1.58 1.6) (layer F.SilkS))
    (fp_text value 300k (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Pin_Headers.pretty:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 236.22 110.49 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0.485 9.605 180) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 /Vout))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /Button))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module KiCad/Pin_Headers.pretty:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 0)
    (at 218.44 102.87)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -0.005 -1.975) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /Button))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /Vin))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module KiCad/Capacitors_SMD.pretty:C_0603_HandSoldering (layer F.Cu) (tedit 575AB843)
    (at 230.525 111.195)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -0.04 1.25) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vout))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Capacitors_SMD.pretty:C_0603_HandSoldering (layer F.Cu) (tedit 575AB84E)
    (at 222.075 104.355)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -0.03 1.18) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 /Vin))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Capacitors_SMD.pretty:C_0603_HandSoldering (layer F.Cu) (tedit 575AB84A)
    (at 222.135 102.585 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -0.09 1.32 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /Button))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:FSM2JSMA (layer B.Cu) (tedit 57596A88)
    (at 227.175 106.845 270)
    (fp_text reference SW1 (at 0.06 -3.98 90) (layer B.SilkS))
    (fp_text value SW_PUSH_SMALL (at 0 0.5 270) (layer B.Fab))
    (pad 2 smd rect (at -2.25 4.55 270) (size 1.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 1 smd rect (at 2.25 -4.55 270) (size 1.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 2 /Button))
    (pad 2 smd rect (at -2.25 -4.55 270) (size 1.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 1 smd rect (at 2.25 4.55 270) (size 1.4 2.1) (layers B.Cu B.Paste B.Mask)
      (net 2 /Button))
  )
  (module KiCad/Housings_SOIC.pretty:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 575AB886)
    (at 228.265 107.255)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference Q1 (at -2.83 -3.07) (layer F.SilkS))
    (fp_text value IRF7309IPBF (at 0 3.5) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /Vin))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vout))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /Vout))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Resistors_SMD.pretty:R_0603_HandSoldering (layer B.Cu) (tedit 575AB935)
    (at 230.465 111.605)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference LED2 (at -2.58 0.06 90) (layer B.SilkS))
    (fp_text value LED (at 0 -1.9) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(LED2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Resistors_SMD.pretty:R_0603_HandSoldering (layer B.Cu) (tedit 5418A00F)
    (at 223.435 111.585 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference LED1 (at -2.67 -0.11 90) (layer B.SilkS))
    (fp_text value LED (at 0 -1.9 180) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(LED1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module KiCad/Diodes_SMD.pretty:MiniMELF_Handsoldering (layer F.Cu) (tedit 575AB88C)
    (at 229.105 101.955)
    (descr "Diode Mini-MELF Handsoldering")
    (tags "Diode Mini-MELF Handsoldering")
    (attr smd)
    (fp_text reference D1 (at 0.06 1.48 180) (layer F.SilkS))
    (fp_text value D (at 0 3.81) (layer F.Fab))
    (fp_text user K (at -5.05 -0.64) (layer F.SilkS))
    (fp_text user A (at 4.97 -0.65) (layer F.SilkS))
    (pad 1 smd rect (at -2.75082 0) (size 3.29946 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 2 /Button))
    (pad 2 smd rect (at 2.75082 0) (size 3.29946 1.69926) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D1-Pad2)"))
    (model Diodes_SMD.3dshapes/MiniMELF_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module mcous/kicad-lib/footprints/jumper.pretty:SOLDER-JUMPER_2-WAY (layer B.Cu) (tedit 575ABC0E)
    (at 227.135 101.915)
    (fp_text reference JP1 (at -4.79 -0.03 90) (layer B.SilkS))
    (fp_text value JUMPER3 (at 0 0) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.35 0) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (pad 3 smd rect (at 1.35 0) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 7 /Vin))
    (pad 2 smd rect (at 0 0) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 7 /Vin))
  )
  (gr_text auto (at 230.536484 102.544954 180) (layer B.SilkS))
  (gr_text auto (at 223.964368 102.544954 180) (layer B.SilkS))
  (gr_text Vout (at 233.95475 110.715 90) (layer B.SilkS))
  (gr_text BTN (at 234.245 108.075 90) (layer B.SilkS))
  (gr_text GND (at 234.245 105.435 90) (layer B.SilkS))
  (gr_text GND (at 234.245 102.795 90) (layer B.SilkS))
  (gr_text Vin (at 220.447 110.758998 90) (layer B.SilkS))
  (gr_text BTN (at 220.73725 108.134332 90) (layer B.SilkS))
  (gr_text GND (at 220.73725 105.509666 90) (layer B.SilkS))
  (gr_text on (at 224.014368 101.454954 180) (layer B.SilkS))
  (gr_text "off\n" (at 230.336484 101.454954 180) (layer B.SilkS))
  (gr_text GND (at 220.73725 102.885 90) (layer B.SilkS))
  (gr_line (start 237.49 100.33) (end 217.17 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 238.76 101.6) (end 237.49 100.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 238.76 111.76) (end 238.76 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 237.49 113.03) (end 238.76 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.17 113.03) (end 237.49 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 215.9 111.76) (end 217.17 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 215.9 101.6) (end 215.9 111.76) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.17 100.33) (end 215.9 101.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 238.765 101.615) (xy 238.765 111.775) (xy 237.495 113.045) (xy 217.175 113.045) (xy 215.905 111.775)
        (xy 215.905 101.615) (xy 217.175 100.345) (xy 237.495 100.345)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 238.765 101.615) (xy 238.765 111.775) (xy 237.495 113.045) (xy 217.175 113.045) (xy 215.905 111.775)
        (xy 215.905 101.615) (xy 217.175 100.345) (xy 237.495 100.345)
      )
    )
  )
)
