(kicad_pcb (version 4) (host pcbnew "(2015-05-09 BZR 5648)-product")
  (general
    (links 60)
    (no_connects 0)
    (area 99.120976 77.12412 158.892224 138.676)
    (thickness 1.6)
    (drawings 31)
    (tracks 232)
    (zones 0)
    (modules 22)
    (nets 22)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.2032)
    (trace_clearance 0.1905)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.0254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 2)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Manufacturing/))
  )
  (net 0 "")
  (net 1 "Net-(CON1-Pad1)")
  (net 2 VCC)
  (net 3 "Net-(CON1-Pad3)")
  (net 4 "Net-(CON1-Pad4)")
  (net 5 /RST)
  (net 6 GND)
  (net 7 "Net-(CON2-Pad5)")
  (net 8 "Net-(CON2-Pad7)")
  (net 9 "Net-(CON2-Pad8)")
  (net 10 "Net-(P2-Pad9)")
  (net 11 "Net-(R1-Pad1)")
  (net 12 "Net-(CON4-Pad3)")
  (net 13 "Net-(CON4-Pad4)")
  (net 14 "Net-(CON4-Pad2)")
  (net 15 +5V)
  (net 16 "Net-(CON4-Pad6)")
  (net 17 "Net-(CON4-Pad7)")
  (net 18 "Net-(CON4-Pad8)")
  (net 19 "Net-(CON4-Pad9)")
  (net 20 +3V3)
  (net 21 +1V8)
  (net_class Default "This is the default net class."
    (clearance 0.1905)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /RST)
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(CON1-Pad3)")
    (add_net "Net-(CON1-Pad4)")
    (add_net "Net-(CON2-Pad5)")
    (add_net "Net-(CON2-Pad7)")
    (add_net "Net-(CON2-Pad8)")
    (add_net "Net-(CON4-Pad2)")
    (add_net "Net-(CON4-Pad3)")
    (add_net "Net-(CON4-Pad4)")
    (add_net "Net-(CON4-Pad6)")
    (add_net "Net-(CON4-Pad7)")
    (add_net "Net-(CON4-Pad8)")
    (add_net "Net-(CON4-Pad9)")
    (add_net "Net-(P2-Pad9)")
    (add_net "Net-(R1-Pad1)")
  )
  (net_class Power ""
    (clearance 0.1905)
    (trace_width 0.508)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V8)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net VCC)
  )
  (module mysensors_buttons:SW_SPST_SMD_J-LEAD_4.3MM (layer F.Cu) (tedit 55C322EC)
    (at 139.73556 85.1408)
    (descr "TE Connectivity SPST SMD J-LEAD,4.3MM")
    (tags "SPST Button Switch")
    (fp_text reference SW1 (at 0.508 -2.921) (layer F.Fab))
    (fp_text value SW_PUSH (at 0 0.381 180) (layer F.Fab))
    (pad 1 smd rect (at -4.8 0) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 4.8 0) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model mysensors.3dshapes/w.lain.3dshapes/switch/smd_push.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5418A00F)
    (at 136.92124 87.91956)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.9) (layer F.SilkS))
    (fp_text value 100 (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /RST))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_3x2 (layer F.Cu) (tedit 55C31CDA)
    (at 113.7412 94.0562 90)
    (descr "Box header 3x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference CON1 (at 0 -5.7 90) (layer F.Fab))
    (fp_text value AVR-ISP-6 (at 0 5.7 90) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -2.54 1.27 90) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(CON1-Pad1)"))
    (pad 2 thru_hole oval (at -2.54 -1.27 90) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 3 thru_hole oval (at 0 1.27 90) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(CON1-Pad3)"))
    (pad 4 thru_hole oval (at 0 -1.27 90) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(CON1-Pad4)"))
    (pad 5 thru_hole oval (at 2.54 1.27 90) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 5 /RST))
    (pad 6 thru_hole oval (at 2.54 -1.27 90) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model walter/conn_strip/vasch_strip_3x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_5x2 (layer F.Cu) (tedit 55C33A6E)
    (at 127.127 94.0562 90)
    (descr "Box header 5x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference CON2 (at 0 -5.7 90) (layer F.Fab))
    (fp_text value AVR-JTAG-10 (at 0 5.7 90) (layer F.SilkS) hide)
    (pad 9 thru_hole oval (at 5.08 1.27 90) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(CON1-Pad4)"))
    (pad 10 thru_hole oval (at 5.08 -1.27 90) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND) (clearance 0.01905))
    (pad 8 thru_hole oval (at 2.54 -1.27 90) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(CON2-Pad8)"))
    (pad 7 thru_hole oval (at 2.54 1.27 90) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(CON2-Pad7)"))
    (pad 1 thru_hole rect (at -5.08 1.27 90) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(CON1-Pad3)"))
    (pad 2 thru_hole oval (at -5.08 -1.27 90) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 3 thru_hole oval (at -2.54 1.27 90) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(CON1-Pad1)"))
    (pad 4 thru_hole oval (at -2.54 -1.27 90) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 5 thru_hole oval (at 0 1.27 90) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(CON2-Pad5)"))
    (pad 6 thru_hole oval (at 0 -1.27 90) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 5 /RST))
    (model walter/conn_strip/vasch_strip_5x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:FCI_10P_HDR (layer F.Cu) (tedit 55C31EEA)
    (at 127.762 125.349)
    (tags "0.05\" ")
    (fp_text reference P1 (at 0 3.5) (layer F.Fab))
    (fp_text value "Jtag ICE3" (at 0 -3.5) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 -0.635) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 1 thru_hole circle (at -2.54 0.635) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(CON1-Pad3)"))
    (pad 4 thru_hole circle (at -1.27 -0.635) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 3 thru_hole circle (at -1.27 0.635) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(CON1-Pad1)"))
    (pad 6 thru_hole circle (at 0 -0.635) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 /RST))
    (pad 5 thru_hole circle (at 0 0.635) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(CON2-Pad5)"))
    (pad 8 thru_hole circle (at 1.27 -0.635) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(CON2-Pad8)"))
    (pad 7 thru_hole circle (at 1.27 0.635) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(CON2-Pad7)"))
    (pad 10 thru_hole circle (at 2.54 -0.635) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 9 thru_hole circle (at 2.54 0.635) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(CON1-Pad4)"))
    (model walter/conn_strip/vasch_strip_5x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:FCI_10P_HDR (layer F.Cu) (tedit 55C31EF8)
    (at 146.431 94.0562 90)
    (tags "0.05\" ")
    (fp_text reference P2 (at 0 3.5 90) (layer F.Fab))
    (fp_text value "Cortex M0 debug" (at 0 -3.5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 -0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(CON2-Pad5)"))
    (pad 1 thru_hole circle (at -2.54 0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 4 thru_hole circle (at -1.27 -0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(CON1-Pad3)"))
    (pad 3 thru_hole circle (at -1.27 0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 6 thru_hole circle (at 0 -0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(CON1-Pad1)"))
    (pad 5 thru_hole circle (at 0 0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 8 thru_hole circle (at 1.27 -0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(CON1-Pad4)"))
    (pad 7 thru_hole circle (at 1.27 0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS))
    (pad 10 thru_hole circle (at 2.54 -0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 /RST))
    (pad 9 thru_hole circle (at 2.54 0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(P2-Pad9)"))
    (model walter/conn_strip/vasch_strip_5x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:FCI_10P_HDR (layer F.Cu) (tedit 55C31EFF)
    (at 137.3632 94.0562 90)
    (tags "0.05\" ")
    (fp_text reference P3 (at 0 3.5 90) (layer F.Fab))
    (fp_text value "ice3 expansion" (at 0 -3.5 90) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 -0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 1 thru_hole circle (at -2.54 0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(CON1-Pad3)"))
    (pad 4 thru_hole circle (at -1.27 -0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 3 thru_hole circle (at -1.27 0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(CON1-Pad1)"))
    (pad 6 thru_hole circle (at 0 -0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 5 /RST))
    (pad 5 thru_hole circle (at 0 0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(CON2-Pad5)"))
    (pad 8 thru_hole circle (at 1.27 -0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(CON2-Pad8)"))
    (pad 7 thru_hole circle (at 1.27 0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(CON2-Pad7)"))
    (pad 10 thru_hole circle (at 2.54 -0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 9 thru_hole circle (at 2.54 0.635 90) (size 1 1) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(CON1-Pad4)"))
    (model walter/conn_strip/vasch_strip_5x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.5 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_connectors:Micro_USB (layer F.Cu) (tedit 55C3A29B)
    (at 141.6177 128.4605)
    (fp_text reference CON4 (at -0.95 9.25) (layer F.Fab))
    (fp_text value USB-MICRO-B (at -0.875 7.925) (layer F.Fab))
    (pad 3 smd rect (at 0 -4.1) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(CON4-Pad3)"))
    (pad 4 smd rect (at 0.65 -4.1) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(CON4-Pad4)"))
    (pad 2 smd rect (at -0.65 -4.1) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(CON4-Pad2)"))
    (pad 1 smd rect (at -1.3 -4.1) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (pad 5 smd rect (at 1.3 -4.1) (size 0.4 1.4) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 6 thru_hole oval (at -3.575 -1.15) (size 1.05 1.85) (drill oval 0.45 1.25) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(CON4-Pad6)"))
    (pad 7 thru_hole oval (at 3.575 -1.15) (size 1.05 1.85) (drill oval 0.45 1.25) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(CON4-Pad7)"))
    (pad 8 thru_hole oval (at -3.575 -4.6) (size 1.05 1.85) (drill oval 0.45 1.25) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(CON4-Pad8)"))
    (pad 9 thru_hole oval (at 3.575 -4.6) (size 1.05 1.85) (drill oval 0.45 1.25) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(CON4-Pad9)"))
    (pad "" np_thru_hole circle (at -2 -3.275) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 2 -3.275) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask F.SilkS))
    (model mysensors.3dshapes/w.lain.3dshapes/conn_pc/usb_B_micro_smd-2.wrl
      (at (xyz 0 0.03 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 55C3A240)
    (at 148.9456 119.7356 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.9464 -0.1016 270) (layer F.SilkS))
    (fp_text value C (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 148.8186 114.2492 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -1.00076 -1.94564 360) (layer F.SilkS))
    (fp_text value C (at 0 1.9 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 20 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 55C3A236)
    (at 139.7889 119.3546 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0.254 1.3208 90) (layer F.SilkS))
    (fp_text value C (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 55C3A227)
    (at 142.99692 106.44124 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 3.4544 -4.6736 90) (layer F.Fab))
    (fp_text value "Supply select" (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 +1V8))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 +3V3))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5V))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 55C355DC)
    (at 151.52116 116.72062)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at 0 -5.1) (layer F.Fab))
    (fp_text value Supply (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 55C35263)
    (at 135.6106 109.2327)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 0 -5.1) (layer F.Fab))
    (fp_text value GND (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module SMD_Packages:SOT-223 (layer F.Cu) (tedit 0)
    (at 135.382 117)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at 0 -0.762) (layer F.SilkS))
    (fp_text value AP1117D18 (at 0 0.762) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 21 +1V8))
    (pad 3 smd rect (at 2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (pad 1 smd rect (at -2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model SMD_Packages.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module SMD_Packages:SOT-223 (layer F.Cu) (tedit 55C39A12)
    (at 144.3736 117)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -0.7112) (layer F.SilkS))
    (fp_text value AP1117D33 (at 0 0.762) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 20 +3V3))
    (pad 3 smd rect (at 2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 15 +5V))
    (pad 1 smd rect (at -2.286 3.302) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model SMD_Packages.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:Symbol_OSHW-Logo_CopperTop_BIG (layer B.Cu) (tedit 55C3C5FC)
    (at 114.4905 89.662 180)
    (descr "Symbol, OSHW-Logo, Copper Top, BIG")
    (tags "Symbol, OSHW-Logo, Copper Top, BIG")
    (fp_text reference REF** (at -0.29972 -11.50112 180) (layer F.Fab))
    (fp_text value Symbol_OSHW-Logo_CopperTop_BIG (at 0.29972 -32.10052 180) (layer B.Fab))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 55C50334)
    (at 150.1902 82.7532)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.Fab))
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 55C5056B)
    (at 107.7468 82.7405)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.Fab) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 55C5054F)
    (at 107.696 125.2601)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.Fab) hide)
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 55C50341)
    (at 150.3172 125.1712)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference REF** (at 0 -4.50088) (layer F.Fab))
    (fp_text value MountingHole_3-5mm (at 0 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 541A9B4D)
    (at 139.9413 111.6711 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.9 180) (layer F.SilkS))
    (fp_text value C (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 21 +1V8))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 1 (at 122.20194 127.69596) (layer F.SilkS))
  (gr_text 1 (at 119.13616 96.64192) (layer F.SilkS))
  (gr_text 1 (at 132.5753 99.09556) (layer F.SilkS))
  (gr_text 1 (at 140.56868 96.70796) (layer F.SilkS))
  (gr_text 1 (at 149.65172 96.48952) (layer F.SilkS))
  (gr_text "PDI\nPDI_D\nVCC\nnc\nnc\nPDI_C\nGND" (at 126.7968 110.3503) (layer F.SilkS))
  (gr_text "Cortex\nVCC\nSWDIO\nGND\nSWDCLK\nGND\nSWO\n(key)\nNC\n-\nReset" (at 113.4491 113.7031) (layer F.SilkS))
  (gr_text "ISP\nMISO\nVCC\nSCK\nMOSI\nRST\nGND\n" (at 121.0945 110.4138) (layer F.SilkS))
  (gr_text "JTAG\nTCK\nGND\nTDO\nVTref\nTMS\nnSRST\nnc\nnTRST\nTDI\nGND" (at 107.6833 113.6904) (layer F.SilkS))
  (gr_text "1\n2\n3\n4\n5\n6\n7\n8\n9\n10" (at 106.9467 114.5032) (layer F.SilkS))
  (gr_text "+5V in" (at 152.51684 110.50016 90) (layer F.SilkS))
  (gr_text "Supply\nonly" (at 138.3284 125.73) (layer F.SilkS))
  (gr_text "Scope\nGND" (at 135.5852 105.5116) (layer F.SilkS))
  (gr_text "5V\n" (at 148.1836 109.474 90) (layer F.SilkS))
  (gr_text 3V3 (at 145.6436 109.7788 90) (layer F.SilkS))
  (gr_text 1V8 (at 143.1544 109.7788 90) (layer F.SilkS))
  (gr_text "JTAGICE3 Breakout board\n" (at 128.9685 82.0293) (layer F.SilkS))
  (gr_text "JTAG / ICE3" (at 133.8834 94.0435 90) (layer F.SilkS))
  (gr_text JTAGICE3 (at 127.254 121.9581) (layer F.SilkS))
  (gr_text Reset (at 143.52778 87.61222) (layer F.SilkS))
  (gr_text Cortex-M (at 143.0528 94.0435 90) (layer F.SilkS))
  (gr_text JTAG (at 121.3739 94.0816 90) (layer F.SilkS))
  (gr_text ISP/PDI (at 107.9246 94.107 90) (layer F.SilkS))
  (gr_arc (start 106 81) (end 104 81) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 152 81) (end 152 79) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 152 127) (end 154 127) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 106 127) (end 106 129) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 152 129) (end 106 129) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 154 81) (end 154 127) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 106 79) (end 152 79) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 104 127) (end 104 81) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 104.14 128.905) (xy 154.051 129.032) (xy 154.051 78.994) (xy 104.14 78.994) (xy 104.013 128.905)
        (xy 104.14 128.905)
      )
    )
  )
)
