(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 72)
    (no_connects 0)
    (area 143.561999 77.521999 193.750001 107.898001)
    (thickness 1.6)
    (drawings 41)
    (tracks 325)
    (zones 0)
    (modules 27)
    (nets 34)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 158.877 98.171)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(C1-Pad1)")
  (net 3 +BATT)
  (net 4 D3/Int1)
  (net 5 "Net-(IC1-Pad2)")
  (net 6 "Net-(IC1-Pad7)")
  (net 7 "Net-(IC1-Pad8)")
  (net 8 "Net-(IC1-Pad10)")
  (net 9 CE)
  (net 10 CSN)
  (net 11 MOSI)
  (net 12 MISO)
  (net 13 SCK)
  (net 14 "Net-(IC1-Pad19)")
  (net 15 "Net-(IC1-Pad22)")
  (net 16 A0)
  (net 17 A1)
  (net 18 A2)
  (net 19 A3)
  (net 20 SDA)
  (net 21 SCL)
  (net 22 RX)
  (net 23 TX)
  (net 24 D2/Int0)
  (net 25 Reset)
  (net 26 DTR)
  (net 27 "Net-(IC1-Pad11)")
  (net 28 D8)
  (net 29 "Net-(D1-Pad2)")
  (net 30 D5)
  (net 31 "Net-(BT1-Pad1)")
  (net 32 "Net-(C2-Pad1)")
  (net 33 "Net-(U3-Pad8)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net CE)
    (add_net CSN)
    (add_net D2/Int0)
    (add_net D3/Int1)
    (add_net D5)
    (add_net D8)
    (add_net DTR)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(U3-Pad8)")
    (add_net RX)
    (add_net Reset)
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net TX)
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 57755767)
    (at 145.669 85.979)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at 0.381 -4.699) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 SCL))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 SDA))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +BATT))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 A2))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 A1))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_radios:NRF24L01-SMD (layer F.Cu) (tedit 577558FA)
    (at 177.419 88.265)
    (fp_text reference U3 (at -1.8415 -0.254) (layer F.SilkS) hide)
    (fp_text value NRF24L01 (at 0.254 -5.3975) (layer F.SilkS))
    (pad 2 smd rect (at -4.4 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 1 smd rect (at -3.13 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.86 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 9 CE))
    (pad 4 smd rect (at -0.59 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 10 CSN))
    (pad 5 smd rect (at 0.68 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 13 SCK))
    (pad 6 smd rect (at 1.95 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 11 MOSI))
    (pad 7 smd rect (at 3.22 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 12 MISO))
    (pad 8 smd rect (at 4.49 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U3-Pad8)"))
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/nrf24smd.wrl
      (at (xyz -5.7625 2.9 0.03))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_5x5mm_Pitch0.65mm.wrl
      (at (xyz 0.0165 -0.109 0.062))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 577557EF)
    (at 183.642 104.394 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference CON1 (at 0 -5.1 90) (layer F.SilkS) hide)
    (fp_text value AVR-ISP-6 (at -2.54 2.6035 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 MISO))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +BATT))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 MOSI))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 Reset))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 57755927)
    (at 163.068 91.694 90)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 0 -6.05 90) (layer F.SilkS) hide)
    (fp_text value ATMEGA328P-A (at 0 6.05 90) (layer F.SilkS))
    (pad 1 smd rect (at -4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 D3/Int1))
    (pad 2 smd rect (at -4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 5 smd rect (at -4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 7 smd rect (at -4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 D5))
    (pad 10 smd rect (at -2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at -1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 D8))
    (pad 13 smd rect (at 0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 CE))
    (pad 14 smd rect (at 1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 CSN))
    (pad 15 smd rect (at 2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 MOSI))
    (pad 16 smd rect (at 2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 MISO))
    (pad 17 smd rect (at 4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 SCK))
    (pad 18 smd rect (at 4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 19 smd rect (at 4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 21 smd rect (at 4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 22 smd rect (at 4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 A0))
    (pad 24 smd rect (at 4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 A1))
    (pad 25 smd rect (at 2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 A2))
    (pad 26 smd rect (at 2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 A3))
    (pad 27 smd rect (at 1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 SDA))
    (pad 28 smd rect (at 0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 SCL))
    (pad 29 smd rect (at -0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 Reset))
    (pad 30 smd rect (at -1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 RX))
    (pad 31 smd rect (at -2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 TX))
    (pad 32 smd rect (at -2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 D2/Int0))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 5775582A)
    (at 149.479 85.979)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 SDA))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 SCL))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +BATT))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 D3/Int1))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 D2/Int0))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module "Batteries:CR2032 Battery Holder" (layer B.Cu) (tedit 57755A8F)
    (at 168.7195 98.425 90)
    (fp_text reference BT1 (at 10.7696 4.5212 90) (layer B.SilkS) hide)
    (fp_text value Battery (at 2.3876 -2.0574 90) (layer B.Fab))
    (pad 2 thru_hole circle (at -5 -5 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 1 thru_hole circle (at 15 -5 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 31 "Net-(BT1-Pad1)"))
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 57759470)
    (at 152.7556 80.391 180)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C8 (at 0 -2.7 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at -0.0508 -2.413 360) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 2 smd rect (at 2 0 180) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_obscurities:2_pin_solder_jumper_smd (layer B.Cu) (tedit 57755A41)
    (at 178.181 89.535)
    (fp_text reference JP1 (at -0.635 3.048) (layer B.SilkS) hide)
    (fp_text value JUMPER (at 0 1.524) (layer B.Fab))
    (pad 2 smd oval (at 0.889 0) (size 1.27 1.524) (layers B.Cu B.Paste B.Mask)
      (net 3 +BATT))
    (pad 1 smd oval (at -0.889 0) (size 1.27 1.524) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(C2-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x06 (layer F.Cu) (tedit 57755821)
    (at 190.881 81.661)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value CONN_01X06 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +BATT))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 RX))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 TX))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 DTR))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x06.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 57755D9B)
    (at 154.6225 86.106 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U4 (at 0 -3.81 180) (layer F.SilkS) hide)
    (fp_text value ATSHA204A (at -2.286 2.794 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 19 A3))
    (pad 2 smd rect (at 0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 3 smd rect (at 0 -1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 57755959)
    (at 186.3725 81.7245)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 -5.1) (layer F.SilkS) hide)
    (fp_text value "Boost Converter Module" (at -2.2225 2.4765 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(C2-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer B.Cu) (tedit 577559C2)
    (at 179.451 83.185 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 0.762 180) (layer B.SilkS) hide)
    (fp_text value AMS1117 (at 0.0635 -0.254 180) (layer B.SilkS))
    (pad 4 smd rect (at 0 3.302 180) (size 3.6576 2.032) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at 0 -3.302 180) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 3 +BATT))
    (pad 3 smd rect (at 2.286 -3.302 180) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -2.286 -3.302 180) (size 1.016 2.032) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 57755CAE)
    (at 167.64 82.169 90)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C1 (at 0 -2.7 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 2.032 -2.286 90) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 57755D55)
    (at 185.547 92.837 180)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C2 (at -0.0635 2.667 180) (layer B.SilkS) hide)
    (fp_text value 100nF (at 0 2.4765 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer B.Cu) (tedit 57755D6E)
    (at 178.181 92.837 180)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C3 (at 0 2.7 180) (layer B.SilkS) hide)
    (fp_text value 22nF (at 3.937 2.6035 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 3 +BATT))
    (pad 2 smd rect (at 2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 5775585E)
    (at 154.813 95.123 90)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C4 (at 0 -2.7 90) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0.0635 -2.413 90) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 26 DTR))
    (pad 2 smd rect (at 2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 25 Reset))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 5775588C)
    (at 167.513 99.695)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C5 (at 0 -2.7) (layer F.SilkS) hide)
    (fp_text value 100nF (at 0.3175 2.413) (layer F.SilkS))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 577557D7)
    (at 176.657 105.7275 90)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C7 (at 2.159 -3.6195 90) (layer F.SilkS) hide)
    (fp_text value 47uF (at 4.8895 0.127 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 +BATT))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_1206 (layer F.Cu) (tedit 57755D2A)
    (at 152.0952 105.029)
    (descr "LED 1206 smd package")
    (tags "LED1206 SMD")
    (attr smd)
    (fp_text reference D1 (at 0 -2) (layer F.SilkS) hide)
    (fp_text value LED (at -0.0635 -2.159) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model LEDs.3dshapes/LED_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 57755CA1)
    (at 160.4645 82.169 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C6 (at 0 -2.7 270) (layer F.SilkS) hide)
    (fp_text value 100nF (at -2.032 -2.4765 270) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 5775960B)
    (at 160.147 99.695 180)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C9 (at 0 -2.7 180) (layer F.SilkS) hide)
    (fp_text value 100nF (at -0.8382 -2.4892 180) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +BATT))
    (pad 2 smd rect (at 2 0 180) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210_HandSoldering (layer B.Cu) (tedit 57755D41)
    (at 152.781 80.391 180)
    (descr "Resistor SMD 1210, hand soldering")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference R1 (at -1.524 4.826 180) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -2.7 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 25 Reset))
    (pad 2 smd rect (at 2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 3 +BATT))
    (model Resistors_SMD.3dshapes/R_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210_HandSoldering (layer F.Cu) (tedit 5775960F)
    (at 158.7754 105.0036 180)
    (descr "Resistor SMD 1210, hand soldering")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference R2 (at 0 -2.7 180) (layer F.SilkS) hide)
    (fp_text value 220 (at 1.9812 2.4638 180) (layer F.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 30 D5))
    (pad 2 smd rect (at 2 0 180) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210_HandSoldering (layer B.Cu) (tedit 57755D68)
    (at 178.181 96.52)
    (descr "Resistor SMD 1210, hand soldering")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference R4 (at 0 2.7) (layer B.SilkS) hide)
    (fp_text value 10k (at 0.0635 2.4765) (layer B.SilkS))
    (pad 1 smd rect (at -2 0) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 20 SDA))
    (pad 2 smd rect (at 2 0) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 3 +BATT))
    (model Resistors_SMD.3dshapes/R_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1210_HandSoldering (layer B.Cu) (tedit 577559E8)
    (at 185.547 96.4565 180)
    (descr "Resistor SMD 1210, hand soldering")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference R5 (at 0 -0.4445 180) (layer B.SilkS) hide)
    (fp_text value 10k (at 0 -2.413 180) (layer B.SilkS))
    (pad 1 smd rect (at -2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 21 SCL))
    (pad 2 smd rect (at 2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 3 +BATT))
    (model Resistors_SMD.3dshapes/R_1210_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 57759467)
    (at 146.2532 80.3148)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 577595CD)
    (at 146.4056 104.9782)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text H (at 151.8666 104.0638) (layer B.SilkS))
  (gr_text O (at 150.749 101.9302) (layer B.SilkS))
  (gr_text - (at 187.1726 85.4202) (layer F.SilkS))
  (gr_text out (at 186.3598 88.5444) (layer F.SilkS))
  (gr_text in (at 186.4106 79.502) (layer F.SilkS))
  (gr_text GND (at 147.4216 91.0844 270) (layer F.SilkS))
  (gr_text SCL (at 147.5232 86.7918 270) (layer F.SilkS))
  (dimension 20 (width 0.3) (layer Dwgs.User)
    (gr_text "20,000 mm" (at 199.227 93.171 90) (layer Dwgs.User))
    (feature1 (pts (xy 163.877 83.171) (xy 200.577 83.171)))
    (feature2 (pts (xy 163.877 103.171) (xy 200.577 103.171)))
    (crossbar (pts (xy 197.877 103.171) (xy 197.877 83.171)))
    (arrow1a (pts (xy 197.877 83.171) (xy 198.463421 84.297504)))
    (arrow1b (pts (xy 197.877 83.171) (xy 197.290579 84.297504)))
    (arrow2a (pts (xy 197.877 103.171) (xy 198.463421 102.044496)))
    (arrow2b (pts (xy 197.877 103.171) (xy 197.290579 102.044496)))
  )
  (dimension 30 (width 0.3) (layer Dwgs.User)
    (gr_text "30,000 mm" (at 137.527 93.171 90) (layer Dwgs.User))
    (feature1 (pts (xy 142.877 78.171) (xy 136.177 78.171)))
    (feature2 (pts (xy 142.877 108.171) (xy 136.177 108.171)))
    (crossbar (pts (xy 138.877 108.171) (xy 138.877 78.171)))
    (arrow1a (pts (xy 138.877 78.171) (xy 139.463421 79.297504)))
    (arrow1b (pts (xy 138.877 78.171) (xy 138.290579 79.297504)))
    (arrow2a (pts (xy 138.877 108.171) (xy 139.463421 107.044496)))
    (arrow2b (pts (xy 138.877 108.171) (xy 138.290579 107.044496)))
  )
  (dimension 50 (width 0.3) (layer Dwgs.User)
    (gr_text "50,000 mm" (at 168.877 71.821) (layer Dwgs.User))
    (feature1 (pts (xy 193.877 77.171) (xy 193.877 70.471)))
    (feature2 (pts (xy 143.877 77.171) (xy 143.877 70.471)))
    (crossbar (pts (xy 143.877 73.171) (xy 193.877 73.171)))
    (arrow1a (pts (xy 193.877 73.171) (xy 192.750496 73.757421)))
    (arrow1b (pts (xy 193.877 73.171) (xy 192.750496 72.584579)))
    (arrow2a (pts (xy 143.877 73.171) (xy 145.003504 73.757421)))
    (arrow2b (pts (xy 143.877 73.171) (xy 145.003504 72.584579)))
  )
  (gr_text D1 (at 151.257 98.679 270) (layer F.SilkS))
  (gr_text D2 (at 151.257 96.012 270) (layer F.SilkS))
  (gr_text BAT+ (at 151.257 93.6244 270) (layer F.SilkS))
  (gr_text SDA (at 151.2824 86.7918 270) (layer F.SilkS))
  (gr_text SCL (at 151.257 88.4936 270) (layer F.SilkS))
  (gr_text GND (at 151.2062 90.4748 270) (layer F.SilkS))
  (gr_text BAT+ (at 147.447 93.218 270) (layer F.SilkS))
  (gr_text A1 (at 147.3708 98.7298 270) (layer F.SilkS))
  (gr_text A2 (at 147.3708 96.0882 270) (layer F.SilkS))
  (gr_text SDA (at 147.3962 88.519 270) (layer F.SilkS))
  (gr_text "Serial Connection" (at 188.6585 82.9945 90) (layer F.SilkS))
  (gr_text Regulator (at 173.6725 88.4555) (layer B.SilkS))
  (gr_text Jumper (at 181.991 88.4555) (layer B.SilkS))
  (gr_text "Coin Cell\nBattery" (at 163.8935 95.758) (layer B.SilkS))
  (gr_line (start 143.637 77.597) (end 143.637 107.823) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.675 77.597) (end 143.637 77.597) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.675 107.823) (end 193.675 77.597) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.637 107.823) (end 193.675 107.823) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.7386 77.851) (xy 193.4972 77.851) (xy 193.421 107.5182) (xy 143.6878 107.5436)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 143.7132 77.851) (xy 193.4972 77.8256) (xy 193.4718 107.4928) (xy 143.6878 107.5436)
      )
    )
  )
)
