(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu16.04.1-stable)
  (general
    (links 57)
    (no_connects 0)
    (area 86.949999 83.449999 136.050001 133.550001)
    (thickness 1.6)
    (drawings 9)
    (tracks 177)
    (zones 0)
    (modules 13)
    (nets 39)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010e0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gbr))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 +5V)
  (net 4 +3V3)
  (net 5 A7)
  (net 6 A6)
  (net 7 "Net-(IC1-Pad1)")
  (net 8 "Net-(IC1-Pad2)")
  (net 9 "Net-(IC1-Pad3)")
  (net 10 D2)
  (net 11 D3)
  (net 12 D4)
  (net 13 D5)
  (net 14 D6)
  (net 15 D7)
  (net 16 D8)
  (net 17 D9)
  (net 18 NSS)
  (net 19 MOSI)
  (net 20 MISO)
  (net 21 SCK)
  (net 22 A0)
  (net 23 A1)
  (net 24 A2)
  (net 25 A3)
  (net 26 "Net-(IC1-Pad22)")
  (net 27 A4)
  (net 28 A5)
  (net 29 "Net-(U2-Pad1)")
  (net 30 "Net-(U2-Pad3)")
  (net 31 "Net-(U2-Pad4)")
  (net 32 "Net-(U2-Pad5)")
  (net 33 "Net-(U2-Pad6)")
  (net 34 "Net-(U2-Pad7)")
  (net 35 "Net-(U2-Pad10)")
  (net 36 "Net-(U2-Pad16)")
  (net 37 "Net-(IC1-Pad23)")
  (net 38 "Net-(CON1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net A6)
    (add_net A7)
    (add_net D2)
    (add_net D3)
    (add_net D4)
    (add_net D5)
    (add_net D6)
    (add_net D7)
    (add_net D8)
    (add_net D9)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net NSS)
    (add_net "Net-(CON1-Pad3)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad23)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
    (add_net SCK)
    (add_net VCC)
  )
  (module mysensors_radios:RFM69HW_SMD_ThroughHole_Handsoldering (layer F.Cu) (tedit 55DEED2C)
    (at 115.1 87.5)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U2 (at 0.254 -1.778) (layer F.SilkS))
    (fp_text value RFM69HW (at 8.382 7.112) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U2-Pad1)"))
    (pad 2 smd rect (at -1.4 2) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 D2))
    (pad 3 smd rect (at -1.4 4) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -1.4 6) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -1.4 8) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at -1.4 10) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -1.4 12) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at -1.4 14) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 +3V3))
    (pad 9 smd rect (at 18.3 14) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 18.3 12) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U2-Pad10)"))
    (pad 11 smd rect (at 18.3 10) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 18.3 8) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 SCK))
    (pad 13 smd rect (at 18.3 6) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 MISO))
    (pad 14 smd rect (at 18.3 4) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 MOSI))
    (pad 15 smd rect (at 18.3 2) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 NSS))
    (pad 16 smd rect (at 18.3 0) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U2-Pad16)"))
    (pad 1 thru_hole rect (at -0.1 0) (size 2 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U2-Pad1)"))
    (pad 2 thru_hole circle (at -0.1 2) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 D2))
    (pad 3 thru_hole circle (at -0.1 4) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U2-Pad3)"))
    (pad 4 thru_hole circle (at -0.1 6) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(U2-Pad4)"))
    (pad 5 thru_hole circle (at -0.1 8) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(U2-Pad5)"))
    (pad 6 thru_hole circle (at -0.1 10) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(U2-Pad6)"))
    (pad 7 thru_hole circle (at -0.1 12) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(U2-Pad7)"))
    (pad 8 thru_hole circle (at -0.1 14) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +3V3))
    (pad 9 thru_hole circle (at 17 14) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole circle (at 17 12) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(U2-Pad10)"))
    (pad 11 thru_hole circle (at 17 10) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 12 thru_hole circle (at 17 8) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 SCK))
    (pad 13 thru_hole circle (at 17 6) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 MISO))
    (pad 14 thru_hole circle (at 17 4) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 MOSI))
    (pad 15 thru_hole circle (at 17 2) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 NSS))
    (pad 16 thru_hole circle (at 17 0) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(U2-Pad16)"))
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/rfm69hw.wrl
      (at (xyz 0.333 -0.275 0.345))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0.332 -0.08 0.375))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_strip_2mm_8.wrl
      (at (xyz -0.004 -0.276 0.31))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_strip_2mm_8.wrl
      (at (xyz 0.669 -0.276 0.31))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_socket_2mm_8.wrl
      (at (xyz -0.004 -0.276 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_socket_2mm_8.wrl
      (at (xyz 0.669 -0.276 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.205 -0.445 0.375))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D6_P5 (layer F.Cu) (tedit 58060E93)
    (at 132.925 117.35 90)
    (descr "Capacitor 6mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C1 (at -2 0.1 180) (layer F.SilkS))
    (fp_text value "0.33 u" (at 7.2 0.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D6_P5 (layer F.Cu) (tedit 58060E7D)
    (at 120 112.5 270)
    (descr "Capacitor 6mm Disc, Pitch 5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 2.1 3.3 450) (layer F.SilkS))
    (fp_text value "0.1 u" (at -2.4 -0.1 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D6_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 58060E9E)
    (at 118 105.5)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C3 (at 5.3 -1.9) (layer F.SilkS))
    (fp_text value 47u (at 5.9 0.2) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_arduino:pro_mini (layer F.Cu) (tedit 58060E3C)
    (at 98 104.5 90)
    (descr "IC, ARDUINO_PRO_MINI x 0,6\"")
    (tags "DIL ARDUINO PRO MINI")
    (fp_text reference IC1 (at -18.5 -7.8 180) (layer F.SilkS))
    (fp_text value ArduinoProMini (at 0 0 90) (layer F.Fab) hide)
    (pad 28 thru_hole oval (at 5.08 -5.08 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 A7))
    (pad 27 thru_hole oval (at 7.62 -5.08 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 A6))
    (pad 1 thru_hole oval (at -13.97 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(IC1-Pad1)"))
    (pad 2 thru_hole oval (at -11.43 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(IC1-Pad2)"))
    (pad 3 thru_hole oval (at -8.89 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(IC1-Pad3)"))
    (pad 4 thru_hole oval (at -6.35 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at -3.81 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 10 D2))
    (pad 6 thru_hole oval (at -1.27 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 11 D3))
    (pad 7 thru_hole oval (at 1.27 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 12 D4))
    (pad 8 thru_hole oval (at 3.81 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 13 D5))
    (pad 9 thru_hole oval (at 6.35 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 14 D6))
    (pad 10 thru_hole oval (at 8.89 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 15 D7))
    (pad 11 thru_hole oval (at 11.43 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 16 D8))
    (pad 12 thru_hole oval (at 13.97 7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 17 D9))
    (pad 13 thru_hole oval (at 13.97 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 18 NSS))
    (pad 14 thru_hole oval (at 11.43 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 19 MOSI))
    (pad 15 thru_hole oval (at 8.89 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 20 MISO))
    (pad 16 thru_hole oval (at 6.35 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 21 SCK))
    (pad 17 thru_hole oval (at 3.81 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 22 A0))
    (pad 18 thru_hole oval (at 1.27 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 23 A1))
    (pad 19 thru_hole oval (at -1.27 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 24 A2))
    (pad 20 thru_hole oval (at -3.81 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 25 A3))
    (pad 21 thru_hole oval (at -6.35 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (pad 22 thru_hole oval (at -8.89 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(IC1-Pad22)"))
    (pad 23 thru_hole oval (at -11.43 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(IC1-Pad23)"))
    (pad 24 thru_hole oval (at -13.97 -7.62 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 25 thru_hole oval (at -2.54 -5.08 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 27 A4))
    (pad 26 thru_hole oval (at -5.08 -5.08 90) (size 1.50114 2.19964) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 28 A5))
    (pad 27 thru_hole oval (at 13.97 -5.08 90) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 6 A6))
    (pad 28 thru_hole oval (at 13.97 -2.54 90) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 5 A7))
    (pad 29 thru_hole oval (at 13.97 0 90) (size 2.19964 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz -0.15 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03.wrl
      (at (xyz 0.55 0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0 0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x12.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.25 0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_arduino.3dshapes/arduino_pro_mini.wrl
      (at (xyz -0.05 0 0.48))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model SMD_Packages.3dshapes/TQFP-32.wrl
      (at (xyz 0.05 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 315))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 -0.3 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x12.wrl
      (at (xyz 0 0.3 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0.55 0.1 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0.25 0.2 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz -0.15 0.2 0.445))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (at (xyz -0.3 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl
      (at (xyz 0.55 -0.175 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Angled_1x06.wrl
      (at (xyz -0.65 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz -0.3 -0.05 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0.55 -0.125 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz -0.3 0.05 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (at (xyz -0.35 0.15 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeS_EIA-3216.wrl
      (at (xyz -0.35 -0.15 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz -0.4 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz -0.5 0 0.5125))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 58060E5D)
    (at 119.2 122.3)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at 0 10.2) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 -3.1) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x04.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 58060E2F)
    (at 112.6 122.9 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 0.1 -2.8 180) (layer F.SilkS))
    (fp_text value CONN_01X08 (at -0.3 -3.4 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 D3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 D4))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 D5))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 D6))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 D7))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 D8))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 D9))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08 (layer F.Cu) (tedit 58060E33)
    (at 108 128.4 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -0.1 -3 270) (layer F.SilkS))
    (fp_text value CONN_01X08 (at 0 -3.1 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 A0))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 A1))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 A2))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 A3))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 A4))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 A5))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 A6))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 A7))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x08.wrl
      (at (xyz 0 -0.35 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_lm7805:TO-220_Neutral123_Vertical (layer F.Cu) (tedit 580618CB)
    (at 126.175 114.55 90)
    (descr "TO-220, Neutral, Vertical,")
    (tags "TO-220, Neutral, Vertical,")
    (fp_text reference U1 (at -6.55 -1.15 180) (layer F.SilkS))
    (fp_text value LM7805 (at -0.3 2.8 90) (layer F.Fab))
    (pad GND thru_hole oval (at 0 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad VI thru_hole oval (at -2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC))
    (pad VO thru_hole oval (at 2.54 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 +5V))
    (model TO_SOT_Packages_THT.3dshapes/TO-220_Neutral123_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 58061EEC)
    (at 114.325 129.975)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_2mmDrill (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask F.SilkS))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 58061ED5)
    (at 130.375 106)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_2mmDrill (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask F.SilkS))
  )
  (module Wire_Pads:SolderWirePad_single_2mmDrill (layer F.Cu) (tedit 58061EE4)
    (at 100.525 100.075)
    (fp_text reference REF** (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value SolderWirePad_single_2mmDrill (at -0.635 3.81) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 4.50088 4.50088) (drill 1.99898) (layers *.Cu *.Mask F.SilkS))
  )
  (module Connect:BARREL_JACK (layer F.Cu) (tedit 582C24E6)
    (at 128.8 129.5 90)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference CON1 (at 10.09904 0 180) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -5.99948 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 6.20014 0 90) (size 3.50012 3.50012) (drill oval 1.00076 2.99974) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole rect (at 0.20066 0 90) (size 3.50012 3.50012) (drill oval 1.00076 2.99974) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole rect (at 3.2004 4.699 90) (size 3.50012 3.50012) (drill oval 2.99974 1.00076) (layers *.Cu *.Mask)
      (net 38 "Net-(CON1-Pad3)"))
  )
  (gr_text FTDI (at 97.8 123.9) (layer F.SilkS))
  (dimension 49.2 (width 0.3) (layer Margin)
    (gr_text "49,200 mm" (at 111.5 141.95) (layer Margin))
    (feature1 (pts (xy 86.9 138.1) (xy 86.9 143.3)))
    (feature2 (pts (xy 136.1 138.1) (xy 136.1 143.3)))
    (crossbar (pts (xy 136.1 140.6) (xy 86.9 140.6)))
    (arrow1a (pts (xy 86.9 140.6) (xy 88.026504 140.013579)))
    (arrow1b (pts (xy 86.9 140.6) (xy 88.026504 141.186421)))
    (arrow2a (pts (xy 136.1 140.6) (xy 134.973496 140.013579)))
    (arrow2b (pts (xy 136.1 140.6) (xy 134.973496 141.186421)))
  )
  (dimension 49.9001 (width 0.3) (layer Margin)
    (gr_text "49,900 mm" (at 78.300021 108.537875 89.88517895) (layer Margin))
    (feature1 (pts (xy 84.4 83.6) (xy 77.000024 83.58517)))
    (feature2 (pts (xy 84.3 133.5) (xy 76.900024 133.48517)))
    (crossbar (pts (xy 79.600019 133.490581) (xy 79.700019 83.590581)))
    (arrow1a (pts (xy 79.700019 83.590581) (xy 80.284181 84.718258)))
    (arrow1b (pts (xy 79.700019 83.590581) (xy 79.111342 84.715907)))
    (arrow2a (pts (xy 79.600019 133.490581) (xy 80.188696 132.365255)))
    (arrow2b (pts (xy 79.600019 133.490581) (xy 79.015857 132.362904)))
  )
  (gr_line (start 136 133.5) (end 136 83.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 87 133.5) (end 136 133.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 87 133.5) (end 87 83.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 87 83.5) (end 136 83.5) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "D3 D4 D5 D6 D7 D8 D9 GND" (at 110.1 113.8 90) (layer F.SilkS))
  (gr_text "A7 A6 A5 A4 A3 A2 A1 A0" (at 99.2 130.9) (layer F.SilkS))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 87 83.5) (xy 136 83.5) (xy 136 133.5) (xy 87 133.5)
      )
    )
  )
)
