(kicad_pcb (version 20170123) (host pcbnew no-vcs-found-c20cf4a~58~ubuntu16.04.1)
  (general
    (links 98)
    (no_connects 0)
    (area 70.790999 72.315476 115.566 93.727001)
    (thickness 1.6)
    (drawings 15)
    (tracks 423)
    (zones 0)
    (modules 39)
    (nets 34)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.12)
    (pad_size 0.8 0.8)
    (pad_drill 0.4)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(C4-Pad2)")
  (net 4 /RST)
  (net 5 /DTR)
  (net 6 +3V3)
  (net 7 "Net-(C12-Pad1)")
  (net 8 /MISO)
  (net 9 /SCK)
  (net 10 /MOSI)
  (net 11 "Net-(D1-Pad2)")
  (net 12 "Net-(D2-Pad2)")
  (net 13 "Net-(D3-Pad2)")
  (net 14 "Net-(P1-Pad2)")
  (net 15 "Net-(P1-Pad3)")
  (net 16 "Net-(P2-Pad1)")
  (net 17 /GW_RX_LED)
  (net 18 /GW_TX_LED)
  (net 19 /GW_ERR_LED)
  (net 20 "Net-(R5-Pad1)")
  (net 21 "Net-(U1-Pad5)")
  (net 22 "Net-(U1-Pad4)")
  (net 23 "Net-(U1-Pad3)")
  (net 24 /SER_TX)
  (net 25 /SER_RX)
  (net 26 "Net-(IC1-Pad8)")
  (net 27 "Net-(IC1-Pad7)")
  (net 28 /ATSHA204A)
  (net 29 /RFM69W_INT)
  (net 30 /RFM69W_SS)
  (net 31 "Net-(C5-Pad2)")
  (net 32 "Net-(R7-Pad1)")
  (net 33 "Net-(R8-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /ATSHA204A)
    (add_net /DTR)
    (add_net /GW_ERR_LED)
    (add_net /GW_RX_LED)
    (add_net /GW_TX_LED)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RFM69W_INT)
    (add_net /RFM69W_SS)
    (add_net /RST)
    (add_net /SCK)
    (add_net /SER_RX)
    (add_net /SER_TX)
    (add_net GND)
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R7-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
  )
  (module myfootprints:USB_A_bottom (layer F.Cu) (tedit 58D0FA2F)
    (at 76.20488 80.30914 270)
    (descr "USB A connector")
    (tags "USB USB_A")
    (fp_text reference P1 (at 5.28886 1.52888 270) (layer B.SilkS))
    (fp_text value USB_A (at 1.98686 1.52888 270) (layer B.SilkS))
    (pad 4 thru_hole circle (at 7.11286 -0.00212 180) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole circle (at 4.57286 -0.00212 180) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 15 "Net-(P1-Pad3)"))
    (pad 2 thru_hole circle (at 2.54086 -0.00212 180) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 14 "Net-(P1-Pad2)"))
    (pad 1 thru_hole circle (at 0.00086 -0.00212 180) (size 1.50114 1.50114) (drill 1.00076) (layers *.Cu *.Mask)
      (net 31 "Net-(C5-Pad2)"))
    (pad 5 thru_hole circle (at 10.16086 2.66488 180) (size 2.99974 2.99974) (drill 2.30124) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -3.55514 2.66488 180) (size 2.99974 2.99974) (drill 2.30124) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connectors_Other.3dshapes/usb_A_male_tht.stp
      (at (xyz 0.2755905511811024 -0.01181102362204724 -0.01181102362204724))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.00mm (layer F.Cu) (tedit 588B057F)
    (at 112.776 92.202)
    (descr "Through hole straight pin header, 1x01, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.00mm single row")
    (fp_text reference P2 (at 0 -2.12) (layer F.SilkS))
    (fp_text value ANTENNA (at -3.376 0.398) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(P2-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.00mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:ZTTCS-3 (layer B.Cu) (tedit 588076C0)
    (at 91.44 78.74 180)
    (attr smd)
    (fp_text reference X1 (at -3.81 2.032 270) (layer B.SilkS))
    (fp_text value 16MHz (at -3.81 -0.762 270) (layer B.SilkS))
    (pad 3 smd rect (at 1.95 0 180) (size 0.8 5.1) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(IC1-Pad7)"))
    (pad 2 smd rect (at 0 0 180) (size 1.3 5.1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.95 0 180) (size 0.8 5.1) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(IC1-Pad8)"))
    (model ${KISYS3DMOD}/Oscillators.3dshapes/ZTTCS_MX_ceramic_resonator.stp
      (at (xyz 0 0 0.0003937007874015749))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:OSHW-Logo_5.7x6mm_SilkScreen locked (layer B.Cu) (tedit 0)
    (at 102.616 89.662 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 587E292F)
    (at 79.502 90.612 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 1.082 -1.414 270) (layer F.SilkS))
    (fp_text value 22u (at -0.95 -1.27 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 587E27E6)
    (at 96.332 74.676 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -5.268 0 180) (layer B.SilkS))
    (fp_text value 100n (at -3.236 0 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 587F2880)
    (at 111.506 78.74 90)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW1 (at -0.254 -2.54 90) (layer F.SilkS))
    (fp_text value RESET (at -0.254 2.794 90) (layer F.SilkS))
    (pad 2 smd rect (at 2.7 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.7 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /RST))
    (model ${KISYS3DMOD}/Button_Switches_SMD.3dshapes/SW_SPST_EVQPE1.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 587E266A)
    (at 98.74 83.566 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -1.336 1.27 180) (layer B.SilkS))
    (fp_text value 100n (at 0.95 1.27 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 587E25EF)
    (at 87.376 84.728 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -1.336 1.162 180) (layer B.SilkS))
    (fp_text value 100n (at 0.95 1.162 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 587E25CA)
    (at 87.376 86.868)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.286 1.27) (layer B.SilkS))
    (fp_text value 100n (at 0.254 1.27) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 587E2648)
    (at 98.74 85.852 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -1.082 1.016 180) (layer B.SilkS))
    (fp_text value 100n (at 0.95 1.016 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C4-Pad2)"))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 587E25DB)
    (at 87.63 91.186 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -1.524 -1.524 180) (layer B.SilkS))
    (fp_text value 100n (at 0.762 -1.524 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 /DTR))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 /RST))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 587E2819)
    (at 83.378 74.76 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 2.606 0.338 180) (layer B.SilkS))
    (fp_text value 1u (at 4.13 0.338 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 587E2831)
    (at 108.27 74.676 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -5.268 0 180) (layer B.SilkS))
    (fp_text value 100n (at -2.982 0 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 587E253C)
    (at 81.31 79.5 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at -0.8 -1.24 270) (layer B.SilkS))
    (fp_text value 1u (at 1.018 -1.24 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 587E2806)
    (at 88.58 74.73)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 4.384 -0.054) (layer B.SilkS))
    (fp_text value 1u (at 2.606 -0.054) (layer B.SilkS))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 587E2524)
    (at 79.07 79.51 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 1.278 -1.092 90) (layer B.SilkS))
    (fp_text value 100n (at -1.008 -1.092 90) (layer B.SilkS))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C12-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:AVR_ISP_SMT_Small_02x03 (layer B.Cu) (tedit 58734B48)
    (at 110.998 79.756 180)
    (descr "SMT pin header")
    (tags "SMT pin header")
    (attr smd)
    (fp_text reference CON1 (at 5.334 0.254 270) (layer B.SilkS))
    (fp_text value AVR-ISP-6 (at 4.318 0 270) (layer B.SilkS))
    (pad 1 smd rect (at -2.5 -2 180) (size 1.27 2.5) (layers B.Cu B.Paste B.Mask)
      (net 8 /MISO))
    (pad 3 smd rect (at 0 -2 180) (size 1.27 2.5) (layers B.Cu B.Paste B.Mask)
      (net 9 /SCK))
    (pad 5 smd rect (at 2.54 -2 180) (size 1.27 2.5) (layers B.Cu B.Paste B.Mask)
      (net 4 /RST))
    (pad 6 smd rect (at 2.54 2 180) (size 1.27 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0 2 180) (size 1.27 2.5) (layers B.Cu B.Paste B.Mask)
      (net 10 /MOSI))
    (pad 2 smd rect (at -2.54 2 180) (size 1.27 2.5) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 587E26E4)
    (at 112.814 84.836 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value RX (at -1.994 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LED_Packages_SMD.3dshapes/led_chip_0603_green.stp
      (at (xyz 0 0 0.0003937007874015749))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 587E26DB)
    (at 112.738 87.376 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 1.27 180) (layer F.SilkS))
    (fp_text value TX (at -2.07 0 270) (layer F.SilkS))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_Packages_SMD.3dshapes/led_chip_0603_blue.stp
      (at (xyz 0 0 0.0003937007874015749))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 587E26D4)
    (at 112.814 89.916 180)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 0.038 1.27 180) (layer F.SilkS))
    (fp_text value ERR (at -1.994 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.8 0) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LED_Packages_SMD.3dshapes/led_chip_0603_red.stp
      (at (xyz 0 0 0.0003937007874015749))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_DFN_QFN:QFN-32-1EP_5x5mm_Pitch0.5mm (layer B.Cu) (tedit 587E261F)
    (at 93.3185 85.878)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference IC1 (at 1.6775 3.53) (layer B.SilkS))
    (fp_text value ATMEGA328P-MU (at -3.9105 3.53) (layer B.SilkS))
    (pad 33 smd rect (at -0.8625 0.8625) (size 1.725 1.725) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 -0.8625) (size 1.725 1.725) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 0.8625) (size 1.725 1.725) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 -0.8625) (size 1.725 1.725) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 32 smd rect (at -1.75 2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 29 /RFM69W_INT))
    (pad 31 smd rect (at -1.25 2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 25 /SER_RX))
    (pad 30 smd rect (at -0.75 2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 24 /SER_TX))
    (pad 29 smd rect (at -0.25 2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 4 /RST))
    (pad 28 smd rect (at 0.25 2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 27 smd rect (at 0.75 2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 26 smd rect (at 1.25 2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 28 /ATSHA204A))
    (pad 25 smd rect (at 1.75 2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 19 /GW_ERR_LED))
    (pad 24 smd rect (at 2.4 1.75) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /GW_TX_LED))
    (pad 23 smd rect (at 2.4 1.25) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 17 /GW_RX_LED))
    (pad 22 smd rect (at 2.4 0.75) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 21 smd rect (at 2.4 0.25) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 20 smd rect (at 2.4 -0.25) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C4-Pad2)"))
    (pad 19 smd rect (at 2.4 -0.75) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 18 smd rect (at 2.4 -1.25) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 17 smd rect (at 2.4 -1.75) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 9 /SCK))
    (pad 16 smd rect (at 1.75 -2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 8 /MISO))
    (pad 15 smd rect (at 1.25 -2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 10 /MOSI))
    (pad 14 smd rect (at 0.75 -2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 30 /RFM69W_SS))
    (pad 13 smd rect (at 0.25 -2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at -0.25 -2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at -0.75 -2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at -1.25 -2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at -1.75 -2.4 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at -2.4 -1.75) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(IC1-Pad8)"))
    (pad 7 smd rect (at -2.4 -1.25) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(IC1-Pad7)"))
    (pad 6 smd rect (at -2.4 -0.75) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 5 smd rect (at -2.4 -0.25) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -2.4 0.25) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at -2.4 0.75) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -2.4 1.25) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd rect (at -2.4 1.75) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/qfn32_5x5_p05.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 587E2609)
    (at 96.35 91.186 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -1.186 -1.524 180) (layer B.SilkS))
    (fp_text value 10K (at 0.846 -1.524 180) (layer B.SilkS))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 /RST))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587E269D)
    (at 108.374 84.836 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 1.186 1.27 180) (layer F.SilkS))
    (fp_text value 330 (at -0.846 1.27 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /GW_RX_LED))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0.0003937007874015749))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587E2692)
    (at 108.374 87.376 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0.932 1.27 180) (layer F.SilkS))
    (fp_text value 330 (at -1.1 1.27 180) (layer F.SilkS))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 /GW_TX_LED))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0.0003937007874015749))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587E26AE)
    (at 108.374 89.916 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0.678 1.27 180) (layer F.SilkS))
    (fp_text value 330 (at -1.1 1.27 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 /GW_ERR_LED))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0.0003937007874015749))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587E2961)
    (at 106.426 77.978 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -1.016 1.27 90) (layer F.SilkS))
    (fp_text value 56K (at 1.27 1.27 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0.0003937007874015749))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-14_4.4x5mm_Pitch0.65mm (layer B.Cu) (tedit 587E28B6)
    (at 100.74 78.232 180)
    (descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at -3.4 -3.302 180) (layer B.SilkS))
    (fp_text value TXB0104 (at -2.638 -4.318 180) (layer B.SilkS))
    (pad 14 smd rect (at 2.95 1.95 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 13 smd rect (at 2.95 1.3 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 30 /RFM69W_SS))
    (pad 12 smd rect (at 2.95 0.65 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 10 /MOSI))
    (pad 11 smd rect (at 2.95 0 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 8 /MISO))
    (pad 10 smd rect (at 2.95 -0.65 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 9 /SCK))
    (pad 9 smd rect (at 2.95 -1.3 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at 2.95 -1.95 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (pad 7 smd rect (at -2.95 -1.95 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.95 -1.3 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -2.95 -0.65 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(U1-Pad5)"))
    (pad 4 smd rect (at -2.95 0 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(U1-Pad4)"))
    (pad 3 smd rect (at -2.95 0.65 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(U1-Pad3)"))
    (pad 2 smd rect (at -2.95 1.3 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(R5-Pad1)"))
    (pad 1 smd rect (at -2.95 1.95 180) (size 1.45 0.45) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/tssop_14_50x44_p065.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT89-3_Housing (layer B.Cu) (tedit 58D2975C)
    (at 85.598 78.74)
    (descr "SOT89-3, Housing,")
    (tags "SOT89-3, Housing,")
    (attr smd)
    (fp_text reference U2 (at -3.198 -2.54) (layer B.SilkS))
    (fp_text value MCP1703A (at -4.498 -1.64) (layer B.SilkS))
    (pad 2 smd trapezoid (at 0 -0.7493 180) (size 1.50114 0.7493) (rect_delta 0 -0.50038 ) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0 1.09982) (size 1.99898 2.99974) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 3 smd rect (at 1.50114 -1.85166) (size 1.00076 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 6 +3V3))
    (pad 2 smd rect (at 0 -1.85166) (size 1.00076 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1.50114 -1.85166) (size 1.00076 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/SOT_Packages_SMD.3dshapes/SOT89-3.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Housings_DFN_QFN:QFN-28-1EP_5x5mm_Pitch0.5mm (layer B.Cu) (tedit 587E2851)
    (at 81.8635 85.1655)
    (descr "28-Lead Plastic Quad Flat, No Lead Package (MQ) - 5x5x0.9 mm Body [QFN or VQFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U3 (at 2.2105 3.7345) (layer B.SilkS))
    (fp_text value CP2102 (at -0.8375 3.7345) (layer B.SilkS))
    (pad 29 smd rect (at -0.8375 0.8375) (size 1.675 1.675) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 29 smd rect (at -0.8375 -0.8375) (size 1.675 1.675) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 29 smd rect (at 0.8375 0.8375) (size 1.675 1.675) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 29 smd rect (at 0.8375 -0.8375) (size 1.675 1.675) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 28 smd oval (at -1.5 2.45 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /DTR))
    (pad 27 smd oval (at -1 2.45 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 26 smd oval (at -0.5 2.45 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 24 /SER_TX))
    (pad 25 smd oval (at 0 2.45 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 25 /SER_RX))
    (pad 24 smd oval (at 0.5 2.45 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 23 smd oval (at 1 2.45 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 22 smd oval (at 1.5 2.45 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 21 smd oval (at 2.45 1.5) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd oval (at 2.45 1) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 19 smd oval (at 2.45 0.5) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 18 smd oval (at 2.45 0) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 17 smd oval (at 2.45 -0.5) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 16 smd oval (at 2.45 -1) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd oval (at 2.45 -1.5) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd oval (at 1.5 -2.45 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd oval (at 1 -2.45 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd oval (at 0.5 -2.45 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd oval (at 0 -2.45 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd oval (at -0.5 -2.45 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd oval (at -1 -2.45 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd oval (at -1.5 -2.45 270) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 7 smd oval (at -2.45 -1.5) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 6 smd oval (at -2.45 -1) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C12-Pad1)"))
    (pad 5 smd oval (at -2.45 -0.5) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 33 "Net-(R8-Pad1)"))
    (pad 4 smd oval (at -2.45 0) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(R7-Pad1)"))
    (pad 3 smd oval (at -2.45 0.5) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd oval (at -2.45 1) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (pad 1 smd oval (at -2.45 1.5) (size 0.85 0.3) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/Housings_DFN_QFN.3dshapes/qfn28_5x5_0.5.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_radios:RFM69HW_SMD_Handsoldering (layer F.Cu) (tedit 587E3757)
    (at 84.88 76.264)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U4 (at 6.306 -1.588) (layer F.SilkS))
    (fp_text value RFM69W (at 9.862 -1.588) (layer F.SilkS))
    (pad 16 smd rect (at 18.3 0) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 18.3 2) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R5-Pad1)"))
    (pad 14 smd rect (at 18.3 4) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U1-Pad3)"))
    (pad 13 smd rect (at 18.3 6) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U1-Pad4)"))
    (pad 12 smd rect (at 18.3 8) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U1-Pad5)"))
    (pad 11 smd rect (at 18.3 10) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 18.3 12) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(P2-Pad1)"))
    (pad 9 smd rect (at 18.3 14) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -1.4 14) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 +3V3))
    (pad 7 smd rect (at -1.4 12) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -1.4 10) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -1.4 8) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -1.4 6) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.4 4) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.4 2) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 /RFM69W_INT))
    (pad 1 smd rect (at -1.4 0) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Radio_Modules.3dshapes/RFM69W.stp
      (at (xyz 0.6692913385826772 -0.5511811023622047 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 587E2722)
    (at 110.048 85.344)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 2.982 -0.254) (layer B.SilkS))
    (fp_text value 100n (at 2.982 0.508) (layer B.SilkS))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 587E27BD)
    (at 108.966 88.562 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 1.44 -1.27 90) (layer B.SilkS))
    (fp_text value 1K (at -0.592 -1.27 90) (layer B.SilkS))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 28 /ATSHA204A))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 587E26F2)
    (at 111.998 88.458)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U5 (at 2.002 1.142) (layer B.SilkS))
    (fp_text value ATSHA204A (at 0.402 2.142) (layer B.SilkS))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 28 /ATSHA204A))
    (model ${KISYS3DMOD}/SOT_Packages_SMD.3dshapes/SOT23-3.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58D0F779)
    (at 80.5 79.4 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at 2.6 0 90) (layer F.SilkS))
    (fp_text value BLM18HE152SN1D (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C5-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58D0F8F6)
    (at 78.4 79.3 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -2.7 0.5 270) (layer F.SilkS))
    (fp_text value 10u (at -2.9 -0.4 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(C5-Pad2)"))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58D0F8D7)
    (at 79.5 83.3)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at -1.4 -1.8) (layer F.SilkS))
    (fp_text value 10n (at -1.3 -1) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58D29314)
    (at 79.1 87.4 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at -1.5 0.2 180) (layer F.SilkS))
    (fp_text value 22 (at -1.5 -0.7 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(R7-Pad1)"))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(P1-Pad3)"))
    (model Resistors_SMD.3dshapes/R_0402.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 58D29320)
    (at 79.1 85.9 180)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R8 (at -1.5 0.6 180) (layer F.SilkS))
    (fp_text value 22 (at -1.5 -0.3 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.35 180) (layer F.Fab))
    (pad 2 smd rect (at 0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P1-Pad2)"))
    (pad 1 smd rect (at -0.45 0 180) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(R8-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0402.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text + (at 77.3 78) (layer F.SilkS))
  (gr_text + (at 80.3 80.5) (layer B.SilkS))
  (gr_text + (at 78.3 89.6) (layer F.SilkS))
  (gr_text "MySensors RFM69W Serial GW" (at 93.472 92.202) (layer F.SilkS))
  (gr_text "Rev. 0.5" (at 81.534 92.202) (layer B.SilkS))
  (gr_text GND (at 108.458 75.692) (layer B.SilkS))
  (gr_text MOSI (at 110.998 75.692) (layer B.SilkS))
  (gr_text +5V (at 113.792 75.692) (layer B.SilkS))
  (gr_text MISO (at 113.538 83.82) (layer B.SilkS))
  (gr_text SCK (at 110.998 83.82) (layer B.SilkS))
  (gr_text RST (at 108.458 83.82) (layer B.SilkS))
  (gr_line (start 70.866 93.472) (end 70.866 73.66) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.316 93.472) (end 70.866 93.472) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 115.316 73.66) (end 115.316 93.472) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 70.866 73.66) (end 115.316 73.66) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 70.866 73.66) (xy 115.316 73.66) (xy 115.316 93.472) (xy 70.866 93.472)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 70.866 73.66) (xy 115.316 73.66) (xy 115.316 93.472) (xy 70.866 93.472)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.4 84) (xy 115.2 84) (xy 115.2 93.4) (xy 106.4 93.4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 106.4 84) (xy 115.2 84) (xy 115.2 93.4) (xy 106.4 93.4)
      )
    )
  )
)
