(kicad_pcb (version 4) (host pcbnew 4.0.4+e1-6308~48~ubuntu15.10.1-stable)
  (general
    (links 35)
    (no_connects 0)
    (area 133.274999 79.159999 183.425001 129.614341)
    (thickness 1.6)
    (drawings 9)
    (tracks 102)
    (zones 0)
    (modules 15)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (user_trace_width 3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 133.35 79.375)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x310f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory OUTPUT_GERBER/))
  )
  (net 0 "")
  (net 1 /GND)
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad2)")
  (net 4 /3V3)
  (net 5 "Net-(D1-Pad2)")
  (net 6 /FP_OUT)
  (net 7 "Net-(D2-Pad1)")
  (net 8 /OPT1)
  (net 9 /OPT2)
  (net 10 /CE)
  (net 11 /CS)
  (net 12 /MOSI)
  (net 13 /MISO)
  (net 14 /SCK)
  (net 15 /PH_IN)
  (net 16 /NEUTRE)
  (net 17 "Net-(R1-Pad1)")
  (net 18 "Net-(R2-Pad1)")
  (net 19 /VCC)
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3V3)
    (add_net /CE)
    (add_net /CS)
    (add_net /FP_OUT)
    (add_net /GND)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /NEUTRE)
    (add_net /OPT1)
    (add_net /OPT2)
    (add_net /PH_IN)
    (add_net /SCK)
    (add_net /VCC)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(R1-Pad1)")
    (add_net "Net-(R2-Pad1)")
  )
  (module Resistors_ThroughHole:RES35 (layer F.Cu) (tedit 57E8E8E7)
    (at 139.065 127.635)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference R1 (at 3.81 0) (layer F.SilkS))
    (fp_text value 220 (at 6.35 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 8 /OPT1))
    (pad 1 thru_hole circle (at 0.00052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(R1-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Diodes_ThroughHole:Diode_TO-220_Dual_CommonCathode_Vertical (layer F.Cu) (tedit 57E8E8D5)
    (at 180.34 110.49 90)
    (descr "TO-220, Diode, Dual, Common Cathode,Vertical,")
    (tags "TO-220, Diode, Dual, Common Cathode, Vertical,")
    (fp_text reference U3 (at 2.54762 -3.83794 90) (layer F.SilkS))
    (fp_text value LD1117V33 (at 2.54 -1.905 90) (layer F.Fab))
    (pad 2 thru_hole rect (at 2.53746 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 /3V3))
    (pad 1 thru_hole oval (at -0.00254 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 3 thru_hole oval (at 5.07746 0 180) (size 2.49936 1.50114) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 19 /VCC))
    (model Diodes_ThroughHole.3dshapes/Diode_TO-220_Dual_CommonCathode_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier3 (layer F.Cu) (tedit 57E8E961)
    (at 141.605 88.9 270)
    (descr "Bornier d'alimentation 3 pins")
    (tags DEV)
    (fp_text reference P1 (at -1.905 -2.54 270) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 5.08 270) (layer F.Fab))
    (pad 1 thru_hole rect (at -5.08 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 15 /PH_IN))
    (pad 2 thru_hole circle (at 0 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 16 /NEUTRE))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 6 /FP_OUT))
    (model Connect.3dshapes/bornier3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57E8E8F3)
    (at 154.94 125.73 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 1.27 -1.905 270) (layer F.SilkS))
    (fp_text value 22p (at 1.27 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 57E8E8F4)
    (at 170.815 125.73 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at 1.27 -1.905 270) (layer F.SilkS))
    (fp_text value 22p (at 1.27 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L11_P2 (layer F.Cu) (tedit 57E8E8DA)
    (at 180.975 119.38 180)
    (descr "Radial Electrolytic Capacitor 5mm x Length 11mm, Pitch 2mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C3 (at 1 -3.8 180) (layer F.SilkS))
    (fp_text value 1u (at 0.635 -5.08 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 /3V3))
    (pad 2 thru_hole circle (at 2 0 180) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L11_P2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 57E8E943)
    (at 135.89 101.219)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D1 (at 5.08 -0.254) (layer F.SilkS))
    (fp_text value "" (at 6.985 -0.254) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254 180) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 -0.00254 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 6 /FP_OUT))
  )
  (module Diodes_ThroughHole:Diode_DO-41_SOD81_Horizontal_RM10 (layer F.Cu) (tedit 57E8E94E)
    (at 159.512 101.219 180)
    (descr "Diode, DO-41, SOD81, Horizontal, RM 10mm,")
    (tags "Diode, DO-41, SOD81, Horizontal, RM 10mm, 1N4007, SB140,")
    (fp_text reference D2 (at 5.842 0.254 180) (layer F.SilkS))
    (fp_text value "" (at 7.112 -0.381 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16 -0.00254) (size 1.99898 1.99898) (drill 1.27) (layers *.Cu *.Mask F.SilkS)
      (net 6 /FP_OUT))
    (pad 1 thru_hole rect (at 0 -0.00254) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(D2-Pad1)"))
  )
  (module Housings_DIP:DIP-28_W7.62mm_LongPads (layer F.Cu) (tedit 57E8E736)
    (at 141.605 122.555 90)
    (descr "28-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference IC1 (at 0 -5.22 90) (layer F.SilkS))
    (fp_text value ATMEGA328P_Arduino (at 3.81 15.24 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /OPT1))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /OPT2))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 /VCC))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad2)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole oval (at 7.62 33.02 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /CE))
    (pad 16 thru_hole oval (at 7.62 30.48 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 /CS))
    (pad 17 thru_hole oval (at 7.62 27.94 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 /MOSI))
    (pad 18 thru_hole oval (at 7.62 25.4 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 /MISO))
    (pad 19 thru_hole oval (at 7.62 22.86 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 /SCK))
    (pad 20 thru_hole oval (at 7.62 20.32 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 /VCC))
    (pad 21 thru_hole oval (at 7.62 17.78 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 22 thru_hole oval (at 7.62 15.24 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 23 thru_hole oval (at 7.62 12.7 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 24 thru_hole oval (at 7.62 10.16 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 25 thru_hole oval (at 7.62 7.62 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 26 thru_hole oval (at 7.62 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 27 thru_hole oval (at 7.62 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 28 thru_hole oval (at 7.62 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (model Housings_DIP.3dshapes/DIP-28_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:RES35 (layer F.Cu) (tedit 57E8E8E6)
    (at 141.605 125.73)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference R2 (at 3.81 0) (layer F.SilkS))
    (fp_text value 220 (at 6.35 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 9 /OPT2))
    (pad 1 thru_hole circle (at 0.00052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(R2-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module MyLibrary:NRF24L01 (layer B.Cu) (tedit 57E8E95C)
    (at 175.26 98.425 180)
    (fp_text reference U4 (at 2.54 -1.27 180) (layer B.SilkS))
    (fp_text value NRF24L01+ (at 15.5 -14.5 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 1.27 -3.175 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 1 /GND))
    (pad 2 thru_hole circle (at 3.81 -3.175 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 4 /3V3))
    (pad 3 thru_hole circle (at 1.27 -5.715 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 10 /CE))
    (pad 4 thru_hole circle (at 3.81 -5.715 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 11 /CS))
    (pad 5 thru_hole circle (at 1.27 -8.255 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 14 /SCK))
    (pad 6 thru_hole circle (at 3.81 -8.255 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 12 /MOSI))
    (pad 7 thru_hole circle (at 1.27 -10.795 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS)
      (net 13 /MISO))
    (pad 8 thru_hole circle (at 3.81 -10.795 180) (size 2 2) (drill 0.762) (layers *.Cu *.Mask B.SilkS))
  )
  (module MyLibrary:HLK-PM01 (layer F.Cu) (tedit 57E8E957)
    (at 151.13 89.535)
    (fp_text reference U5 (at 11.43 -8.89) (layer F.SilkS))
    (fp_text value HLK-PM01 (at 16.9 -9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.54) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 15 /PH_IN))
    (pad 2 thru_hole circle (at 0 2.54) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 16 /NEUTRE))
    (pad 3 thru_hole circle (at 29.464 -7.62) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 4 thru_hole circle (at 29.464 7.62) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 19 /VCC))
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 57E8E72E)
    (at 163.195 127)
    (descr "Crystal Quarz HC49/U vertical stehend")
    (tags "Crystal Quarz HC49/U vertical stehend")
    (fp_text reference Y1 (at 0 -3.81) (layer F.SilkS))
    (fp_text value Crystal (at 0 1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at -2.44094 0) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 2.44094 0) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad2)"))
  )
  (module Housings_DIP:DIP-6_W7.62mm_LongPads (layer F.Cu) (tedit 57E8E903)
    (at 140.97 111.887 90)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 5.207 2.54 360) (layer F.SilkS))
    (fp_text value MOC3041M (at 3.175 2.54 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(R1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 7.62 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(D1-Pad2)"))
    (pad 5 thru_hole oval (at 7.62 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 7.62 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 /PH_IN))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-6_W7.62mm_LongPads (layer F.Cu) (tedit 57E8E8FF)
    (at 154.432 111.887 90)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at 5.207 2.413 180) (layer F.SilkS))
    (fp_text value MOC3041M (at 3.175 2.54 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(R2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 7.62 5.08 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(D2-Pad1)"))
    (pad 5 thru_hole oval (at 7.62 2.54 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 7.62 0 90) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 /PH_IN))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "MySensors\nFil Pilote" (at 164.465 88.9) (layer B.SilkS))
  (gr_text "MySensors\nFil Pilote" (at 164.465 83.82) (layer F.SilkS))
  (gr_text Out (at 135.255 93.98) (layer F.SilkS))
  (gr_text N (at 135.255 88.9) (layer F.SilkS))
  (gr_text L (at 135.255 83.82) (layer F.SilkS))
  (gr_line (start 133.35 129.375) (end 133.35 79.375) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.35 129.375) (end 133.35 129.375) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.35 79.375) (end 183.35 129.375) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 133.35 79.375) (end 183.35 79.375) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.35 129.375) (xy 183.35 129.375) (xy 183.35 79.375) (xy 172.85 79.375) (xy 170.85 81.375)
        (xy 170.85 96.375) (xy 168.35 98.875) (xy 168.35 107.875) (xy 166.85 109.375) (xy 133.35 109.375)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 183.35 129.375) (xy 133.35 129.375) (xy 133.35 109.375) (xy 166.85 109.375) (xy 168.35 107.875)
        (xy 168.35 98.875) (xy 170.85 96.375) (xy 170.85 81.375) (xy 172.85 79.375) (xy 183.35 79.375)
      )
    )
  )
)
