(kicad_pcb (version 20170123) (host pcbnew no-vcs-found-7591~57~ubuntu16.04.1)
  (general
    (links 126)
    (no_connects 0)
    (area 98.374999 77.229407 146.671501 99.491001)
    (thickness 1.6)
    (drawings 19)
    (tracks 401)
    (zones 0)
    (modules 64)
    (nets 48)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.45)
    (trace_clearance 0.3)
    (zone_clearance 0.5)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.35 0.35)
    (mod_text_width 0.0875)
    (pad_size 0.8 0.8)
    (pad_drill 0.4)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 "Net-(BT1-Pad1)")
  (net 2 GND)
  (net 3 +3V3)
  (net 4 "Net-(C2-Pad2)")
  (net 5 "Net-(C4-Pad2)")
  (net 6 "Net-(C5-Pad1)")
  (net 7 "Net-(C6-Pad2)")
  (net 8 /RESET)
  (net 9 /V_BOOST_IN)
  (net 10 /MISO)
  (net 11 /SCK)
  (net 12 /MOSI)
  (net 13 /C0)
  (net 14 /C1)
  (net 15 "Net-(IC1-Pad7)")
  (net 16 "Net-(IC1-Pad8)")
  (net 17 /C2)
  (net 18 /C3)
  (net 19 /C4)
  (net 20 /C5)
  (net 21 /C6)
  (net 22 /SS)
  (net 23 "Net-(IC1-Pad19)")
  (net 24 "Net-(IC1-Pad22)")
  (net 25 /V_BATT)
  (net 26 "Net-(IC1-Pad31)")
  (net 27 /INT)
  (net 28 "Net-(L2-Pad1)")
  (net 29 "Net-(P1-Pad1)")
  (net 30 "Net-(S1-Pad8)")
  (net 31 "Net-(U1-Pad2)")
  (net 32 "Net-(U1-Pad3)")
  (net 33 "Net-(U2-Pad1)")
  (net 34 "Net-(U2-Pad3)")
  (net 35 "Net-(U2-Pad4)")
  (net 36 "Net-(U2-Pad5)")
  (net 37 "Net-(U2-Pad6)")
  (net 38 "Net-(U2-Pad7)")
  (net 39 "Net-(U2-Pad16)")
  (net 40 /SDA)
  (net 41 /SCL)
  (net 42 "Net-(C12-Pad1)")
  (net 43 "Net-(C13-Pad1)")
  (net 44 /HALL_SENSOR)
  (net 45 /A0)
  (net 46 /A1)
  (net 47 /D0)
  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.45)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /A0)
    (add_net /A1)
    (add_net /C0)
    (add_net /C1)
    (add_net /C2)
    (add_net /C3)
    (add_net /C4)
    (add_net /C5)
    (add_net /C6)
    (add_net /D0)
    (add_net /HALL_SENSOR)
    (add_net /INT)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SS)
    (add_net /V_BATT)
    (add_net /V_BOOST_IN)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad31)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(L2-Pad1)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(S1-Pad8)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
  )
  (module myfootprints:DLJ-3015 (layer F.Cu) (tedit 580DAC1C)
    (at 143.1925 83.693)
    (fp_text reference L2 (at -3.048 1.3462 90) (layer F.SilkS))
    (fp_text value 10uH (at -3.0734 -0.5842 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.3 0) (size 2 3) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(L2-Pad1)"))
    (pad 2 smd rect (at 1.3 0) (size 2 3) (layers F.Cu F.Paste F.Mask)
      (net 9 /V_BOOST_IN))
    (model ${KISYS3DMOD}/Inductors.3dshapes/SDR0302.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:ZTTCR-3 (layer B.Cu) (tedit 5809CF68)
    (at 123.7615 80.9625 90)
    (attr smd)
    (fp_text reference X1 (at -2.794 1.27 180) (layer B.SilkS))
    (fp_text value 8MHz (at -3.6195 0.9525 180) (layer B.SilkS))
    (pad 2 smd rect (at 1.5 0 90) (size 0.8 3) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(IC1-Pad7)"))
    (pad 3 smd rect (at 0 0 90) (size 0.8 3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 0.8 3) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(IC1-Pad8)"))
    (model ${KISYS3DMOD}/Oscillators.3dshapes/zttcr_MG_ceramic_resonator.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 135.5344 84.2607)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 135.5344 83.2607)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 135.5344 82.2607)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 135.5344 81.2607)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 135.5344 80.2607)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 135.5344 79.2607)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 118.2464 88.6046)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 117.2464 88.6046)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 118.2464 87.6046)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 117.2464 87.6046)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 100.8474 98.409)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 99.8474 98.409)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 100.8474 97.409)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 99.8474 97.409)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 132.1148 97.7994)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 131.1148 97.7994)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 132.1148 96.7994)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 131.1148 96.7994)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 136.5217 89.2203)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 135.5217 89.2203)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 136.5217 88.2203)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 135.5217 88.2203)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 136.5217 87.2203)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 135.5217 87.2203)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 136.5217 86.2203)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO14580_Pad (layer F.Cu) (tedit 5809CED3)
    (at 145.161 87.9475)
    (descr "Mounting Hole 2.2mm, M2, ISO14580")
    (tags "mounting hole 2.2mm m2 iso14580")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO14580_Pad (at 0 2.9) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 2 2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (zone_connect 2))
  )
  (module mysensors_connectors:CR123_holder (layer B.Cu) (tedit 5809CED3)
    (at 103.404 87.884 270)
    (descr "CR123 battery holder")
    (tags "Battery holder, CR123")
    (fp_text reference BT1 (at -0.0635 -1.879 90) (layer B.SilkS))
    (fp_text value "CR123A - 3V" (at 0.635 1.931 270) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask B.SilkS)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole circle (at 0 -37.82 270) (size 2.54 2.54) (drill 1.3) (layers *.Cu *.Mask B.SilkS)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 8.1 0 270) (size 1.98 1.98) (drill 1.98) (layers *.Cu Dwgs.User))
    (model ${KISYS3DMOD}/Battery_Holders.3dshapes/cr123_holder.stp
      (at (xyz 0 0 0.07874015748031496))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5809CED3)
    (at 104.8385 90.805 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R7 (at 1.0795 0 180) (layer F.SilkS))
    (fp_text value VB_DIS (at 0.381 1.143 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(BT1-Pad1)"))
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeA_EIA-3216_Wave (layer F.Cu) (tedit 5809CED3)
    (at 136.9695 94.2975 90)
    (descr "Tantal Cap. , Size A, EIA-3216, Wave,")
    (tags "Tantal Cap. , Size A, EIA-3216, Wave,")
    (attr smd)
    (fp_text reference C6 (at -3.7465 -0.381 180) (layer F.SilkS))
    (fp_text value 47u (at -3.81 1.143 180) (layer F.SilkS))
    (fp_text user + (at -3.59918 -1.80086 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.50114 0 90) (size 2.14884 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (pad 1 smd rect (at -1.50114 0 90) (size 2.14884 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/Tantalum_A_3216H18.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5809CED3)
    (at 118.3005 79.9465 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 1.651 1.3335 180) (layer B.SilkS))
    (fp_text value 100n (at 0.9525 1.7145 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_0603_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5809CED3)
    (at 120.523 93.98 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at -1.1455 -1.2065 180) (layer B.SilkS))
    (fp_text value 100n (at 0.5055 -1.143 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/c_0603_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5809CED3)
    (at 116.078 79.883 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0.127 1.651) (layer B.SilkS))
    (fp_text value 100n (at 0.9525 1.8415) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/c_0603_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5809CED3)
    (at 116.9645 93.98)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0.828 1.143) (layer B.SilkS))
    (fp_text value 100n (at -1.0135 1.143) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/c_0603_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5809CED3)
    (at 144.145 95.377 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -1.458 1.27 90) (layer F.SilkS))
    (fp_text value 100n (at 0.828 1.27 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_0603_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5809CED3)
    (at 109.2835 87.4395)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 1.016 1.2065) (layer B.SilkS))
    (fp_text value 100n (at -1.016 1.2065) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 8 /RESET))
    (model Capacitors_SMD.3dshapes/c_0603_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5809CED3)
    (at 134.3025 95.316 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at 1.5215 1.143 90) (layer F.SilkS))
    (fp_text value 100n (at -0.2565 1.143 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_0603_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5809CED3)
    (at 101.6635 90.932 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 1.8415 1.0795 180) (layer F.SilkS))
    (fp_text value 100n (at 2.286 -0.3175 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_0603_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer B.Cu) (tedit 5809CED3)
    (at 117.348 87.376 270)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 0 -1.27 270) (layer B.SilkS) hide)
    (fp_text value ATMEGA328P-A (at -0.4445 0) (layer B.SilkS))
    (fp_text user %R (at -1.4605 -2.0955) (layer B.SilkS))
    (pad 1 smd rect (at -4.25 2.8 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 13 /C0))
    (pad 2 smd rect (at -4.25 2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 14 /C1))
    (pad 3 smd rect (at -4.25 1.2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -4.25 0.4 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 5 smd rect (at -4.25 -0.4 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.25 -1.2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 7 smd rect (at -4.25 -2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -4.25 -2.8 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -2.8 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 17 /C2))
    (pad 10 smd rect (at -2 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 18 /C3))
    (pad 11 smd rect (at -1.2 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 19 /C4))
    (pad 12 smd rect (at -0.4 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 20 /C5))
    (pad 13 smd rect (at 0.4 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 21 /C6))
    (pad 14 smd rect (at 1.2 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 22 /SS))
    (pad 15 smd rect (at 2 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 12 /MOSI))
    (pad 16 smd rect (at 2.8 -4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 10 /MISO))
    (pad 17 smd rect (at 4.25 -2.8 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 11 /SCK))
    (pad 18 smd rect (at 4.25 -2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 19 smd rect (at 4.25 -1.2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.25 -0.4 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C4-Pad2)"))
    (pad 21 smd rect (at 4.25 0.4 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 4.25 1.2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.25 2 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 45 /A0))
    (pad 24 smd rect (at 4.25 2.8 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 46 /A1))
    (pad 25 smd rect (at 2.8 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 25 /V_BATT))
    (pad 26 smd rect (at 2 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 44 /HALL_SENSOR))
    (pad 27 smd rect (at 1.2 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 40 /SDA))
    (pad 28 smd rect (at 0.4 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 41 /SCL))
    (pad 29 smd rect (at -0.4 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /RESET))
    (pad 30 smd rect (at -1.2 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 47 /D0))
    (pad 31 smd rect (at -2 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(IC1-Pad31)"))
    (pad 32 smd rect (at -2.8 4.25 180) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 27 /INT))
    (model Housings_QFP.3dshapes/qfp32_7x7_p08.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5809CED3)
    (at 124.2695 94.234 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference L1 (at -2.3495 0.635 180) (layer B.SilkS))
    (fp_text value BLM18HE152SN1D (at -5.2705 -0.1905 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/c_0603_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5809CED3)
    (at 134.3025 92.329 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R1 (at 1.3335 0.0635 180) (layer F.SilkS))
    (fp_text value VB_EN (at 0.8255 -1.0795 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5809CED3)
    (at 109.1565 85.7885)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0.635 -1.2065) (layer B.SilkS))
    (fp_text value 10K (at -1.2065 -1.143) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 /RESET))
    (model Resistors_SMD.3dshapes/r_0603_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5809CED3)
    (at 125.4125 91.5465 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -0.9955 -1.5875) (layer B.SilkS))
    (fp_text value 10K (at -0.1065 -1.651) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 22 /SS))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (model Resistors_SMD.3dshapes/r_0603_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5809CED3)
    (at 112.395 93.2815 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -1.1 -1.27 270) (layer B.SilkS))
    (fp_text value 1M (at 0.424 -1.27 270) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 25 /V_BATT))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (model Resistors_SMD.3dshapes/r_0603_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5809CED3)
    (at 110.236 90.678 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -1.016 1.8415) (layer B.SilkS))
    (fp_text value 470K (at 0.1905 1.9685) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 25 /V_BATT))
    (model Resistors_SMD.3dshapes/r_0603_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0402 (layer F.Cu) (tedit 5809CED3)
    (at 144.272 91.8845 90)
    (descr "Resistor SMD 0402, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0402")
    (attr smd)
    (fp_text reference R6 (at 0.254 -1.0795 270) (layer F.SilkS))
    (fp_text value VB_EN (at 0.0635 1.143 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at 0.45 0 90) (size 0.4 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /V_BOOST_IN))
  )
  (module myfootprints:DIPSWITCH_SMD_1.27-16 (layer F.Cu) (tedit 5809CED3)
    (at 134.9375 84.201 270)
    (attr smd)
    (fp_text reference S1 (at 3.4798 0.5207 90) (layer F.SilkS))
    (fp_text value MCDHA-08TQR (at -0.0762 0.5715 270) (layer F.SilkS))
    (pad 16 smd rect (at -4.445 -3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -4.445 3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 13 /C0))
    (pad 15 smd rect (at -3.175 -3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -3.175 3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 14 /C1))
    (pad 14 smd rect (at -1.905 -3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.905 3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 17 /C2))
    (pad 13 smd rect (at -0.635 -3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -0.635 3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 18 /C3))
    (pad 12 smd rect (at 0.635 -3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 0.635 3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 19 /C4))
    (pad 11 smd rect (at 1.905 -3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 1.905 3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 20 /C5))
    (pad 10 smd rect (at 3.175 -3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 3.175 3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 21 /C6))
    (pad 9 smd rect (at 4.445 -3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 8 smd rect (at 4.445 3.175 270) (size 0.76 1.27) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(S1-Pad8)"))
    (model ${KISYS3DMOD}/DIP_Switches.3dshapes/dip_sw_8_smd.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:MSOP-8_3x3mm_Pitch0.65mm (layer F.Cu) (tedit 5809CED3)
    (at 140.716 94.107 90)
    (descr "8-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0.762 -1.016 90) (layer F.SilkS))
    (fp_text value L6920 (at 0 0.508 90) (layer F.SilkS))
    (pad 1 smd rect (at -2.2 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at -2.2 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad2)"))
    (pad 3 smd rect (at -2.2 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -2.2 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C5-Pad1)"))
    (pad 5 smd rect (at 2.2 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (pad 6 smd rect (at 2.2 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 2.2 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(L2-Pad1)"))
    (pad 8 smd rect (at 2.2 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (model Housings_SSOP.3dshapes/msop_8_3x3mm_p065mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors_radios:RFM69HW_SMD_Handsoldering (layer F.Cu) (tedit 5809CED3)
    (at 109.982 79.756)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U2 (at 2.921 1.5875) (layer F.SilkS))
    (fp_text value RFM69HW (at 4.191 2.54) (layer F.SilkS))
    (pad 1 smd rect (at -1.4 0) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U2-Pad1)"))
    (pad 2 smd rect (at -1.4 2) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 27 /INT))
    (pad 3 smd rect (at -1.4 4) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -1.4 6) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -1.4 8) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at -1.4 10) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -1.4 12) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at -1.4 14) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 9 smd rect (at 18.3 14) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 18.3 12) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(P1-Pad1)"))
    (pad 11 smd rect (at 18.3 10) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 18.3 8) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 /SCK))
    (pad 13 smd rect (at 18.3 6) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 10 /MISO))
    (pad 14 smd rect (at 18.3 4) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 /MOSI))
    (pad 15 smd rect (at 18.3 2) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 /SS))
    (pad 16 smd rect (at 18.3 0) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U2-Pad16)"))
    (model ${KISYS3DMOD}/Radio_Modules.3dshapes/RFM69W.stp
      (at (xyz 0.6692913385826772 -0.5511811023622047 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 5809CED3)
    (at 131.5085 91.821)
    (fp_text reference P1 (at -0.508 1.778 90) (layer F.SilkS))
    (fp_text value ANTENNA (at 0.381 2.7305 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(P1-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 5809CED3)
    (at 104.013 84.328 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference CON1 (at 4.5085 2.667 270) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at -1.905 2.667 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /MISO))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (model Pin_Headers.3dshapes/PinHeader_Straight_2x03x2.54mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeA_EIA-3216_Wave (layer F.Cu) (tedit 5809CED3)
    (at 143.1925 79.756)
    (descr "Tantal Cap. , Size A, EIA-3216, Wave,")
    (tags "Tantal Cap. , Size A, EIA-3216, Wave,")
    (attr smd)
    (fp_text reference C9 (at -1.27 -1.7145) (layer F.SilkS))
    (fp_text value 47u (at 0.35814 -1.7145) (layer F.SilkS))
    (fp_text user + (at -3.59918 -1.80086) (layer F.SilkS))
    (pad 2 smd rect (at 1.50114 0) (size 2.14884 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 9 /V_BOOST_IN))
    (pad 1 smd rect (at -1.50114 0) (size 2.14884 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/Tantalum_A_3216H18.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeA_EIA-3216_Wave (layer F.Cu) (tedit 5809CED3)
    (at 102.51186 93.345 180)
    (descr "Tantal Cap. , Size A, EIA-3216, Wave,")
    (tags "Tantal Cap. , Size A, EIA-3216, Wave,")
    (attr smd)
    (fp_text reference C10 (at 1.92786 -2.032 180) (layer F.SilkS))
    (fp_text value 10u (at 1.86436 -3.048 180) (layer F.SilkS))
    (fp_text user + (at -3.59918 -1.80086 180) (layer F.SilkS))
    (pad 2 smd rect (at 1.50114 0 180) (size 2.14884 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.50114 0 180) (size 2.14884 1.50114) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/Tantalum_A_3216H18.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:TantalC_SizeA_EIA-3216_Wave (layer B.Cu) (tedit 5809CED3)
    (at 138.811 96.139)
    (descr "Tantal Cap. , Size A, EIA-3216, Wave,")
    (tags "Tantal Cap. , Size A, EIA-3216, Wave,")
    (attr smd)
    (fp_text reference C12 (at 1.143 1.8415) (layer B.SilkS))
    (fp_text value 10u (at -0.8255 1.778) (layer B.SilkS))
    (fp_text user + (at -3.59918 1.80086) (layer B.SilkS))
    (pad 2 smd rect (at 1.50114 0) (size 2.14884 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.50114 0) (size 2.14884 1.50114) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Capacitors_SMD.3dshapes/c_1206_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer B.Cu) (tedit 5809CED3)
    (at 140.335 92.6465 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at -0.9525 -1.3335 270) (layer B.SilkS))
    (fp_text value 10n (at 0.8255 -1.27 270) (layer B.SilkS))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/c_0603_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer B.Cu) (tedit 5809CED3)
    (at 137.498 92.517)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at -0.0635 -2.3495) (layer B.SilkS))
    (fp_text value MIC5205-3.3 (at -2.3495 0.1905 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C6-Pad2)"))
    (pad 4 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 43 "Net-(C13-Pad1)"))
    (pad 5 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers B.Cu B.Paste B.Mask)
      (net 42 "Net-(C12-Pad1)"))
    (model SOT_Packages_SMD.3dshapes/SOT23-5_wLABEL.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.00mm (layer F.Cu) (tedit 5809CED3)
    (at 106.331 96.8375 90)
    (descr "Through hole pin header, 1x03, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference P3 (at 1.4605 1.492 180) (layer F.SilkS))
    (fp_text value A3212 (at 1.4605 3.651 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole circle (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole circle (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /HALL_SENSOR))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 5809CED3)
    (at 109.347 94.2975)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0.635 -1.143) (layer B.SilkS))
    (fp_text value 51K (at -1.143 -1.143) (layer B.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 44 /HALL_SENSOR))
    (model Resistors_SMD.3dshapes/r_0603_h078.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.00mm (layer F.Cu) (tedit 5809CED3)
    (at 116.8715 96.8375 270)
    (descr "Through hole pin header, 1x03, 2.00mm pitch, single row")
    (tags "pin header single row")
    (fp_text reference P4 (at -1.4605 4.54) (layer F.SilkS))
    (fp_text value OTHER (at -1.4605 2.254) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /A0))
    (pad 2 thru_hole circle (at 0 2 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /A1))
    (pad 3 thru_hole circle (at 0 4 270) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /D0))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04 (layer F.Cu) (tedit 5809CED3)
    (at 121.031 96.901 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 1.651 2.413 180) (layer F.SilkS))
    (fp_text value HTU21D (at 1.651 4.8895 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /SDA))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /SCL))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2_ISO14580_Pad (layer F.Cu) (tedit 5809CED3)
    (at 99.822 88.011)
    (descr "Mounting Hole 2.2mm, M2, ISO14580")
    (tags "mounting hole 2.2mm m2 iso14580")
    (fp_text reference REF** (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2_ISO14580_Pad (at 0 2.9) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 2 2) (drill 1.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND) (zone_connect 2))
  )
  (module myfootprints:my_logo (layer B.Cu) (tedit 57629D29)
    (at 141.4526 81.0514)
    (attr virtual)
    (fp_text reference REF** (at 0.2032 5.4864) (layer B.SilkS) hide)
    (fp_text value my_logo (at -0.0254 -4.6482) (layer B.Fab) hide)
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 5809CED3)
    (at 135.5217 86.2203)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 2 GND) (zone_connect 2))
  )
  (gr_text "Use CR123(A) 3V battery" (at 145.4785 94.1705 90) (layer B.SilkS))
  (gr_text "MySensors RFM69 Node - Rev 1.4" (at 118.3005 78.0415) (layer F.SilkS))
  (gr_text BATT+ (at 101.5365 87.884 90) (layer F.SilkS))
  (gr_text BATT- (at 143.3195 87.884 90) (layer F.SilkS))
  (gr_text "Node ID Switch" (at 135.0645 77.9145) (layer F.SilkS))
  (gr_text GND (at 123.5075 98.933) (layer F.SilkS))
  (gr_text +3V3 (at 120.777 98.933) (layer F.SilkS))
  (gr_text SDA (at 126.111 98.933) (layer F.SilkS))
  (gr_text SCL (at 128.651 98.933) (layer F.SilkS))
  (gr_text +3V3 (at 106.3625 98.8695) (layer F.SilkS))
  (gr_text GND (at 108.458 98.8695) (layer F.SilkS))
  (gr_text HS (at 110.363 98.8695) (layer F.SilkS))
  (gr_text D0 (at 112.903 98.8695) (layer F.SilkS))
  (gr_text A1 (at 114.8715 98.8695) (layer F.SilkS))
  (gr_text A0 (at 116.9035 98.8695) (layer F.SilkS))
  (gr_line (start 98.425 99.441) (end 98.425 77.2795) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.6215 99.441) (end 98.425 99.441) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 146.6215 77.279408) (end 146.6215 99.441) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 98.425 77.2795) (end 146.6215 77.2795) (layer Edge.Cuts) (width 0.1))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 98.425 77.2795) (xy 146.6215 77.2795) (xy 146.6215 99.441) (xy 98.425 99.441)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 98.425 77.2795) (xy 146.6215 77.2795) (xy 146.6215 99.441) (xy 98.425 99.441)
      )
    )
  )
)
