(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 39)
    (no_connects 0)
    (area 125.250599 93.924999 191.850334 130.052133)
    (thickness 1.6)
    (drawings 4)
    (tracks 119)
    (zones 0)
    (modules 15)
    (nets 53)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory GERBER/))
  )
  (net 0 "")
  (net 1 /VUSB)
  (net 2 GND)
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D2-Pad2)")
  (net 5 "Net-(D3-Pad2)")
  (net 6 "Net-(P1-Pad1)")
  (net 7 /LED_TX)
  (net 8 /LED_RX)
  (net 9 /LED_ERR)
  (net 10 /SCK)
  (net 11 "Net-(U2-Pad2)")
  (net 12 "Net-(U2-Pad3)")
  (net 13 "Net-(U2-Pad7)")
  (net 14 "Net-(U2-Pad8)")
  (net 15 "Net-(U2-Pad9)")
  (net 16 "Net-(U2-Pad10)")
  (net 17 "Net-(U2-Pad11)")
  (net 18 "Net-(U2-Pad13)")
  (net 19 "Net-(U2-Pad15)")
  (net 20 "Net-(U2-Pad16)")
  (net 21 "Net-(U2-Pad17)")
  (net 22 "Net-(U2-Pad18)")
  (net 23 /IRQ)
  (net 24 "Net-(U2-Pad21)")
  (net 25 "Net-(U2-Pad22)")
  (net 26 "Net-(U2-Pad23)")
  (net 27 "Net-(U2-Pad24)")
  (net 28 "Net-(U2-Pad25)")
  (net 29 "Net-(U2-Pad26)")
  (net 30 "Net-(U2-Pad27)")
  (net 31 /CS)
  (net 32 /MOSI)
  (net 33 /MISO)
  (net 34 "Net-(U3-Pad1)")
  (net 35 "Net-(U3-Pad3)")
  (net 36 "Net-(U3-Pad4)")
  (net 37 "Net-(U3-Pad5)")
  (net 38 "Net-(U3-Pad6)")
  (net 39 "Net-(U3-Pad7)")
  (net 40 "Net-(U3-Pad16)")
  (net 41 VCC)
  (net 42 /IRQ3)
  (net 43 /SCK3)
  (net 44 /MISO3)
  (net 45 /MOSI3)
  (net 46 /CS3)
  (net 47 "Net-(U4-Pad7)")
  (net 48 "Net-(U4-Pad8)")
  (net 49 "Net-(U4-Pad9)")
  (net 50 "Net-(U4-Pad11)")
  (net 51 "Net-(U4-Pad12)")
  (net 52 "Net-(U4-Pad13)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CS)
    (add_net /CS3)
    (add_net /IRQ)
    (add_net /IRQ3)
    (add_net /LED_ERR)
    (add_net /LED_RX)
    (add_net /LED_TX)
    (add_net /MISO)
    (add_net /MISO3)
    (add_net /MOSI)
    (add_net /MOSI3)
    (add_net /SCK)
    (add_net /SCK3)
    (add_net /VUSB)
    (add_net GND)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(U2-Pad10)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad15)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U2-Pad23)")
    (add_net "Net-(U2-Pad24)")
    (add_net "Net-(U2-Pad25)")
    (add_net "Net-(U2-Pad26)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad7)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U2-Pad9)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U4-Pad11)")
    (add_net "Net-(U4-Pad12)")
    (add_net "Net-(U4-Pad13)")
    (add_net "Net-(U4-Pad7)")
    (add_net "Net-(U4-Pad8)")
    (add_net "Net-(U4-Pad9)")
    (add_net VCC)
  )
  (module Mysensors_Radio:RFM69HW_SMD_Handsoldering (layer F.Cu) (tedit 558806AF)
    (at 170.18 116.713 90)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U3 (at 0.254 -1.778 90) (layer F.SilkS))
    (fp_text value RFM69HW (at 8.382 7.112 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U3-Pad1)"))
    (pad 2 smd rect (at -1.4 2 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 /IRQ3))
    (pad 3 smd rect (at -1.4 4 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U3-Pad3)"))
    (pad 4 smd rect (at -1.4 6 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U3-Pad4)"))
    (pad 5 smd rect (at -1.4 8 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(U3-Pad5)"))
    (pad 6 smd rect (at -1.4 10 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(U3-Pad6)"))
    (pad 7 smd rect (at -1.4 12 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(U3-Pad7)"))
    (pad 8 smd rect (at -1.4 14 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 VCC))
    (pad 9 smd rect (at 18.3 14 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 10 smd rect (at 18.3 12 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P1-Pad1)"))
    (pad 11 smd rect (at 18.3 10 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 12 smd rect (at 18.3 8 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 /SCK3))
    (pad 13 smd rect (at 18.3 6 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 /MISO3))
    (pad 14 smd rect (at 18.3 4 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 /MOSI3))
    (pad 15 smd rect (at 18.3 2 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 /CS3))
    (pad 16 smd rect (at 18.3 0 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U3-Pad16)"))
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/rfm69hw.wrl
      (at (xyz 0.332 -0.275 0.03))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0.332 -0.08 0.06))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.204 -0.445 0.06))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 0)
    (at 162.433 115.951 270)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 -3.8 270) (layer F.SilkS))
    (fp_text value C (at 1.25 3.8 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /VUSB))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_THT:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 0)
    (at 166.243 120.523 270)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at 1.25 -3.8 270) (layer F.SilkS))
    (fp_text value C (at 1.25 3.8 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 VCC))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 587F14BB)
    (at 134.366 125.349 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D1 (at -1.778 0 180) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 587F14C4)
    (at 139.573 125.349 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D2 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 587F14CB)
    (at 144.78 125.349 90)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D3 (at -1.905 0 180) (layer F.SilkS))
    (fp_text value LED (at 1.3 -2.9 90) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 587F153B)
    (at 186.817 102.108)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P1 (at 0 -2.39) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 2.39) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(P1-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 134.493 117.856 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value R (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 /LED_TX))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 139.573 117.856 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value R (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 8 /LED_RX))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58307C0D)
    (at 144.78 117.856 90)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value R (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 2 0 90) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 /LED_ERR))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 583F3B4E)
    (at 154.178 118.237 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -4.5 180) (layer F.SilkS))
    (fp_text value AP111733 (at 0 4.5 180) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 41 VCC))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 41 VCC))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /VUSB))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module arduino:arduino_mini (layer F.Cu) (tedit 507C2E55)
    (at 148.5011 105.0036)
    (descr "30 pins DIL package, elliptical pads, width 600mil (arduino mini)")
    (tags "DIL arduino mini")
    (fp_text reference U2 (at -13.97 -3.81) (layer F.SilkS))
    (fp_text value arduino_mini (at -0.635 3.175) (layer F.SilkS))
    (pad 1 thru_hole rect (at -19.05 7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 /SCK))
    (pad 2 thru_hole oval (at -16.51 7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(U2-Pad2)"))
    (pad 3 thru_hole oval (at -13.97 7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(U2-Pad3)"))
    (pad 4 thru_hole oval (at -11.43 7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 /LED_TX))
    (pad 5 thru_hole oval (at -8.89 7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 /LED_RX))
    (pad 6 thru_hole oval (at -6.35 7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 /LED_ERR))
    (pad 7 thru_hole oval (at -3.81 7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(U2-Pad7)"))
    (pad 8 thru_hole oval (at -1.27 7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(U2-Pad8)"))
    (pad 9 thru_hole oval (at 1.27 7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(U2-Pad9)"))
    (pad 10 thru_hole oval (at 3.81 7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U2-Pad10)"))
    (pad 11 thru_hole oval (at 6.35 7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(U2-Pad11)"))
    (pad 12 thru_hole oval (at 8.89 7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 /VUSB))
    (pad 13 thru_hole oval (at 11.43 7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(U2-Pad13)"))
    (pad 14 thru_hole oval (at 13.97 7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 15 thru_hole oval (at 16.51 7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(U2-Pad15)"))
    (pad 16 thru_hole oval (at 16.51 -7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(U2-Pad16)"))
    (pad 17 thru_hole oval (at 13.97 -7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(U2-Pad17)"))
    (pad 18 thru_hole oval (at 11.43 -7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(U2-Pad18)"))
    (pad 19 thru_hole oval (at 8.89 -7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 20 thru_hole oval (at 6.35 -7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 /IRQ))
    (pad 21 thru_hole oval (at 3.81 -7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U2-Pad21)"))
    (pad 22 thru_hole oval (at 1.27 -7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(U2-Pad22)"))
    (pad 23 thru_hole oval (at -1.27 -7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(U2-Pad23)"))
    (pad 24 thru_hole oval (at -3.81 -7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(U2-Pad24)"))
    (pad 25 thru_hole oval (at -6.35 -7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(U2-Pad25)"))
    (pad 26 thru_hole oval (at -8.89 -7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U2-Pad26)"))
    (pad 27 thru_hole oval (at -11.43 -7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(U2-Pad27)"))
    (pad 28 thru_hole oval (at -13.97 -7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 31 /CS))
    (pad 29 thru_hole oval (at -16.51 -7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 32 /MOSI))
    (pad 30 thru_hole oval (at -19.05 -7.62) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /MISO))
    (model arduino_nano.wrl
      (at (xyz -0.978 -0.385 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 587F1534)
    (at 150.368 124.968 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P2 (at -2.286 1.27 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.93 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VUSB))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 587F14DF)
    (at 159.8168 125.0188 270)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P3 (at 2.2352 1.1938 360) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.93 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 VCC))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer B.Cu) (tedit 57503549)
    (at 176.784 108.585 90)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at 0 7.5 90) (layer B.SilkS))
    (fp_text value 74HC245 (at 0 -7.5 90) (layer B.Fab))
    (pad 1 smd rect (at -4.7 5.715 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 41 VCC))
    (pad 2 smd rect (at -4.7 4.445 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 10 /SCK))
    (pad 3 smd rect (at -4.7 3.175 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 32 /MOSI))
    (pad 4 smd rect (at -4.7 1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 31 /CS))
    (pad 5 smd rect (at -4.7 0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 44 /MISO3))
    (pad 6 smd rect (at -4.7 -0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 42 /IRQ3))
    (pad 7 smd rect (at -4.7 -1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(U4-Pad7)"))
    (pad 8 smd rect (at -4.7 -3.175 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(U4-Pad8)"))
    (pad 9 smd rect (at -4.7 -4.445 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(U4-Pad9)"))
    (pad 10 smd rect (at -4.7 -5.715 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 11 smd rect (at 4.7 -5.715 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 50 "Net-(U4-Pad11)"))
    (pad 12 smd rect (at 4.7 -4.445 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 51 "Net-(U4-Pad12)"))
    (pad 13 smd rect (at 4.7 -3.175 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 52 "Net-(U4-Pad13)"))
    (pad 14 smd rect (at 4.7 -1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 23 /IRQ))
    (pad 15 smd rect (at 4.7 -0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 33 /MISO))
    (pad 16 smd rect (at 4.7 0.635 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 46 /CS3))
    (pad 17 smd rect (at 4.7 1.905 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 45 /MOSI3))
    (pad 18 smd rect (at 4.7 3.175 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 43 /SCK3))
    (pad 19 smd rect (at 4.7 4.445 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 4.7 5.715 90) (size 1.95 0.6) (layers B.Cu B.Paste B.Mask)
      (net 41 VCC))
    (model Housings_SOIC.3dshapes/SOIC-20_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 126 128) (end 126 94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190 128) (end 126 128) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190 94) (end 190 128) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 126 94) (end 190 94) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126 94) (xy 190 94) (xy 190 128) (xy 126 128)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 126 94) (xy 190 94) (xy 190 128) (xy 126 128)
      )
    )
  )
)
