(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 49)
    (no_connects 0)
    (area 81.547999 51.476 131.779334 82.355)
    (thickness 1.6)
    (drawings 5)
    (tracks 205)
    (zones 0)
    (modules 16)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7272 1.7272)
    (pad_drill 0.3)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory GERBER/))
  )
  (net 0 "")
  (net 1 /GND)
  (net 2 /3V3)
  (net 3 "Net-(IC1-Pad1)")
  (net 4 "Net-(IC1-Pad2)")
  (net 5 "Net-(IC1-Pad7)")
  (net 6 "Net-(IC1-Pad8)")
  (net 7 "Net-(IC1-Pad9)")
  (net 8 "Net-(IC1-Pad10)")
  (net 9 "Net-(IC1-Pad11)")
  (net 10 "Net-(IC1-Pad12)")
  (net 11 "Net-(IC1-Pad20)")
  (net 12 "Net-(IC1-Pad22)")
  (net 13 "Net-(IC1-Pad25)")
  (net 14 "Net-(IC1-Pad26)")
  (net 15 "Net-(IC1-Pad27)")
  (net 16 "Net-(IC1-Pad30)")
  (net 17 "Net-(IC1-Pad31)")
  (net 18 "Net-(L1-Pad2)")
  (net 19 "Net-(P2-Pad1)")
  (net 20 /PC0)
  (net 21 /PC1)
  (net 22 /MISO)
  (net 23 /SCK)
  (net 24 /MOSI)
  (net 25 /RST)
  (net 26 /IRQ)
  (net 27 /CE)
  (net 28 /CSN)
  (net 29 "Net-(U3-Pad1)")
  (net 30 "Net-(U3-Pad3)")
  (net 31 "Net-(U3-Pad4)")
  (net 32 "Net-(U3-Pad5)")
  (net 33 "Net-(U3-Pad6)")
  (net 34 "Net-(U3-Pad7)")
  (net 35 "Net-(U3-Pad16)")
  (net 36 /VIN)
  (net 37 "Net-(IC1-Pad19)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3V3)
    (add_net /CE)
    (add_net /CSN)
    (add_net /GND)
    (add_net /IRQ)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /PC0)
    (add_net /PC1)
    (add_net /RST)
    (add_net /SCK)
    (add_net /VIN)
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad25)")
    (add_net "Net-(IC1-Pad26)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad30)")
    (add_net "Net-(IC1-Pad31)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 587DC503)
    (at 91.44 77.089 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference 10uF (at 0 -1.905 270) (layer F.SilkS))
    (fp_text value C (at 0 2.3 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /VIN))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_radios:RFM69HW_SMD_Handsoldering (layer F.Cu) (tedit 587DC4ED)
    (at 115.7224 77.6224 90)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference RFM69HW (at 0.254 -1.778 90) (layer F.SilkS))
    (fp_text value RFM69HW (at 8.382 7.112 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U3-Pad1)"))
    (pad 2 smd rect (at -1.4 2 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 /IRQ))
    (pad 3 smd rect (at -1.4 4 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U3-Pad3)"))
    (pad 4 smd rect (at -1.4 6 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U3-Pad4)"))
    (pad 5 smd rect (at -1.4 8 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U3-Pad5)"))
    (pad 6 smd rect (at -1.4 10 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U3-Pad6)"))
    (pad 7 smd rect (at -1.4 12 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U3-Pad7)"))
    (pad 8 smd rect (at -1.4 14 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 9 smd rect (at 18.3 14 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 10 smd rect (at 18.3 12 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(P2-Pad1)"))
    (pad 11 smd rect (at 18.3 10 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 12 smd rect (at 18.3 8 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 /SCK))
    (pad 13 smd rect (at 18.3 6 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 /MISO))
    (pad 14 smd rect (at 18.3 4 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 /MOSI))
    (pad 15 smd rect (at 18.3 2 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 /CSN))
    (pad 16 smd rect (at 18.3 0 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U3-Pad16)"))
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/rfm69hw.wrl
      (at (xyz 0.332 -0.275 0.03))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0.332 -0.08 0.06))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.204 -0.445 0.06))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 587DC56C)
    (at 99.695 66.421 90)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference 328p (at -5.969 0 180) (layer F.SilkS))
    (fp_text value ATMEGA328P-AU (at 0 6.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at -4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 4 smd rect (at -4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 5 smd rect (at -4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 6 smd rect (at -4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 7 smd rect (at -4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad9)"))
    (pad 10 smd rect (at -2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at -1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at 0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 /CE))
    (pad 14 smd rect (at 1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 /CSN))
    (pad 15 smd rect (at 2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 /MOSI))
    (pad 16 smd rect (at 2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 /MISO))
    (pad 17 smd rect (at 4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 /SCK))
    (pad 18 smd rect (at 4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 19 smd rect (at 4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 22 smd rect (at 4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 /PC1))
    (pad 24 smd rect (at 4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /PC0))
    (pad 25 smd rect (at 2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(IC1-Pad25)"))
    (pad 26 smd rect (at 2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(IC1-Pad26)"))
    (pad 27 smd rect (at 1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad27)"))
    (pad 28 smd rect (at 0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 /VIN))
    (pad 29 smd rect (at -0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 /RST))
    (pad 30 smd rect (at -1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad30)"))
    (pad 31 smd rect (at -2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad31)"))
    (pad 32 smd rect (at -2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 /IRQ))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Choke_SMD:Choke_SMD_1206_Handsoldering (layer F.Cu) (tedit 587CB04E)
    (at 84.4423 73.2409 90)
    (descr "Choke, Drossel, SMD, 1206, Handsoldering,")
    (tags "Choke, Drossel, SMD, 1206, Handsoldering,")
    (attr smd)
    (fp_text reference L1 (at 0.0889 -1.5113 90) (layer F.SilkS))
    (fp_text value L (at 0 2.54 90) (layer F.Fab))
    (pad 1 smd rect (at -2.30124 0 90) (size 2.59842 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 36 /VIN))
    (pad 2 smd rect (at 2.30124 0 90) (size 2.60096 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(L1-Pad2)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 587CB08D)
    (at 127.6985 54.6608)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference ANT (at -2.8575 -0.1778) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -0.9525 -2.0828) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P2-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 587DC4BB)
    (at 84.1629 54.4449 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference S0 (at -0.1651 7.9121 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 1.7399 3.2131 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PC0))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 587DC4C3)
    (at 100.1903 54.4322 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference S1 (at -0.3048 -2.6543 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 1.9812 3.0607 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 /3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /PC1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 587DC667)
    (at 108.585 63.627)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference ICSP (at 1.27 7.62) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 22 /MISO))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 2 /3V3))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 23 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 24 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 25 /RST))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 0.3) (layers *.Cu *.Mask F.SilkS)
      (net 1 /GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:TSOT-6-MK06A_Handsoldering (layer F.Cu) (tedit 587CB09D)
    (at 87.4903 73.2409)
    (descr "TSOP-6 MK06A housing 6pin")
    (attr smd)
    (fp_text reference U1 (at 0.1397 0.0381) (layer F.SilkS))
    (fp_text value MAX1724 (at -0.03048 5.22986) (layer F.Fab))
    (pad 1 smd rect (at -0.94996 1.80086) (size 0.69088 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 36 /VIN))
    (pad 2 smd rect (at 0 1.80086) (size 0.69088 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 3 smd rect (at 0.94996 1.80086) (size 0.69088 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 36 /VIN))
    (pad 4 smd rect (at 0.94996 -1.80086) (size 0.69088 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 5 smd rect (at 0 -1.80086) (size 0.69088 1.99898) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -0.94996 -1.80086) (size 0.69088 1.99898) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(L1-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/TSOT-6-MK06A_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 587DC4AB)
    (at 86.36 58.293)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference 4K7 (at 4.191 0) (layer F.SilkS))
    (fp_text value 4K7 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 /PC0))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 587DC509)
    (at 99.822 77.724 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference 3V3 (at 0 -2.39 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.93 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /3V3))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Batteries:BU2032_smd (layer B.Cu) (tedit 587DC58C)
    (at 89.154 67.818)
    (fp_text reference 3V3 (at 0.863015 -3.860095) (layer B.SilkS))
    (fp_text value CR2032 (at 14 -2) (layer B.SilkS))
    (pad 2 smd rect (at 29.3 0) (size 5 4.2) (layers B.Cu B.Paste B.Mask)
      (net 1 /GND))
    (pad 1 smd rect (at 0 0) (size 5 4.2) (layers B.Cu B.Paste B.Mask)
      (net 36 /VIN))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 587DC50E)
    (at 84.455 79.629 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference VIN (at -1.651 1.397 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at -1.143 9.017 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /VIN))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 587DC54B)
    (at 92.329 69.723 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference 10uF (at 0.127 -1.778 90) (layer F.SilkS))
    (fp_text value C (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 587DC4D2)
    (at 100.711 58.293)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference 4K7 (at 4.191 -0.381) (layer F.SilkS))
    (fp_text value 4K7 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 /PC1))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 587DC550)
    (at 87.63 63.627)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference 1117 (at -0.254 0 90) (layer F.SilkS))
    (fp_text value AP111733 (at -0.381 2.286) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 3 smd rect (at -3.15 2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 36 /VIN))
    (pad 1 smd rect (at -3.15 -2.3) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 131.623 81.938) (end 131.623 51.938) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.623 81.938) (end 131.623 81.938) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.623 51.938) (end 81.623 81.938) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 131.623 51.938) (end 81.623 51.938) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 81.623 51.938) (end 131.623 51.938) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.572 81.915) (xy 81.661 81.915) (xy 81.661 52.07) (xy 131.572 51.943)
      )
    )
  )
  (zone (net 1) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 131.6355 51.943) (xy 81.5975 51.943) (xy 81.661 82.042) (xy 131.6355 81.9785)
      )
    )
  )
)
