(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 51)
    (no_connects 0)
    (area 102.865 55.274 178.68 123.659)
    (thickness 1.6)
    (drawings 24)
    (tracks 225)
    (zones 0)
    (modules 20)
    (nets 51)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1)
    (user_trace_width 2)
    (user_trace_width 3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 163.83 45.974)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory GERBER/))
  )
  (net 0 "")
  (net 1 "Net-(IC1-Pad1)")
  (net 2 "Net-(IC1-Pad2)")
  (net 3 /3V3)
  (net 4 "Net-(IC1-Pad7)")
  (net 5 "Net-(IC1-Pad8)")
  (net 6 "Net-(IC1-Pad9)")
  (net 7 "Net-(IC1-Pad10)")
  (net 8 "Net-(IC1-Pad11)")
  (net 9 "Net-(IC1-Pad12)")
  (net 10 "Net-(IC1-Pad13)")
  (net 11 /CS)
  (net 12 /MOSI)
  (net 13 /MISO)
  (net 14 /SCK)
  (net 15 "Net-(IC1-Pad18)")
  (net 16 "Net-(IC1-Pad19)")
  (net 17 "Net-(IC1-Pad20)")
  (net 18 "Net-(IC1-Pad22)")
  (net 19 /RESET)
  (net 20 /IRQ)
  (net 21 "Net-(P2-Pad1)")
  (net 22 /S0)
  (net 23 /S1)
  (net 24 "Net-(U2-Pad1)")
  (net 25 "Net-(U2-Pad3)")
  (net 26 "Net-(U2-Pad4)")
  (net 27 "Net-(U2-Pad5)")
  (net 28 "Net-(U2-Pad6)")
  (net 29 "Net-(U2-Pad7)")
  (net 30 "Net-(U2-Pad16)")
  (net 31 /VCC)
  (net 32 /GND)
  (net 33 /SL7)
  (net 34 /SL6)
  (net 35 /SL5)
  (net 36 /SL4)
  (net 37 /SL3)
  (net 38 /SL2)
  (net 39 /SL1)
  (net 40 /SL0)
  (net 41 "Net-(P4-Pad1)")
  (net 42 "Net-(P4-Pad2)")
  (net 43 "Net-(P4-Pad3)")
  (net 44 "Net-(P5-Pad3)")
  (net 45 "Net-(P5-Pad2)")
  (net 46 "Net-(P5-Pad1)")
  (net 47 "Net-(P1-Pad2)")
  (net 48 "Net-(P1-Pad1)")
  (net 49 "Net-(Q1-Pad1)")
  (net 50 "Net-(Q2-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3V3)
    (add_net /CS)
    (add_net /GND)
    (add_net /IRQ)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /S0)
    (add_net /S1)
    (add_net /SCK)
    (add_net /SL0)
    (add_net /SL1)
    (add_net /SL2)
    (add_net /SL3)
    (add_net /SL4)
    (add_net /SL5)
    (add_net /SL6)
    (add_net /SL7)
    (add_net /VCC)
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad18)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
  )
  (net_class Big ""
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P2-Pad1)")
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5885B116)
    (at 109.855 89.408 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at 0.127 0 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.3 270) (layer F.Fab))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /GND))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 31 /VCC))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5885B110)
    (at 121.92 89.408 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at 0 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V3))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 136.525 92.329 90)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 0 -6.05 90) (layer F.SilkS))
    (fp_text value ATMEGA328-A (at 0 6.05 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 32 smd rect (at -2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /IRQ))
    (pad 31 smd rect (at -2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 /SL0))
    (pad 30 smd rect (at -1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 /SL1))
    (pad 29 smd rect (at -0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 /RESET))
    (pad 28 smd rect (at 0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 /SL2))
    (pad 27 smd rect (at 1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 37 /SL3))
    (pad 26 smd rect (at 2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 36 /SL4))
    (pad 25 smd rect (at 2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 35 /SL5))
    (pad 24 smd rect (at 4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 /SL6))
    (pad 23 smd rect (at 4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 /SL7))
    (pad 22 smd rect (at 4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(IC1-Pad22)"))
    (pad 21 smd rect (at 4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 /GND))
    (pad 20 smd rect (at 4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad20)"))
    (pad 19 smd rect (at 4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad19)"))
    (pad 18 smd rect (at 4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad18)"))
    (pad 17 smd rect (at 4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 /SCK))
    (pad 16 smd rect (at 2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 /MISO))
    (pad 15 smd rect (at 2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 /MOSI))
    (pad 14 smd rect (at 1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /CS))
    (pad 13 smd rect (at 0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad13)"))
    (pad 12 smd rect (at -0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad12)"))
    (pad 11 smd rect (at -1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad11)"))
    (pad 10 smd rect (at -2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad10)"))
    (pad 9 smd rect (at -2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad9)"))
    (pad 8 smd rect (at -4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad8)"))
    (pad 7 smd rect (at -4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad7)"))
    (pad 6 smd rect (at -4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V3))
    (pad 5 smd rect (at -4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 /GND))
    (pad 4 smd rect (at -4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V3))
    (pad 3 smd rect (at -4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 /GND))
    (pad 2 smd rect (at -4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad2)"))
    (pad 1 smd rect (at -4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(IC1-Pad1)"))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:bornier2 (layer F.Cu) (tedit 587FD522)
    (at 110.49 71.374 270)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P1 (at 2.54 -5.08 270) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 2.54 5.08 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 47 "Net-(P1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 48 "Net-(P1-Pad1)"))
    (model Connectors.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5885B23C)
    (at 151.765 85.344)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference ANT (at 0 -2.39) (layer F.SilkS))
    (fp_text value ANT (at 0 2.39) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(P2-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5885B239)
    (at 157.099 76.708 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference ICSP (at 1.27 -2.39 180) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 1.27 7.47 180) (layer F.Fab))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /GND))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /RESET))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /MOSI))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /SCK))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /3V3))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /MISO))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors:bornier3 (layer F.Cu) (tedit 5885B267)
    (at 156.845 118.364 90)
    (descr "Bornier d'alimentation 3 pins")
    (tags DEV)
    (fp_text reference P4 (at 5.05 -4.65 90) (layer F.SilkS))
    (fp_text value "" (at 5.08 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 41 "Net-(P4-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 42 "Net-(P4-Pad2)"))
    (pad 3 thru_hole circle (at 10.16 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 43 "Net-(P4-Pad3)"))
    (model Connectors.3dshapes/bornier3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:bornier3 (layer F.Cu) (tedit 5885B269)
    (at 109.22 108.204 270)
    (descr "Bornier d'alimentation 3 pins")
    (tags DEV)
    (fp_text reference P5 (at 5.05 -4.65 270) (layer F.SilkS))
    (fp_text value "" (at 5.08 5.08 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 10.16 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 44 "Net-(P5-Pad3)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 45 "Net-(P5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 46 "Net-(P5-Pad1)"))
    (model Connectors.3dshapes/bornier3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:bornier3 (layer F.Cu) (tedit 5885B264)
    (at 156.845 100.584 90)
    (descr "Bornier d'alimentation 3 pins")
    (tags DEV)
    (fp_text reference "IN1   IN2   COM" (at 5.05 -4.65 90) (layer F.SilkS))
    (fp_text value "" (at 5.08 5.08 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 10.16 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 32 /GND))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 8 "Net-(IC1-Pad11)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 7 "Net-(IC1-Pad10)"))
    (model Connectors.3dshapes/bornier3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5885B0F7)
    (at 140.1445 100.457)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 1.8415 -1.27) (layer F.SilkS))
    (fp_text value PZT2222A (at 0 2.5) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 /S0))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 /GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5885B0FE)
    (at 115.57 101.473)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 1.778 -1.397) (layer F.SilkS))
    (fp_text value PZT2222A (at 0 2.5) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 /GND))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 /S1))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(Q2-Pad1)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5885B0EE)
    (at 132.969 99.5045 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference 390 (at 0 -0.0635 180) (layer F.SilkS))
    (fp_text value R (at 0 2.3 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 40 /SL0))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5885B0D0)
    (at 116.84 97.663)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference 390 (at 0 0.127) (layer F.SilkS))
    (fp_text value R (at 0 2.3) (layer F.Fab))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 39 /SL1))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(Q2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLibrary:SRD_Relay_TypeC (layer F.Cu) (tedit 5885B0BD)
    (at 142.875 113.284)
    (fp_text reference RLY1 (at 0 5.08) (layer F.SilkS))
    (fp_text value SRD_Type_C (at 0.25 -6.75) (layer F.Fab))
    (pad 1 thru_hole circle (at -6.1 -6) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 /VCC))
    (pad 2 thru_hole circle (at -6.1 6) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 /S0))
    (pad 4 thru_hole circle (at 6.1 6) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 41 "Net-(P4-Pad1)"))
    (pad 3 thru_hole circle (at 6.1 -6) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 43 "Net-(P4-Pad3)"))
    (pad 5 thru_hole circle (at -8.1 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 42 "Net-(P4-Pad2)"))
  )
  (module MyLibrary:SRD_Relay_TypeC (layer F.Cu) (tedit 5885B0C3)
    (at 123.19 113.284 180)
    (fp_text reference RLY2 (at 0 -5.08 180) (layer F.SilkS))
    (fp_text value SRD_Type_C (at 0.25 -6.75 180) (layer F.Fab))
    (pad 5 thru_hole circle (at -8.1 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 45 "Net-(P5-Pad2)"))
    (pad 3 thru_hole circle (at 6.1 -6 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 "Net-(P5-Pad3)"))
    (pad 4 thru_hole circle (at 6.1 6 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 46 "Net-(P5-Pad1)"))
    (pad 2 thru_hole circle (at -6.1 6 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 /S1))
    (pad 1 thru_hole circle (at -6.1 -6 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 31 /VCC))
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 5885B111)
    (at 116.205 90.043 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -0.127 270) (layer F.SilkS))
    (fp_text value AMS1117 (at 0 4.5 270) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -2.3 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 32 /GND))
    (pad 3 smd rect (at -3.15 2.3 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 31 /VCC))
    (pad 2 smd rect (at -3.15 0 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V3))
    (pad 4 smd rect (at 3.15 0 270) (size 2 3.8) (layers F.Cu F.Paste F.Mask))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module mysensors-radio:RFM69HW_SMD_Handsoldering (layer B.Cu) (tedit 558806AF)
    (at 128.27 101.219)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U2 (at 0.254 1.778) (layer B.SilkS))
    (fp_text value RFM69HW (at 8.382 -7.112) (layer B.Fab) hide)
    (pad 16 smd rect (at 18.3 0) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(U2-Pad16)"))
    (pad 15 smd rect (at 18.3 -2) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 11 /CS))
    (pad 14 smd rect (at 18.3 -4) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 12 /MOSI))
    (pad 13 smd rect (at 18.3 -6) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 13 /MISO))
    (pad 12 smd rect (at 18.3 -8) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 14 /SCK))
    (pad 11 smd rect (at 18.3 -10) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 32 /GND))
    (pad 10 smd rect (at 18.3 -12) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(P2-Pad1)"))
    (pad 9 smd rect (at 18.3 -14) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 32 /GND))
    (pad 8 smd rect (at -1.4 -14) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 /3V3))
    (pad 7 smd rect (at -1.4 -12) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(U2-Pad7)"))
    (pad 6 smd rect (at -1.4 -10) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(U2-Pad6)"))
    (pad 5 smd rect (at -1.4 -8) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(U2-Pad5)"))
    (pad 4 smd rect (at -1.4 -6) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(U2-Pad4)"))
    (pad 3 smd rect (at -1.4 -4) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(U2-Pad3)"))
    (pad 2 smd rect (at -1.4 -2) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 20 /IRQ))
    (pad 1 smd rect (at -1.4 0) (size 3 1.2) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(U2-Pad1)"))
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/rfm69hw.wrl
      (at (xyz 0.332 -0.275 0.03))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0.332 -0.08 0.06))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.204 -0.445 0.06))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLibrary:HLK-PM01 (layer F.Cu) (tedit 57E3C36D)
    (at 118.031001 73.921001)
    (fp_text reference U3 (at 16.7 9) (layer F.SilkS))
    (fp_text value HLK-PM01 (at 16.9 -9) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 -2.54) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(P1-Pad1)"))
    (pad 2 thru_hole circle (at 0 2.54) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(P1-Pad2)"))
    (pad 3 thru_hole circle (at 29.464 -7.62) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 31 /VCC))
    (pad 4 thru_hole circle (at 29.464 7.62) (size 2 2) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 32 /GND))
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5885B0DD)
    (at 133.858 102.108)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 0) (layer F.SilkS))
    (fp_text value D (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 /VCC))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 /S0))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 5885B10A)
    (at 111.125 100.838 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 0 1.651 270) (layer F.SilkS))
    (fp_text value D (at 0 2.1 270) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 /S1))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 /VCC))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "AC\nIN" (at 110.363 81.407) (layer F.SilkS))
  (gr_text "C\n" (at 153.924 112.395) (layer B.SilkS))
  (gr_text "C\n" (at 112.268 112.268) (layer B.SilkS))
  (gr_text NO (at 112.395 117.475) (layer B.SilkS))
  (gr_text NO (at 153.162 107.188) (layer B.SilkS))
  (gr_text NC (at 153.035 117.348) (layer B.SilkS))
  (gr_text NC (at 113.03 107.061) (layer B.SilkS))
  (gr_line (start 104.83 63.974) (end 104.83 120.974) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.83 120.974) (end 160.83 63.974) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 160.83 63.974) (end 104.83 63.974) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.83 120.974) (end 160.83 120.974) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 32) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.83 102.974) (xy 104.83 102.974) (xy 104.83 83.974) (xy 137.83 83.974) (xy 145.83 75.974)
        (xy 145.83 63.974) (xy 160.83 63.974)
      )
    )
  )
  (zone (net 32) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.83 63.974) (xy 160.83 63.974) (xy 160.83 102.974) (xy 104.83 102.974) (xy 104.83 83.974)
        (xy 137.83 83.974) (xy 145.83 75.974)
      )
    )
  )
)
