(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 120)
    (no_connects 0)
    (area 44.759999 39.679999 145.075001 140.533001)
    (thickness 1.6)
    (drawings 5)
    (tracks 340)
    (zones 0)
    (modules 68)
    (nets 91)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (user_trace_width 3)
    (user_trace_width 5)
    (trace_clearance 0.25)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory GERBER/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 "Net-(D1-Pad2)")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D2-Pad2)")
  (net 6 "Net-(D2-Pad1)")
  (net 7 "Net-(D3-Pad2)")
  (net 8 "Net-(D3-Pad1)")
  (net 9 "Net-(D4-Pad2)")
  (net 10 "Net-(D4-Pad1)")
  (net 11 "Net-(D5-Pad2)")
  (net 12 "Net-(D5-Pad1)")
  (net 13 "Net-(D6-Pad2)")
  (net 14 "Net-(D6-Pad1)")
  (net 15 "Net-(D7-Pad2)")
  (net 16 "Net-(D7-Pad1)")
  (net 17 "Net-(D8-Pad2)")
  (net 18 "Net-(D8-Pad1)")
  (net 19 "Net-(F1-Pad1)")
  (net 20 /PH_IN)
  (net 21 "Net-(F2-Pad1)")
  (net 22 "Net-(F3-Pad1)")
  (net 23 "Net-(F4-Pad1)")
  (net 24 "Net-(F5-Pad1)")
  (net 25 "Net-(F6-Pad1)")
  (net 26 "Net-(F7-Pad1)")
  (net 27 "Net-(F8-Pad1)")
  (net 28 /N)
  (net 29 /PH_0)
  (net 30 /PH_1)
  (net 31 /PH_2)
  (net 32 /PH_3)
  (net 33 /PH_4)
  (net 34 /PH_5)
  (net 35 /PH_6)
  (net 36 "Net-(R1-Pad2)")
  (net 37 "Net-(R10-Pad1)")
  (net 38 "Net-(R11-Pad1)")
  (net 39 "Net-(R12-Pad1)")
  (net 40 "Net-(R13-Pad1)")
  (net 41 "Net-(R14-Pad1)")
  (net 42 "Net-(R15-Pad1)")
  (net 43 "Net-(R16-Pad1)")
  (net 44 "Net-(R17-Pad1)")
  (net 45 "Net-(U14-Pad3)")
  (net 46 "Net-(U15-Pad3)")
  (net 47 "Net-(U16-Pad3)")
  (net 48 "Net-(U17-Pad3)")
  (net 49 "Net-(U10-Pad4)")
  (net 50 "Net-(U11-Pad4)")
  (net 51 "Net-(U12-Pad4)")
  (net 52 "Net-(U13-Pad4)")
  (net 53 /C7)
  (net 54 /C6)
  (net 55 /C5)
  (net 56 /C4)
  (net 57 /C3)
  (net 58 /C2)
  (net 59 /C0)
  (net 60 /C1)
  (net 61 /PH_7)
  (net 62 /CS)
  (net 63 /SCK)
  (net 64 /ZCD)
  (net 65 "Net-(IC1-Pad11)")
  (net 66 /3V3)
  (net 67 "Net-(IC1-Pad2)")
  (net 68 "Net-(IC1-Pad7)")
  (net 69 "Net-(IC1-Pad8)")
  (net 70 "Net-(IC1-Pad9)")
  (net 71 "Net-(IC1-Pad10)")
  (net 72 "Net-(IC1-Pad13)")
  (net 73 "Net-(IC1-Pad14)")
  (net 74 /MOSI)
  (net 75 /MISO)
  (net 76 "Net-(IC1-Pad18)")
  (net 77 "Net-(IC1-Pad19)")
  (net 78 "Net-(IC1-Pad20)")
  (net 79 "Net-(IC1-Pad22)")
  (net 80 /IRQ)
  (net 81 "Net-(P1-Pad1)")
  (net 82 "Net-(R18-Pad2)")
  (net 83 "Net-(U3-Pad1)")
  (net 84 "Net-(U3-Pad3)")
  (net 85 "Net-(U3-Pad4)")
  (net 86 "Net-(U3-Pad5)")
  (net 87 "Net-(U3-Pad6)")
  (net 88 "Net-(U3-Pad7)")
  (net 89 "Net-(U3-Pad16)")
  (net 90 /RESET)
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.25)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3V3)
    (add_net /C0)
    (add_net /C1)
    (add_net /C2)
    (add_net /C3)
    (add_net /C4)
    (add_net /C5)
    (add_net /C6)
    (add_net /C7)
    (add_net /CS)
    (add_net /IRQ)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /N)
    (add_net /PH_0)
    (add_net /PH_1)
    (add_net /PH_2)
    (add_net /PH_3)
    (add_net /PH_4)
    (add_net /PH_5)
    (add_net /PH_6)
    (add_net /PH_7)
    (add_net /PH_IN)
    (add_net /RESET)
    (add_net /SCK)
    (add_net /ZCD)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(F2-Pad1)")
    (add_net "Net-(F3-Pad1)")
    (add_net "Net-(F4-Pad1)")
    (add_net "Net-(F5-Pad1)")
    (add_net "Net-(F6-Pad1)")
    (add_net "Net-(F7-Pad1)")
    (add_net "Net-(F8-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad18)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R11-Pad1)")
    (add_net "Net-(R12-Pad1)")
    (add_net "Net-(R13-Pad1)")
    (add_net "Net-(R14-Pad1)")
    (add_net "Net-(R15-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R17-Pad1)")
    (add_net "Net-(R18-Pad2)")
    (add_net "Net-(U10-Pad4)")
    (add_net "Net-(U11-Pad4)")
    (add_net "Net-(U12-Pad4)")
    (add_net "Net-(U13-Pad4)")
    (add_net "Net-(U14-Pad3)")
    (add_net "Net-(U15-Pad3)")
    (add_net "Net-(U16-Pad3)")
    (add_net "Net-(U17-Pad3)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net VCC)
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 58417B02)
    (at 138.43 45.085 90)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P2 (at 0 -5.08 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PH_IN))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 28 /N))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 58417AFB)
    (at 138.43 55.245 90)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P3 (at 0 -5.08 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 29 /PH_0))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 28 /N))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 58417B08)
    (at 138.43 66.04 90)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P4 (at 0 -5.08 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 30 /PH_1))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 28 /N))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 58417B0E)
    (at 138.43 77.47 90)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P5 (at 0 -5.08 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 31 /PH_2))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 28 /N))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 58417B17)
    (at 138.43 88.9 90)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P6 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 32 /PH_3))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 28 /N))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 58417B1B)
    (at 138.43 100.33 90)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P7 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 33 /PH_4))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 28 /N))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 58417B22)
    (at 138.43 111.76 90)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P8 (at 0.635 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 34 /PH_5))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 28 /N))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 58417B2B)
    (at 138.43 123.19 90)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P9 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 35 /PH_6))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 28 /N))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 58417B26)
    (at 138.43 134.62 90)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P10 (at 0 -2.54 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 61 /PH_7))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 28 /N))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-4_W7.62mm_LongPads (layer F.Cu) (tedit 58345D86)
    (at 91.44 45.085 180)
    (descr "4-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 5.715 -9.525 270) (layer F.SilkS))
    (fp_text value LTV-814 (at 2.54 1.27 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(R1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(R18-Pad2)"))
    (pad 3 thru_hole oval (at 7.62 2.54 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole oval (at 7.62 0 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 64 /ZCD))
    (model Housings_DIP.3dshapes/DIP-4_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-6_W7.62mm_LongPads (layer F.Cu) (tedit 58345D89)
    (at 83.82 52.07)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U6 (at 2.54 -8.255 90) (layer F.SilkS))
    (fp_text value MOC3023M (at 4.445 2.54 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(U14-Pad3)"))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(R10-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-6_W7.62mm_LongPads (layer F.Cu) (tedit 58345E31)
    (at 83.82 63.5)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U7 (at 2.54 2.54 90) (layer F.SilkS))
    (fp_text value MOC3023M (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U15-Pad3)"))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(R11-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-6_W7.62mm_LongPads (layer F.Cu) (tedit 58345E35)
    (at 83.82 74.93)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U8 (at 2.54 2.54 90) (layer F.SilkS))
    (fp_text value MOC3023M (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U16-Pad3)"))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(R12-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-6_W7.62mm_LongPads (layer F.Cu) (tedit 58345E0C)
    (at 83.82 86.36)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U9 (at 2.54 2.54 90) (layer F.SilkS))
    (fp_text value MOC3023M (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(D4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U17-Pad3)"))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(R13-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-6_W7.62mm_LongPads (layer F.Cu) (tedit 58345E05)
    (at 83.82 97.79)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U10 (at 2.54 2.54 90) (layer F.SilkS))
    (fp_text value MOC3023M (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U10-Pad4)"))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(R14-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-6_W7.62mm_LongPads (layer F.Cu) (tedit 58345E00)
    (at 83.82 109.22)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U11 (at 2.54 2.54 90) (layer F.SilkS))
    (fp_text value MOC3023M (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(D6-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U11-Pad4)"))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(R15-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-6_W7.62mm_LongPads (layer F.Cu) (tedit 5832FD06)
    (at 83.82 120.65)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U12 (at 2.54 2.54 90) (layer F.SilkS))
    (fp_text value MOC3023M (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(D7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U12-Pad4)"))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(R16-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-6_W7.62mm_LongPads (layer F.Cu) (tedit 5832FCFC)
    (at 83.82 132.08)
    (descr "6-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U13 (at 2.54 2.54 90) (layer F.SilkS))
    (fp_text value MOC3023M (at 5.08 2.54 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(D8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(U13-Pad4)"))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(R17-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-6_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 58417A73)
    (at 99.695 57.15 180)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U14 (at 0 -0.635 180) (layer F.SilkS))
    (fp_text value TRIAC_small (at 0 -1.905 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(F1-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(U14-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 29 /PH_0))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 58417A68)
    (at 99.695 68.58 180)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U15 (at 0 0 180) (layer F.SilkS))
    (fp_text value TRIAC_small (at 0 -1.905 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(F2-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U15-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 30 /PH_1))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 58417A54)
    (at 99.695 80.01 180)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U16 (at 0 0 180) (layer F.SilkS))
    (fp_text value TRIAC_small (at -0.635 -1.905 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(F3-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U16-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 31 /PH_2))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 58417A44)
    (at 99.695 91.44 180)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U17 (at 0 0.635 180) (layer F.SilkS))
    (fp_text value TRIAC_small (at 0 -1.905 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(F4-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U17-Pad3)"))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 32 /PH_3))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 58417A2F)
    (at 99.695 102.87 180)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U18 (at 0 0.635 180) (layer F.SilkS))
    (fp_text value TRIAC_small (at 0 -1.905 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(F5-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U10-Pad4)"))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 33 /PH_4))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 58417A11)
    (at 99.695 114.3 180)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U19 (at 0 0 180) (layer F.SilkS))
    (fp_text value TRIAC_small (at 0 -1.905 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(F6-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U11-Pad4)"))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 34 /PH_5))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 584179E2)
    (at 99.695 125.73 180)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U20 (at -0.305 0.23 180) (layer F.SilkS))
    (fp_text value TRIAC_small (at -0.305 -1.77 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(F7-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U12-Pad4)"))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 35 /PH_6))
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 584179F8)
    (at 99.695 137.16 180)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference U21 (at 0 0.635 180) (layer F.SilkS))
    (fp_text value TRIAC_small (at -0.305 -0.84 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(F8-Pad1)"))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(U13-Pad4)"))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask F.SilkS)
      (net 61 /PH_7))
  )
  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer F.Cu) (tedit 587DCF22)
    (at 56.515 45.085 90)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at -2.667 1.143 180) (layer F.SilkS))
    (fp_text value 100µF (at 1.25 4.4 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D6.3_L11.2_P2.5 (layer F.Cu) (tedit 587DCF26)
    (at 64.135 45.085 90)
    (descr "Radial Electrolytic Capacitor, Diameter 6.3mm x Length 11.2mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C5 (at -2.921 1.397 180) (layer F.SilkS))
    (fp_text value 100µF (at 1.25 4.4 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 66 /3V3))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D6.3_L11.2_P2.5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:bornier2 (layer F.Cu) (tedit 587DD060)
    (at 48.895 45.085 270)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference 5V (at 4.445 -5.207 360) (layer F.SilkS))
    (fp_text value 5VIN (at 5.715 0 540) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 587DD053)
    (at 53.34 55.88 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference 1117 (at 0 -0.762 90) (layer F.SilkS))
    (fp_text value AP1117D33 (at 0 0.762 90) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302 90) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 3.302 90) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 66 /3V3))
    (pad 3 smd rect (at 2.286 3.302 90) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 1 smd rect (at -2.286 3.302 90) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLibrary:Fuseholder5x20 (layer F.Cu) (tedit 58417CBA)
    (at 109.22 52.07)
    (descr http://www.schurter.com/var/schurter/storage/ilcatalogue/files/document/datasheet/en/pdf/typ_OGN.pdf)
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F1 (at 11.25 -6) (layer F.SilkS))
    (fp_text value F_Small (at 11.25 6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 22.5 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PH_IN))
  )
  (module MyLibrary:Fuseholder5x20 (layer F.Cu) (tedit 58417CBA)
    (at 109.22 63.5)
    (descr http://www.schurter.com/var/schurter/storage/ilcatalogue/files/document/datasheet/en/pdf/typ_OGN.pdf)
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F2 (at 11.25 -6) (layer F.SilkS))
    (fp_text value F_Small (at 11.25 6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(F2-Pad1)"))
    (pad 2 thru_hole circle (at 22.5 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PH_IN))
  )
  (module MyLibrary:Fuseholder5x20 (layer F.Cu) (tedit 58417CBA)
    (at 109.22 74.93)
    (descr http://www.schurter.com/var/schurter/storage/ilcatalogue/files/document/datasheet/en/pdf/typ_OGN.pdf)
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F3 (at 11.25 -6) (layer F.SilkS))
    (fp_text value F_Small (at 11.25 6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(F3-Pad1)"))
    (pad 2 thru_hole circle (at 22.5 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PH_IN))
  )
  (module MyLibrary:Fuseholder5x20 (layer F.Cu) (tedit 58417CBA)
    (at 109.22 86.36)
    (descr http://www.schurter.com/var/schurter/storage/ilcatalogue/files/document/datasheet/en/pdf/typ_OGN.pdf)
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F4 (at 11.25 -6) (layer F.SilkS))
    (fp_text value F_Small (at 11.25 6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(F4-Pad1)"))
    (pad 2 thru_hole circle (at 22.5 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PH_IN))
  )
  (module MyLibrary:Fuseholder5x20 (layer F.Cu) (tedit 58417CBA)
    (at 109.22 97.79)
    (descr http://www.schurter.com/var/schurter/storage/ilcatalogue/files/document/datasheet/en/pdf/typ_OGN.pdf)
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F5 (at 11.25 -6) (layer F.SilkS))
    (fp_text value F_Small (at 11.25 6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(F5-Pad1)"))
    (pad 2 thru_hole circle (at 22.5 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PH_IN))
  )
  (module MyLibrary:Fuseholder5x20 (layer F.Cu) (tedit 58417CBA)
    (at 109.22 109.22)
    (descr http://www.schurter.com/var/schurter/storage/ilcatalogue/files/document/datasheet/en/pdf/typ_OGN.pdf)
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F6 (at 11.25 -6) (layer F.SilkS))
    (fp_text value F_Small (at 11.25 6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(F6-Pad1)"))
    (pad 2 thru_hole circle (at 22.5 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PH_IN))
  )
  (module MyLibrary:Fuseholder5x20 (layer F.Cu) (tedit 58417CBA)
    (at 109.22 120.65)
    (descr http://www.schurter.com/var/schurter/storage/ilcatalogue/files/document/datasheet/en/pdf/typ_OGN.pdf)
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F7 (at 11.25 -6) (layer F.SilkS))
    (fp_text value F_Small (at 11.25 6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(F7-Pad1)"))
    (pad 2 thru_hole circle (at 22.5 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PH_IN))
  )
  (module MyLibrary:Fuseholder5x20 (layer F.Cu) (tedit 58417CBA)
    (at 109.22 132.08)
    (descr http://www.schurter.com/var/schurter/storage/ilcatalogue/files/document/datasheet/en/pdf/typ_OGN.pdf)
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (fp_text reference F8 (at 11.25 -6) (layer F.SilkS))
    (fp_text value F_Small (at 11.25 6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(F8-Pad1)"))
    (pad 2 thru_hole circle (at 22.5 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PH_IN))
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 80.01 52.07 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D1 (at 1.91 3.06 180) (layer F.SilkS))
    (fp_text value Led (at 1.3 -2.9 180) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 80.01 63.5 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D2 (at 1.91 3.06 180) (layer F.SilkS))
    (fp_text value Led (at 1.3 -2.9 180) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 6 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 80.01 74.93 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D3 (at 1.91 3.06 180) (layer F.SilkS))
    (fp_text value Led (at 1.3 -2.9 180) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 8 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 80.01 86.36 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D4 (at 1.91 3.06 180) (layer F.SilkS))
    (fp_text value Led (at 1.3 -2.9 180) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 10 "Net-(D4-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 80.01 97.79 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D5 (at 1.91 3.06 180) (layer F.SilkS))
    (fp_text value Led (at 1.3 -2.9 180) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 12 "Net-(D5-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 11 "Net-(D5-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 80.01 109.22 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D6 (at 1.91 3.06 180) (layer F.SilkS))
    (fp_text value Led (at 1.3 -2.9 180) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 14 "Net-(D6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 13 "Net-(D6-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 80.01 120.65 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D7 (at 1.91 3.06 180) (layer F.SilkS))
    (fp_text value Led (at 1.3 -2.9 180) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 16 "Net-(D7-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 15 "Net-(D7-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-3MM (layer F.Cu) (tedit 559B82F6)
    (at 80.01 132.08 180)
    (descr "LED 3mm round vertical")
    (tags "LED  3mm round vertical")
    (fp_text reference D8 (at 1.91 3.06 180) (layer F.SilkS))
    (fp_text value Led (at 1.3 -2.9 180) (layer F.Fab))
    (fp_text user K (at -1.69 1.74 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 18 "Net-(D8-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2 2) (drill 1.00076) (layers *.Cu *.Mask)
      (net 17 "Net-(D8-Pad2)"))
    (model LEDs.3dshapes/LED-3MM.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 587DD036)
    (at 56.134 88.265 270)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference 328p (at 0 -6.05 270) (layer F.SilkS))
    (fp_text value ATMEGA328-A (at 0 6.05 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 64 /ZCD))
    (pad 2 smd rect (at -4.25 -2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -4.25 -1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -4.25 -0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 66 /3V3))
    (pad 5 smd rect (at -4.25 0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -4.25 1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 66 /3V3))
    (pad 7 smd rect (at -4.25 2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -4.25 2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -2.8 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(IC1-Pad9)"))
    (pad 10 smd rect (at -2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at -1.2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 62 /CS))
    (pad 13 smd rect (at 0.4 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at 1.2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 73 "Net-(IC1-Pad14)"))
    (pad 15 smd rect (at 2 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 74 /MOSI))
    (pad 16 smd rect (at 2.8 4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 75 /MISO))
    (pad 17 smd rect (at 4.25 2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 63 /SCK))
    (pad 18 smd rect (at 4.25 2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(IC1-Pad18)"))
    (pad 19 smd rect (at 4.25 1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(IC1-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 22 smd rect (at 4.25 -1.2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.25 -2 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 53 /C7))
    (pad 24 smd rect (at 4.25 -2.8 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 54 /C6))
    (pad 25 smd rect (at 2.8 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 55 /C5))
    (pad 26 smd rect (at 2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 56 /C4))
    (pad 27 smd rect (at 1.2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 57 /C3))
    (pad 28 smd rect (at 0.4 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 58 /C2))
    (pad 29 smd rect (at -0.4 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 90 /RESET))
    (pad 30 smd rect (at -1.2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 60 /C1))
    (pad 31 smd rect (at -2 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 59 /C0))
    (pad 32 smd rect (at -2.8 -4.25) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 80 /IRQ))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 587DD03E)
    (at 68.58 126.365)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference ANT (at 0 -2.39) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 2.39) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 81 "Net-(P1-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 587DCED3)
    (at 76.2 55.88)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 2.286) (layer F.SilkS))
    (fp_text value 390 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 59 /C0))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 587DCECF)
    (at 76.2 68.58)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at -0.254 2.286) (layer F.SilkS))
    (fp_text value 390 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 60 /C1))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 587DCECC)
    (at 76.2 78.74)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R4 (at -0.254 2.286) (layer F.SilkS))
    (fp_text value 390 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 58 /C2))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 587DCECA)
    (at 76.2 90.17)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R5 (at 0 2.286) (layer F.SilkS))
    (fp_text value 390 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 57 /C3))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 587DCEB6)
    (at 76.2 101.6)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R6 (at 0 2.032) (layer F.SilkS))
    (fp_text value 390 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 56 /C4))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D5-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 587DCEBA)
    (at 76.2 113.03)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R7 (at 0 2.286) (layer F.SilkS))
    (fp_text value 390 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 55 /C5))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D6-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 587DCEBC)
    (at 76.2 124.46)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R8 (at -0.254 2.286) (layer F.SilkS))
    (fp_text value 390 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 54 /C6))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D7-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 587DCEC4)
    (at 75.438 135.89)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R9 (at -0.254 2.286) (layer F.SilkS))
    (fp_text value 390 (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 53 /C7))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D8-Pad2)"))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mysensors_Radio:RFM69HW_SMD_Handsoldering (layer F.Cu) (tedit 587DD045)
    (at 51.435 130.81 90)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference RFM69HW (at 0.254 -1.778 90) (layer F.SilkS))
    (fp_text value RFM69HW (at 8.382 7.112 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 83 "Net-(U3-Pad1)"))
    (pad 2 smd rect (at -1.4 2 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 80 /IRQ))
    (pad 3 smd rect (at -1.4 4 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 84 "Net-(U3-Pad3)"))
    (pad 4 smd rect (at -1.4 6 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 85 "Net-(U3-Pad4)"))
    (pad 5 smd rect (at -1.4 8 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 86 "Net-(U3-Pad5)"))
    (pad 6 smd rect (at -1.4 10 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U3-Pad6)"))
    (pad 7 smd rect (at -1.4 12 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U3-Pad7)"))
    (pad 8 smd rect (at -1.4 14 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 66 /3V3))
    (pad 9 smd rect (at 18.3 14 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 18.3 12 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 81 "Net-(P1-Pad1)"))
    (pad 11 smd rect (at 18.3 10 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 18.3 8 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 63 /SCK))
    (pad 13 smd rect (at 18.3 6 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 75 /MISO))
    (pad 14 smd rect (at 18.3 4 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 74 /MOSI))
    (pad 15 smd rect (at 18.3 2 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 62 /CS))
    (pad 16 smd rect (at 18.3 0 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U3-Pad16)"))
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/rfm69hw.wrl
      (at (xyz 0.332 -0.275 0.03))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0.332 -0.08 0.06))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.204 -0.445 0.06))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:RES35 (layer F.Cu) (tedit 57A1F3C5)
    (at 105.41 45.085 180)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference R1 (at 4.8895 0.0635 180) (layer F.SilkS))
    (fp_text value 100k (at 5.08 -1.4605 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(R1-Pad2)"))
    (pad 1 thru_hole circle (at 0.00052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 20 /PH_IN))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_ThroughHole:RES35 (layer F.Cu) (tedit 57A1F3C5)
    (at 95.25 52.07)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference R10 (at 4.8895 0.0635) (layer F.SilkS))
    (fp_text value 4k7 (at 5.08 -1.4605) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(F1-Pad1)"))
    (pad 1 thru_hole circle (at 0.00052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(R10-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_ThroughHole:RES35 (layer F.Cu) (tedit 57A1F3C5)
    (at 95.885 63.5)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference R11 (at 4.8895 0.0635) (layer F.SilkS))
    (fp_text value 4k7 (at 5.08 -1.4605) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(F2-Pad1)"))
    (pad 1 thru_hole circle (at 0.00052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(R11-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_ThroughHole:RES35 (layer F.Cu) (tedit 57A1F3C5)
    (at 95.25 74.93)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference R12 (at 4.8895 0.0635) (layer F.SilkS))
    (fp_text value 4k7 (at 5.08 -1.4605) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(F3-Pad1)"))
    (pad 1 thru_hole circle (at 0.00052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(R12-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_ThroughHole:RES35 (layer F.Cu) (tedit 57A1F3C5)
    (at 95.885 86.36)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference R13 (at 4.8895 0.0635) (layer F.SilkS))
    (fp_text value 4k7 (at 5.08 -1.4605) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(F4-Pad1)"))
    (pad 1 thru_hole circle (at 0.00052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(R13-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_ThroughHole:RES35 (layer F.Cu) (tedit 57A1F3C5)
    (at 95.885 97.79)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference R14 (at 4.8895 0.0635) (layer F.SilkS))
    (fp_text value 4k7 (at 5.08 -1.4605) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(F5-Pad1)"))
    (pad 1 thru_hole circle (at 0.00052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(R14-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_ThroughHole:RES35 (layer F.Cu) (tedit 57A1F3C5)
    (at 95.885 109.22)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference R15 (at 4.8895 0.0635) (layer F.SilkS))
    (fp_text value 4k7 (at 5.08 -1.4605) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(F6-Pad1)"))
    (pad 1 thru_hole circle (at 0.00052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(R15-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_ThroughHole:RES35 (layer F.Cu) (tedit 57A1F3C5)
    (at 95.885 120.65)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference R16 (at 4.8895 0.0635) (layer F.SilkS))
    (fp_text value 4k7 (at 5.08 -1.4605) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(F7-Pad1)"))
    (pad 1 thru_hole circle (at 0.00052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(R16-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_ThroughHole:RES35 (layer F.Cu) (tedit 57A1F3C5)
    (at 95.25 132.08)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference R17 (at 4.8895 0.0635) (layer F.SilkS))
    (fp_text value 4k7 (at 5.08 -1.4605) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(F8-Pad1)"))
    (pad 1 thru_hole circle (at 0.00052 -0.00254 180) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(R17-Pad1)"))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_ThroughHole:RES35 (layer F.Cu) (tedit 57A1F3C5)
    (at 110.49 42.545 180)
    (descr "Diode, DO-35,  SOD27, Horizontal, RM 10mm")
    (tags "Diode, DO-35, SOD27, Horizontal, RM 10mm, 1N4148,")
    (fp_text reference R18 (at 4.8895 0.0635 180) (layer F.SilkS))
    (fp_text value 100k (at 5.08 -1.4605 180) (layer F.Fab))
    (pad 2 thru_hole circle (at 10.16052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(R18-Pad2)"))
    (pad 1 thru_hole circle (at 0.00052 -0.00254) (size 1.69926 1.69926) (drill 0.70104) (layers *.Cu *.Mask F.SilkS)
      (net 28 /N))
    (model Diodes_ThroughHole.3dshapes/Diode_DO-35_SOD27_Horizontal_RM10.wrl
      (at (xyz 0.2 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 587DD04A)
    (at 55.88 104.14 90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference ICSP (at -2.286 2.794 180) (layer F.SilkS))
    (fp_text value ICSP (at 1.27 7.47 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 /MISO))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 66 /3V3))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 63 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 /RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "0V\n" (at 53.848 47.498) (layer F.SilkS))
  (gr_line (start 145 140) (end 145 40) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 45 140) (end 45 40) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 145 140) (end 45 140) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 45 40) (end 145 40) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 140) (xy 84 140) (xy 84 40) (xy 45 40)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 84 140) (xy 45 140) (xy 45 40) (xy 84 40)
      )
    )
  )
)
