(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 76)
    (no_connects 0)
    (area 113.187143 44.274 224.68 153.521)
    (thickness 1.6)
    (drawings 5)
    (tracks 287)
    (zones 0)
    (modules 29)
    (nets 71)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 1)
    (user_trace_width 2)
    (user_trace_width 3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.7 1.7)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 163.83 45.974)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory GERBER/))
  )
  (net 0 "")
  (net 1 "Net-(IC1-Pad1)")
  (net 2 "Net-(IC1-Pad2)")
  (net 3 /3V3)
  (net 4 "Net-(IC1-Pad7)")
  (net 5 "Net-(IC1-Pad8)")
  (net 6 "Net-(IC1-Pad9)")
  (net 7 "Net-(IC1-Pad10)")
  (net 8 "Net-(IC1-Pad11)")
  (net 9 "Net-(IC1-Pad12)")
  (net 10 "Net-(IC1-Pad13)")
  (net 11 /CS)
  (net 12 /MOSI)
  (net 13 /MISO)
  (net 14 /SCK)
  (net 15 "Net-(IC1-Pad18)")
  (net 16 "Net-(IC1-Pad19)")
  (net 17 "Net-(IC1-Pad20)")
  (net 18 "Net-(IC1-Pad22)")
  (net 19 /RESET)
  (net 20 /IRQ)
  (net 21 "Net-(P2-Pad1)")
  (net 22 /S0)
  (net 23 /S1)
  (net 24 /S2)
  (net 25 /S3)
  (net 26 /S4)
  (net 27 /S5)
  (net 28 /S6)
  (net 29 /S7)
  (net 30 "Net-(U2-Pad1)")
  (net 31 "Net-(U2-Pad3)")
  (net 32 "Net-(U2-Pad4)")
  (net 33 "Net-(U2-Pad5)")
  (net 34 "Net-(U2-Pad6)")
  (net 35 "Net-(U2-Pad7)")
  (net 36 "Net-(U2-Pad16)")
  (net 37 /VCC)
  (net 38 /GND)
  (net 39 /SL7)
  (net 40 /SL6)
  (net 41 /SL5)
  (net 42 /SL4)
  (net 43 /SL3)
  (net 44 /SL2)
  (net 45 /SL1)
  (net 46 /SL0)
  (net 47 "Net-(P4-Pad1)")
  (net 48 "Net-(P4-Pad2)")
  (net 49 "Net-(P4-Pad3)")
  (net 50 "Net-(P5-Pad3)")
  (net 51 "Net-(P5-Pad2)")
  (net 52 "Net-(P5-Pad1)")
  (net 53 "Net-(P6-Pad1)")
  (net 54 "Net-(P6-Pad2)")
  (net 55 "Net-(P6-Pad3)")
  (net 56 "Net-(P7-Pad3)")
  (net 57 "Net-(P7-Pad2)")
  (net 58 "Net-(P7-Pad1)")
  (net 59 "Net-(P8-Pad3)")
  (net 60 "Net-(P8-Pad2)")
  (net 61 "Net-(P8-Pad1)")
  (net 62 "Net-(P9-Pad1)")
  (net 63 "Net-(P9-Pad2)")
  (net 64 "Net-(P9-Pad3)")
  (net 65 "Net-(P10-Pad3)")
  (net 66 "Net-(P10-Pad2)")
  (net 67 "Net-(P10-Pad1)")
  (net 68 "Net-(P11-Pad1)")
  (net 69 "Net-(P11-Pad2)")
  (net 70 "Net-(P11-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3V3)
    (add_net /CS)
    (add_net /GND)
    (add_net /IRQ)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /S0)
    (add_net /S1)
    (add_net /S2)
    (add_net /S3)
    (add_net /S4)
    (add_net /S5)
    (add_net /S6)
    (add_net /S7)
    (add_net /SCK)
    (add_net /SL0)
    (add_net /SL1)
    (add_net /SL2)
    (add_net /SL3)
    (add_net /SL4)
    (add_net /SL5)
    (add_net /SL6)
    (add_net /SL7)
    (add_net /VCC)
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad18)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(P10-Pad1)")
    (add_net "Net-(P10-Pad2)")
    (add_net "Net-(P10-Pad3)")
    (add_net "Net-(P11-Pad1)")
    (add_net "Net-(P11-Pad2)")
    (add_net "Net-(P11-Pad3)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P4-Pad2)")
    (add_net "Net-(P4-Pad3)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P5-Pad2)")
    (add_net "Net-(P5-Pad3)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P6-Pad3)")
    (add_net "Net-(P7-Pad1)")
    (add_net "Net-(P7-Pad2)")
    (add_net "Net-(P7-Pad3)")
    (add_net "Net-(P8-Pad1)")
    (add_net "Net-(P8-Pad2)")
    (add_net "Net-(P8-Pad3)")
    (add_net "Net-(P9-Pad1)")
    (add_net "Net-(P9-Pad2)")
    (add_net "Net-(P9-Pad3)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
  )
  (net_class Big ""
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(P2-Pad1)")
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 587DCB16)
    (at 149.352 101.219)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 0 -6.05) (layer F.SilkS))
    (fp_text value ATMEGA328-A (at 0 6.05) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at -4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 /GND))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V3))
    (pad 5 smd rect (at -4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 /GND))
    (pad 6 smd rect (at -4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V3))
    (pad 7 smd rect (at -4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad9)"))
    (pad 10 smd rect (at -2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 /CS))
    (pad 15 smd rect (at 2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 /MOSI))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 /MISO))
    (pad 17 smd rect (at 4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 /SCK))
    (pad 18 smd rect (at 4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad18)"))
    (pad 19 smd rect (at 4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 38 /GND))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 /SL7))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 40 /SL6))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 41 /SL5))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 42 /SL4))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 43 /SL3))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 44 /SL2))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 /RESET))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 45 /SL1))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 46 /SL0))
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /IRQ))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:bornier2 (layer F.Cu) (tedit 587DCB1E)
    (at 195.326 114.554 90)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P1 (at 0 -5.08 90) (layer F.SilkS))
    (fp_text value 5VIN (at 0 5.08 90) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 38 /GND))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 37 /VCC))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 587DCB0A)
    (at 172.847 94.234)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P2 (at 0 -2.39) (layer F.SilkS))
    (fp_text value ANT (at 0 2.39) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(P2-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 587DCB00)
    (at 164.592 105.029 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference P3 (at 1.27 -2.39 180) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 1.27 7.47 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /MISO))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /3V3))
    (pad 3 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 /GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 587DCB51)
    (at 172.974 114.046 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0 -4.5 180) (layer F.SilkS))
    (fp_text value AMS1117 (at 0 4.5 180) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V3))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 37 /VCC))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 38 /GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mysensors_Radio:RFM69HW_SMD_Handsoldering (layer F.Cu) (tedit 587DCB06)
    (at 195.707 106.299 180)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U2 (at 0.254 -1.778 180) (layer F.SilkS))
    (fp_text value RFM69HW (at 8.382 7.112 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U2-Pad1)"))
    (pad 2 smd rect (at -1.4 2 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 /IRQ))
    (pad 3 smd rect (at -1.4 4 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -1.4 6 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -1.4 8 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at -1.4 10 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -1.4 12 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at -1.4 14 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 /3V3))
    (pad 9 smd rect (at 18.3 14 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 /GND))
    (pad 10 smd rect (at 18.3 12 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(P2-Pad1)"))
    (pad 11 smd rect (at 18.3 10 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 38 /GND))
    (pad 12 smd rect (at 18.3 8 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 /SCK))
    (pad 13 smd rect (at 18.3 6 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 /MISO))
    (pad 14 smd rect (at 18.3 4 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 12 /MOSI))
    (pad 15 smd rect (at 18.3 2 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 11 /CS))
    (pad 16 smd rect (at 18.3 0 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(U2-Pad16)"))
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/rfm69hw.wrl
      (at (xyz 0.332 -0.275 0.03))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0.332 -0.08 0.06))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.204 -0.445 0.06))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 0)
    (at 184.15 110.998)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 1.25 -3.8) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 3.8) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 /VCC))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_THT:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 587DCB4D)
    (at 181.102 114.046 270)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C2 (at -1.905 2.54 270) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 3.8 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /3V3))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 /GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_SOIC:SOIC-18W_7.5x11.6mm_Pitch1.27mm (layer B.Cu) (tedit 5750353E)
    (at 135.89 102.362 180)
    (descr "18-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC2 (at 0 6.875 180) (layer B.SilkS))
    (fp_text value ULN2803A (at 0 -6.875 180) (layer B.Fab))
    (pad 18 smd rect (at 4.7 5.08 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 22 /S0))
    (pad 17 smd rect (at 4.7 3.81 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 23 /S1))
    (pad 16 smd rect (at 4.7 2.54 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 24 /S2))
    (pad 15 smd rect (at 4.7 1.27 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 25 /S3))
    (pad 14 smd rect (at 4.7 0 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 26 /S4))
    (pad 13 smd rect (at 4.7 -1.27 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 27 /S5))
    (pad 12 smd rect (at 4.7 -2.54 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 28 /S6))
    (pad 11 smd rect (at 4.7 -3.81 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 29 /S7))
    (pad 10 smd rect (at 4.7 -5.08 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 37 /VCC))
    (pad 9 smd rect (at -4.7 -5.08 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 38 /GND))
    (pad 8 smd rect (at -4.7 -3.81 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 39 /SL7))
    (pad 7 smd rect (at -4.7 -2.54 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 40 /SL6))
    (pad 6 smd rect (at -4.7 -1.27 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 41 /SL5))
    (pad 5 smd rect (at -4.7 0 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 42 /SL4))
    (pad 4 smd rect (at -4.7 1.27 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 43 /SL3))
    (pad 3 smd rect (at -4.7 2.54 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 44 /SL2))
    (pad 2 smd rect (at -4.7 3.81 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 45 /SL1))
    (pad 1 smd rect (at -4.7 5.08 180) (size 2 0.6) (layers B.Cu B.Paste B.Mask)
      (net 46 /SL0))
    (model Housings_SOIC.3dshapes/SOIC-18_7.5x11.6mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:bornier3 (layer F.Cu) (tedit 587FD5F2)
    (at 142.494 60.071 180)
    (descr "Bornier d'alimentation 3 pins")
    (tags DEV)
    (fp_text reference P4 (at 5.05 -4.65 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 5.08 5.08 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 47 "Net-(P4-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 48 "Net-(P4-Pad2)"))
    (pad 3 thru_hole circle (at 10.16 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 49 "Net-(P4-Pad3)"))
    (model Connectors.3dshapes/bornier3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:bornier3 (layer F.Cu) (tedit 587FD5F2)
    (at 159.766 60.071 180)
    (descr "Bornier d'alimentation 3 pins")
    (tags DEV)
    (fp_text reference P5 (at 5.05 -4.65 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 5.08 5.08 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 10.16 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 50 "Net-(P5-Pad3)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 51 "Net-(P5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 52 "Net-(P5-Pad1)"))
    (model Connectors.3dshapes/bornier3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:bornier3 (layer F.Cu) (tedit 587FD5F2)
    (at 177.038 60.071 180)
    (descr "Bornier d'alimentation 3 pins")
    (tags DEV)
    (fp_text reference P6 (at 5.05 -4.65 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 5.08 5.08 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 53 "Net-(P6-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 54 "Net-(P6-Pad2)"))
    (pad 3 thru_hole circle (at 10.16 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 55 "Net-(P6-Pad3)"))
    (model Connectors.3dshapes/bornier3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:bornier3 (layer F.Cu) (tedit 587FD5F2)
    (at 194.31 60.071 180)
    (descr "Bornier d'alimentation 3 pins")
    (tags DEV)
    (fp_text reference P7 (at 5.05 -4.65 180) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 5.08 5.08 180) (layer F.Fab))
    (pad 3 thru_hole circle (at 10.16 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 56 "Net-(P7-Pad3)"))
    (pad 2 thru_hole circle (at 5.08 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 57 "Net-(P7-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 58 "Net-(P7-Pad1)"))
    (model Connectors.3dshapes/bornier3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:bornier3 (layer F.Cu) (tedit 587FD5F2)
    (at 182.626 147.066)
    (descr "Bornier d'alimentation 3 pins")
    (tags DEV)
    (fp_text reference P8 (at 5.05 -4.65) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 5.08 5.08) (layer F.Fab))
    (pad 3 thru_hole circle (at 10.16 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 59 "Net-(P8-Pad3)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 60 "Net-(P8-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 61 "Net-(P8-Pad1)"))
    (model Connectors.3dshapes/bornier3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:bornier3 (layer F.Cu) (tedit 587FD5F2)
    (at 165.862 147.066)
    (descr "Bornier d'alimentation 3 pins")
    (tags DEV)
    (fp_text reference P9 (at 5.05 -4.65) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 5.08 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 62 "Net-(P9-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 63 "Net-(P9-Pad2)"))
    (pad 3 thru_hole circle (at 10.16 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 64 "Net-(P9-Pad3)"))
    (model Connectors.3dshapes/bornier3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:bornier3 (layer F.Cu) (tedit 587FD5F2)
    (at 149.098 147.066)
    (descr "Bornier d'alimentation 3 pins")
    (tags DEV)
    (fp_text reference P10 (at 5.05 -4.65) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 5.08 5.08) (layer F.Fab))
    (pad 3 thru_hole circle (at 10.16 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 65 "Net-(P10-Pad3)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 66 "Net-(P10-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 67 "Net-(P10-Pad1)"))
    (model Connectors.3dshapes/bornier3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:bornier3 (layer F.Cu) (tedit 587FD5F2)
    (at 132.334 147.066)
    (descr "Bornier d'alimentation 3 pins")
    (tags DEV)
    (fp_text reference P11 (at 5.05 -4.65) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 5.08 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 68 "Net-(P11-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 69 "Net-(P11-Pad2)"))
    (pad 3 thru_hole circle (at 10.16 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 70 "Net-(P11-Pad3)"))
    (model Connectors.3dshapes/bornier3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLibrary:SRD_Relay_TypeC (layer F.Cu) (tedit 58822E33)
    (at 137.414 74.295 90)
    (fp_text reference RLY1 (at 0 9 90) (layer F.SilkS))
    (fp_text value SRD_Type_C (at 0.25 -6.75 90) (layer F.Fab))
    (pad 5 thru_hole circle (at -8.1 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 48 "Net-(P4-Pad2)"))
    (pad 3 thru_hole circle (at 6.1 -6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 49 "Net-(P4-Pad3)"))
    (pad 4 thru_hole circle (at 6.1 6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 47 "Net-(P4-Pad1)"))
    (pad 2 thru_hole circle (at -6.1 6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 22 /S0))
    (pad 1 thru_hole circle (at -6.1 -6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 /VCC))
  )
  (module MyLibrary:SRD_Relay_TypeC (layer F.Cu) (tedit 58822E33)
    (at 154.686 74.295 90)
    (fp_text reference RLY2 (at 0 9 90) (layer F.SilkS))
    (fp_text value SRD_Type_C (at 0.25 -6.75 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -6.1 -6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 /VCC))
    (pad 2 thru_hole circle (at -6.1 6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 23 /S1))
    (pad 4 thru_hole circle (at 6.1 6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 52 "Net-(P5-Pad1)"))
    (pad 3 thru_hole circle (at 6.1 -6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 50 "Net-(P5-Pad3)"))
    (pad 5 thru_hole circle (at -8.1 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 51 "Net-(P5-Pad2)"))
  )
  (module MyLibrary:SRD_Relay_TypeC (layer F.Cu) (tedit 58822E33)
    (at 171.958 74.295 90)
    (fp_text reference RLY3 (at 0 9 90) (layer F.SilkS))
    (fp_text value SRD_Type_C (at 0.25 -6.75 90) (layer F.Fab))
    (pad 5 thru_hole circle (at -8.1 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 54 "Net-(P6-Pad2)"))
    (pad 3 thru_hole circle (at 6.1 -6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 55 "Net-(P6-Pad3)"))
    (pad 4 thru_hole circle (at 6.1 6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 53 "Net-(P6-Pad1)"))
    (pad 2 thru_hole circle (at -6.1 6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 24 /S2))
    (pad 1 thru_hole circle (at -6.1 -6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 /VCC))
  )
  (module MyLibrary:SRD_Relay_TypeC (layer F.Cu) (tedit 58822E33)
    (at 189.23 74.295 90)
    (fp_text reference RLY4 (at 0 9 90) (layer F.SilkS))
    (fp_text value SRD_Type_C (at 0.25 -6.75 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -6.1 -6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 /VCC))
    (pad 2 thru_hole circle (at -6.1 6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 /S3))
    (pad 4 thru_hole circle (at 6.1 6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 58 "Net-(P7-Pad1)"))
    (pad 3 thru_hole circle (at 6.1 -6 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 56 "Net-(P7-Pad3)"))
    (pad 5 thru_hole circle (at -8.1 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 57 "Net-(P7-Pad2)"))
  )
  (module MyLibrary:SRD_Relay_TypeC (layer F.Cu) (tedit 58822E33)
    (at 187.706 133.35 270)
    (fp_text reference RLY5 (at 0 9 270) (layer F.SilkS))
    (fp_text value SRD_Type_C (at 0.25 -6.75 270) (layer F.Fab))
    (pad 5 thru_hole circle (at -8.1 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 60 "Net-(P8-Pad2)"))
    (pad 3 thru_hole circle (at 6.1 -6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 59 "Net-(P8-Pad3)"))
    (pad 4 thru_hole circle (at 6.1 6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 61 "Net-(P8-Pad1)"))
    (pad 2 thru_hole circle (at -6.1 6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 /S4))
    (pad 1 thru_hole circle (at -6.1 -6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 /VCC))
  )
  (module MyLibrary:SRD_Relay_TypeC (layer F.Cu) (tedit 58822E33)
    (at 170.942 133.35 270)
    (fp_text reference RLY6 (at 0 9 270) (layer F.SilkS))
    (fp_text value SRD_Type_C (at 0.25 -6.75 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -6.1 -6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 /VCC))
    (pad 2 thru_hole circle (at -6.1 6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 /S5))
    (pad 4 thru_hole circle (at 6.1 6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 62 "Net-(P9-Pad1)"))
    (pad 3 thru_hole circle (at 6.1 -6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 64 "Net-(P9-Pad3)"))
    (pad 5 thru_hole circle (at -8.1 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 63 "Net-(P9-Pad2)"))
  )
  (module MyLibrary:SRD_Relay_TypeC (layer F.Cu) (tedit 58822E33)
    (at 154.178 133.35 270)
    (fp_text reference RLY7 (at 0 9 270) (layer F.SilkS))
    (fp_text value SRD_Type_C (at 0.25 -6.75 270) (layer F.Fab))
    (pad 5 thru_hole circle (at -8.1 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 66 "Net-(P10-Pad2)"))
    (pad 3 thru_hole circle (at 6.1 -6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 65 "Net-(P10-Pad3)"))
    (pad 4 thru_hole circle (at 6.1 6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 67 "Net-(P10-Pad1)"))
    (pad 2 thru_hole circle (at -6.1 6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 /S6))
    (pad 1 thru_hole circle (at -6.1 -6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 /VCC))
  )
  (module MyLibrary:SRD_Relay_TypeC (layer F.Cu) (tedit 58822E33)
    (at 137.414 133.35 270)
    (fp_text reference RLY8 (at 0 9 270) (layer F.SilkS))
    (fp_text value SRD_Type_C (at 0.25 -6.75 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -6.1 -6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 37 /VCC))
    (pad 2 thru_hole circle (at -6.1 6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 /S7))
    (pad 4 thru_hole circle (at 6.1 6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 68 "Net-(P11-Pad1)"))
    (pad 3 thru_hole circle (at 6.1 -6 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 70 "Net-(P11-Pad3)"))
    (pad 5 thru_hole circle (at -8.1 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 69 "Net-(P11-Pad2)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5885B47C)
    (at 201.83 77.927)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5885B47F)
    (at 124.83 77.927)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5885B484)
    (at 124.83 126.974)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5885B488)
    (at 201.83 126.974)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference "" (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_line (start 120.83 55.974) (end 120.83 150.974) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 205.83 55.974) (end 120.83 55.974) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 205.83 150.974) (end 205.83 55.974) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 204.83 150.974) (end 205.83 150.974) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 120.83 150.974) (end 204.83 150.974) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 38) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 205.83 86.974) (xy 120.83 86.974) (xy 120.83 120.974) (xy 205.83 120.974)
      )
    )
  )
  (zone (net 38) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 205.83 120.974) (xy 205.83 86.974) (xy 120.83 86.974) (xy 120.83 120.974)
      )
    )
  )
)
