(kicad_pcb (version 20170123) (host pcbnew no-vcs-found-7652~57~ubuntu16.04.1)
  (general
    (links 280)
    (no_connects 0)
    (area 106.702381 54.9195 191.532143 125.8365)
    (thickness 1.6)
    (drawings 23)
    (tracks 337)
    (zones 0)
    (modules 231)
    (nets 32)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.35)
    (trace_clearance 0.3)
    (zone_clearance 0.6)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.8 0.8)
    (mod_text_width 0.15)
    (pad_size 0.8 0.8)
    (pad_drill 0.4)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +3V3)
  (net 3 "Net-(C4-Pad2)")
  (net 4 /RST)
  (net 5 /MISO)
  (net 6 /SCK)
  (net 7 /MOSI)
  (net 8 "Net-(D1-Pad2)")
  (net 9 +5V)
  (net 10 "Net-(D2-Pad2)")
  (net 11 "Net-(D3-Pad2)")
  (net 12 "Net-(D4-Pad2)")
  (net 13 "Net-(D5-Pad2)")
  (net 14 "Net-(F1-Pad1)")
  (net 15 "Net-(F1-Pad2)")
  (net 16 /H_RELAY_CMD)
  (net 17 /ATSHA204A)
  (net 18 /ERR_LED)
  (net 19 /TX_LED)
  (net 20 /RX_LED)
  (net 21 /SPI_FLASH_SS)
  (net 22 "Net-(IC1-Pad8)")
  (net 23 "Net-(IC1-Pad7)")
  (net 24 "Net-(P1-Pad1)")
  (net 25 "Net-(Q1-Pad2)")
  (net 26 /HEATER_ON_LED)
  (net 27 "Net-(RL1-Pad11)")
  (net 28 "Net-(RL1-Pad14)")
  (net 29 "Net-(U4-Pad2)")
  (net 30 /RFM69W_INT)
  (net 31 /RFM69W_SS)
  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.35)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /ATSHA204A)
    (add_net /ERR_LED)
    (add_net /HEATER_ON_LED)
    (add_net /H_RELAY_CMD)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RFM69W_INT)
    (add_net /RFM69W_SS)
    (add_net /RST)
    (add_net /RX_LED)
    (add_net /SCK)
    (add_net /SPI_FLASH_SS)
    (add_net /TX_LED)
    (add_net GND)
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(Q1-Pad2)")
    (add_net "Net-(RL1-Pad11)")
    (add_net "Net-(RL1-Pad14)")
    (add_net "Net-(U4-Pad2)")
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 147.775 116.65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 147.775 118.15)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 146.275 118.15)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 146.275 116.65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 141.25 116.4)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 141.25 117.9)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 139.75 117.9)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 139.75 116.4)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 135.675 82.075)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 135.675 83.575)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 134.175 83.575)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 134.175 82.075)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 121.15 67.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 119.65 65.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 121.15 64.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 119.65 64.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 119.65 67.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 121.15 65.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 127.625 66.425)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 127.625 64.925)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 127.625 63.425)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 130.65 59.025)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 132.15 59.025)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 133.65 59.025)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 135.15 59.025)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 129.15 59.025)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 122.65 62.025)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 124.15 60.525)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 121.15 62.025)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 125.65 60.525)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 124.15 59.025)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 122.65 60.525)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 121.15 60.525)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 125.65 59.025)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 124.15 62.025)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 127.15 60.525)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 121.15 59.025)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 127.15 62.025)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 125.65 62.025)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 127.15 59.025)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 122.65 59.025)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.225 82.3)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.225 83.8)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.725 83.8)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.725 82.3)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 148.4 86.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 146.9 85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 148.4 85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 146.9 86.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 144.25 86.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 145.6 85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 144.25 85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 142.75 85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 142.75 86.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 145.6 86.5)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 167.85 120.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 167.85 121.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 166.35 121.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 166.35 120.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 170.7 120.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 170.7 121.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 169.2 121.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 172.2 121.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 169.2 120.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 172.2 120.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 127.425 121.65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 130.425 121.65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 128.925 121.65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 130.425 120.15)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 127.425 120.15)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 128.925 120.15)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 151.275 120.125)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 151.275 121.625)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 149.775 121.625)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 152.775 121.625)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 149.775 120.125)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 152.775 120.125)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 144.775 121.625)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 147.775 121.625)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 146.275 121.625)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 147.775 120.125)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 144.775 120.125)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 146.275 120.125)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 133.875 121.65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 133.875 120.15)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 135.375 120.15)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 135.375 121.65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 132.375 121.65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 132.375 120.15)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.7 80.725)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.7 79.225)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.2 80.725)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.2 77.725)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.7 76.225)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.2 79.225)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.2 76.225)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.7 77.725)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.175 73.2)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.675 71.7)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.175 70.2)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.675 70.2)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.175 74.7)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.675 74.7)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.675 73.2)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.175 71.7)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.675 65.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.175 68.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.175 67.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.175 65.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.175 64.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.675 64.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.675 68.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.675 67.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 122.6 121.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 122.6 116.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 121.1 116.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 121.1 121.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 122.6 119.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 121.1 119.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 121.1 118.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 124.1 116.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 124.1 119.85)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 122.6 118.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 124.1 118.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 124.1 121.35)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 163.25 118.55)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 164.75 120.05)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 161.75 118.55)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 164.75 118.55)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 164.75 115.55)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 163.25 117.05)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 163.25 115.55)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 164.75 117.05)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 161.75 120.05)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 161.75 115.55)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 163.25 120.05)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 161.75 117.05)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.7 93.65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 119.7 95.15)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.2 95.15)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.7 95.15)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 119.7 98.15)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.2 96.65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.7 98.15)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 119.7 93.65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.2 98.15)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 116.7 96.65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 119.7 96.65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 118.2 93.65)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 130.5 83.4)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 129 83.4)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 127.5 83.4)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 130.5 81.9)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 129 81.9)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 127.5 81.9)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 130.5 80.4)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 129 80.4)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 127.5 80.4)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 130.5 78.9)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 129 78.9)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 127.5 78.9)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 135.15 66.45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 133.65 66.45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 132.15 66.45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 130.65 66.45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 129.15 66.45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 135.15 64.95)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 133.65 64.95)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 132.15 64.95)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 130.65 64.95)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 129.15 64.95)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 135.15 63.45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 133.65 63.45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 132.15 63.45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 130.65 63.45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 129.15 63.45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 135.15 61.95)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 133.65 61.95)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 132.15 61.95)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 130.65 61.95)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 129.15 61.95)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 135.15 60.45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 133.65 60.45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 132.15 60.45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 130.65 60.45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:1pin (layer F.Cu) (tedit 589825D6)
    (at 129.15 60.45)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF** (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad "" thru_hole circle (at 0 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu)
      (net 1 GND) (zone_connect 2))
  )
  (module myfootprints:Symbol_HighVoltage_Type2_FrontSilk_VerySmall (layer B.Cu) (tedit 58908E48)
    (at 170.8 73.3 180)
    (descr "Symbol, High Voltage, Type 2, Copper Top, Very Small,")
    (tags "Symbol, High Voltage, Type 2, Copper Top, Very Small,")
    (fp_text reference REF** (at -0.127 5.715 180) (layer B.SilkS) hide)
    (fp_text value "High Voltage" (at -0.381 -4.572 180) (layer B.SilkS))
  )
  (module Symbols:OSHW-Logo_5.7x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 118.875 112.15)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 588F5A71)
    (at 117.65 59.875)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 588F5A71)
    (at 181.8 59.925)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 588F5A71)
    (at 181.8 95.275)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 588F5A71)
    (at 181.8 120.475)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 588F5A71)
    (at 117.75 87.175)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 588F5A71)
    (at 117.65 120.475)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (fp_text reference REF** (at 0 -3.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.2mm_M2 (at 0 3.2) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Resistors_ThroughHole:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 588F5D02)
    (at 174.27 117.775 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R8 (at 5.82 1.875 180) (layer F.SilkS))
    (fp_text value 330 (at 3.42 1.85 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 "Net-(D5-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 26 /HEATER_ON_LED))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/RES-0.125W-H-MF.stp
      (at (xyz 0.1496062992125984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 588F5CEC)
    (at 174.27 113.275 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 5.795 1.75 180) (layer F.SilkS))
    (fp_text value 330 (at 3.37 1.75 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 20 /RX_LED))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/RES-0.125W-H-MF.stp
      (at (xyz 0.1496062992125984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 588F5CE8)
    (at 174.27 108.475 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at 5.845 1.8 180) (layer F.SilkS))
    (fp_text value 330 (at 3.495 1.825 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(D3-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 19 /TX_LED))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/RES-0.125W-H-MF.stp
      (at (xyz 0.1496062992125984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 588F5CDC)
    (at 174.37 104.075 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R7 (at 5.87 1.95 180) (layer F.SilkS))
    (fp_text value 330 (at 3.445 1.9 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 12 "Net-(D4-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 /ERR_LED))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/RES-0.125W-H-MF.stp
      (at (xyz 0.1496062992125984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:ZTTCR-3 (layer F.Cu) (tedit 588B71E3)
    (at 122.65 95.975 90)
    (attr smd)
    (fp_text reference Y1 (at -3.7 -2.075) (layer F.SilkS))
    (fp_text value 8MHz (at -3.7 0.525) (layer F.SilkS))
    (pad 3 smd rect (at 1.5 0 90) (size 0.8 3) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC1-Pad7)"))
    (pad 2 smd rect (at 0 0 90) (size 0.8 3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 0.8 3) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(IC1-Pad8)"))
    (model ${KISYS3DMOD}/Oscillators.3dshapes/zttcr_MG_ceramic_resonator.stp
      (at (xyz 0 -0.01968503937007874 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_ThroughHole:SW_PUSH_6mm (layer F.Cu) (tedit 588F5D76)
    (at 117.5 102.375)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference SW1 (at 9.175 4.825 270) (layer F.SilkS))
    (fp_text value RESET (at 9.25 0.8 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 /RST))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 4 /RST))
    (model ${KISYS3DMOD}/Button_Switches_THT.3dshapes/tactile_sw_6x6x17.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 588F5E5F)
    (at 138.2 95.925 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 1.575 1.375 180) (layer F.SilkS))
    (fp_text value 100n (at -1.2 1.45 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 588F5D88)
    (at 122.1 91.275)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -1.6 -1.675) (layer F.SilkS))
    (fp_text value 100n (at 0.975 -1.725) (layer F.SilkS))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 588F5E52)
    (at 138.2 92.975 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 1.4 1.5 180) (layer F.SilkS))
    (fp_text value 100n (at -1.35 1.525 180) (layer F.SilkS))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C4-Pad2)"))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 588F5DE8)
    (at 141.8 109.275 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 1.65 2 90) (layer B.SilkS))
    (fp_text value 100n (at -1.325 1.975 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 588F5E17)
    (at 138.65 85.775)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 1.175 -1.55) (layer B.SilkS))
    (fp_text value 100n (at -1.65 -1.575) (layer B.SilkS))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-B_EIA-3528-21_Hand (layer B.Cu) (tedit 588F5C6F)
    (at 123 72.925 270)
    (descr "Tantalum capacitor, Case B, EIA 3528-21, 3.5x2.8x1.9mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C8 (at -1.625 2.775 270) (layer B.SilkS))
    (fp_text value 22u (at 1.175 2.8 270) (layer B.SilkS))
    (pad 1 smd rect (at -2.15 0 270) (size 3.2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 2.15 0 270) (size 3.2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-B_EIA-3528-21_Hand (layer F.Cu) (tedit 588F5E05)
    (at 126.95 114.475 90)
    (descr "Tantalum capacitor, Case B, EIA 3528-21, 3.5x2.8x1.9mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C9 (at -0.25 -2.625 90) (layer F.SilkS))
    (fp_text value 10u (at 2.475 -2.65 90) (layer F.SilkS))
    (pad 2 smd rect (at 2.15 0 90) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.15 0 90) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch2.54mm (layer F.Cu) (tedit 588F5D0C)
    (at 156.725 109.905)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference CON1 (at 0.525 -3.905 180) (layer F.SilkS))
    (fp_text value AVR-ISP-10 (at 1.15 -2.405 180) (layer F.SilkS))
    (pad 10 thru_hole oval (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /MISO))
    (pad 8 thru_hole oval (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /SCK))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /RST))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /MOSI))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/PinHeader_Straight_2x05x2.54mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 588F5E95)
    (at 150.95 87.615 270)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 7.835 1.825 270) (layer F.SilkS))
    (fp_text value 1N4148 (at 4.035 1.925 270) (layer F.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 +5V))
    (model Diodes_ThroughHole.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.stp
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Diode_Packages.3dshapes/DO35.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 588F5D5D)
    (at 182.215 110.325 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 5.765 0.125 270) (layer F.SilkS))
    (fp_text value GW_RX (at 4.49 0 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(D2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_Packages.3dshapes/led_3mm_green_short.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 588F5D5A)
    (at 182.215 105.525 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D3 (at 5.74 -0.2 270) (layer F.SilkS))
    (fp_text value GW_TX (at 4.49 -0.3 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(D3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_Packages.3dshapes/led_3mm_blue_short.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 588F5D56)
    (at 182.215 100.725 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D4 (at 5.79 -0.1 270) (layer F.SilkS))
    (fp_text value GW_ERR (at 4.59 -0.025 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LED_Packages.3dshapes/led_3mm_red_short.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 588F5D60)
    (at 182.215 114.925 180)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D5 (at 5.815 -0.95 270) (layer F.SilkS))
    (fp_text value HEATER_ON (at 4.465 -1.15 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LED_Packages.3dshapes/led_3mm_yellow_short.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_lateral_Type-II (layer F.Cu) (tedit 588F5C90)
    (at 170.75 77.875)
    (descr "Fuseholder, 5x20, open, horizontal, Type-II, lateral,")
    (tags "Fuseholder, 5x20, open, horizontal, Type-II, lateral, Sicherungshalter, offen,")
    (fp_text reference F1 (at -2.05 -4.375) (layer F.SilkS))
    (fp_text value 0.5A (at 0.625 -4.4) (layer F.SilkS))
    (pad 1 thru_hole circle (at -7.66064 2.54) (size 2.3495 2.3495) (drill 1.34874) (layers *.Cu *.Mask)
      (net 14 "Net-(F1-Pad1)"))
    (pad 1 thru_hole circle (at -7.66064 -2.54) (size 2.3495 2.3495) (drill 1.34874) (layers *.Cu *.Mask)
      (net 14 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 7.66064 2.54) (size 2.3495 2.3495) (drill 1.34874) (layers *.Cu *.Mask)
      (net 15 "Net-(F1-Pad2)"))
    (pad 2 thru_hole circle (at 7.66064 -2.54) (size 2.3495 2.3495) (drill 1.34874) (layers *.Cu *.Mask)
      (net 15 "Net-(F1-Pad2)"))
    (model ${KISYS3DMOD}/Fuse_Holders_Packages.3dshapes/fuse_clips_5mm_typeII.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 588F5DB8)
    (at 130.35 93.275)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at -4.25 5.475) (layer F.SilkS))
    (fp_text value ATMEGA328P-A (at 0.675 6.725) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 /RFM69W_INT))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 /RST))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 /HEATER_ON_LED))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 16 /H_RELAY_CMD))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 /ATSHA204A))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 /ERR_LED))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 /TX_LED))
    (pad 23 smd rect (at 4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /RX_LED))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 20 smd rect (at 4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C4-Pad2)"))
    (pad 19 smd rect (at 4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 17 smd rect (at 4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 /SCK))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 /MISO))
    (pad 15 smd rect (at 2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 /MOSI))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 /RFM69W_SS))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 /SPI_FLASH_SS))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(IC1-Pad8)"))
    (pad 7 smd rect (at -4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC1-Pad7)"))
    (pad 6 smd rect (at -4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 5 smd rect (at -4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 1 smd rect (at -4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 588F5D15)
    (at 139.35 120.675)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference P1 (at 2.525 -1.45) (layer F.SilkS))
    (fp_text value ANTENNA (at 6.25 -1.45) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(P1-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 588F5E86)
    (at 146.35 90.875 180)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 3.1 2.85 180) (layer F.SilkS))
    (fp_text value BC337 (at -0.175 2.85 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.27 -1.27 270) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 25 "Net-(Q1-Pad2)"))
    (model ${KISYS3DMOD}/TO_Packages.3dshapes/TO-92.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 588F5E81)
    (at 144.95 96.675 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 1.475 1.725 180) (layer F.SilkS))
    (fp_text value 5K6 (at -1.1 1.725 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(Q1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /H_RELAY_CMD))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 588F5DF8)
    (at 136.825 112.9)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 1.45 1.725) (layer B.SilkS))
    (fp_text value 56K (at -1.075 1.75) (layer B.SilkS))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 /SPI_FLASH_SS))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 588F5DA1)
    (at 130.95 86.375 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 1.4 1.525 180) (layer F.SilkS))
    (fp_text value 10K (at -1.225 1.55 180) (layer F.SilkS))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /RST))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 +5V))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 588F5EF8)
    (at 134.85 88.975 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 1.125 -1.575 90) (layer B.SilkS))
    (fp_text value 1K (at -1.15 -1.625 90) (layer B.SilkS))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 17 /ATSHA204A))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 588F5E63)
    (at 138.275 98.725)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at -1.3 -1.375) (layer F.SilkS))
    (fp_text value 56K (at 1.8 -1.325) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 31 /RFM69W_SS))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:RM50_SP (layer F.Cu) (tedit 588F5C83)
    (at 155.55 93.275)
    (descr "relay, Sanyou SRD series Form C")
    (fp_text reference RL1 (at 7.55 -8.65) (layer F.SilkS))
    (fp_text value RM50-SP (at 12.35 -8.65) (layer F.SilkS))
    (pad A2 thru_hole circle (at 1.95 6.05 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(D1-Pad2)"))
    (pad A1 thru_hole circle (at 1.95 -5.95 90) (size 2.5 2.5) (drill 1.2) (layers *.Cu *.Mask F.SilkS)
      (net 9 +5V))
    (pad 11 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 27 "Net-(RL1-Pad11)"))
    (pad 14 thru_hole circle (at 14.2 6 90) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 28 "Net-(RL1-Pad14)"))
    (model ${KISYS3DMOD}/Relays.3dshapes/rm50-sp.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 588F5DDD)
    (at 136.65 108.675)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -0.175 -4.825) (layer B.SilkS))
    (fp_text value AT25DF512C (at 0 -3.5) (layer B.SilkS))
    (pad 8 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 7 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 6 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 /SCK))
    (pad 5 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 /MOSI))
    (pad 4 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 5 /MISO))
    (pad 1 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 21 /SPI_FLASH_SS))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 588F5E28)
    (at 139.05 89.075)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at -0.425 2.2) (layer B.SilkS))
    (fp_text value ATSHA204A (at -0.175 3.325) (layer B.SilkS))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 1 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 17 /ATSHA204A))
    (model ${KISYS3DMOD}/SOT_Packages_SMD.3dshapes/SOT23-3.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer B.Cu) (tedit 588F5C5E)
    (at 130 73.025)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U3 (at 0 -5.25 180) (layer B.SilkS))
    (fp_text value AMS1117-3.3 (at -0.125 -4.175 180) (layer B.SilkS))
    (pad 1 smd rect (at -3.15 2.3) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -3.15 -2.3) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 9 +5V))
    (pad 2 smd rect (at -3.15 0) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 4 smd rect (at 3.15 0) (size 2 3.8) (layers B.Cu B.Paste B.Mask))
    (model ${KISYS3DMOD}/SOT_Packages_SMD.3dshapes/SOT223-3.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:HLK-PM01 placed (layer F.Cu) (tedit 588F5C45)
    (at 153.35 75.175 180)
    (fp_text reference U4 (at 16.95 15.6) (layer F.SilkS))
    (fp_text value HLK-PM01 (at 11.75 15.6 180) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 0 5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U4-Pad2)"))
    (pad 4 thru_hole circle (at 29.4 -5.2 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at 29.4 10.2 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask F.SilkS)
      (net 9 +5V))
    (model ${KISYS3DMOD}/Power_Supply.3dshapes/hlk-pm01.stp
      (at (xyz 0.5787401574803149 -0.09842519685039371 0.0007874015748031497))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_radios:RFM69HW_SMD_Handsoldering (layer F.Cu) (tedit 588F5DCE)
    (at 132.95 103.475)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U5 (at 9.325 -1.85) (layer F.SilkS))
    (fp_text value RFM69W (at 13.475 -1.85) (layer F.SilkS))
    (pad 16 smd rect (at 18.3 0) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 18.3 2) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 /RFM69W_SS))
    (pad 14 smd rect (at 18.3 4) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 /MOSI))
    (pad 13 smd rect (at 18.3 6) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 /MISO))
    (pad 12 smd rect (at 18.3 8) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /SCK))
    (pad 11 smd rect (at 18.3 10) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 18.3 12) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P1-Pad1)"))
    (pad 9 smd rect (at 18.3 14) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -1.4 14) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 7 smd rect (at -1.4 12) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -1.4 10) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -1.4 8) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -1.4 6) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -1.4 4) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.4 2) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 /RFM69W_INT))
    (pad 1 smd rect (at -1.4 0) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Radio_Modules.3dshapes/RFM69W.stp
      (at (xyz 0.6692913385826772 -0.5511811023622047 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Varistors:RV_Disc_D12_W6.3_P7.5 (layer F.Cu) (tedit 588F5C93)
    (at 169.75 66.875 180)
    (tags "varistor SIOV")
    (fp_text reference VR1 (at 3.75 5.7 180) (layer F.SilkS))
    (fp_text value VAR10-300 (at 3.75 -2.6 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 7.5 3.1 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U4-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(F1-Pad1)"))
    (model ${KISYS3DMOD}/Varistor_Packages.3dshapes/RV_Disc_D10_P7.5.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer F.Cu) (tedit 588F5CBA)
    (at 179.45 90.275 90)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference X1 (at 1.475 -4.5 90) (layer F.SilkS))
    (fp_text value HEATER_SW (at 6.4 0.8 180) (layer F.SilkS))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 27 "Net-(RL1-Pad11)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 28 "Net-(RL1-Pad14)"))
    (model ${KISYS3DMOD}/Terminal_Block_Packages.3dshapes/mkds-3.5-02.stp
      (at (xyz 0 0 0.0007874015748031497))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_PT-3.5mm_2pol (layer F.Cu) (tedit 588F5CAE)
    (at 179.35 69.375 90)
    (descr "2-way 3.5mm pitch terminal block, Phoenix PT series")
    (fp_text reference X2 (at 1.6 -4.4 90) (layer F.SilkS))
    (fp_text value 230Vac~~ (at 6.15 0.5 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(F1-Pad2)"))
    (pad 2 thru_hole circle (at 3.5 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 29 "Net-(U4-Pad2)"))
    (model ${KISYS3DMOD}/Terminal_Block_Packages.3dshapes/mkds-3.5-02.stp
      (at (xyz 0 0 0.0007874015748031497))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 151.1 64.7) (end 147.22492 64.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.1 71.85) (end 151.1 64.699607) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.1 80.675) (end 147.22492 80.675) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.1 80.675393) (end 151.1 73.525) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.225 64.7) (end 147.225 80.675) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.95 73.525) (end 151.1 73.525) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.95 71.85) (end 156.95 73.525) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 156.950053 71.85) (end 151.1 71.85) (layer Edge.Cuts) (width 0.1))
  (gr_text NC (at 154.375 112.525 90) (layer F.SilkS))
  (gr_text GND (at 161.625 120.125 90) (layer F.SilkS))
  (gr_text GND (at 161.625 117.5 90) (layer F.SilkS))
  (gr_text GND (at 161.65 115.025 90) (layer F.SilkS))
  (gr_text "Rev. 0.2" (at 175.45 121.525) (layer F.SilkS))
  (gr_text GND (at 161.625 112.575 90) (layer F.SilkS))
  (gr_text +3V3 (at 161.675 109.825 90) (layer F.SilkS))
  (gr_text MISO (at 154.4 120.1 90) (layer F.SilkS))
  (gr_text SCK (at 154.425 117.525 90) (layer F.SilkS))
  (gr_text RST (at 154.4 114.925 90) (layer F.SilkS))
  (gr_text MOSI (at 154.425 109.825 90) (layer F.SilkS))
  (gr_line (start 115.15 122.975) (end 115.15 57.475) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 184.25 122.975) (end 115.15 122.975) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 184.25 57.475) (end 184.25 122.975) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.15 57.475) (end 184.25 57.475) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.6))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.175 57.475) (xy 184.2 57.475) (xy 184.2 123.025) (xy 115.175 123.025)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.42637 57.8) (xy 184.25 57.8) (xy 184.25 98.475) (xy 176.124869 98.5) (xy 176.125 102.95)
        (xy 149.526326 102.95) (xy 149.525 84.05) (xy 136.425685 84.029)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.6))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.15 57.5) (xy 184.25 57.5) (xy 184.25 122.975) (xy 115.15 122.975)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 136.42637 57.8) (xy 184.25 57.8) (xy 184.25 98.475) (xy 176.125 98.5) (xy 176.125 102.95)
        (xy 149.526326 102.95) (xy 149.525 84.05) (xy 136.425685 84.029)
      )
    )
  )
)
