(kicad_pcb (version 4) (host pcbnew 4.0.5-e0-6337~49~ubuntu16.04.1)
  (general
    (links 36)
    (no_connects 0)
    (area 159.274999 50.82 186.925001 127.682001)
    (thickness 1.6)
    (drawings 4)
    (tracks 137)
    (zones 0)
    (modules 12)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (user_trace_width 3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 133.35 79.375)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory OUTPUT_GERBER/))
  )
  (net 0 "")
  (net 1 /GND)
  (net 2 /3V3)
  (net 3 "Net-(R1-Pad1)")
  (net 4 /CS)
  (net 5 /MOSI)
  (net 6 /MISO)
  (net 7 /SCK)
  (net 8 /RESET)
  (net 9 /IRQ)
  (net 10 /VIN)
  (net 11 /T+)
  (net 12 /T-)
  (net 13 /T_IN)
  (net 14 "Net-(P3-Pad2)")
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3V3)
    (add_net /CS)
    (add_net /GND)
    (add_net /IRQ)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /SCK)
    (add_net /T+)
    (add_net /T-)
    (add_net /T_IN)
    (add_net /VIN)
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(R1-Pad1)")
  )
  (module Capacitors_THT:C_Radial_D10_L20_P5 (layer F.Cu) (tedit 5899BDD4)
    (at 164.85 77.375)
    (descr "Radial Electrolytic Capacitor Diameter 10mm x Length 20mm, Pitch 5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at -0.004 -1.937) (layer F.SilkS))
    (fp_text value 2200u (at 0.885 1.619) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /VIN))
    (pad 2 thru_hole circle (at 5 0) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L20_P5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 5899BDCA)
    (at 176.85 76.875)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -0.066 0.087) (layer F.SilkS))
    (fp_text value 1u (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model Capacitors_SMD.3dshapes/C_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 172.85 93.875)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 0 -6.05) (layer F.SilkS))
    (fp_text value ATMEGA328-A (at 0 6.05) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 4 smd rect (at -4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 5 smd rect (at -4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 6 smd rect (at -4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 7 smd rect (at -4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 0.4 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 1.2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 /CS))
    (pad 15 smd rect (at 2 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 /MOSI))
    (pad 16 smd rect (at 2.8 4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 /MISO))
    (pad 17 smd rect (at 4.25 2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCK))
    (pad 18 smd rect (at 4.25 2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 4.25 1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 4.25 0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 4.25 -0.4) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 22 smd rect (at 4.25 -1.2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 4.25 -2) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 4.25 -2.8) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 26 smd rect (at 2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at -0.4 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 /RESET))
    (pad 30 smd rect (at -1.2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 /T_IN))
    (pad 31 smd rect (at -2 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 32 smd rect (at -2.8 -4.25 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 /IRQ))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:bornier2 (layer F.Cu) (tedit 5899BDC1)
    (at 171.85 56.875 180)
    (descr "Bornier d'alimentation 2 pins")
    (tags DEV)
    (fp_text reference P1 (at 0.019 -2.688 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 5.08 180) (layer F.Fab))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 12 /T-))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.54 2.54) (drill 1.524) (layers *.Cu *.Mask)
      (net 11 /T+))
    (model Connect.3dshapes/bornier2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5862ED53)
    (at 177.35 102.875 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference P2 (at 1.27 -2.39 270) (layer F.SilkS))
    (fp_text value ICSP (at 1.27 7.47 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /MISO))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /3V3))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /SCK))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5899BDBD)
    (at 174.85 62.375 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at -0.156 0.145 180) (layer F.SilkS))
    (fp_text value 1k2 (at -3.458 -0.109 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 11 /T+))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 5899BDD7)
    (at 167.85 85.875)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at -0.083 0.104) (layer F.SilkS))
    (fp_text value 4k7 (at 0.044 1.882) (layer F.Fab))
    (pad 1 smd rect (at -2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 13 /T_IN))
    (model Resistors_SMD.3dshapes/R_1206_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-4_W7.62mm_SMD (layer F.Cu) (tedit 5899BDB6)
    (at 175.35 69.375 270)
    (descr "4-lead dip package, row spacing 7.62 mm (300 mils), SMD")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil SMD")
    (attr smd)
    (fp_text reference U1 (at 0 -3.66 270) (layer F.SilkS))
    (fp_text value SFH620 (at -0.033 -0.164 270) (layer F.Fab))
    (pad 1 smd rect (at -3.81 -1.27 270) (size 2 1.78) (layers F.Cu F.Mask)
      (net 3 "Net-(R1-Pad1)"))
    (pad 3 smd rect (at 3.81 1.27 270) (size 2 1.78) (layers F.Cu F.Mask)
      (net 1 /GND))
    (pad 2 smd rect (at -3.81 1.27 270) (size 2 1.78) (layers F.Cu F.Mask)
      (net 12 /T-))
    (pad 4 smd rect (at 3.81 -1.27 270) (size 2 1.78) (layers F.Cu F.Mask)
      (net 13 /T_IN))
    (model Housings_DIP.3dshapes/DIP-4_W7.62mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 5899BDD0)
    (at 176.35 82.875 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U3 (at 0.183 0.074 360) (layer F.SilkS))
    (fp_text value AMS1117 (at 0 4.5 270) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 270) (size 2 3.8) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -3.15 0 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 3 smd rect (at -3.15 2.3 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /VIN))
    (pad 1 smd rect (at -3.15 -2.3 270) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mysensors_Radio:RFM69HW_SMD_Handsoldering (layer F.Cu) (tedit 558806AF)
    (at 164.85 108.875)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U4 (at 0.254 -1.778) (layer F.SilkS))
    (fp_text value RFM69HW (at 8.382 7.112) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.4 2) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 /IRQ))
    (pad 3 smd rect (at -1.4 4) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -1.4 6) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -1.4 8) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -1.4 10) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -1.4 12) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -1.4 14) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 /3V3))
    (pad 9 smd rect (at 18.3 14) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 10 smd rect (at 18.3 12) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P3-Pad2)"))
    (pad 11 smd rect (at 18.3 10) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 12 smd rect (at 18.3 8) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCK))
    (pad 13 smd rect (at 18.3 6) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /MISO))
    (pad 14 smd rect (at 18.3 4) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 /MOSI))
    (pad 15 smd rect (at 18.3 2) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /CS))
    (pad 16 smd rect (at 18.3 0) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/rfm69hw.wrl
      (at (xyz 0.332 -0.275 0.03))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0.332 -0.08 0.06))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.204 -0.445 0.06))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MyLibrary:TO-269AA (layer F.Cu) (tedit 5899BF68)
    (at 168.021 65.786 180)
    (fp_text reference D1 (at 0.09398 4.83616 180) (layer F.SilkS))
    (fp_text value MB6S (at 0.23622 -4.63296 180) (layer F.Fab))
    (pad 1 smd rect (at -1.28524 3.24104 180) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 11 /T+))
    (pad 2 smd rect (at 1.3843 3.24104 180) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 12 /T-))
    (pad 4 smd rect (at -1.28524 -3.36042 180) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 1 /GND))
    (pad 3 smd rect (at 1.3843 -3.36042 180) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 10 /VIN))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5862ED52)
    (at 176.784 125.857 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P3 (at 0 -2.39 90) (layer F.SilkS))
    (fp_text value ANT (at 0 4.93 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(P3-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 159.35 127.375) (end 159.35 52.875) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.85 127.375) (end 159.35 127.375) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.85 52.875) (end 186.85 127.375) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 159.35 52.875) (end 186.85 52.875) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.85 127.375) (xy 159.35 127.375) (xy 159.35 52.875) (xy 186.85 52.875)
      )
    )
  )
)
