(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~52~ubuntu16.10.1)
  (general
    (links 71)
    (no_connects 0)
    (area 186.424999 57.024999 213.575001 100.075001)
    (thickness 1.6)
    (drawings 20)
    (tracks 480)
    (zones 0)
    (modules 26)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user hide)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.16)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.5)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.35 1.35)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 145 100)
    (grid_origin 145 100)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x030f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber))
  )
  (net 0 "")
  (net 1 /VCC)
  (net 2 /D10)
  (net 3 /MOSI)
  (net 4 /MISO)
  (net 5 /SCK)
  (net 6 /RESET)
  (net 7 /D2)
  (net 8 /ANT)
  (net 9 /D3)
  (net 10 /D4)
  (net 11 /D5)
  (net 12 /D6)
  (net 13 /D7)
  (net 14 /A3)
  (net 15 GND)
  (net 16 "Net-(D1-Pad4)")
  (net 17 "Net-(D1-Pad5)")
  (net 18 "Net-(D1-Pad6)")
  (net 19 /A0)
  (net 20 /A1)
  (net 21 /A2)
  (net 22 /TXO)
  (net 23 "Net-(BT1-Pad1)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.16)
    (trace_width 0.25)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A2)
    (add_net /A3)
    (add_net /D10)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /SCK)
    (add_net /TXO)
    (add_net /VCC)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(D1-Pad4)")
    (add_net "Net-(D1-Pad5)")
    (add_net "Net-(D1-Pad6)")
  )
  (net_class Antenna ""
    (clearance 0.2)
    (trace_width 0.85)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ANT)
  )
  (module parts:CR2032Holder (layer B.Cu) (tedit 59298EB2)
    (at 200 90)
    (fp_text reference BT1 (at -9 -9) (layer B.SilkS))
    (fp_text value Battery (at -6 9) (layer B.Fab))
    (pad 1 smd rect (at -11.45 0) (size 2.3 5.08) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(BT1-Pad1)"))
    (pad 1 smd rect (at 11.45 0) (size 2.3 5.08) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at 0 0) (size 5.08 5.08) (layers B.Cu B.Paste B.Mask)
      (net 15 GND))
  )
  (module parts:868MHz_Spring_Antenna (layer F.Cu) (tedit 5904583C)
    (at 211.2 60)
    (fp_text reference P1 (at 0 6.35) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 -7.62) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 /ANT))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 198.3 89.45 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value R (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D1-Pad6)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /A2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 200 89.4 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value R (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D1-Pad5)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 /A1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 201.71 89.45 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value R (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D1-Pad4)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 /A0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun-LED:LED-TRICOLOR-5050 (layer F.Cu) (tedit 200000)
    (at 200 94.4 90)
    (descr "5050 SMD RGB LED")
    (tags "5050 SMD RGB LED")
    (attr smd)
    (fp_text reference D1 (at -0.635 -3.175 90) (layer B.SilkS))
    (fp_text value LED_RGB (at -0.254 3.175 90) (layer B.SilkS))
    (pad 1 smd oval (at -2.39776 -1.69926 90) (size 1.99898 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 15 GND))
    (pad 2 smd oval (at -2.39776 0 90) (size 1.99898 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 15 GND))
    (pad 3 smd oval (at -2.39776 1.69926 90) (size 1.99898 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 15 GND))
    (pad 4 smd oval (at 2.39776 1.69926 90) (size 1.99898 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D1-Pad4)"))
    (pad 5 smd oval (at 2.39776 0 90) (size 1.99898 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D1-Pad5)"))
    (pad 6 smd oval (at 2.39776 -1.69926 90) (size 1.99898 1.09982) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D1-Pad6)"))
  )
  (module parts:4mm_Rubber_Button (layer F.Cu) (tedit 58FA554E)
    (at 200 68.1)
    (fp_text reference SW1 (at 0 3.81) (layer F.SilkS))
    (fp_text value SW_SPST (at 0 -3.81) (layer F.Fab))
    (pad 1 smd rect (at -1.9 0) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /D5))
    (pad 2 smd rect (at 1.9 0) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 GND))
  )
  (module parts:4mm_Rubber_Button (layer F.Cu) (tedit 58FA554E)
    (at 192.2 76.2)
    (fp_text reference SW2 (at 0 3.81) (layer F.SilkS))
    (fp_text value SW_SPST (at 0 -3.81) (layer F.Fab))
    (pad 1 smd rect (at -1.9 0) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /D4))
    (pad 2 smd rect (at 1.9 0) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 GND))
  )
  (module parts:4mm_Rubber_Button (layer F.Cu) (tedit 58FA554E)
    (at 207.8 76)
    (fp_text reference SW4 (at 0 3.81) (layer F.SilkS))
    (fp_text value SW_SPST (at 0 -3.81) (layer F.Fab))
    (pad 1 smd rect (at -1.9 0) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 /D7))
    (pad 2 smd rect (at 1.9 0) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 GND))
  )
  (module parts:4mm_Rubber_Button (layer F.Cu) (tedit 58FA554E)
    (at 200 83.7)
    (fp_text reference SW5 (at 0 3.81) (layer F.SilkS))
    (fp_text value SW_SPST (at 0 -3.81) (layer F.Fab))
    (pad 1 smd rect (at -1.9 0) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /D3))
    (pad 2 smd rect (at 1.9 0) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 GND))
  )
  (module parts:4mm_Rubber_Button (layer F.Cu) (tedit 58FA554E)
    (at 199.95 76.03)
    (fp_text reference SW3 (at 0 3.81) (layer F.SilkS))
    (fp_text value SW_SPST (at 0 -3.81) (layer F.Fab))
    (pad 1 smd rect (at -1.9 0) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 /D6))
    (pad 2 smd rect (at 1.9 0) (size 0.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 15 GND))
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Reflow (layer B.Cu) (tedit 57B6E980)
    (at 209.5 81)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C3 (at 0 2.55) (layer B.SilkS))
    (fp_text value CP (at 0 -2.55) (layer B.Fab))
    (pad 1 smd rect (at -1.375 0) (size 1.95 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 /VCC))
    (pad 2 smd rect (at 1.375 0) (size 1.95 1.5) (layers B.Cu B.Paste B.Mask)
      (net 15 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58AA844E)
    (at 191.1 72.775)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 1.5) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.5) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 15 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 /VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58AA844E)
    (at 191.25 81.4)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 0 1.5) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.5) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 15 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 /VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer B.Cu) (tedit 58CD4EC5)
    (at 190.54 58.66 180)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference P2 (at 1.27 2.33 180) (layer B.SilkS))
    (fp_text value CONN_02X03 (at 1.27 -7.41 180) (layer B.Fab))
    (fp_text user %R (at 1.27 2.33 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /MISO))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /VCC))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /SCK))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /MOSI))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /RESET))
    (pad 6 thru_hole oval (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E)
    (at 191.6 69)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U1 (at 0 2.5) (layer B.SilkS))
    (fp_text value ATSHA204A (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 14 /A3))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 /VCC))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 15 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58AA844E)
    (at 208.9 62.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 0 1.5 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 1.5 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 15 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 /VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 58AA844E)
    (at 188.4 66.8)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.5) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 1.5) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 15 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 /VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 188.4 68.4 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 1.45 180) (layer B.SilkS))
    (fp_text value 1K (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 /VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 14 /A3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-32-1EP_5x5mm_Pitch0.5mm (layer B.Cu) (tedit 54130A77)
    (at 190.6 76.8 270)
    (descr "UH Package; 32-Lead Plastic QFN (5mm x 5mm); (see Linear Technology QFN_32_05-08-1693.pdf)")
    (tags "QFN 0.5")
    (attr smd)
    (fp_text reference U3 (at 0 3.75 270) (layer B.SilkS))
    (fp_text value ATMEGA328P-MU (at 0 -3.75 270) (layer B.Fab))
    (pad 1 smd rect (at -2.4 1.75 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 9 /D3))
    (pad 2 smd rect (at -2.4 1.25 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 10 /D4))
    (pad 3 smd rect (at -2.4 0.75 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 15 GND))
    (pad 4 smd rect (at -2.4 0.25 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 /VCC))
    (pad 5 smd rect (at -2.4 -0.25 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 15 GND))
    (pad 6 smd rect (at -2.4 -0.75 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 /VCC))
    (pad 7 smd rect (at -2.4 -1.25 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at -2.4 -1.75 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at -1.75 -2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 11 /D5))
    (pad 10 smd rect (at -1.25 -2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 12 /D6))
    (pad 11 smd rect (at -0.75 -2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 13 /D7))
    (pad 12 smd rect (at -0.25 -2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd rect (at 0.25 -2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 14 smd rect (at 0.75 -2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 2 /D10))
    (pad 15 smd rect (at 1.25 -2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 3 /MOSI))
    (pad 16 smd rect (at 1.75 -2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 4 /MISO))
    (pad 17 smd rect (at 2.4 -1.75 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 5 /SCK))
    (pad 18 smd rect (at 2.4 -1.25 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 /VCC))
    (pad 19 smd rect (at 2.4 -0.75 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd rect (at 2.4 -0.25 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 1 /VCC))
    (pad 21 smd rect (at 2.4 0.25 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 15 GND))
    (pad 22 smd rect (at 2.4 0.75 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 23 smd rect (at 2.4 1.25 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 19 /A0))
    (pad 24 smd rect (at 2.4 1.75 270) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 20 /A1))
    (pad 25 smd rect (at 1.75 2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 21 /A2))
    (pad 26 smd rect (at 1.25 2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 14 /A3))
    (pad 27 smd rect (at 0.75 2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 28 smd rect (at 0.25 2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 29 smd rect (at -0.25 2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 6 /RESET))
    (pad 30 smd rect (at -0.75 2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask))
    (pad 31 smd rect (at -1.25 2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 22 /TXO))
    (pad 32 smd rect (at -1.75 2.4 180) (size 0.7 0.25) (layers B.Cu B.Paste B.Mask)
      (net 7 /D2))
    (pad 33 smd rect (at 0.8625 -0.8625 270) (size 1.725 1.725) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at 0.8625 0.8625 270) (size 1.725 1.725) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 -0.8625 270) (size 1.725 1.725) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 33 smd rect (at -0.8625 0.8625 270) (size 1.725 1.725) (layers B.Cu B.Paste B.Mask)
      (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/QFN-32-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SparkFun-RF:RFM69HCW-XXXS2 (layer B.Cu) (tedit 200000)
    (at 204.3 71.65)
    (attr smd)
    (fp_text reference U2 (at -5.82422 9.63422) (layer F.SilkS))
    (fp_text value RFM69HCW (at 12.80922 9.63422) (layer F.SilkS))
    (fp_text user 1 (at -4.84886 6.985) (layer F.SilkS))
    (pad 1 smd rect (at -7.49808 6.9977) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 15 GND))
    (pad 2 smd rect (at -7.49808 4.99872) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 4 /MISO))
    (pad 3 smd rect (at -7.49808 2.99974) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 3 /MOSI))
    (pad 4 smd rect (at -7.49808 0.99822) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 5 /SCK))
    (pad 5 smd rect (at -7.49808 -0.99822) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 2 /D10))
    (pad 6 smd rect (at -7.49808 -2.99974) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -7.49808 -4.99872) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at -7.49808 -6.9977) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 15 GND))
    (pad 9 smd rect (at 7.49808 -6.9977) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 8 /ANT))
    (pad 10 smd rect (at 7.49808 -4.99872) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 15 GND))
    (pad 11 smd rect (at 7.49808 -2.99974) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at 7.49808 -0.99822) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd rect (at 7.49808 0.99822) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 1 /VCC))
    (pad 14 smd rect (at 7.49808 2.99974) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask)
      (net 7 /D2))
    (pad 15 smd rect (at 7.49808 4.99872) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask))
    (pad 16 smd rect (at 7.49808 6.9977) (size 2.99974 1.19888) (layers B.Cu B.Paste B.Mask))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 193.95 90.3 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value C (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 /VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 195.4 98.5 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value C (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 GND))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(BT1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-89-3 (layer F.Cu) (tedit 591F0203)
    (at 193.9 93.8 270)
    (descr SOT-89-3)
    (tags SOT-89-3)
    (attr smd)
    (fp_text reference U4 (at 0.45 -3.2 270) (layer F.SilkS))
    (fp_text value HT7333 (at 0.45 3.25 270) (layer F.Fab))
    (fp_text user %R (at 0.38 0 270) (layer F.Fab))
    (pad 2 smd trapezoid (at 2.667 0 180) (size 1.6 0.85) (rect_delta 0 0.6 ) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(BT1-Pad1)"))
    (pad 1 smd rect (at -1.48 -1.5 180) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 15 GND))
    (pad 2 smd rect (at -1.3335 0 180) (size 1 1.8) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(BT1-Pad1)"))
    (pad 3 smd rect (at -1.48 1.5 180) (size 1 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 /VCC))
    (pad 2 smd rect (at 1.3335 0 180) (size 2.2 1.84) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(BT1-Pad1)"))
    (pad 2 smd trapezoid (at -0.0762 0) (size 1.5 1) (rect_delta 0 0.7 ) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(BT1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-89-3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.00mm (layer F.Cu) (tedit 592A8B48)
    (at 188.55 85.45 90)
    (descr "Through hole straight pin header, 1x02, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.00mm single row")
    (fp_text reference J1 (at 0 -2.06 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 4.06 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.06 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0 90) (size 1.35 1.35) (layers F.Cu F.Paste F.Mask)
      (net 22 /TXO))
    (pad 2 smd circle (at 0 2 90) (size 1.35 1.35) (layers F.Cu F.Paste F.Mask)
      (net 15 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 58E0A804)
    (at 194.1 69 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 1.45 90) (layer B.SilkS))
    (fp_text value R (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 -0.024999 90) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 /D10))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 /VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 193.15 100) (end 206.85 100) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.5 83.35) (end 213.5 93.35) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.5 57.1) (end 213.5 80.95) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 192.4 57.1) (end 192.4 63.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 192.4 57.1) (end 186.5 57.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 213.5 57.1) (end 206.5 57.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 192.4 63.2) (end 206.5 63.2) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 206.5 57.1) (end 206.5 63.2) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 186.5 82.15) (end 186.5 80.95) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 213.5 82.15) (end 213.5 83.35) (angle 180) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 206.85 100) (end 213.5 93.35) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 193.15 100) (end 186.5 93.35) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.5 83.35) (end 186.5 93.35) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.5 57.1) (end 186.5 80.95) (layer Edge.Cuts) (width 0.15))
  (zone (net 15) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.7 57.3) (xy 186.7 79.8) (xy 188.2 81.3) (xy 188.2 83.4) (xy 187.4 84.2)
        (xy 187.1 84.5) (xy 186.7 84.9) (xy 186.7 93.1) (xy 193.3 99.7) (xy 206.5 99.7)
        (xy 212.8 93.4) (xy 213.1 93.1) (xy 213.1 84.4) (xy 211.5 82.8) (xy 213.3 81)
        (xy 213.3 57.3) (xy 206.8 57.3) (xy 206.8 63.1) (xy 191.9 63.1) (xy 191.9 57.3)
      )
    )
  )
  (zone (net 15) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 186.7 57.394581) (xy 186.7 79.894581) (xy 188.2 81.394581) (xy 188.2 83.494581) (xy 187.4 84.294581)
        (xy 187.1 84.594581) (xy 186.7 84.994581) (xy 186.7 93.194581) (xy 193.3 99.794581) (xy 206.5 99.794581)
        (xy 212.8 93.494581) (xy 213.1 93.194581) (xy 213.1 84.494581) (xy 211.5 82.894581) (xy 213.3 81.094581)
        (xy 213.3 57.394581) (xy 206.8 57.394581) (xy 206.8 63.194581) (xy 191.9 63.194581) (xy 191.9 57.394581)
      )
    )
  )
  (zone (net 15) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 210.4 57.6) (xy 213.2 57.6) (xy 213.2 64) (xy 210.4 64)
      )
    )
  )
)
