(kicad_pcb (version 20170123) (host pcbnew no-vcs-found-6cefb68~58~ubuntu16.04.1)
  (general
    (links 114)
    (no_connects 0)
    (area 119.6 70 165.400001 113.934921)
    (thickness 1.6)
    (drawings 35)
    (tracks 563)
    (zones 0)
    (modules 52)
    (nets 34)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.3)
    (trace_clearance 0.3)
    (zone_clearance 0.38)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.4 0.4)
    (mod_text_width 0.1)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 "Net-(C4-Pad2)")
  (net 4 "Net-(C6-Pad1)")
  (net 5 "Net-(C7-Pad1)")
  (net 6 /RESET)
  (net 7 "Net-(C9-Pad2)")
  (net 8 "Net-(C9-Pad1)")
  (net 9 /12Vcc)
  (net 10 "Net-(C11-Pad1)")
  (net 11 "Net-(C12-Pad1)")
  (net 12 /MISO)
  (net 13 /SCK)
  (net 14 /MOSI)
  (net 15 "Net-(D3-Pad2)")
  (net 16 "Net-(D4-Pad1)")
  (net 17 "Net-(D5-Pad1)")
  (net 18 "Net-(D6-Pad2)")
  (net 19 /INT)
  (net 20 /TS2)
  (net 21 /S2_LEDs)
  (net 22 /TS1)
  (net 23 /S1_LEDs)
  (net 24 "Net-(P3-Pad1)")
  (net 25 "Net-(R1-Pad1)")
  (net 26 /Relay2_Reset)
  (net 27 /Relay1_Reset)
  (net 28 /Relay2_Set)
  (net 29 /Relay1_Set)
  (net 30 /ATSHA204A)
  (net 31 /RADIO_SS)
  (net 32 /FLASH_SS)
  (net 33 "Net-(C5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.3)
    (trace_width 0.3)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /12Vcc)
    (add_net /ATSHA204A)
    (add_net /FLASH_SS)
    (add_net /INT)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RADIO_SS)
    (add_net /RESET)
    (add_net /Relay1_Reset)
    (add_net /Relay1_Set)
    (add_net /Relay2_Reset)
    (add_net /Relay2_Set)
    (add_net /S1_LEDs)
    (add_net /S2_LEDs)
    (add_net /SCK)
    (add_net /TS1)
    (add_net /TS2)
    (add_net GND)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(R1-Pad1)")
  )
  (module myfootprints:Livolo_EU_SW_2_Channel_1Way_Frame_VL-C702X-2_Ver_C1 locked (layer B.Cu) (tedit 590C6ABA)
    (at 142.3 92 180)
    (fp_text reference REF** (at -0.3 -0.5 180) (layer B.SilkS) hide)
    (fp_text value Livolo_EU_SW_2Ways_Frame_VL-C702X-2_Ver_C1 (at 0 0.5 180) (layer B.Fab) hide)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59101D79)
    (at 150 111.6)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -1.1 1.3) (layer F.SilkS))
    (fp_text value 10u/25V (at 1.1 1.3) (layer F.SilkS))
    (fp_text user %R (at 0 -1.5) (layer F.Fab) hide)
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 9 /12Vcc))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:VLCF4020T-150MR68 (layer F.Cu) (tedit 590C5D79)
    (at 157.4 107.1)
    (fp_text reference L2 (at -0.9 3.2 -180) (layer F.SilkS))
    (fp_text value 15uH (at 0.5 3.2 -180) (layer F.SilkS))
    (pad 1 smd rect (at 0 -1.75) (size 4 2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0 1.5) (size 4 2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C9-Pad2)"))
    (model ${KISYS3DMOD}/Inductors.3dshapes/VLCF4020T-150MR68.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:SS14M (layer F.Cu) (tedit 58E37FED)
    (at 154.2 109.3 270)
    (fp_text reference D2 (at 2.6 0.2) (layer F.SilkS))
    (fp_text value SS14M (at 3.3 -0.3) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 270) (size 2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C9-Pad2)"))
    (pad 2 smd rect (at 1.5 0 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/DO_Packages_SMD.3dshapes/DO-219AB.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 586E4F31)
    (at 145.8 108.8 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.4 -0.6 90) (layer F.SilkS))
    (fp_text value 10K (at -2.6 0 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R1-Pad1)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58933BCC)
    (at 150 108.8 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U2 (at -2.6 1.1) (layer F.SilkS))
    (fp_text value MCP16301 (at -2 0.8 180) (layer F.SilkS))
    (pad 5 smd rect (at 1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 /12Vcc))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C9-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 9 /12Vcc))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/SOT_Packages_SMD.3dshapes/SOT23-6.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:AVR_ISP_SMT_Small_02x03 (layer F.Cu) (tedit 58C6B9BA)
    (at 128.05 79.9 90)
    (descr "SMT pin header")
    (tags "SMT pin header")
    (attr smd)
    (fp_text reference CON1 (at -0.45 -5.03 90) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at -0.43 -4.17 270) (layer F.SilkS))
    (pad 2 smd rect (at -2.54 -2 90) (size 1.27 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 4 smd rect (at 0 -2 90) (size 1.27 2.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /MOSI))
    (pad 6 smd rect (at 2.54 -2 90) (size 1.27 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.54 2 90) (size 1.27 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 /RESET))
    (pad 3 smd rect (at 0 2 90) (size 1.27 2.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /SCK))
    (pad 1 smd rect (at -2.5 2 90) (size 1.27 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /MISO))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_SMT_02x03.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-R_EIA-2012-12_Wave (layer F.Cu) (tedit 58C6B5AC)
    (at 143.05 101.092)
    (descr "Tantalum capacitor, Case R, EIA 2012-12, 2.0x1.3x1.2mm, Wave soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C5 (at -2.15 -1.892) (layer F.SilkS))
    (fp_text value 10u (at -2.05 -1.292) (layer F.SilkS))
    (pad 1 smd rect (at -1.275 0) (size 1.75 1.26) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C5-Pad1)"))
    (pad 2 smd rect (at 1.275 0) (size 1.75 1.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module myfootprints:touch_pad_16mm locked (layer F.Cu) (tedit 58C1C47E)
    (at 156.25 92.15)
    (fp_text reference P1 (at 0.025 0.9) (layer F.SilkS) hide)
    (fp_text value "Sense Pad 1" (at 0 -0.5) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 15.5 15.5) (layers B.Cu)
      (net 10 "Net-(C11-Pad1)"))
  )
  (module myfootprints:touch_pad_16mm locked (layer F.Cu) (tedit 58C1C466)
    (at 128.65 92.15)
    (fp_text reference P2 (at -0.075 0.85) (layer F.SilkS) hide)
    (fp_text value "Sense Pad 2" (at 0 -0.5) (layer F.SilkS))
    (pad 1 smd circle (at 0 0) (size 15.5 15.5) (layers B.Cu)
      (net 11 "Net-(C12-Pad1)"))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 587E330A)
    (at 159.766 83.312 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0.866 -1.238 180) (layer F.SilkS))
    (fp_text value 1K (at -0.762 -1.27 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 /ATSHA204A))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen locked (layer B.Cu) (tedit 0)
    (at 141.975 79.275 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58734590)
    (at 153.625 72.6)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at -1.425 -1 180) (layer F.SilkS))
    (fp_text value 100n (at 1.375 -1 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:hole_1.5mm locked (layer F.Cu) (tedit 587347E2)
    (at 152.1 100.85)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole_1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module myfootprints:hole_1.5mm locked (layer F.Cu) (tedit 587347E2)
    (at 160.3 100.85)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole_1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module myfootprints:hole_1.5mm locked (layer F.Cu) (tedit 587347E2)
    (at 132.7 100.9)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole_1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module myfootprints:hole_1.5mm locked (layer F.Cu) (tedit 587347E2)
    (at 124.5 100.9)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole_1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 586E53C5)
    (at 137.15 96.9)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at -1.75 -1.35 180) (layer F.SilkS))
    (fp_text value 100n (at -1.3 -0.65 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 586E5227)
    (at 137.35 87.5 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C2 (at 1.5 0.275 180) (layer F.SilkS))
    (fp_text value 100n (at 1.85 -0.4 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0402.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 586E5221)
    (at 147.5 87.5)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 1.525 -0.3) (layer F.SilkS))
    (fp_text value 100n (at 1.95 0.375) (layer F.SilkS))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0402.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 586E5461)
    (at 140.5 104 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -1.3 -1.1 90) (layer F.SilkS))
    (fp_text value 22u (at -0.1 -1.1 270) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 586E52D1)
    (at 146.1 103.7 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 1 0.85 270) (layer F.SilkS))
    (fp_text value 470p (at -1.15 0.9 270) (layer F.SilkS))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 586E52DF)
    (at 152.6 108.8 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 2.5 0.3 270) (layer F.SilkS))
    (fp_text value 100n (at 2.8 -0.4 90) (layer F.SilkS))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C9-Pad2)"))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C9-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 586E525C)
    (at 149.1 104.4 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 1.7 -1 180) (layer F.SilkS))
    (fp_text value 0-50pf* (at -0.3 -1 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 586E5261)
    (at 136 99.35 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at -1.25 -1 90) (layer F.SilkS))
    (fp_text value 0-50pf* (at 1.55 -1 90) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 586E5244)
    (at 149.2 99.1 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at -0.925 1.825 180) (layer F.SilkS))
    (fp_text value 100n (at -1.125 1.075 180) (layer F.SilkS))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 586E532E)
    (at 138.2 102 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 2.5 0.4) (layer F.SilkS))
    (fp_text value 100n (at 2.6 -0.4 180) (layer F.SilkS))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 586E52DA)
    (at 153.1 105.6)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at -0.7 -0.6 180) (layer F.SilkS))
    (fp_text value 1N4148 (at 0 0.7) (layer F.SilkS))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/SOD_Packages_SMD.3dshapes/SOD123.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Diodes_SMD:D_0603 (layer B.Cu) (tedit 586E517C)
    (at 130.5 102.15 180)
    (descr "Diode SMD in 0603 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D3 (at -0.9 1.05 180) (layer B.SilkS))
    (fp_text value Blue (at 0.6 1.05 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.85 0 180) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.85 0 180) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_Packages_SMD.3dshapes/led_chip_0603_blue.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer B.Cu) (tedit 586E517F)
    (at 126.85 102.15)
    (descr "Diode SMD in 0603 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D4 (at 0.9 -1.05) (layer B.SilkS))
    (fp_text value Red (at -0.6 -1.05) (layer B.SilkS))
    (pad 1 smd rect (at -0.85 0) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.85 0) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/LED_Packages_SMD.3dshapes/led_chip_0603_red.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer B.Cu) (tedit 586E5177)
    (at 157.95 102.15 180)
    (descr "Diode SMD in 0603 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D5 (at -0.85 1.05 180) (layer B.SilkS))
    (fp_text value Red (at 0.65 1.05 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.85 0 180) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 0.85 0 180) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/LED_Packages_SMD.3dshapes/led_chip_0603_red.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer B.Cu) (tedit 586E5173)
    (at 154.6 102.15)
    (descr "Diode SMD in 0603 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D6 (at 1 -1.05) (layer B.SilkS))
    (fp_text value Blue (at -0.6 -1.05) (layer B.SilkS))
    (pad 2 smd rect (at 0.85 0) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -0.85 0) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_Packages_SMD.3dshapes/led_chip_0603_blue.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 586E5114)
    (at 142.45 92.3 180)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 1.35 0.3) (layer F.SilkS))
    (fp_text value ATMEGA328P-AU (at -0.05 -0.5) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 32 smd rect (at -2.8 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 19 /INT))
    (pad 31 smd rect (at -2 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 /Relay2_Reset))
    (pad 30 smd rect (at -1.2 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 /Relay2_Set))
    (pad 29 smd rect (at -0.4 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 /RESET))
    (pad 28 smd rect (at 0.4 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 /Relay1_Reset))
    (pad 27 smd rect (at 1.2 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 29 /Relay1_Set))
    (pad 26 smd rect (at 2 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 /ATSHA204A))
    (pad 25 smd rect (at 2.8 -4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 4.25 -2.8 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 /TS2))
    (pad 23 smd rect (at 4.25 -2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 21 /S2_LEDs))
    (pad 22 smd rect (at 4.25 -1.2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 4.25 -0.4 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 20 smd rect (at 4.25 0.4 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C4-Pad2)"))
    (pad 19 smd rect (at 4.25 1.2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 4.25 2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 17 smd rect (at 4.25 2.8 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 /SCK))
    (pad 16 smd rect (at 2.8 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 12 /MISO))
    (pad 15 smd rect (at 2 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 /MOSI))
    (pad 14 smd rect (at 1.2 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 /RADIO_SS))
    (pad 13 smd rect (at 0.4 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -0.4 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 /FLASH_SS))
    (pad 11 smd rect (at -1.2 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -2 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at -2.8 4.25 270) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -4.25 2.8 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -4.25 2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -4.25 1.2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at -4.25 0.4 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -4.25 -0.4 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at -4.25 -1.2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -4.25 -2 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 23 /S1_LEDs))
    (pad 1 smd rect (at -4.25 -2.8 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 22 /TS1))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_single_0-8mmDrill (layer F.Cu) (tedit 586E520A)
    (at 131.55 72.55)
    (fp_text reference P3 (at -1.625 -0.15) (layer F.SilkS))
    (fp_text value ANTENNA (at 1.05 -1.35) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 0.8001) (layers *.Cu *.Mask)
      (net 24 "Net-(P3-Pad1)"))
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 586E4F9D)
    (at 147.4 108.8 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.3 -0.4 90) (layer F.SilkS))
    (fp_text value 31K6 (at -2.7 0.3 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 586E524A)
    (at 146.1 99.7 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1.7 -1.1 180) (layer F.SilkS))
    (fp_text value 10K (at 1.1 -1.2) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /RESET))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 586E5213)
    (at 132.5 82.3 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -2.35 0.075 180) (layer F.SilkS))
    (fp_text value 56K (at -3.125 0.05 180) (layer F.SilkS))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 /RADIO_SS))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58933CFE)
    (at 154.2 103.4 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0.9 1.2 180) (layer F.SilkS))
    (fp_text value 1K* (at -0.7 1.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /S1_LEDs))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58933CF9)
    (at 158.3 103.4 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 1.2 1.2) (layer F.SilkS))
    (fp_text value 1K* (at -0.1 1.2) (layer F.SilkS))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /S1_LEDs))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58933CDD)
    (at 130.7 103.4)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -0.7 -1.2) (layer F.SilkS))
    (fp_text value 1K* (at 0.7 -1.2) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /S2_LEDs))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58933CD7)
    (at 126.6 103.4)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -0.3 -1.2 -180) (layer F.SilkS))
    (fp_text value 1K* (at 1 -1.2 -180) (layer F.SilkS))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /S2_LEDs))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 586E52C3)
    (at 143.05 103.75 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U1 (at -2.15 -1.85 180) (layer F.SilkS))
    (fp_text value MIC5205-3.3 (at -2.15 0.85 180) (layer F.SilkS))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C5-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C6-Pad1)"))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C7-Pad1)"))
    (model ${KISYS3DMOD}/SOT_Packages_SMD.3dshapes/SOT23-5.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 586E52B6)
    (at 149.1 101.75 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U3 (at 0 -2.1 270) (layer F.SilkS))
    (fp_text value TTP223 (at -0.075 0) (layer F.SilkS))
    (pad 5 smd rect (at 1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 6 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 22 /TS1))
    (model ${KISYS3DMOD}/SOT_Packages_SMD.3dshapes/SOT23-6.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 586E540D)
    (at 138.6 99.45)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U4 (at -0.05 -2) (layer F.SilkS))
    (fp_text value TTP223 (at 0 0.025 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 20 /TS2))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C12-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 6 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/SOT_Packages_SMD.3dshapes/SOT23-6.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:RFM69CW (layer F.Cu) (tedit 586E5591)
    (at 142.45 78.55)
    (tags "RF12, RFM12B, RFM69CW")
    (fp_text reference U5 (at 1.15 -0.05) (layer F.SilkS))
    (fp_text value RFM69CW (at 1.15 1) (layer F.SilkS))
    (pad 1 smd rect (at -7.9502 -5.95122) (size 1.99898 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P3-Pad1)"))
    (pad 2 smd rect (at -7.97814 -3.9497) (size 1.99898 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at -7.97814 -1.95072) (size 1.99898 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -7.97814 0) (size 1.99898 1.39954) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -7.97814 1.95072) (size 1.99898 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 14 /MOSI))
    (pad 6 smd rect (at -7.97814 3.9497) (size 1.99898 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 13 /SCK))
    (pad 7 smd rect (at -7.97814 5.95122) (size 1.99898 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 31 /RADIO_SS))
    (pad 8 smd rect (at 7.92226 5.95122) (size 1.99898 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 12 /MISO))
    (pad 9 smd rect (at 7.92226 3.9497) (size 1.99898 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 19 /INT))
    (pad 10 smd rect (at 7.92226 1.95072) (size 1.99898 1.39954) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 7.92226 0) (size 1.99898 1.39954) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at 7.92226 -1.95072) (size 1.99898 1.39954) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 7.92226 -3.9497) (size 1.99898 1.39954) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 7.92226 -5.95122) (size 1.99898 1.39954) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Radio_Modules.3dshapes/RFM69CW.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58734586)
    (at 162.2 82 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 2.95 0.45 270) (layer F.SilkS))
    (fp_text value 100n (at 2.7 -0.3 270) (layer F.SilkS))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 5873458D)
    (at 154.3 81.7 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0.475 -1.375 180) (layer F.SilkS))
    (fp_text value 56K (at -1.05 -1.375 180) (layer F.SilkS))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 /FLASH_SS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 5911806B)
    (at 154.305 77.1 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U6 (at -1.1 6.375 270) (layer F.SilkS))
    (fp_text value AT25DF512C (at 0.1 3.695 270) (layer F.SilkS))
    (pad 8 smd rect (at 2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 7 smd rect (at 2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 6 smd rect (at 2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 /SCK))
    (pad 5 smd rect (at 2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /MOSI))
    (pad 4 smd rect (at -2.7 1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -2.7 0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at -2.7 -0.635 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /MISO))
    (pad 1 smd rect (at -2.7 -1.905 90) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /FLASH_SS))
    (model Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 58734582)
    (at 159.9 79.85 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U7 (at 2.85 -2.5 270) (layer F.SilkS))
    (fp_text value ATSHA204A (at 1.45 2.2 270) (layer F.SilkS))
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 30 /ATSHA204A))
    (model ${KISYS3DMOD}/SOT_Packages_SMD.3dshapes/SOT23-3.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58C1C6FD)
    (at 142.95 99.3 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at 0.266 1.27 180) (layer F.SilkS))
    (fp_text value BLM18HE152SN1D (at 0 1.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(C5-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-R_EIA-2012-12_Wave (layer F.Cu) (tedit 58C6B578)
    (at 132.4 76 270)
    (descr "Tantalum capacitor, Case R, EIA 2012-12, 2.0x1.3x1.2mm, Wave soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C15 (at -1.5 1.8) (layer F.SilkS))
    (fp_text value 10u (at -0.8 1.8) (layer F.SilkS))
    (pad 2 smd rect (at 1.275 0 270) (size 1.75 1.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.275 0 270) (size 1.75 1.26) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x07_Pitch2.00mm locked (layer F.Cu) (tedit 590C33F6)
    (at 131.65 109.55 90)
    (descr "Through hole straight pin header, 2x07, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x07 2.00mm double row")
    (fp_text reference P4 (at -2.2 2.5 180) (layer F.SilkS))
    (fp_text value "Power Board" (at -2.2 7.8 180) (layer F.SilkS))
    (fp_text user %R (at 1 -2.06 90) (layer F.Fab) hide)
    (pad 14 thru_hole oval (at 2 12 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 13 thru_hole oval (at 0 12 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 12 thru_hole oval (at 2 10 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 11 thru_hole oval (at 0 10 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 9 thru_hole oval (at 0 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 8 thru_hole oval (at 2 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 7 thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad 6 thru_hole oval (at 2 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /Relay1_Reset))
    (pad 5 thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /Relay2_Set))
    (pad 4 thru_hole oval (at 2 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 /Relay1_Set))
    (pad 3 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 /Relay2_Reset))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /12Vcc))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Female/female_header_2row_14pins_2mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text +3V (at 143.6 111.1) (layer B.SilkS))
  (gr_line (start 158.90064 111.60234) (end 162.91 107.59) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 157.89988 74.60216) (end 159.89886 76.60114) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.89842 111.60234) (end 128.9007 113.60132) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.89936 105.60032) (end 163.89936 78.60012) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.89918 74.60216) (end 125.40058 73.10102) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.9 70.2) (end 159.39848 73.10102) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.91 107.59) (end 163.89936 105.60032) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.8997 105.60032) (end 120.8997 78.60012) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 123.39906 75.1) (end 124.9002 76.60114) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 124.9002 76.60114) (end 126.89918 74.60216) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.40058 73.10102) (end 128.9 70.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.9 70.2) (end 155.89766 70.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 159.89886 76.60114) (end 161.4 75.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.94 108.61) (end 125.89842 111.60234) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.89836 113.60132) (end 158.90064 111.60234) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.9007 113.60132) (end 155.89836 113.60132) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.8997 105.60032) (end 122.94 108.61) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 159.39848 73.10102) (end 157.89988 74.60216) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.8997 78.60012) (end 123.39906 75.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161.4 75.1) (end 163.89936 78.60012) (layer Edge.Cuts) (width 0.1))
  (gr_text REL1_SET (at 134.8 105.1 45) (layer B.SilkS))
  (gr_text REL1_RST (at 137.2 105.1 45) (layer B.SilkS))
  (gr_text REL2_RST (at 136.7 111.7 135) (layer B.SilkS))
  (gr_text REL2_SET (at 134.4 111.8 135) (layer B.SilkS))
  (gr_text "Rev. 0.1" (at 125.6 106.3) (layer F.SilkS))
  (gr_text RES (at 130.1 78.5) (layer F.SilkS))
  (gr_text SCK (at 130.1 81.2) (layer F.SilkS))
  (gr_text MISO (at 130.125 84.35) (layer F.SilkS))
  (gr_text GND (at 125.9 78.5) (layer F.SilkS))
  (gr_text MOSI (at 125.9 81.2) (layer F.SilkS))
  (gr_text 3V3 (at 125.975 84.375) (layer F.SilkS))
  (gr_text GND (at 141.65 111.1) (layer B.SilkS))
  (gr_text +12V (at 131.55 105.85) (layer B.SilkS))
  (gr_text "Mysensors RFM69CW Livolo Node" (at 142.4 74.4) (layer B.SilkS))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 147.5 104.2) (xy 159.4 104.2) (xy 159.4 109.8) (xy 147.5 109.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.8 83.1) (xy 134 83.1) (xy 138.1 87.2) (xy 138.1 96.5) (xy 135 101.4)
        (xy 122.5 101.4) (xy 119.6 96.5) (xy 119.6 86.6)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.38))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.38) (thermal_bridge_width 0.38) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 120.8 70) (xy 163.9 70) (xy 163.9 113.7) (xy 120.8 113.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150.1 83.218218) (xy 161.3 83.218218) (xy 165.4 87.318218) (xy 165.4 96.618218) (xy 162.3 101.518218)
        (xy 149.8 101.518218) (xy 146.9 96.618218) (xy 146.9 86.718218)
      )
    )
  )
)
