(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 56)
    (no_connects 0)
    (area 133.653572 30.17 257 118.700001)
    (thickness 1.6)
    (drawings 32)
    (tracks 300)
    (zones 0)
    (modules 25)
    (nets 58)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x020f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 "Net-(U1-Pad3)")
  (net 2 "Net-(U1-Pad4)")
  (net 3 "Net-(U1-Pad5)")
  (net 4 "Net-(U1-Pad6)")
  (net 5 "Net-(U1-Pad7)")
  (net 6 "Net-(U1-Pad9)")
  (net 7 "Net-(U1-Pad10)")
  (net 8 "Net-(U1-Pad11)")
  (net 9 "Net-(U1-Pad13)")
  (net 10 "Net-(U1-Pad15)")
  (net 11 "Net-(U1-Pad16)")
  (net 12 "Net-(U1-Pad17)")
  (net 13 "Net-(U1-Pad18)")
  (net 14 GND)
  (net 15 "Net-(U1-Pad21)")
  (net 16 "Net-(U1-Pad26)")
  (net 17 SCK)
  (net 18 +5V)
  (net 19 433RX)
  (net 20 ErrLed)
  (net 21 TXled)
  (net 22 RXled)
  (net 23 433TX)
  (net 24 CE)
  (net 25 CSN)
  (net 26 MOSI)
  (net 27 MISO)
  (net 28 +3V3)
  (net 29 "Net-(U2-Pad8)")
  (net 30 "Net-(P1-Pad2)")
  (net 31 "Net-(P1-Pad3)")
  (net 32 "Net-(P1-Pad4)")
  (net 33 "Net-(U5-Pad3)")
  (net 34 "Net-(D1-Pad1)")
  (net 35 "Net-(D2-Pad1)")
  (net 36 "Net-(D3-Pad1)")
  (net 37 "Net-(JP1-Pad1)")
  (net 38 SDA)
  (net 39 "Net-(JP2-Pad1)")
  (net 40 "Net-(U7-Pad1)")
  (net 41 "Net-(U7-Pad2)")
  (net 42 "Net-(U7-Pad3)")
  (net 43 "Net-(U7-Pad4)")
  (net 44 "Net-(U7-Pad5)")
  (net 45 "Net-(U7-Pad6)")
  (net 46 "Net-(U7-Pad7)")
  (net 47 "Net-(U7-Pad8)")
  (net 48 "Net-(U7-Pad9)")
  (net 49 "Net-(U7-Pad10)")
  (net 50 "Net-(U7-Pad11)")
  (net 51 "Net-(U7-Pad12)")
  (net 52 "Net-(U7-Pad13)")
  (net 53 "Net-(U7-Pad18)")
  (net 54 "Net-(U7-Pad19)")
  (net 55 "Net-(U7-Pad25)")
  (net 56 "Net-(U7-Pad26)")
  (net 57 "Net-(U7-Pad24)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net 433RX)
    (add_net 433TX)
    (add_net CE)
    (add_net CSN)
    (add_net ErrLed)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(JP1-Pad1)")
    (add_net "Net-(JP2-Pad1)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P1-Pad4)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad8)")
    (add_net "Net-(U5-Pad3)")
    (add_net "Net-(U7-Pad1)")
    (add_net "Net-(U7-Pad10)")
    (add_net "Net-(U7-Pad11)")
    (add_net "Net-(U7-Pad12)")
    (add_net "Net-(U7-Pad13)")
    (add_net "Net-(U7-Pad18)")
    (add_net "Net-(U7-Pad19)")
    (add_net "Net-(U7-Pad2)")
    (add_net "Net-(U7-Pad24)")
    (add_net "Net-(U7-Pad25)")
    (add_net "Net-(U7-Pad26)")
    (add_net "Net-(U7-Pad3)")
    (add_net "Net-(U7-Pad4)")
    (add_net "Net-(U7-Pad5)")
    (add_net "Net-(U7-Pad6)")
    (add_net "Net-(U7-Pad7)")
    (add_net "Net-(U7-Pad8)")
    (add_net "Net-(U7-Pad9)")
    (add_net RXled)
    (add_net SCK)
    (add_net SDA)
    (add_net TXled)
  )
  (module mysensors_radios:NRF24L01 (layer F.Cu) (tedit 58FBD1F7)
    (at 180.34 77.47 270)
    (descr NRF24L01)
    (tags "nRF 24 NRF24L01 NRF24L01+")
    (fp_text reference U2 (at -1.016 -1.016 270) (layer F.SilkS) hide)
    (fp_text value NRF24L01 (at -11.938 2.794 360) (layer F.SilkS))
    (pad 7 thru_hole oval (at -9.144 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 MISO))
    (pad 8 thru_hole oval (at -9.144 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U2-Pad8)"))
    (pad 5 thru_hole oval (at -6.604 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 SCK))
    (pad 6 thru_hole oval (at -6.604 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 MOSI))
    (pad 3 thru_hole oval (at -4.064 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 CE))
    (pad 4 thru_hole oval (at -4.064 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 CSN))
    (pad 1 thru_hole rect (at -1.524 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (pad 2 thru_hole oval (at -1.524 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0.442))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/nrf24l01.wrl
      (at (xyz -0.3 -0.5669999999999999 0.475))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz -0.22 -0.51 0.509))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_hc-49s.wrl
      (at (xyz -0.5 -0.475 0.51))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module arduino:arduino_mini (layer F.Cu) (tedit 58FBD423)
    (at 211.836 76.2 180)
    (descr "30 pins DIL package, elliptical pads, width 600mil (arduino mini)")
    (tags "DIL arduino mini")
    (fp_text reference U1 (at -13.97 -3.81 180) (layer F.SilkS) hide)
    (fp_text value "Arduino Nano" (at -0.381 2.921 180) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -19.05 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 SCK))
    (pad 2 thru_hole oval (at -16.51 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(JP1-Pad1)"))
    (pad 3 thru_hole oval (at -13.97 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(U1-Pad3)"))
    (pad 4 thru_hole oval (at -11.43 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(U1-Pad4)"))
    (pad 5 thru_hole oval (at -8.89 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(U1-Pad5)"))
    (pad 6 thru_hole oval (at -6.35 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(U1-Pad6)"))
    (pad 7 thru_hole oval (at -3.81 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(U1-Pad7)"))
    (pad 8 thru_hole oval (at -1.27 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 SDA))
    (pad 9 thru_hole oval (at 1.27 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(U1-Pad9)"))
    (pad 10 thru_hole oval (at 3.81 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(U1-Pad10)"))
    (pad 11 thru_hole oval (at 6.35 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(U1-Pad11)"))
    (pad 12 thru_hole oval (at 8.89 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 18 +5V))
    (pad 13 thru_hole oval (at 11.43 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(U1-Pad13)"))
    (pad 14 thru_hole oval (at 13.97 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (pad 15 thru_hole oval (at 16.51 7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(U1-Pad15)"))
    (pad 16 thru_hole oval (at 16.51 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(U1-Pad16)"))
    (pad 17 thru_hole oval (at 13.97 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(U1-Pad17)"))
    (pad 18 thru_hole oval (at 11.43 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(U1-Pad18)"))
    (pad 19 thru_hole oval (at 8.89 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (pad 20 thru_hole oval (at 6.35 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 19 433RX))
    (pad 21 thru_hole oval (at 3.81 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(U1-Pad21)"))
    (pad 22 thru_hole oval (at 1.27 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 20 ErrLed))
    (pad 23 thru_hole oval (at -1.27 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 21 TXled))
    (pad 24 thru_hole oval (at -3.81 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 22 RXled))
    (pad 25 thru_hole oval (at -6.35 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 23 433TX))
    (pad 26 thru_hole oval (at -8.89 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U1-Pad26)"))
    (pad 27 thru_hole oval (at -11.43 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 CE))
    (pad 28 thru_hole oval (at -13.97 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 25 CSN))
    (pad 29 thru_hole oval (at -16.51 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 26 MOSI))
    (pad 30 thru_hole oval (at -19.05 -7.62 180) (size 1.5748 2.286) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 27 MISO))
    (model arduino_nano.wrl
      (at (xyz -0.978 -0.385 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58F511C7)
    (at 177.546 80.264)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -1.27 -3.048) (layer F.SilkS) hide)
    (fp_text value 0.1uFC (at 0.254 2.032) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 28 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58F511CC)
    (at 177.546 83.82)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C2 (at -4.064 -2.286) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0 2) (layer F.SilkS))
    (fp_text user %R (at 4.064 1.524) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 28 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58FBD2CE)
    (at 177.546 87.376)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at -5.588 1.27) (layer F.SilkS) hide)
    (fp_text value 10uF (at 0 2.032) (layer F.SilkS))
    (fp_text user %R (at -5.334 -1.524) (layer F.Fab) hide)
    (pad 1 smd rect (at -2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 28 +3V3))
    (pad 2 smd rect (at 2 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58FD231C)
    (at 209.55 103.378 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at 0 -1.75 180) (layer F.SilkS) hide)
    (fp_text value 22uF (at 0.254 -2.286 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 28 +3V3))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 58F516CF)
    (at 223.012 91.694)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value MicroUSBBreakout (at 4.838 5.472 90) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(P1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(P1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(P1-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58FD230B)
    (at 193.04 105.41 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference U4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value 433Mhz_Sender (at 2.54 1.778 180) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 433TX))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58FD22FE)
    (at 154.94 105.41 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference U5 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value 433Mhz_Receiver (at 2.54 5.08 180) (layer F.SilkS))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 433RX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(U5-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 58F5120B)
    (at 144 59)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 58F51205)
    (at 231 59)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 58F51211)
    (at 144 106)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 58F51215)
    (at 231 106)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (fp_text reference REF** (at 0 -3.7) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.7mm_M2.5 (at 0 3.7) (layer F.Fab) hide)
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module mysensors_obscurities:2_pin_solder_jumper_smd (layer F.Cu) (tedit 58FBD118)
    (at 159.512 58.674 90)
    (fp_text reference JP1 (at -0.254 -3.556 180) (layer F.SilkS))
    (fp_text value JUMPER (at 0 -1.524 90) (layer F.Fab) hide)
    (pad 2 smd oval (at 0.889 0 90) (size 1.27 1.524) (layers F.Cu F.Paste F.Mask)
      (net 28 +3V3))
    (pad 1 smd oval (at -0.889 0 90) (size 1.27 1.524) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(JP1-Pad1)"))
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 153.67 99.06 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R1 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 270 (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 22 RXled))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 153.67 91.44 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R2 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 270 (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 21 TXled))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(D2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_1206_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 153.67 83.82 180)
    (descr "Resistor SMD 1206, hand soldering")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference R3 (at 0 -1.85 180) (layer F.SilkS))
    (fp_text value 270 (at 0 1.9 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 20 ErrLed))
    (pad 2 smd rect (at 2 0 180) (size 2 1.7) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58F51296)
    (at 143.51 99.06 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -3.96 90) (layer F.SilkS) hide)
    (fp_text value LEDRX (at 1.27 3.96 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 +5V))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58F51292)
    (at 143.51 91.44 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D2 (at 1.27 -3.96 90) (layer F.SilkS) hide)
    (fp_text value LEDTX (at 1.27 3.96 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 +5V))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 58F51287)
    (at 143.51 83.82 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D3 (at 1.27 -3.96 90) (layer F.SilkS) hide)
    (fp_text value LEDERR (at 1.27 3.96 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 36 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 +5V))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223-3Lead_TabPin2 (layer F.Cu) (tedit 58FBD262)
    (at 211.074 96.266 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U3 (at 0 -4.5 90) (layer F.SilkS) hide)
    (fp_text value "AMS1117 3.3V" (at 0 4.5 90) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 3.15 0 90) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 28 +3V3))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 28 +3V3))
    (pad 3 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 +5V))
    (pad 1 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206_HandSoldering (layer F.Cu) (tedit 58FBD468)
    (at 173.99 97.536 270)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C5 (at 0 -1.75 270) (layer F.SilkS) hide)
    (fp_text value 0.1uFC (at 0 -2.0955 270) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 28 +3V3))
    (pad 2 smd rect (at 2 0 270) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module SOT-23_Handsoldering (layer F.Cu) (tedit 58F511F6)
    (at 167.386 97.282 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U6 (at 0 -2.5 180) (layer F.SilkS) hide)
    (fp_text value ATSHA204A (at -0.508 -2.794 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 38 SDA))
    (pad 2 smd rect (at -1.5 0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 28 +3V3))
    (pad 3 smd rect (at 1.5 0 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_obscurities:2_pin_solder_jumper_smd (layer F.Cu) (tedit 58FBD115)
    (at 165.1 58.674 90)
    (fp_text reference JP2 (at 0 2.54 180) (layer F.SilkS))
    (fp_text value JUMPER (at 0 -1.524 90) (layer F.Fab) hide)
    (pad 2 smd oval (at 0.889 0 90) (size 1.27 1.524) (layers F.Cu F.Paste F.Mask)
      (net 28 +3V3))
    (pad 1 smd oval (at -0.889 0 90) (size 1.27 1.524) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(JP2-Pad1)"))
  )
  (module nodemcu:NodeMCU_Amica_R2 (layer F.Cu) (tedit 58FBD427)
    (at 192.278 87.63 90)
    (descr "Through-hole-mounted NodeMCU 0.9")
    (tags nodemcu)
    (fp_text reference U7 (at 11.43 12.68 90) (layer F.SilkS) hide)
    (fp_text value NodeMCU_Amica_R2 (at 9.779 19.685 180) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(U7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(U7-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(U7-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(U7-Pad4)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(U7-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(U7-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(U7-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(U7-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(U7-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(U7-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(U7-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(U7-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(U7-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (pad 15 thru_hole oval (at 0 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 +5V))
    (pad 30 thru_hole oval (at 22.86 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 ErrLed))
    (pad 18 thru_hole oval (at 22.86 30.48 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(U7-Pad18)"))
    (pad 17 thru_hole oval (at 22.86 33.02 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 GND))
    (pad 19 thru_hole oval (at 22.86 27.94 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(U7-Pad19)"))
    (pad 25 thru_hole oval (at 22.86 12.7 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(U7-Pad25)"))
    (pad 26 thru_hole oval (at 22.86 10.16 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(U7-Pad26)"))
    (pad 24 thru_hole oval (at 22.86 15.24 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(U7-Pad24)"))
    (pad 16 thru_hole oval (at 22.86 35.56 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(JP2-Pad1)"))
    (pad 22 thru_hole oval (at 22.86 20.32 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 MISO))
    (pad 23 thru_hole oval (at 22.86 17.78 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 SCK))
    (pad 21 thru_hole oval (at 22.86 22.86 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 26 MOSI))
    (pad 20 thru_hole oval (at 22.86 25.4 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 CSN))
    (pad 28 thru_hole oval (at 22.86 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 CE))
    (pad 27 thru_hole oval (at 22.86 7.62 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 TXled))
    (pad 29 thru_hole oval (at 22.86 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 RXled))
  )
  (gr_text + (at 145.288 95.25) (layer F.SilkS))
  (gr_text + (at 145.288 87.63) (layer F.SilkS))
  (gr_text + (at 145.288 80.01) (layer F.SilkS))
  (gr_text - (at 145.288 100.584) (layer F.SilkS))
  (gr_text - (at 145.288 92.964) (layer F.SilkS))
  (gr_text - (at 145.288 85.344) (layer F.SilkS))
  (gr_text "Inner == Arduino Nano\nOuter == NodeMCU" (at 197.866 75.7555) (layer F.SilkS))
  (gr_text "OH MySensors Gateway\n+ 433Mhz Bridge" (at 192.786 96.266) (layer F.SilkS))
  (gr_text "Close to power radio from\n\nJP1 == Nano\nJP2 == NodeMUC\n\nIf closed the AMS1117 \nis not needed." (at 153.924 66.802) (layer F.SilkS))
  (gr_text H (at 162.56 81.788) (layer B.SilkS))
  (gr_text O (at 165.354 76.708) (layer B.SilkS))
  (gr_text "OH MySensors Gateway\n+ 433Mhz Bridge" (at 195.58 96.266) (layer B.SilkS))
  (gr_text GND (at 223.012 104.648) (layer F.SilkS))
  (dimension 40.64 (width 0.3) (layer Dwgs.User)
    (gr_text "40,640 mm" (at 160.02 31.67) (layer Dwgs.User))
    (feature1 (pts (xy 180.34 68.58) (xy 180.34 30.32)))
    (feature2 (pts (xy 139.7 68.58) (xy 139.7 30.32)))
    (crossbar (pts (xy 139.7 33.02) (xy 180.34 33.02)))
    (arrow1a (pts (xy 180.34 33.02) (xy 179.213496 33.606421)))
    (arrow1b (pts (xy 180.34 33.02) (xy 179.213496 32.433579)))
    (arrow2a (pts (xy 139.7 33.02) (xy 140.826504 33.606421)))
    (arrow2b (pts (xy 139.7 33.02) (xy 140.826504 32.433579)))
  )
  (dimension 12 (width 0.3) (layer Dwgs.User)
    (gr_text "12,000 mm" (at 229 117.35) (layer Dwgs.User))
    (feature1 (pts (xy 223 98) (xy 223 118.7)))
    (feature2 (pts (xy 235 98) (xy 235 118.7)))
    (crossbar (pts (xy 235 116) (xy 223 116)))
    (arrow1a (pts (xy 223 116) (xy 224.126504 115.413579)))
    (arrow1b (pts (xy 223 116) (xy 224.126504 116.586421)))
    (arrow2a (pts (xy 235 116) (xy 233.873496 115.413579)))
    (arrow2b (pts (xy 235 116) (xy 233.873496 116.586421)))
  )
  (dimension 55 (width 0.3) (layer Dwgs.User)
    (gr_text "55,000 mm" (at 250.35 82.5 270) (layer Dwgs.User))
    (feature1 (pts (xy 235 110) (xy 251.7 110)))
    (feature2 (pts (xy 235 55) (xy 251.7 55)))
    (crossbar (pts (xy 249 55) (xy 249 110)))
    (arrow1a (pts (xy 249 110) (xy 248.413579 108.873496)))
    (arrow1b (pts (xy 249 110) (xy 249.586421 108.873496)))
    (arrow2a (pts (xy 249 55) (xy 248.413579 56.126504)))
    (arrow2b (pts (xy 249 55) (xy 249.586421 56.126504)))
  )
  (dimension 95 (width 0.3) (layer Dwgs.User)
    (gr_text "95,000 mm" (at 187.5 42.65) (layer Dwgs.User))
    (feature1 (pts (xy 235 55) (xy 235 41.3)))
    (feature2 (pts (xy 140 55) (xy 140 41.3)))
    (crossbar (pts (xy 140 44) (xy 235 44)))
    (arrow1a (pts (xy 235 44) (xy 233.873496 44.586421)))
    (arrow1b (pts (xy 235 44) (xy 233.873496 43.413579)))
    (arrow2a (pts (xy 140 44) (xy 141.126504 44.586421)))
    (arrow2b (pts (xy 140 44) (xy 141.126504 43.413579)))
  )
  (dimension 47 (width 0.3) (layer Dwgs.User)
    (gr_text "47,000 mm" (at 243.35 82.5 90) (layer Dwgs.User))
    (feature1 (pts (xy 231 59) (xy 244.7 59)))
    (feature2 (pts (xy 231 106) (xy 244.7 106)))
    (crossbar (pts (xy 242 106) (xy 242 59)))
    (arrow1a (pts (xy 242 59) (xy 242.586421 60.126504)))
    (arrow1b (pts (xy 242 59) (xy 241.413579 60.126504)))
    (arrow2a (pts (xy 242 106) (xy 242.586421 104.873496)))
    (arrow2b (pts (xy 242 106) (xy 241.413579 104.873496)))
  )
  (dimension 87 (width 0.3) (layer Dwgs.User)
    (gr_text "87,000 mm" (at 187.5 49.65) (layer Dwgs.User))
    (feature1 (pts (xy 231 59) (xy 231 48.3)))
    (feature2 (pts (xy 144 59) (xy 144 48.3)))
    (crossbar (pts (xy 144 51) (xy 231 51)))
    (arrow1a (pts (xy 231 51) (xy 229.873496 51.586421)))
    (arrow1b (pts (xy 231 51) (xy 229.873496 50.413579)))
    (arrow2a (pts (xy 144 51) (xy 145.126504 51.586421)))
    (arrow2b (pts (xy 144 51) (xy 145.126504 50.413579)))
  )
  (zone (net 14) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 234.442 55.626) (xy 234.696 109.474) (xy 140.462 109.22) (xy 140.462 55.118) (xy 234.442 55.626)
      )
    )
  )
  (zone (net 14) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.462 55.118) (xy 234.442 55.626) (xy 234.696 109.474) (xy 140.462 109.22)
      )
    )
  )
)
