(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~53~ubuntu16.04.1)
  (general
    (links 65)
    (no_connects 0)
    (area 149.924999 110.396999 190.175001 151.883)
    (thickness 1.6)
    (drawings 29)
    (tracks 314)
    (zones 0)
    (modules 25)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.25)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.63 0.45)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 190 150)
    (visible_elements FFFFEFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 /RESET)
  (net 5 /S2)
  (net 6 /CE)
  (net 7 /CSN)
  (net 8 /MOSI)
  (net 9 /MISO)
  (net 10 /SCK)
  (net 11 /LDR_IN)
  (net 12 /LDR_VCC)
  (net 13 /ATSHA_SDA)
  (net 14 /SDA)
  (net 15 /SCL)
  (net 16 /TX)
  (net 17 /S1)
  (net 18 "Net-(J2-Pad1)")
  (net 19 "Net-(R1-Pad2)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ATSHA_SDA)
    (add_net /CE)
    (add_net /CSN)
    (add_net /LDR_IN)
    (add_net /LDR_VCC)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /S1)
    (add_net /S2)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TX)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(R1-Pad2)")
  )
  (net_class power ""
    (clearance 0.3)
    (trace_width 0.4)
    (via_dia 0.7)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net VCC)
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 170.942 140.97 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference P2 (at 0 7.62 180) (layer F.SilkS))
    (fp_text value Switches (at 2.032 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 7.62 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /S1))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /S2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module battery_holders:CR2032-battery-holder (layer F.Cu) (tedit 58FFA26C)
    (at 160.02 133.5 90)
    (fp_text reference BT1 (at -11.5 4.572 180) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 0 90) (layer F.Fab))
    (fp_text user - (at -15.09 -2.54 180) (layer F.SilkS))
    (fp_text user + (at 15 -2.54 90) (layer F.SilkS))
    (pad 1 smd rect (at 15 0 90) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at -15 0 90) (size 2 3.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 594A1545)
    (at 158.75 112.522 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J2 (at 0.127 -2.54 180) (layer F.SilkS))
    (fp_text value LED (at -0.508 -3.175 180) (layer F.Fab))
    (fp_text user %R (at 0.127 -2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 173.8198 132.7658 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 3.35 0 180) (layer F.SilkS))
    (fp_text value 10k (at -3.65 1 180) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 /SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 173.8198 125.6284)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -3.208 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 4.5 -1.25) (layer F.Fab))
    (fp_text user %R (at -3.208 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:DFN-6-1EP_3x3mm_Pitch0.95mm (layer F.Cu) (tedit 594F82C9)
    (at 173.7498 128.4884 180)
    (descr "DFN6 3*3 MM, 0.95 PITCH; CASE 506AH-01 (see ON Semiconductor 506AH.PDF)")
    (tags "DFN 0.95")
    (attr smd)
    (fp_text reference U3 (at 0.09 -2.474 180) (layer F.SilkS))
    (fp_text value Si7021 (at 2.925 0.1 270) (layer F.Fab))
    (pad 1 smd oval (at -1.84 -0.95 180) (size 1.63 0.45) (layers F.Cu F.Paste F.Mask)
      (net 14 /SDA))
    (pad 2 smd oval (at -1.84 0 180) (size 1.63 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd oval (at -1.84 0.95 180) (size 1.63 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd oval (at 1.84 0.95 180) (size 1.63 0.45) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd oval (at 1.84 0 180) (size 1.63 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 6 smd oval (at 1.84 -0.95 180) (size 1.63 0.45) (layers F.Cu F.Paste F.Mask)
      (net 15 /SCL))
    (pad 7 smd rect (at 0.425 0.65 180) (size 0.85 1.3) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at 0.425 -0.65 180) (size 0.85 1.3) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at -0.425 0.65 180) (size 0.85 1.3) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (pad 7 smd rect (at -0.425 -0.65 180) (size 0.85 1.3) (layers F.Cu F.Paste F.Mask)
      (solder_paste_margin_ratio -0.2))
    (model Housings_DFN_QFN.3dshapes/DFN-6-1EP_3x3mm_Pitch0.95mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 173.8198 135.3058 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 3.35 0 180) (layer F.SilkS))
    (fp_text value 10k (at -3.65 1.25 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_radios:NRF24L01-SMD (layer F.Cu) (tedit 574A9E44)
    (at 183.8 120.5)
    (fp_text reference U1 (at 0 1.1) (layer F.SilkS))
    (fp_text value NRF24L01 (at 0 -4.8) (layer F.Fab))
    (pad 2 smd rect (at -4.4 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 1 smd rect (at -3.13 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -1.86 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 6 /CE))
    (pad 4 smd rect (at -0.59 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 7 /CSN))
    (pad 5 smd rect (at 0.68 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 10 /SCK))
    (pad 6 smd rect (at 1.95 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 8 /MOSI))
    (pad 7 smd rect (at 3.22 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask)
      (net 9 /MISO))
    (pad 8 smd rect (at 4.49 8.7) (size 1 2) (layers F.Cu F.Paste F.Mask))
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/nrf24smd.wrl
      (at (xyz -5.7625 2.9 0.03))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_5x5mm_Pitch0.65mm.wrl
      (at (xyz 0.0165 -0.109 0.062))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 152.908 131.826 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.25 0 360) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 3.25 0 360) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 167.132 132.842 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 3.25 0 360) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 3.25 0 360) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:CP_Elec_3x5.3 (layer F.Cu) (tedit 58AA85CF)
    (at 183 134.5 90)
    (descr "SMT capacitor, aluminium electrolytic, 3x5.3")
    (attr smd)
    (fp_text reference C3 (at -3.75 0 180) (layer F.SilkS))
    (fp_text value 4.7uF (at 1 2.75 90) (layer F.Fab))
    (fp_text user + (at -0.94 -0.08 90) (layer F.Fab))
    (fp_text user + (at -2.22 1.4 90) (layer F.SilkS))
    (fp_text user %R (at -3.75 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.5 0 90) (size 2.2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.5 0 90) (size 2.2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (model Capacitors_SMD.3dshapes/CP_Elec_3x5.3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 179.75 134 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -3.25 0 180) (layer F.SilkS))
    (fp_text value 100nF (at 0.25 -1.5 270) (layer F.Fab))
    (fp_text user %R (at -3.25 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 162.56 144.125 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 3.195 0 360) (layer B.SilkS))
    (fp_text value 100nF (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 3.195 0 360) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 158.75 121.412 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 3.048 0 360) (layer B.SilkS))
    (fp_text value 220 (at 0 1.524 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 155.575 142.955 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 3.349 0 540) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 /ATSHA_SDA))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 153.035 142.955 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -3.349 0 360) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 4 /RESET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 183.0324 141.5034 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 3.302 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0.9 -1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /S1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 180.4924 141.5034 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 3.302 0 360) (layer F.SilkS))
    (fp_text value 10k (at 0.9 -1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0.254 450) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /S2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 161.29 121.412 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at -3.048 0 180) (layer B.SilkS))
    (fp_text value 10k (at 0 1.524 90) (layer B.Fab))
    (fp_text user %R (at 0.635 1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 /LDR_IN))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer B.Cu) (tedit 58CE4E7E)
    (at 159.385 144.375 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at 3.707 -0.127 360) (layer B.SilkS))
    (fp_text value ATSHA204A (at 0 -2.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 13 /ATSHA_SDA))
    (pad 2 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 594A15E8)
    (at 158.75 115.57 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P3 (at 0 -2.54 180) (layer F.SilkS))
    (fp_text value LDR (at -0.635 -3.175 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /LDR_VCC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /LDR_IN))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 152.4 121.158 90)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J1 (at 5.08 1.27 180) (layer F.SilkS))
    (fp_text value Power (at 2.54 1.27 180) (layer F.Fab))
    (fp_text user %R (at 4.315 -2.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer B.Cu) (tedit 58CC9A48)
    (at 160.02 131.885)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U4 (at 0 6.05) (layer B.SilkS))
    (fp_text value ATMEGA328P-AU (at 0 -6.05) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -4.25 2.8) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 5 /S2))
    (pad 2 smd rect (at -4.25 2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 3 smd rect (at -4.25 1.2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -4.25 0.4) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 5 smd rect (at -4.25 -0.4) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.25 -1.2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 7 smd rect (at -4.25 -2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at -4.25 -2.8) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at -2.8 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at -2 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(R1-Pad2)"))
    (pad 11 smd rect (at -1.2 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at -0.4 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 13 smd rect (at 0.4 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 6 /CE))
    (pad 14 smd rect (at 1.2 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 7 /CSN))
    (pad 15 smd rect (at 2 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 8 /MOSI))
    (pad 16 smd rect (at 2.8 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 9 /MISO))
    (pad 17 smd rect (at 4.25 -2.8) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 10 /SCK))
    (pad 18 smd rect (at 4.25 -2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 19 smd rect (at 4.25 -1.2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd rect (at 4.25 -0.4) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 21 smd rect (at 4.25 0.4) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 4.25 1.2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 23 smd rect (at 4.25 2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 12 /LDR_VCC))
    (pad 24 smd rect (at 4.25 2.8) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 11 /LDR_IN))
    (pad 25 smd rect (at 2.8 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 26 smd rect (at 2 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 13 /ATSHA_SDA))
    (pad 27 smd rect (at 1.2 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 14 /SDA))
    (pad 28 smd rect (at 0.4 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 15 /SCL))
    (pad 29 smd rect (at -0.4 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 4 /RESET))
    (pad 30 smd rect (at -1.2 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 31 smd rect (at -2 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 16 /TX))
    (pad 32 smd rect (at -2.8 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 17 /S1))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x05_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 165.1 121.158 90)
    (descr "Through hole angled pin header, 1x05, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x05 2.54mm single row")
    (fp_text reference J3 (at 5.08 1.27 180) (layer F.SilkS))
    (fp_text value "ISP and TX" (at 2.54 5.08 180) (layer F.Fab))
    (fp_text user %R (at 4.315 -2.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /TX))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /RESET))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /MOSI))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /MISO))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /SCK))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_PTS645 (layer F.Cu) (tedit 58724A80)
    (at 173.736 146.558)
    (descr "C&K Components SPST SMD PTS645 Series 6mm Tact Switch")
    (tags "SPST Button Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 0) (layer F.SilkS))
    (fp_text value SW_DIP_x01 (at 0 4.15) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at -3.98 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -3.98 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /S1))
    (pad 1 smd rect (at 3.98 -2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 /S1))
    (pad 2 smd rect (at 3.98 2.25) (size 1.55 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Buttons_Switches_SMD.3dshapes/SW_SPST_PTS645.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Platine für\nUniflächentaster\nV 2.0" (at 153.67 147.066) (layer F.SilkS))
  (gr_text GND (at 173.482 142.748) (layer F.SilkS))
  (gr_text S1 (at 170.942 142.748) (layer F.SilkS))
  (gr_text S2 (at 176.022 142.748) (layer F.SilkS))
  (gr_text - (at 163.195 113.665) (layer F.SilkS))
  (gr_text + (at 156.845 113.665) (layer F.SilkS))
  (gr_text LDR (at 163.576 115.57) (layer F.SilkS))
  (gr_text LED (at 163.576 112.268) (layer F.SilkS))
  (gr_text "SCK\n" (at 175.26 122.555) (layer F.SilkS))
  (gr_text MISO (at 172.72 122.555) (layer F.SilkS))
  (gr_text MOSI (at 170.18 122.555) (layer F.SilkS))
  (gr_text RESET (at 167.64 122.555) (layer F.SilkS))
  (gr_text TX (at 165.1 122.555) (layer F.SilkS))
  (gr_text VCC (at 154.94 122.555) (layer F.SilkS))
  (gr_text GND (at 152.4 122.555) (layer F.SilkS))
  (gr_line (start 185.5 150) (end 190 150) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 185.5 148.25) (end 185.5 150) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 183.5 148.25) (end 183.5 150) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 184.5 148.25) (end 184.5 147.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 184.5 148.25) (end 183.5 148.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190 144) (end 190 150) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 188.25 137) (end 190 137) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 188.25 144) (end 188.25 142.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 188.25 140.5) (end 188.25 142.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 188.25 140.5) (end 186.5 140.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 190 111) (end 190 137) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150 111) (end 190 111) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150 111) (end 150 150) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150 150) (end 183.5 150) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.25 111) (xy 190 111) (xy 190 118) (xy 177.25 118)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 177.25 111) (xy 190 111) (xy 190 118) (xy 177.25 118)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150 111) (xy 150 150) (xy 190 150) (xy 190 111)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 150 111) (xy 150 150) (xy 190 150) (xy 190 111)
      )
    )
  )
)
