(kicad_pcb (version 4) (host pcbnew 4.0.6-e0-6349~52~ubuntu17.04.1)
  (general
    (links 182)
    (no_connects 0)
    (area 79.524999 58.904999 180.390001 161.195)
    (thickness 1.6)
    (drawings 15)
    (tracks 644)
    (zones 0)
    (modules 86)
    (nets 94)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 80.264 158.496)
    (visible_elements FFFFFFFF)
    (pcbplotparams
      (layerselection 0x01030_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerbers/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(AE1-Pad1)")
  (net 3 "Net-(C1-Pad1)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C3-Pad2)")
  (net 6 /V3)
  (net 7 /V5)
  (net 8 "Net-(C9-Pad1)")
  (net 9 /RST)
  (net 10 /V12)
  (net 11 "Net-(D1-Pad2)")
  (net 12 "Net-(D3-Pad2)")
  (net 13 /TX0)
  (net 14 "Net-(D5-Pad2)")
  (net 15 "Net-(D6-Pad1)")
  (net 16 "Net-(D6-Pad2)")
  (net 17 /LGC)
  (net 18 "Net-(D7-Pad2)")
  (net 19 /LGO)
  (net 20 "Net-(D8-Pad2)")
  (net 21 /RGC)
  (net 22 "Net-(D9-Pad2)")
  (net 23 /RGO)
  (net 24 "Net-(D10-Pad2)")
  (net 25 "Net-(D11-Pad2)")
  (net 26 "Net-(D12-Pad2)")
  (net 27 "Net-(D13-Pad2)")
  (net 28 "Net-(D14-Pad2)")
  (net 29 /FTDI_P4)
  (net 30 "Net-(F2-Pad1)")
  (net 31 /L)
  (net 32 /COMMON_L)
  (net 33 "Net-(H1-Pad2)")
  (net 34 /MISO)
  (net 35 /D13)
  (net 36 /MOSI)
  (net 37 "Net-(J1-Pad1)")
  (net 38 "Net-(J1-Pad2)")
  (net 39 "Net-(J2-Pad1)")
  (net 40 "Net-(J2-Pad2)")
  (net 41 /RX1)
  (net 42 /TX1)
  (net 43 /KEYFOB)
  (net 44 /KEYPAD)
  (net 45 /INTERCOM)
  (net 46 /REED_SW)
  (net 47 /PHOTO)
  (net 48 /WALL_SW)
  (net 49 /N)
  (net 50 "Net-(K1-Pad3)")
  (net 51 "Net-(K2-Pad3)")
  (net 52 "Net-(K3-Pad3)")
  (net 53 "Net-(K4-Pad3)")
  (net 54 "Net-(LED1-Pad1)")
  (net 55 "Net-(LED1-Pad2)")
  (net 56 "Net-(Q2-Pad2)")
  (net 57 "Net-(Q3-Pad2)")
  (net 58 "Net-(Q4-Pad2)")
  (net 59 "Net-(Q5-Pad2)")
  (net 60 /RX0)
  (net 61 /SS)
  (net 62 /NSS_3)
  (net 63 /SCK)
  (net 64 /SCK_3)
  (net 65 /MOSI_3)
  (net 66 "Net-(R19-Pad1)")
  (net 67 "Net-(R20-Pad1)")
  (net 68 "Net-(R21-Pad1)")
  (net 69 "Net-(R22-Pad1)")
  (net 70 "Net-(R23-Pad2)")
  (net 71 "Net-(R24-Pad2)")
  (net 72 "Net-(R25-Pad2)")
  (net 73 "Net-(R26-Pad2)")
  (net 74 "Net-(U1-Pad1)")
  (net 75 "Net-(U1-Pad2)")
  (net 76 "Net-(U1-Pad22)")
  (net 77 /INT)
  (net 78 "Net-(U1-Pad23)")
  (net 79 "Net-(U1-Pad4)")
  (net 80 "Net-(U1-Pad34)")
  (net 81 "Net-(U1-Pad35)")
  (net 82 "Net-(U1-Pad36)")
  (net 83 "Net-(U1-Pad37)")
  (net 84 "Net-(U1-Pad38)")
  (net 85 "Net-(U1-Pad39)")
  (net 86 "Net-(U1-Pad40)")
  (net 87 "Net-(U2-Pad1)")
  (net 88 "Net-(U2-Pad3)")
  (net 89 "Net-(U2-Pad4)")
  (net 90 "Net-(U2-Pad5)")
  (net 91 "Net-(U2-Pad6)")
  (net 92 "Net-(U2-Pad7)")
  (net 93 "Net-(U2-Pad16)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /D13)
    (add_net /FTDI_P4)
    (add_net /INT)
    (add_net /INTERCOM)
    (add_net /KEYFOB)
    (add_net /KEYPAD)
    (add_net /LGC)
    (add_net /LGO)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /MOSI_3)
    (add_net /NSS_3)
    (add_net /PHOTO)
    (add_net /REED_SW)
    (add_net /RGC)
    (add_net /RGO)
    (add_net /RST)
    (add_net /RX0)
    (add_net /RX1)
    (add_net /SCK)
    (add_net /SCK_3)
    (add_net /SS)
    (add_net /TX0)
    (add_net /TX1)
    (add_net /V12)
    (add_net /V3)
    (add_net /V5)
    (add_net /WALL_SW)
    (add_net GND)
    (add_net "Net-(AE1-Pad1)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D10-Pad2)")
    (add_net "Net-(D11-Pad2)")
    (add_net "Net-(D12-Pad2)")
    (add_net "Net-(D13-Pad2)")
    (add_net "Net-(D14-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad2)")
    (add_net "Net-(D9-Pad2)")
    (add_net "Net-(H1-Pad2)")
    (add_net "Net-(K1-Pad3)")
    (add_net "Net-(K2-Pad3)")
    (add_net "Net-(K3-Pad3)")
    (add_net "Net-(K4-Pad3)")
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(Q2-Pad2)")
    (add_net "Net-(Q3-Pad2)")
    (add_net "Net-(Q4-Pad2)")
    (add_net "Net-(Q5-Pad2)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R20-Pad1)")
    (add_net "Net-(R21-Pad1)")
    (add_net "Net-(R22-Pad1)")
    (add_net "Net-(R23-Pad2)")
    (add_net "Net-(R24-Pad2)")
    (add_net "Net-(R25-Pad2)")
    (add_net "Net-(R26-Pad2)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad34)")
    (add_net "Net-(U1-Pad35)")
    (add_net "Net-(U1-Pad36)")
    (add_net "Net-(U1-Pad37)")
    (add_net "Net-(U1-Pad38)")
    (add_net "Net-(U1-Pad39)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad40)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad16)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U2-Pad7)")
  )
  (net_class AC_PWR ""
    (clearance 1.7)
    (trace_width 1.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /COMMON_L)
    (add_net /L)
    (add_net /N)
    (add_net "Net-(F2-Pad1)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
  )
  (module Connectors:SMA_THT_Jack_Straight (layer F.Cu) (tedit 5954CD20)
    (at 99.06 64.77)
    (descr "SMA pcb through hole jack")
    (tags "SMA THT Jack Straight")
    (fp_text reference AE1 (at -5.08 -2.286) (layer F.SilkS))
    (fp_text value Antenna_Shield (at 5.08 0 90) (layer F.Fab))
    (fp_text user %R (at 0 -5) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "Net-(AE1-Pad1)"))
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5920C254)
    (at 156.21 90.17 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C1 (at 1.25 -1.86 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 1.86 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5920C254)
    (at 118.11 105.41 180)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C2 (at 1.25 -1.86 180) (layer F.SilkS))
    (fp_text value 22pf (at 1.25 1.86 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5954CBAA)
    (at 111.76 96.52 90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C3 (at 2.54 -2.54 180) (layer F.SilkS))
    (fp_text value 22pf (at 1.27 -2.54 180) (layer F.Fab))
    (fp_text user %R (at 1.25 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5954C972)
    (at 162.56 86.36)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C8 (at 1.25 -1.86) (layer F.SilkS))
    (fp_text value 0.1uF (at -2.54 0 90) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /V5))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5954C926)
    (at 156.21 68.58 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C9 (at 1.25 -1.86 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 3.81 -2.54 360) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(C9-Pad1)"))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /RST))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5920C254)
    (at 109.22 80.01 270)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C14 (at 1.25 -1.86 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 1.86 270) (layer F.Fab))
    (fp_text user %R (at 1.25 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /V3))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm (layer F.Cu) (tedit 5920C254)
    (at 109.22 100.33)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
    (fp_text reference C15 (at 1.25 -1.86) (layer F.SilkS))
    (fp_text value 0.1uF (at 1.25 1.86) (layer F.Fab))
    (fp_text user %R (at 1.25 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /V5))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D1.8mm_W3.3mm_H2.4mm locked (layer F.Cu) (tedit 5954CD27)
    (at 82.55 62.23)
    (descr "LED, Round,  Rectangular size 3.3x2.4mm^2 diameter 1.8mm, 2 pins")
    (tags "LED Round  Rectangular size 3.3x2.4mm^2 diameter 1.8mm 2 pins")
    (fp_text reference D1 (at 4.826 -0.254) (layer F.SilkS))
    (fp_text value GREEN (at 1.27 2.26) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(D1-Pad2)"))
    (model LEDs.3dshapes/LED_D1.8mm_W3.3mm_H2.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp (layer F.Cu) (tedit 5921392E)
    (at 151.13 100.33)
    (descr "D, DO-35_SOD27 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Vertical pin pitch 2.54mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 1.27 -2.266371) (layer F.SilkS))
    (fp_text value 1N4148 (at 1.27 3.155371) (layer F.Fab))
    (fp_text user K (at -1.966371 0) (layer F.Fab))
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /V5))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /RST))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P2.54mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp (layer F.Cu) (tedit 5954CC79)
    (at 143.51 71.12 90)
    (descr "D, DO-41_SOD81 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "D DO-41_SOD81 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D3 (at 1.27 -2.690635 90) (layer F.SilkS))
    (fp_text value 1N5817 (at 5.08 0 180) (layer F.Fab))
    (fp_text user K (at -2.390635 0 90) (layer F.Fab))
    (fp_text user %R (at 1.27 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 7 /V5))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-41_SOD81_P2.54mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 147.32 76.2 270)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D5 (at 1.27 -3.96 270) (layer F.SilkS))
    (fp_text value GREEN (at 1.27 3.96 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 /TX0))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(D5-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 158.75 76.2 270)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D6 (at 1.27 -3.96 270) (layer F.SilkS))
    (fp_text value RED (at 1.27 3.96 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(D6-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 96.52 130.81 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D7 (at 1.27 -3.96 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 /LGC))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "Net-(D7-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 5954CAD6)
    (at 86.36 132.08 90)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D8 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 /LGO))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 "Net-(D8-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 172.72 130.81)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D9 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 /RGC))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 "Net-(D9-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D5.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 165.1 124.46)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D10 (at 1.27 -3.96) (layer F.SilkS))
    (fp_text value LED (at 1.27 3.96) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 /RGO))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 "Net-(D10-Pad2)"))
    (model LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_A-405_P2.54mm_Vertical_AnodeUp (layer F.Cu) (tedit 5954CB69)
    (at 115.57 119.38 180)
    (descr "D, A-405 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D11 (at 1.27 -2.41 180) (layer F.SilkS))
    (fp_text value 1N4007 (at 1.27 2.54 180) (layer F.Fab))
    (fp_text user K (at -2.11 0 180) (layer F.Fab))
    (fp_text user %R (at 1.27 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 /V12))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P2.54mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_A-405_P2.54mm_Vertical_AnodeUp (layer F.Cu) (tedit 5954CB71)
    (at 116.84 111.76 180)
    (descr "D, A-405 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D12 (at -2.54 0 180) (layer F.SilkS))
    (fp_text value 1N4007 (at 2.54 -2.54 180) (layer F.Fab))
    (fp_text user K (at -2.11 0 180) (layer F.Fab))
    (fp_text user %R (at 1.27 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 /V12))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 "Net-(D12-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P2.54mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_A-405_P2.54mm_Vertical_AnodeUp (layer F.Cu) (tedit 5954C990)
    (at 147.32 115.57)
    (descr "D, A-405 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D13 (at -3.81 0) (layer F.SilkS))
    (fp_text value 1N4007 (at 1.27 2.54) (layer F.Fab))
    (fp_text user K (at -2.11 0) (layer F.Fab))
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 /V12))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 27 "Net-(D13-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P2.54mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_A-405_P2.54mm_Vertical_AnodeUp (layer F.Cu) (tedit 5954C98D)
    (at 147.32 120.65)
    (descr "D, A-405 series, Axial, Vertical, pin pitch=2.54mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Vertical pin pitch 2.54mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D14 (at -3.81 0) (layer F.SilkS))
    (fp_text value 1N4007 (at 1.27 3.299) (layer F.Fab))
    (fp_text user K (at -2.11 0) (layer F.Fab))
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 /V12))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 28 "Net-(D14-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P2.54mm_Vertical_AnodeUp.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5954CC7F)
    (at 148.59 68.58)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference F1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Fuse (at -1.27 5.08) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /FTDI_P4))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer F.Cu) (tedit 5954C90B)
    (at 156.21 63.5 270)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference H1 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value FTDI (at 2.54 2.54 360) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(C9-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(H1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(D6-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /FTDI_P4))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 -0.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC5)
    (at 151.13 107.95 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference H4 (at 1.27 -2.33 270) (layer F.SilkS))
    (fp_text value ICSP (at 1.27 7.41 270) (layer F.Fab))
    (fp_text user %R (at 1.27 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /MISO))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /V5))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /D13))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 /MOSI))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /RST))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 5954CD42)
    (at 104.14 153.67)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J1 (at 8.636 -4.318) (layer F.SilkS))
    (fp_text value "LEFT GATE" (at 11.43 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad2)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 5954CD72)
    (at 151.13 153.67)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J2 (at 8.382 -4.318) (layer F.SilkS))
    (fp_text value "RIGHT GATE" (at 10.16 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 40 "Net-(J2-Pad2)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 58CD4EC1)
    (at 118.11 63.5 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value GSM (at 0 12.49 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /V5))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /V5))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 /RX1))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /TX1))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5954C8E6)
    (at 176.53 74.93 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value KEYFOB (at 2.54 3.81 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /KEYFOB))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /V12))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5954C8B9)
    (at 176.53 102.87)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33) (layer F.SilkS))
    (fp_text value KEYPAD (at -2.54 5.08 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /KEYPAD))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /V12))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5954CCD5)
    (at 176.53 93.98)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J9 (at 0.254 4.572) (layer F.SilkS))
    (fp_text value INTERCOM (at -2.54 2.54 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /INTERCOM))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5954CCCF)
    (at 176.53 90.17 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J10 (at -0.254 -1.778 180) (layer F.SilkS))
    (fp_text value REED_SW (at 2.54 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 /REED_SW))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5954C8EF)
    (at 163.83 63.5 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J11 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value PHOTOCELLS (at -2.54 3.81 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 /PHOTO))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /V12))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5954C8D6)
    (at 176.53 82.55 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J12 (at 0 -2.33 180) (layer F.SilkS))
    (fp_text value WALL_SW (at 2.54 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 /WALL_SW))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MKDS1.5-2pol (layer F.Cu) (tedit 5954CD6E)
    (at 137.16 153.67)
    (descr "2-way 5mm pitch terminal block, Phoenix MKDS series")
    (fp_text reference J14 (at 8.636 -4.826) (layer F.SilkS))
    (fp_text value AC_PWR (at 8.89 -1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 31 /L))
    (pad 2 thru_hole circle (at 5 0) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 49 /N))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MKDS1.5-2pol.wrl
      (at (xyz 0.0984 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relays_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C locked (layer F.Cu) (tedit 5954CAEA)
    (at 109.22 129.54 270)
    (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
    (tags "relay Sanyu SRD form C")
    (fp_text reference K1 (at 1.27 8.89 270) (layer F.SilkS))
    (fp_text value L_CLOSE (at -3.81 -2.54 360) (layer F.Fab))
    (fp_text user 1 (at 0 -2.3 270) (layer F.Fab))
    (fp_text user %R (at 7.1 0.025 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.95 6.05) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(D11-Pad2)"))
    (pad 3 thru_hole circle (at 14.15 6.05) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 50 "Net-(K1-Pad3)"))
    (pad 4 thru_hole circle (at 14.2 -6) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad2)"))
    (pad 5 thru_hole circle (at 1.95 -5.95) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 /V12))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 32 /COMMON_L))
    (model ${KISYS3DMOD}/Relays_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relays_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C locked (layer F.Cu) (tedit 5954CADE)
    (at 92.71 139.7 270)
    (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
    (tags "relay Sanyu SRD form C")
    (fp_text reference K2 (at -2.54 5.08 360) (layer F.SilkS))
    (fp_text value L_OPEN (at -3.81 5.08 360) (layer F.Fab))
    (fp_text user 1 (at 0 -2.3 270) (layer F.Fab))
    (fp_text user %R (at 7.1 0.025 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.95 6.05) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(D12-Pad2)"))
    (pad 3 thru_hole circle (at 14.15 6.05) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 51 "Net-(K2-Pad3)"))
    (pad 4 thru_hole circle (at 14.2 -6) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad1)"))
    (pad 5 thru_hole circle (at 1.95 -5.95) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 /V12))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 32 /COMMON_L))
    (model ${KISYS3DMOD}/Relays_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relays_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C locked (layer F.Cu) (tedit 5954C9FB)
    (at 170.18 139.7 270)
    (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
    (tags "relay Sanyu SRD form C")
    (fp_text reference K3 (at 8.1 9.2 270) (layer F.SilkS))
    (fp_text value R_CLOSE (at -3.81 1.27 360) (layer F.Fab))
    (fp_text user 1 (at 0 -2.3 270) (layer F.Fab))
    (fp_text user %R (at 7.1 0.025 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.95 6.05) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(D13-Pad2)"))
    (pad 3 thru_hole circle (at 14.15 6.05) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 52 "Net-(K3-Pad3)"))
    (pad 4 thru_hole circle (at 14.2 -6) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 40 "Net-(J2-Pad2)"))
    (pad 5 thru_hole circle (at 1.95 -5.95) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 /V12))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 32 /COMMON_L))
    (model ${KISYS3DMOD}/Relays_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relays_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C locked (layer F.Cu) (tedit 5954CA00)
    (at 153.67 129.54 270)
    (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
    (tags "relay Sanyu SRD form C")
    (fp_text reference K4 (at 8.1 9.2 270) (layer F.SilkS))
    (fp_text value R_OPEN (at -2.54 6.35 360) (layer F.Fab))
    (fp_text user 1 (at 0 -2.3 270) (layer F.Fab))
    (fp_text user %R (at 7.1 0.025 270) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.95 6.05) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(D14-Pad2)"))
    (pad 3 thru_hole circle (at 14.15 6.05) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 53 "Net-(K4-Pad3)"))
    (pad 4 thru_hole circle (at 14.2 -6) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 39 "Net-(J2-Pad1)"))
    (pad 5 thru_hole circle (at 1.95 -5.95) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 10 /V12))
    (pad 1 thru_hole circle (at 0 0) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 32 /COMMON_L))
    (model ${KISYS3DMOD}/Relays_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D1.8mm_W3.3mm_H2.4mm (layer F.Cu) (tedit 5880A862)
    (at 162.56 91.44)
    (descr "LED, Round,  Rectangular size 3.3x2.4mm^2 diameter 1.8mm, 2 pins")
    (tags "LED Round  Rectangular size 3.3x2.4mm^2 diameter 1.8mm 2 pins")
    (fp_text reference LED1 (at 1.27 -2.26) (layer F.SilkS))
    (fp_text value AMBER (at 1.27 2.26) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 54 "Net-(LED1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 55 "Net-(LED1-Pad2)"))
    (model LEDs.3dshapes/LED_D1.8mm_W3.3mm_H2.4mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 58CE52AF)
    (at 157.48 104.14)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value 2N7000 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 54 "Net-(LED1-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 35 /D13))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 58CE52AF)
    (at 105.41 120.65 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q2 (at 1.27 -3.56 90) (layer F.SilkS))
    (fp_text value BC548 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 56 "Net-(Q2-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 25 "Net-(D11-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 58CE52AF)
    (at 105.41 109.22)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q3 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value BC548 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 57 "Net-(Q3-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 26 "Net-(D12-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 58CE52AF)
    (at 154.94 115.57)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q4 (at 1.27 -3.56) (layer F.SilkS))
    (fp_text value BC548 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 58 "Net-(Q4-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 27 "Net-(D13-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Narrow (layer F.Cu) (tedit 58CE52AF)
    (at 157.48 123.19 90)
    (descr "TO-92 leads molded, narrow, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q5 (at 1.27 -3.56 90) (layer F.SilkS))
    (fp_text value BC548 (at 1.27 2.79 90) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.27 -1.27 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 59 "Net-(Q5-Pad2)"))
    (pad 3 thru_hole circle (at 2.54 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1 1) (drill 0.6) (layers *.Cu *.Mask)
      (net 28 "Net-(D14-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Narrow.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 170.18 88.9 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R3 (at 1.27 -1.86 270) (layer F.SilkS))
    (fp_text value 1K (at 1.27 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 /V5))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 55 "Net-(LED1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5954CBBC)
    (at 118.11 88.9 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R4 (at 3.81 -1.27 180) (layer F.SilkS))
    (fp_text value 1M (at 1.27 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5954CC87)
    (at 152.4 68.58 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R5 (at 1.27 -1.86 270) (layer F.SilkS))
    (fp_text value 1K (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 33 "Net-(H1-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 13 /TX0))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5954C94A)
    (at 151.13 83.82 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R6 (at -2.54 0 360) (layer F.SilkS))
    (fp_text value 1K (at 1.27 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 15 "Net-(D6-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 60 /RX0))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5954C950)
    (at 154.94 83.82 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R7 (at -2.54 0 360) (layer F.SilkS))
    (fp_text value 2K (at 1.27 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 "Net-(D6-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 /V5))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5954C953)
    (at 147.32 83.82 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R8 (at -2.54 0 360) (layer F.SilkS))
    (fp_text value 2K (at 1.27 1.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 14 "Net-(D5-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 /V5))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 158.75 96.52 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R9 (at 1.27 -1.86 180) (layer F.SilkS))
    (fp_text value 10K (at 1.27 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 35 /D13))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 144.78 100.33)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R10 (at 1.27 -1.86) (layer F.SilkS))
    (fp_text value 10K (at 1.27 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 /RST))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 /V5))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 91.44 64.77 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R11 (at 1.27 -1.86 180) (layer F.SilkS))
    (fp_text value 1K (at 1.27 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 /V5))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 "Net-(D1-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 91.44 99.06 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R12 (at 1.27 -1.86 180) (layer F.SilkS))
    (fp_text value 4.7K (at 1.27 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 61 /SS))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 62 /NSS_3))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 85.09 99.06 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R13 (at 1.27 -1.86 180) (layer F.SilkS))
    (fp_text value 10K (at 1.27 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 62 /NSS_3))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 91.44 93.98 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R14 (at 1.27 -1.86 180) (layer F.SilkS))
    (fp_text value 4.7K (at 1.27 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 63 /SCK))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 64 /SCK_3))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 85.09 93.98 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R15 (at 1.27 -1.86 180) (layer F.SilkS))
    (fp_text value 10K (at 1.27 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 64 /SCK_3))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 91.44 88.9 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R16 (at 1.27 -1.86 180) (layer F.SilkS))
    (fp_text value 4.7K (at 1.27 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 36 /MOSI))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 65 /MOSI_3))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 85.09 88.9 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R17 (at 1.27 -1.86 180) (layer F.SilkS))
    (fp_text value 10K (at 1.27 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 65 /MOSI_3))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5954C967)
    (at 143.51 86.36 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R18 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 220 (at 1.27 -2.54 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 /V5))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 48 /WALL_SW))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5954CB58)
    (at 96.52 121.92)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R19 (at -1.27 1.27) (layer F.SilkS))
    (fp_text value 1K (at 1.27 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 66 "Net-(R19-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 /V5))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 96.52 116.84)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R20 (at 1.27 -1.86) (layer F.SilkS))
    (fp_text value 1K (at 1.27 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 67 "Net-(R20-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 /V5))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5954C9BA)
    (at 171.45 113.03 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R21 (at 1.27 -1.86 180) (layer F.SilkS))
    (fp_text value 1K (at -2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 68 "Net-(R21-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 /V5))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5954C9AA)
    (at 165.1 115.57 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R22 (at 1.27 -1.86 180) (layer F.SilkS))
    (fp_text value 1K (at 3.81 -1.27 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 69 "Net-(R22-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 7 /V5))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5954CB50)
    (at 99.06 111.76 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R23 (at 5.08 0 180) (layer F.SilkS))
    (fp_text value 510 (at 1.27 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 56 "Net-(Q2-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 70 "Net-(R23-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5954CB4C)
    (at 99.06 106.68 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R24 (at -2.54 1.27 180) (layer F.SilkS))
    (fp_text value 510 (at 1.27 1.86 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 57 "Net-(Q3-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 71 "Net-(R24-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5874F706)
    (at 163.83 99.06)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R25 (at 1.27 -1.86) (layer F.SilkS))
    (fp_text value 510 (at 1.27 1.86) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 58 "Net-(Q4-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 72 "Net-(R25-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical (layer F.Cu) (tedit 5954C9B2)
    (at 161.29 111.76)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R26 (at 1.27 -1.86) (layer F.SilkS))
    (fp_text value 510 (at -2.54 -1.27) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 59 "Net-(Q5-Pad2)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 73 "Net-(R26-Pad2)"))
    (model Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5923F252)
    (at 144.78 90.17)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference S1 (at 3.25 -2) (layer F.SilkS))
    (fp_text value RST_SW (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 /RST))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 9 /RST))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (at (xyz 0.005 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Damian:HLK-PM01 locked (layer F.Cu) (tedit 5954CAFB)
    (at 130.81 130.81 90)
    (fp_text reference T1 (at 5.08 -3.81 90) (layer F.SilkS))
    (fp_text value "HI-Link 12V" (at -3.81 -11.43 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -14.7 -2.5 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(F2-Pad1)"))
    (pad 2 thru_hole circle (at -14.7 2.5 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 49 /N))
    (pad 3 thru_hole circle (at 14.7 -7.7 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole circle (at 14.7 7.7 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 10 /V12))
  )
  (module Housings_DIP:DIP-40_W15.24mm_LongPads (layer F.Cu) (tedit 5954CD34)
    (at 123.19 63.5)
    (descr "40-lead dip package, row spacing 15.24 mm (600 mils), LongPads")
    (tags "DIL DIP PDIP 2.54mm 15.24mm 600mil LongPads")
    (fp_text reference U1 (at 17.018 1.016) (layer F.SilkS))
    (fp_text value ATMEGA1284P-PU (at -2.54 8.89 90) (layer F.Fab))
    (fp_text user %R (at 7.62 24.13) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(U1-Pad1)"))
    (pad 21 thru_hole oval (at 15.24 48.26) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /LGO))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(U1-Pad2)"))
    (pad 22 thru_hole oval (at 15.24 45.72) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(U1-Pad22)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 /INT))
    (pad 23 thru_hole oval (at 15.24 43.18) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "Net-(U1-Pad23)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(U1-Pad4)"))
    (pad 24 thru_hole oval (at 15.24 40.64) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /LGC))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 /SS))
    (pad 25 thru_hole oval (at 15.24 38.1) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 /INTERCOM))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 /MOSI))
    (pad 26 thru_hole oval (at 15.24 35.56) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 /KEYPAD))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 /MISO))
    (pad 27 thru_hole oval (at 15.24 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 /KEYFOB))
    (pad 8 thru_hole oval (at 0 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 /SCK))
    (pad 28 thru_hole oval (at 15.24 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 /REED_SW))
    (pad 9 thru_hole oval (at 0 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 /RST))
    (pad 29 thru_hole oval (at 15.24 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 /PHOTO))
    (pad 10 thru_hole oval (at 0 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /V5))
    (pad 30 thru_hole oval (at 15.24 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /V5))
    (pad 11 thru_hole oval (at 0 25.4) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole oval (at 15.24 22.86) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole oval (at 0 27.94) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 32 thru_hole oval (at 15.24 20.32) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 33 thru_hole oval (at 15.24 17.78) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 /WALL_SW))
    (pad 14 thru_hole oval (at 0 33.02) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 /RX0))
    (pad 34 thru_hole oval (at 15.24 15.24) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(U1-Pad34)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 /TX0))
    (pad 35 thru_hole oval (at 15.24 12.7) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "Net-(U1-Pad35)"))
    (pad 16 thru_hole oval (at 0 38.1) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 /RX1))
    (pad 36 thru_hole oval (at 15.24 10.16) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "Net-(U1-Pad36)"))
    (pad 17 thru_hole oval (at 0 40.64) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 /TX1))
    (pad 37 thru_hole oval (at 15.24 7.62) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "Net-(U1-Pad37)"))
    (pad 18 thru_hole oval (at 0 43.18) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 /RGO))
    (pad 38 thru_hole oval (at 15.24 5.08) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "Net-(U1-Pad38)"))
    (pad 19 thru_hole oval (at 0 45.72) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 /D13))
    (pad 39 thru_hole oval (at 15.24 2.54) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(U1-Pad39)"))
    (pad 20 thru_hole oval (at 0 48.26) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 /RGC))
    (pad 40 thru_hole oval (at 15.24 0) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 "Net-(U1-Pad40)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-40_W15.24mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_radios:RFM69HW_SMD_Handsoldering locked (layer F.Cu) (tedit 5954CC23)
    (at 101.6 85.09 180)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U2 (at 16.51 16.51 180) (layer F.SilkS))
    (fp_text value RFM69HW (at 8.382 7.112 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 87 "Net-(U2-Pad1)"))
    (pad 2 smd rect (at -1.4 2 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 77 /INT))
    (pad 3 smd rect (at -1.4 4 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 88 "Net-(U2-Pad3)"))
    (pad 4 smd rect (at -1.4 6 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 89 "Net-(U2-Pad4)"))
    (pad 5 smd rect (at -1.4 8 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 90 "Net-(U2-Pad5)"))
    (pad 6 smd rect (at -1.4 10 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at -1.4 12 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 92 "Net-(U2-Pad7)"))
    (pad 8 smd rect (at -1.4 14 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /V3))
    (pad 9 smd rect (at 18.3 14 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 18.3 12 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(AE1-Pad1)"))
    (pad 11 smd rect (at 18.3 10 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 18.3 8 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 64 /SCK_3))
    (pad 13 smd rect (at 18.3 6 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 34 /MISO))
    (pad 14 smd rect (at 18.3 4 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 65 /MOSI_3))
    (pad 15 smd rect (at 18.3 2 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 62 /NSS_3))
    (pad 16 smd rect (at 18.3 0 180) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 93 "Net-(U2-Pad16)"))
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/rfm69hw.wrl
      (at (xyz 0.332 -0.275 0.03))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0.332 -0.08 0.06))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.204 -0.445 0.06))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220_Vertical (layer F.Cu) (tedit 5954CB8A)
    (at 105.41 100.33 90)
    (descr "TO-220, Vertical, RM 2.54mm")
    (tags "TO-220 Vertical RM 2.54mm")
    (fp_text reference U3 (at 8.89 0 180) (layer F.SilkS))
    (fp_text value L7805 (at -3.81 0 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 10 /V12))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 /V5))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 5954CBD7)
    (at 115.57 85.09 90)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U4 (at 1.27 -3.56 90) (layer F.SilkS))
    (fp_text value 3VREG (at 5.08 1.27 180) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 1.27 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 7 /V5))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 6 /V3))
    (pad 1 thru_hole rect (at 0 0 270) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-92_Inline_Narrow_Oval.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Housings_DIP:DIP-4_W7.62mm (layer F.Cu) (tedit 5954AB1E)
    (at 85.09 116.84)
    (descr "4-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U5 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value LTV-817 (at 3.81 4.93) (layer F.Fab))
    (fp_text user %R (at 3.81 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(R19-Pad1)"))
    (pad 3 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(R23-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(D7-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /V12))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-4_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-4_W7.62mm (layer F.Cu) (tedit 58CC8E31)
    (at 83.82 106.68)
    (descr "4-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U6 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value LTV-817 (at 3.81 4.93) (layer F.Fab))
    (fp_text user %R (at 3.81 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "Net-(R20-Pad1)"))
    (pad 3 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Net-(R24-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(D8-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /V12))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-4_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-4_W7.62mm (layer F.Cu) (tedit 58CC8E31)
    (at 163.83 105.41)
    (descr "4-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U7 (at 3.81 -2.39) (layer F.SilkS))
    (fp_text value LTV-817 (at 3.81 4.93) (layer F.Fab))
    (fp_text user %R (at 3.81 1.27) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 "Net-(R21-Pad1)"))
    (pad 3 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Net-(R25-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(D9-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /V12))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-4_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-4_W7.62mm (layer F.Cu) (tedit 58CC8E31)
    (at 172.72 124.46 90)
    (descr "4-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U8 (at 3.81 -2.39 90) (layer F.SilkS))
    (fp_text value LTV-817 (at 3.81 4.93 90) (layer F.Fab))
    (fp_text user %R (at 3.81 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(R22-Pad1)"))
    (pad 3 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(R26-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(D10-Pad2)"))
    (pad 4 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /V12))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-4_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 58CD2E9C)
    (at 116.84 95.25 270)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (fp_text reference Y1 (at 2.44 -3.525 270) (layer F.SilkS))
    (fp_text value "16 Mhz" (at 2.44 3.525 270) (layer F.Fab))
    (fp_text user %R (at 2.44 0 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C3-Pad2)"))
    (pad 2 thru_hole circle (at 4.88 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5920C257)
    (at 113.03 74.93 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C4 (at 1.25 -3.56 90) (layer F.SilkS))
    (fp_text value 4.7uF (at 1.25 3.56 90) (layer F.Fab))
    (fp_text user %R (at 0.775 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /V3))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5920C257)
    (at 97.79 100.33 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C11 (at 1.25 -3.56 90) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 3.56 90) (layer F.Fab))
    (fp_text user %R (at 0.775 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /V12))
    (pad 2 thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5954CB9A)
    (at 109.22 88.9)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C12 (at 1.25 -3.56) (layer F.SilkS))
    (fp_text value 10uF (at -2.54 -1.27) (layer F.Fab))
    (fp_text user %R (at 0.775 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 /V5))
    (pad 2 thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:CP_Radial_D5.0mm_P2.50mm (layer F.Cu) (tedit 5920C257)
    (at 97.79 88.9 270)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C13 (at 1.25 -3.56 270) (layer F.SilkS))
    (fp_text value 10uF (at 1.25 3.56 270) (layer F.Fab))
    (fp_text user %R (at 0.775 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /V3))
    (pad 2 thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_A-405_P10.16mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 120.65 151.13)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference F2 (at 5.08 -2.41) (layer F.SilkS))
    (fp_text value "Fuse 0.5A" (at 5.08 2.41) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 30 "Net-(F2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 /L))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_THT:D_A-405_P10.16mm_Horizontal (layer F.Cu) (tedit 5954C876)
    (at 120.65 156.21)
    (descr "D, A-405 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/A-405.pdf")
    (tags "D A-405 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference F3 (at 5.08 -2.41) (layer F.SilkS))
    (fp_text value "Fuse 3A" (at 5.08 2.41) (layer F.Fab))
    (fp_text user %R (at 5.08 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 32 /COMMON_L))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 31 /L))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_A-405_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Varistors:RV_Disc_D12_W4_P7.5 (layer F.Cu) (tedit 5954C9D2)
    (at 142.24 144.78 90)
    (tags "varistor SIOV")
    (fp_text reference RV1 (at 11.43 1.27 180) (layer F.SilkS))
    (fp_text value Varistor (at 3.81 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(F2-Pad1)"))
    (pad 2 thru_hole circle (at 7.5 1.45 90) (size 1.8 1.8) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 /N))
  )
  (gr_text RFM69 (at 91.44 68.58) (layer F.SilkS))
  (gr_text Close (at 112.776 155.448 90) (layer F.SilkS))
  (gr_text Open (at 101.092 157.48 90) (layer F.SilkS))
  (gr_text N (at 146.05 157.48) (layer F.SilkS))
  (gr_text L (at 133.35 157.48) (layer F.SilkS))
  (gr_text Close (at 160.02 153.67 90) (layer F.SilkS))
  (gr_text Open (at 147.32 153.67 90) (layer F.SilkS))
  (gr_line (start 132.08 148.59) (end 129.54 148.59) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 132.08 142.24) (end 132.08 148.59) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.54 142.24) (end 132.08 142.24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 129.54 148.59) (end 129.54 142.24) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80.01 158.75) (end 80.01 59.69) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.34 158.75) (end 80.01 158.75) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.34 59.69) (end 180.34 158.75) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 80.01 59.69) (end 180.34 59.69) (angle 90) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80.01 59.69) (xy 81.28 144.78) (xy 88.9 143.51) (xy 88.9 135.89) (xy 104.14 135.89)
        (xy 105.41 132.08) (xy 105.41 128.27) (xy 109.22 125.73) (xy 111.76 125.73) (xy 118.11 127)
        (xy 140.97 127) (xy 143.51 127) (xy 146.05 134.62) (xy 149.86 133.35) (xy 149.86 125.73)
        (xy 156.21 127) (xy 162.56 129.54) (xy 162.56 138.43) (xy 162.56 140.97) (xy 165.1 143.51)
        (xy 166.37 140.97) (xy 167.64 135.89) (xy 180.34 137.16) (xy 180.34 132.08) (xy 179.07 59.69)
      )
    )
  )
)
