(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 32)
    (no_connects 0)
    (area 130.734999 84.379999 153.110001 104.850001)
    (thickness 1.6)
    (drawings 26)
    (tracks 156)
    (zones 0)
    (modules 18)
    (nets 14)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 130.81 104.775)
    (grid_origin 130.81 104.775)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad1)")
  (net 5 "Net-(J3-Pad2)")
  (net 6 "Net-(J4-Pad1)")
  (net 7 "Net-(J4-Pad2)")
  (net 8 "Net-(JP1-Pad2)")
  (net 9 "Net-(JP2-Pad2)")
  (net 10 "Net-(J4-Pad5)")
  (net 11 "Net-(J4-Pad6)")
  (net 12 "Net-(J4-Pad4)")
  (net 13 "Net-(J4-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad3)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(JP1-Pad2)")
    (add_net "Net-(JP2-Pad2)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm (layer B.Cu) (tedit 59650532)
    (at 133.35 87.63 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (fp_text reference J4 (at 0 2.33 180) (layer B.SilkS))
    (fp_text value CONN_01X06 (at 0 -15.03 180) (layer B.Fab))
    (fp_text user %R (at 0 -6.35 450) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J4-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J4-Pad3)"))
    (pad 4 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J4-Pad4)"))
    (pad 5 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J4-Pad5)"))
    (pad 6 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J4-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_2pol (layer F.Cu) (tedit 59A2D1B5)
    (at 147.955 99.695)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J1 (at 3.429 -4.064) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x02 (at 1.27 4.50088) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_2pol.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer B.Cu) (tedit 59A35ADC)
    (at 145.415 90.17 270)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C1 (at -2.286 -1.905 360) (layer B.SilkS))
    (fp_text value 10u (at 0 -2 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.5 0 270) (size 1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 59A2BE38)
    (at 137.16 90.805 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.27 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_2pol (layer F.Cu) (tedit 59A2D1B7)
    (at 141.605 99.695)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J2 (at 3.429 -4.064) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x02 (at 1.27 4.50088) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_2pol.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer B.Cu) (tedit 59A35B15)
    (at 148.59 95.25)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J3 (at 0.635 -7.0485) (layer B.SilkS))
    (fp_text value CONN_01X03 (at 0 -7.41) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 270) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 2 thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J3-Pad2)"))
    (pad 3 thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59A2D541)
    (at 137.16 102.87 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at 2.794 -0.127 180) (layer F.SilkS))
    (fp_text value Jumper (at 0 4.87 180) (layer F.Fab))
    (fp_text user %R (at 0 1.27 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(JP1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59A2F25B)
    (at 144.145 102.235 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.413 0 180) (layer B.SilkS))
    (fp_text value 120R (at 0 -1.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(JP1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59A2DEEF)
    (at 136.525 86.995 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 1.27 450) (layer B.SilkS))
    (fp_text value 10k0 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J4-Pad2)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59A2D1A1)
    (at 136.525 93.345)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 1.905 0.254 90) (layer B.SilkS))
    (fp_text value 10k0 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(JP2-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59A2D1A5)
    (at 136.525 95.25)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 1.905 0.381 90) (layer B.SilkS))
    (fp_text value 10k0 (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J4-Pad5)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59A2DF0C)
    (at 145.415 86.36 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.905 450) (layer B.SilkS))
    (fp_text value 10k0 (at 0 -1.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J4-Pad1)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59A35AEF)
    (at 140.97 95.25)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0.381 1.524 180) (layer B.SilkS))
    (fp_text value 20k (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 59A2D19B)
    (at 141.605 93.345)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -1.905 0.254 90) (layer B.SilkS))
    (fp_text value 20k (at 0 -1.5) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer B.Cu) (tedit 59A2DF03)
    (at 140.97 88.9 270)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 3.81 360) (layer B.SilkS))
    (fp_text value MAX485E (at 0 -3.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J4-Pad2)"))
    (pad 2 smd rect (at -2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(JP2-Pad2)"))
    (pad 3 smd rect (at -2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J4-Pad5)"))
    (pad 4 smd rect (at -2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J4-Pad1)"))
    (pad 5 smd rect (at 2.7 -1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.7 -0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad1)"))
    (pad 7 smd rect (at 2.7 0.635 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 8 smd rect (at 2.7 1.905 270) (size 1.55 0.6) (layers B.Cu B.Paste B.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:GS3 (layer B.Cu) (tedit 59A2D7A2)
    (at 137.16 97.79 270)
    (descr "3-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference JP2 (at 0 -2.667 270) (layer B.SilkS))
    (fp_text value Jumper_NC_Dual (at 1.8 0 540) (layer B.Fab))
    (pad 1 smd rect (at 0 1.27 270) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J4-Pad5)"))
    (pad 2 smd rect (at 0 0 270) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(JP2-Pad2)"))
    (pad 3 smd rect (at 0 -1.27 270) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J4-Pad6)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer B.Cu) (tedit 59A2D1ED)
    (at 133.35 102.87)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP1 (at 1.778 0.127 90) (layer B.SilkS))
    (fp_text value TEST (at 0 -2) (layer B.Fab))
    (pad 1 smd circle (at 0 0) (size 1.5 1.5) (layers B.Cu B.Mask)
      (net 12 "Net-(J4-Pad4)"))
  )
  (module Symbols:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 144.78 95.631 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (gr_text NC (at 151.3205 92.71 90) (layer B.SilkS))
  (gr_text NC (at 135.6995 95.3135 90) (layer F.SilkS))
  (gr_text ENI (at 131.572 100.33 90) (layer F.SilkS))
  (gr_text NC (at 135.763 92.7735 90) (layer F.SilkS))
  (gr_text ENO (at 131.572 97.79 90) (layer F.SilkS))
  (gr_text RX (at 135.763 90.297 90) (layer F.SilkS))
  (gr_text TX (at 135.6995 87.6935 90) (layer F.SilkS))
  (gr_text GND (at 151.257 89.662 90) (layer B.SilkS))
  (gr_text +5V (at 151.257 95.631 90) (layer B.SilkS))
  (gr_text 2017-08-27 (at 213.868 193.04) (layer Dwgs.User))
  (gr_text "RS485 - MAX485 breakout board" (at 205.867 189.611) (layer Dwgs.User))
  (gr_text V1.1 (at 270.891 193.167) (layer Dwgs.User))
  (gr_line (start 130.81 84.455) (end 130.81 104.775) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.035 84.455) (end 130.81 84.455) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.035 104.775) (end 153.035 84.455) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 130.81 104.775) (end 153.035 104.775) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 20.32 (width 0.3) (layer Dwgs.User)
    (gr_text "20,320 mm" (at 158.195 94.615 270) (layer Dwgs.User))
    (feature1 (pts (xy 153.035 104.775) (xy 159.545 104.775)))
    (feature2 (pts (xy 153.035 84.455) (xy 159.545 84.455)))
    (crossbar (pts (xy 156.845 84.455) (xy 156.845 104.775)))
    (arrow1a (pts (xy 156.845 104.775) (xy 156.258579 103.648496)))
    (arrow1b (pts (xy 156.845 104.775) (xy 157.431421 103.648496)))
    (arrow2a (pts (xy 156.845 84.455) (xy 156.258579 85.581504)))
    (arrow2b (pts (xy 156.845 84.455) (xy 157.431421 85.581504)))
  )
  (gr_text Term (at 137.16 97.79) (layer F.SilkS))
  (gr_text "RS485\nArduino\nPro mini\nV1.1" (at 141.5415 90.17) (layer F.SilkS))
  (gr_text B (at 150.495 103.759) (layer F.SilkS))
  (gr_text A (at 147.955 103.759) (layer F.SilkS))
  (gr_text B (at 144.145 103.759) (layer F.SilkS))
  (gr_text A (at 141.605 103.759) (layer F.SilkS))
  (dimension 22.098 (width 0.3) (layer Dwgs.User)
    (gr_text "22,098 mm" (at 141.859 73.199) (layer Dwgs.User))
    (feature1 (pts (xy 152.908 83.185) (xy 152.908 71.849)))
    (feature2 (pts (xy 130.81 83.185) (xy 130.81 71.849)))
    (crossbar (pts (xy 130.81 74.549) (xy 152.908 74.549)))
    (arrow1a (pts (xy 152.908 74.549) (xy 151.781496 75.135421)))
    (arrow1b (pts (xy 152.908 74.549) (xy 151.781496 73.962579)))
    (arrow2a (pts (xy 130.81 74.549) (xy 131.936504 75.135421)))
    (arrow2b (pts (xy 130.81 74.549) (xy 131.936504 73.962579)))
  )
  (dimension 15.24 (width 0.3) (layer Dwgs.User)
    (gr_text "15,240 mm" (at 140.97 78.025) (layer Dwgs.User))
    (feature1 (pts (xy 148.59 87.63) (xy 148.59 76.675)))
    (feature2 (pts (xy 133.35 87.63) (xy 133.35 76.675)))
    (crossbar (pts (xy 133.35 79.375) (xy 148.59 79.375)))
    (arrow1a (pts (xy 148.59 79.375) (xy 147.463496 79.961421)))
    (arrow1b (pts (xy 148.59 79.375) (xy 147.463496 78.788579)))
    (arrow2a (pts (xy 133.35 79.375) (xy 134.476504 79.961421)))
    (arrow2b (pts (xy 133.35 79.375) (xy 134.476504 78.788579)))
  )
  (zone (net 1) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.97 93.98) (xy 140.97 97.79) (xy 135.89 97.79) (xy 135.89 90.805) (xy 140.335 90.805)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.81 83.185) (xy 153.035 83.185) (xy 153.035 104.775) (xy 130.81 104.775)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.035 104.775) (xy 130.81 104.775) (xy 130.81 88.9) (xy 130.81 83.185) (xy 153.035 83.185)
      )
    )
    (polygon
      (pts        (xy 142.24 98.425) (xy 142.24 90.17) (xy 136.525 90.17) (xy 136.525 88.9) (xy 134.62 88.9)
        (xy 134.62 98.425)
      )
    )
  )
)
