(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 72)
    (no_connects 0)
    (area 115.924999 101.424999 181.075001 131.575001)
    (thickness 1.6)
    (drawings 51)
    (tracks 430)
    (zones 0)
    (modules 29)
    (nets 49)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 1)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerber/))
  )
  (net 0 "")
  (net 1 /L_ERR)
  (net 2 "Net-(D1-Pad2)")
  (net 3 /L_RX)
  (net 4 "Net-(D2-Pad2)")
  (net 5 /L_TX)
  (net 6 "Net-(D3-Pad2)")
  (net 7 GND)
  (net 8 /ANT)
  (net 9 "Net-(J2-Pad1)")
  (net 10 "Net-(J2-Pad3)")
  (net 11 "Net-(J2-Pad5)")
  (net 12 "Net-(J2-Pad7)")
  (net 13 "Net-(J2-Pad8)")
  (net 14 "Net-(J2-Pad10)")
  (net 15 "Net-(J2-Pad11)")
  (net 16 "Net-(J2-Pad13)")
  (net 17 /IRQ)
  (net 18 +3V3)
  (net 19 /MOSI)
  (net 20 /MISO)
  (net 21 /CE)
  (net 22 /SCLK)
  (net 23 /CS0)
  (net 24 "Net-(J2-Pad26)")
  (net 25 "Net-(J2-Pad27)")
  (net 26 "Net-(J2-Pad28)")
  (net 27 "Net-(U1-Pad1)")
  (net 28 "Net-(U1-Pad3)")
  (net 29 "Net-(U1-Pad4)")
  (net 30 "Net-(U1-Pad5)")
  (net 31 "Net-(U1-Pad6)")
  (net 32 "Net-(U1-Pad7)")
  (net 33 "Net-(U1-Pad16)")
  (net 34 "Net-(J3-Pad1)")
  (net 35 +5V)
  (net 36 "Net-(J2-Pad17)")
  (net 37 /IRQ_1)
  (net 38 /MISO_1)
  (net 39 /CS0_1)
  (net 40 /CE_1)
  (net 41 /MOSI_1)
  (net 42 /SCLK_1)
  (net 43 /L_ERR_1)
  (net 44 "Net-(D4-Pad2)")
  (net 45 /L_RX_1)
  (net 46 "Net-(D5-Pad2)")
  (net 47 /L_TX_1)
  (net 48 "Net-(D6-Pad2)")
  (net_class Default "Ceci est la Netclass par défaut"
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /CE)
    (add_net /CE_1)
    (add_net /CS0)
    (add_net /CS0_1)
    (add_net /IRQ)
    (add_net /IRQ_1)
    (add_net /L_ERR)
    (add_net /L_ERR_1)
    (add_net /L_RX)
    (add_net /L_RX_1)
    (add_net /L_TX)
    (add_net /L_TX_1)
    (add_net /MISO)
    (add_net /MISO_1)
    (add_net /MOSI)
    (add_net /MOSI_1)
    (add_net /SCLK)
    (add_net /SCLK_1)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad2)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad17)")
    (add_net "Net-(J2-Pad26)")
    (add_net "Net-(J2-Pad27)")
    (add_net "Net-(J2-Pad28)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad7)")
    (add_net "Net-(J2-Pad8)")
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
  )
  (net_class ant ""
    (clearance 0.2)
    (trace_width 2.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ANT)
    (add_net "Net-(J3-Pad1)")
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
  )
  (module Symbols:KiCad-Logo2_6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 132.4 119.5 180)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module _LaurentPerso:RaspberryPiZeroHAT (layer F.Cu) (tedit 59D53C92)
    (at 148.5011 105.0036)
    (fp_text reference J2 (at 26.1989 -2.1036) (layer F.SilkS) hide)
    (fp_text value CONN_02X20 (at 22.4989 -2.7036) (layer F.Fab))
    (pad 1 thru_hole circle (at -24.13 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at -24.13 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 +5V))
    (pad 3 thru_hole circle (at -21.59 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(J2-Pad3)"))
    (pad 4 thru_hole circle (at -21.59 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 35 +5V))
    (pad 5 thru_hole circle (at -19.05 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(J2-Pad5)"))
    (pad 6 thru_hole circle (at -19.05 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 7 thru_hole circle (at -16.51 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(J2-Pad7)"))
    (pad 8 thru_hole circle (at -16.51 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad8)"))
    (pad 9 thru_hole circle (at -13.97 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 10 thru_hole circle (at -13.97 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad10)"))
    (pad 11 thru_hole circle (at -11.43 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(J2-Pad11)"))
    (pad 12 thru_hole circle (at -11.43 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 /L_ERR))
    (pad 13 thru_hole circle (at -8.89 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(J2-Pad13)"))
    (pad 14 thru_hole circle (at -8.89 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 15 thru_hole circle (at -6.35 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 17 /IRQ))
    (pad 16 thru_hole circle (at -6.35 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 /L_RX))
    (pad 17 thru_hole circle (at -3.81 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 36 "Net-(J2-Pad17)"))
    (pad 18 thru_hole circle (at -3.81 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 /L_TX))
    (pad 19 thru_hole circle (at -1.27 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 19 /MOSI))
    (pad 20 thru_hole circle (at -1.27 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 21 thru_hole circle (at 1.27 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 20 /MISO))
    (pad 22 thru_hole circle (at 1.27 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 21 /CE))
    (pad 23 thru_hole circle (at 3.81 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 22 /SCLK))
    (pad 24 thru_hole circle (at 3.81 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 23 /CS0))
    (pad 25 thru_hole circle (at 6.35 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 26 thru_hole circle (at 6.35 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad26)"))
    (pad 27 thru_hole circle (at 8.89 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad27)"))
    (pad 28 thru_hole circle (at 8.89 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 26 "Net-(J2-Pad28)"))
    (pad 29 thru_hole circle (at 11.43 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 43 /L_ERR_1))
    (pad 30 thru_hole circle (at 11.43 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 31 thru_hole circle (at 13.97 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 45 /L_RX_1))
    (pad 32 thru_hole circle (at 13.97 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 47 /L_TX_1))
    (pad 33 thru_hole circle (at 16.51 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 37 /IRQ_1))
    (pad 34 thru_hole circle (at 16.51 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 35 thru_hole circle (at 19.05 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 38 /MISO_1))
    (pad 36 thru_hole circle (at 19.05 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 39 /CS0_1))
    (pad 37 thru_hole circle (at 21.59 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 40 /CE_1))
    (pad 38 thru_hole circle (at 21.59 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 41 /MOSI_1))
    (pad 39 thru_hole circle (at 24.13 1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 40 thru_hole circle (at 24.13 -1.27) (size 1.524 1.524) (drill 0.9) (layers *.Cu *.Mask)
      (net 42 /SCLK_1))
    (pad "" np_thru_hole circle (at -29 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.72) (clearance 1.72))
    (pad "" np_thru_hole circle (at 29 0) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.72) (clearance 1.72))
    (pad "" np_thru_hole circle (at 29 23) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.72) (clearance 1.72))
    (pad "" np_thru_hole circle (at -29 23) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.72) (clearance 1.72))
  )
  (module mysensors_radios:NRF24L01 (layer F.Cu) (tedit 59D53D89)
    (at 145 124 270)
    (descr NRF24L01)
    (tags "nRF 24 NRF24L01 NRF24L01+")
    (fp_text reference U2 (at -0.8 -1 360) (layer F.SilkS))
    (fp_text value "NRF24L01 SPI0" (at -4.8 5.9 270) (layer F.SilkS))
    (pad 7 thru_hole oval (at -9.144 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 /MISO))
    (pad 8 thru_hole oval (at -9.144 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 /IRQ))
    (pad 5 thru_hole oval (at -6.604 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 /SCLK))
    (pad 6 thru_hole oval (at -6.604 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 /MOSI))
    (pad 3 thru_hole oval (at -4.064 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 /CE))
    (pad 4 thru_hole oval (at -4.064 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 /CS0))
    (pad 1 thru_hole rect (at -1.524 1.524 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 2 thru_hole oval (at -1.524 4.064 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0.442))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/nrf24l01.wrl
      (at (xyz -0.3 -0.5669999999999999 0.475))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz -0.22 -0.51 0.509))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_hc-49s.wrl
      (at (xyz -0.5 -0.475 0.51))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 59D5394F)
    (at 158 130)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D1 (at 0.1 0) (layer F.SilkS) hide)
    (fp_text value ERR (at -4 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 /L_ERR))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 59D5395A)
    (at 165 130)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value RX (at -3.5 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 /L_RX))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 59D539EA)
    (at 172 130)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D3 (at 0 0.1) (layer F.SilkS) hide)
    (fp_text value TX (at -3.5 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /L_TX))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:SMA_THT_Jack_Straight (layer F.Cu) (tedit 59A86F46)
    (at 129.5 127)
    (descr "SMA pcb through hole jack")
    (tags "SMA THT Jack Straight")
    (fp_text reference J1 (at 0.05 -2.4) (layer F.SilkS))
    (fp_text value ANT (at -5.6 3) (layer F.SilkS))
    (fp_text user %R (at 0 -5) (layer F.Fab))
    (pad 2 thru_hole circle (at -2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 2 thru_hole circle (at 2.54 2.54) (size 2.2 2.2) (drill 1.7) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 1 thru_hole circle (at 0 0) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (net 8 /ANT))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59D53A5A)
    (at 158 128.15)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -3.2 -0.1) (layer F.SilkS))
    (fp_text value 470 (at 0 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59D53A53)
    (at 165 128.1)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -3.3 -0.1) (layer F.SilkS))
    (fp_text value 470 (at 0 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59D53A7A)
    (at 172 128.1)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at -3.2 -0.1) (layer F.SilkS))
    (fp_text value 470 (at 0 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59A86E2C)
    (at 128 127)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 1 1.5) (layer F.SilkS))
    (fp_text value 0 (at 0.1 0.1) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J3-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /ANT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors:PINTST (layer F.Cu) (tedit 59D62E6D)
    (at 123.95 127)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference J3 (at -0.2 1.7) (layer F.SilkS))
    (fp_text value CONN_01X01 (at -2.65 3.7) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J3-Pad1)"))
    (model ${KISYS3DMOD}/Connectors.3dshapes/PINTST.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_obscurities:MySensors-logo-sticker-large (layer F.Cu) (tedit 0)
    (at 164.55 114.1)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Symbols:OSHW-Logo_5.7x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 136.2 112.1 180)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo_5.7x6mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (module mysensors_radios:RFM69HW_SMD_Handsoldering (layer F.Cu) (tedit 59D53BD5)
    (at 150 111 270)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U1 (at 0.8 -0.2 360) (layer F.SilkS))
    (fp_text value RFM69HW (at 8.382 7.112 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad1)"))
    (pad 2 smd rect (at -1.4 2 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 /CE))
    (pad 3 smd rect (at -1.4 4 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U1-Pad3)"))
    (pad 4 smd rect (at -1.4 6 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U1-Pad4)"))
    (pad 5 smd rect (at -1.4 8 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U1-Pad5)"))
    (pad 6 smd rect (at -1.4 10 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U1-Pad6)"))
    (pad 7 smd rect (at -1.4 12 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(U1-Pad7)"))
    (pad 8 smd rect (at -1.4 14 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 9 smd rect (at 18.3 14 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 10 smd rect (at 18.3 12 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 /ANT))
    (pad 11 smd rect (at 18.3 10 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (pad 12 smd rect (at 18.3 8 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 /SCLK))
    (pad 13 smd rect (at 18.3 6 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 /MISO))
    (pad 14 smd rect (at 18.3 4 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 /MOSI))
    (pad 15 smd rect (at 18.3 2 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 /CS0))
    (pad 16 smd rect (at 18.3 0 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(U1-Pad16)"))
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/rfm69hw.wrl
      (at (xyz 0.332 -0.275 0.03))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals.3dshapes/crystal_FA238-TSX3225.wrl
      (at (xyz 0.332 -0.08 0.06))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (at (xyz 0.204 -0.445 0.06))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59A87157)
    (at 131.4 108.6)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 2.8 -0.4) (layer F.SilkS))
    (fp_text value 10u (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 35 +5V))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59A87524)
    (at 127.8 108.6 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 2.8 0.4 180) (layer F.SilkS))
    (fp_text value 100n (at 0.1 0.1 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 35 +5V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59A871CA)
    (at 131.4 117.4)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 2.6 0) (layer F.SilkS))
    (fp_text value 10u (at 0 0) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59A871D4)
    (at 127.8 117.4 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 1 1.2 180) (layer F.SilkS))
    (fp_text value 100n (at 0 0 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 59A87179)
    (at 130 113 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U3 (at 3.2 2.8 180) (layer F.SilkS))
    (fp_text value AP1117 (at 0.8 0 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 4 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 35 +5V))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59D53D0C)
    (at 159.5 109.6 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 1.7 -1.8 180) (layer F.SilkS))
    (fp_text value 10u (at 0.1 0 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 59D53D01)
    (at 161.4 109.6 90)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 1.7 1.6 180) (layer F.SilkS))
    (fp_text value 100n (at 0 0 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 90) (layer F.Fab))
    (pad 1 smd rect (at -1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1 0 90) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_radios:NRF24L01 (layer F.Cu) (tedit 59D53D71)
    (at 152.1 108.8 90)
    (descr NRF24L01)
    (tags "nRF 24 NRF24L01 NRF24L01+")
    (fp_text reference U4 (at 0.7 0.7 180) (layer F.SilkS))
    (fp_text value "NRF24L01 SPI1" (at -5.9 -0.4 90) (layer F.SilkS))
    (pad 7 thru_hole oval (at -9.144 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 /MISO_1))
    (pad 8 thru_hole oval (at -9.144 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 /IRQ_1))
    (pad 5 thru_hole oval (at -6.604 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 /SCLK_1))
    (pad 6 thru_hole oval (at -6.604 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 /MOSI_1))
    (pad 3 thru_hole oval (at -4.064 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 /CE_1))
    (pad 4 thru_hole oval (at -4.064 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 /CS0_1))
    (pad 1 thru_hole rect (at -1.524 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 2 thru_hole oval (at -1.524 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 +3V3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x04.wrl
      (at (xyz -0.21 -0.11 0.442))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/nrf24l01.wrl
      (at (xyz -0.3 -0.5669999999999999 0.475))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 0))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_Pitch0.5mm.wrl
      (at (xyz -0.22 -0.51 0.509))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_hc-49s.wrl
      (at (xyz -0.5 -0.475 0.51))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 59D54BF0)
    (at 158 126.3)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D4 (at -0.1 0.05) (layer F.SilkS) hide)
    (fp_text value ERR (at -3.95 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 43 /L_ERR_1))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 59D54C29)
    (at 165 126.25)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D5 (at 0 0.05) (layer F.SilkS) hide)
    (fp_text value RX (at -3.5 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 45 /L_RX_1))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805_HandSoldering (layer F.Cu) (tedit 59D54C2F)
    (at 172 126.25)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference D6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value TX (at -3.45 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 47 /L_TX_1))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59D54C36)
    (at 158 124.45)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -3.25 0) (layer F.SilkS))
    (fp_text value 470 (at -0.05 0.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59D54C3C)
    (at 165 124.4)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -3.2 0) (layer F.SilkS))
    (fp_text value 470 (at 0 0.05) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59D54C44)
    (at 170.55 122.9 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 1.75 -1.85 360) (layer F.SilkS))
    (fp_text value 470 (at -0.2 -0.1 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(D6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 181 124) (end 181 128) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181 105) (end 181 109) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 172.5 109.5) (end 172 109.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 172.5 123.5) (end 172.5 124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 172 109.5) (end 172 123.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181 124) (end 172.5 124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 181 109) (end 172.5 109) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text v3 (at 136.6 130) (layer B.SilkS))
  (gr_text "433Mhz\n868Mhz\n915Mhz" (at 128 120.8) (layer F.SilkS))
  (gr_text "Designed by Laurent Le Goff (2017)\n(http://github.com/llegoff)" (at 158.6 127.8) (layer B.SilkS))
  (gr_text "RFMHW69\n" (at 150.2 127 90) (layer F.SilkS))
  (gr_text Gateway (at 164.35 121.65) (layer F.SilkS))
  (gr_arc (start 124.5 123.5) (end 125 123.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 124.5 109.5) (end 124.5 109) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 124.5 109) (end 116 109) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 125 123.5) (end 125 109.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116 124) (end 124.5 124) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 119.5 105) (end 116 105) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 119.5 128) (end 119.5 131.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 177.5 128) (end 181 128) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 177.5 105) (end 177.5 101.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 177.5 131.5) (end 119.5 131.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.5 101.5) (end 177.5 101.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116 124) (end 116 128) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116 105) (end 116 109) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116 101.5) (xy 181 101.5) (xy 181 131.5) (xy 116 131.5)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116 101.5) (xy 181 101.5) (xy 181 131.5) (xy 116 131.5)
      )
    )
  )
)
