(kicad_pcb (version 20170922) (host pcbnew no-vcs-found-72d4889~60~ubuntu16.04.1)
(general
  (thickness 1.6)
  (drawings 36)
  (tracks 379)
  (zones 0)
  (modules 42)
  (nets 45)
)
(page A4)
(layers
  (0 F.Cu signal)
  (31 B.Cu signal)
  (32 B.Adhes user)
  (33 F.Adhes user)
  (34 B.Paste user)
  (35 F.Paste user)
  (36 B.SilkS user)
  (37 F.SilkS user)
  (38 B.Mask user)
  (39 F.Mask user)
  (40 Dwgs.User user hide)
  (41 Cmts.User user)
  (42 Eco1.User user)
  (43 Eco2.User user)
  (44 Edge.Cuts user)
  (45 Margin user)
  (46 B.CrtYd user)
  (47 F.CrtYd user)
  (48 B.Fab user)
  (49 F.Fab user)
)
(setup
  (last_trace_width 0.3)
  (trace_clearance 0.3)
  (zone_clearance 0.45)
  (zone_45_only no)
  (trace_min 0.2)
  (segment_width 0.2)
  (edge_width 0.1)
  (via_size 0.8)
  (via_drill 0.4)
  (via_min_size 0.4)
  (via_min_drill 0.3)
  (uvia_size 0.3)
  (uvia_drill 0.1)
  (uvias_allowed no)
  (uvia_min_size 0.2)
  (uvia_min_drill 0.1)
  (pcb_text_width 0.3)
  (pcb_text_size 1.5 1.5)
  (mod_edge_width 0.15)
  (mod_text_size 0.5 0.5)
  (mod_text_width 0.1)
  (pad_size 1.5 1.5)
  (pad_drill 0.6)
  (pad_to_mask_clearance 0)
  (aux_axis_origin 0 0)
  (visible_elements 7FFFFF7F)
  (pcbplotparams
    (layerselection 0x010fc_ffffffff)
    (usegerberextensions true)
    (usegerberattributes true)
    (usegerberadvancedattributes true)
    (creategerberjobfile true)
    (excludeedgelayer true)
    (linewidth 0.100000)
    (plotframeref false)
    (viasonmask false)
    (mode 1)
    (useauxorigin false)
    (hpglpennumber 1)
    (hpglpenspeed 20)
    (hpglpendiameter 15)
    (psnegative false)
    (psa4output false)
    (plotreference true)
    (plotvalue true)
    (plotinvisibletext false)
    (padsonsilk false)
    (subtractmaskfromsilk true)
    (outputformat 1)
    (mirror false)
    (drillshape 0)
    (scaleselection 1)
    (outputdirectory gerber/))
)
(net 0 "")
(net 1 +3V3)
(net 2 GND)
(net 3 "Net-(C7-Pad1)")
(net 4 "Net-(C9-Pad2)")
(net 5 "Net-(C9-Pad1)")
(net 6 /12Vcc)
(net 7 "Net-(D3-Pad2)")
(net 8 "Net-(D4-Pad1)")
(net 9 "Net-(D5-Pad1)")
(net 10 "Net-(D6-Pad2)")
(net 11 /TS2)
(net 12 /S2_LEDs)
(net 13 /TS1)
(net 14 /S1_LEDs)
(net 15 "Net-(R1-Pad1)")
(net 16 /Relay2_Reset)
(net 17 /Relay1_Reset)
(net 18 /Relay2_Set)
(net 19 /Relay1_Set)
(net 20 /SWCLK)
(net 21 /SWDIO)
(net 22 "Net-(C4-Pad2)")
(net 23 "Net-(R3-Pad2)")
(net 24 "Net-(R3-Pad1)")
(net 25 "Net-(R4-Pad1)")
(net 26 "Net-(R4-Pad2)")
(net 27 "Net-(R9-Pad2)")
(net 28 "Net-(R10-Pad2)")
(net 29 "Net-(R10-Pad1)")
(net 30 /MTSA)
(net 31 /MTPM)
(net 32 "Net-(J2-Pad1)")
(net 33 "Net-(P4-Pad14)")
(net 34 "Net-(P4-Pad12)")
(net 35 "Net-(P4-Pad10)")
(net 36 "Net-(P4-Pad9)")
(net 37 "Net-(P4-Pad8)")
(net 38 "Net-(P4-Pad7)")
(net 39 "Net-(P4-Pad1)")
(net 40 "Net-(U5-Pad11)")
(net 41 "Net-(U7-Pad9)")
(net 42 "Net-(U7-Pad8)")
(net 43 "Net-(U7-Pad7)")
(net 44 "Net-(U7-Pad6)")
(net_class Default "This is the default net class."
  (clearance 0.3)
  (trace_width 0.3)
  (via_dia 0.8)
  (via_drill 0.4)
  (uvia_dia 0.3)
  (uvia_drill 0.1)
  (add_net +3V3)
  (add_net /12Vcc)
  (add_net /MTPM)
  (add_net /MTSA)
  (add_net /Relay1_Reset)
  (add_net /Relay1_Set)
  (add_net /Relay2_Reset)
  (add_net /Relay2_Set)
  (add_net /S1_LEDs)
  (add_net /S2_LEDs)
  (add_net /SWCLK)
  (add_net /SWDIO)
  (add_net /TS1)
  (add_net /TS2)
  (add_net GND)
  (add_net "Net-(C4-Pad2)")
  (add_net "Net-(C7-Pad1)")
  (add_net "Net-(C9-Pad1)")
  (add_net "Net-(C9-Pad2)")
  (add_net "Net-(D3-Pad2)")
  (add_net "Net-(D4-Pad1)")
  (add_net "Net-(D5-Pad1)")
  (add_net "Net-(D6-Pad2)")
  (add_net "Net-(J2-Pad1)")
  (add_net "Net-(P4-Pad1)")
  (add_net "Net-(P4-Pad10)")
  (add_net "Net-(P4-Pad12)")
  (add_net "Net-(P4-Pad14)")
  (add_net "Net-(P4-Pad7)")
  (add_net "Net-(P4-Pad8)")
  (add_net "Net-(P4-Pad9)")
  (add_net "Net-(R1-Pad1)")
  (add_net "Net-(R10-Pad1)")
  (add_net "Net-(R10-Pad2)")
  (add_net "Net-(R3-Pad1)")
  (add_net "Net-(R3-Pad2)")
  (add_net "Net-(R4-Pad1)")
  (add_net "Net-(R4-Pad2)")
  (add_net "Net-(R9-Pad2)")
  (add_net "Net-(U5-Pad11)")
  (add_net "Net-(U7-Pad6)")
  (add_net "Net-(U7-Pad7)")
  (add_net "Net-(U7-Pad8)")
  (add_net "Net-(U7-Pad9)")
)
  (module Symbols:KiCad-Logo2_6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 124.5 84.5 90)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0 90) (layer F.Fab) hide)
  )
  (module myfootprints:PTR5518 (layer F.Cu) (tedit 5964C9D8)
    (at 142.6294 79.8332)
    (attr smd)
    (fp_text reference U5 (at -0.4826 0.4572) (layer F.SilkS))
    (fp_text value PTR5518 (at -0.3294 1.3668) (layer F.SilkS))
    (pad 15 smd rect (at -8.1294 4.8768 270) (size 0.8128 2) (layers F.Cu F.Paste F.Mask)
      (net 16 /Relay2_Reset))
    (pad 1 smd rect (at 7.3166 4.8768 270) (size 0.8128 2) (layers F.Cu F.Paste F.Mask)
      (net 11 /TS2))
    (pad 14 smd rect (at -8.1294 3.6068 270) (size 0.8128 2) (layers F.Cu F.Paste F.Mask)
      (net 18 /Relay2_Set))
    (pad 2 smd rect (at 7.3166 3.6068 270) (size 0.8128 2) (layers F.Cu F.Paste F.Mask)
      (net 13 /TS1))
    (pad 13 smd rect (at -8.1294 2.3368 270) (size 0.8128 2) (layers F.Cu F.Paste F.Mask)
      (net 17 /Relay1_Reset))
    (pad 3 smd rect (at 7.3166 2.3368 270) (size 0.8128 2) (layers F.Cu F.Paste F.Mask)
      (net 31 /MTPM))
    (pad 12 smd rect (at -8.1294 1.0668 270) (size 0.8128 2) (layers F.Cu F.Paste F.Mask)
      (net 19 /Relay1_Set))
    (pad 4 smd rect (at 7.3166 1.0668 270) (size 0.8128 2) (layers F.Cu F.Paste F.Mask)
      (net 21 /SWDIO))
    (pad 11 smd rect (at -8.1294 -0.2032 270) (size 0.8128 2) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(U5-Pad11)"))
    (pad 5 smd rect (at 7.3166 -0.2032 270) (size 0.8128 2) (layers F.Cu F.Paste F.Mask)
      (net 20 /SWCLK))
    (pad 10 smd rect (at -8.1294 -1.4732 270) (size 0.8128 2) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 6 smd rect (at 7.3166 -1.4732 270) (size 0.8128 2) (layers F.Cu F.Paste F.Mask)
      (net 30 /MTSA))
    (pad 9 smd rect (at -8.1294 -2.7432 270) (size 0.8128 2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 7.3166 -2.7432 270) (size 0.8128 2) (layers F.Cu F.Paste F.Mask)
      (net 14 /S1_LEDs))
    (pad 8 smd rect (at 7.3166 -4.0132 270) (size 0.8128 2) (layers F.Cu F.Paste F.Mask)
      (net 12 /S2_LEDs))
    (model ${KISYS3DMOD}/Radio_Modules.3dshapes/PTR5518.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5964C74D)
    (at 147.1 100.8)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -0.5 1.1) (layer F.SilkS))
    (fp_text value 4K7 (at 0.9 1.1) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5964C720)
    (at 147.1 99.2)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 -1.1) (layer F.SilkS))
    (fp_text value 0 (at 0 0) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R3-Pad2)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(R9-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5964C64D)
    (at 136.85 100.7)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -1.1 1.4) (layer F.SilkS))
    (fp_text value 4K7 (at 0.6 1.4) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(R10-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R10-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5964C66A)
    (at 136.85 99.1)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.1) (layer F.SilkS))
    (fp_text value 0 (at 0 0) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02_Pitch2.00mm_SMD (layer F.Cu) (tedit 594A0E13)
    (at 156.275 80.6)
    (descr "surface-mounted straight pin header, 2x02, 2.00mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x02 2.00mm double row")
    (attr smd)
    (fp_text reference J1 (at -0.775 -2.9) (layer F.SilkS))
    (fp_text value SWD (at 0.525 -2.9) (layer F.SilkS))
    (fp_text user %R (at 0 -3.06) (layer F.Fab) hide)
    (pad 4 smd rect (at 3.125 1) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3 smd rect (at -3.125 1) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 21 /SWDIO))
    (pad 2 smd rect (at 3.125 -1) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -3.125 -1) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 20 /SWCLK))
  )
  (module myfootprints:Livolo_EU_SW_2_Channel_1Way_Frame_VL-C702X-2_Ver_C1 locked (layer B.Cu) (tedit 590C6ABA)
    (at 142.3 92.4 180)
    (fp_text reference REF** (at -0.3 -0.5 180) (layer B.SilkS) hide)
    (fp_text value Livolo_EU_SW_2Ways_Frame_VL-C702X-2_Ver_C1 (at 0 0.5 180) (layer B.Fab) hide)
  )
  (module myfootprints:VLCF4020T-150MR68 (layer F.Cu) (tedit 590C5D79)
    (at 157.7 107.6)
    (fp_text reference L2 (at -1.2 3.2 -180) (layer F.SilkS))
    (fp_text value 15uH (at 0.5 3.2 -180) (layer F.SilkS))
    (pad 1 smd rect (at 0 -1.75) (size 4 2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0 1.5) (size 4 2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C9-Pad2)"))
    (model ${KISYS3DMOD}/Inductors.3dshapes/IFSC-1515AH-01_sp.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:SS14M (layer F.Cu) (tedit 58E37FED)
    (at 154.2 109.3 270)
    (fp_text reference D2 (at 2.45 -1.3) (layer F.SilkS))
    (fp_text value SS14M (at 3.3 -0.8) (layer F.SilkS))
    (pad 1 smd rect (at -1.5 0 270) (size 2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C9-Pad2)"))
    (pad 2 smd rect (at 1.5 0 270) (size 1.4 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/DO_Packages_SMD.3dshapes/DO-219AB.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 586E4F31)
    (at 145.8 108.8 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.6 -1.05 90) (layer F.SilkS))
    (fp_text value 10K (at -2.7 -0.3 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad1)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-6 (layer F.Cu) (tedit 58933BCC)
    (at 150 108.8 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U2 (at -2.3 4.25) (layer F.SilkS))
    (fp_text value MCP16301 (at -2.3 1.5 180) (layer F.SilkS))
    (pad 5 smd rect (at 1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 /12Vcc))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C9-Pad2)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 6 /12Vcc))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/SOT_Packages_SMD.3dshapes/SOT23-6.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module myfootprints:hole_1.5mm locked (layer F.Cu) (tedit 587347E2)
    (at 152.1 100.85)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole_1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module myfootprints:hole_1.5mm locked (layer F.Cu) (tedit 587347E2)
    (at 160.3 100.85)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole_1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module myfootprints:hole_1.5mm locked (layer F.Cu) (tedit 587347E2)
    (at 132.7 100.9)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole_1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module myfootprints:hole_1.5mm locked (layer F.Cu) (tedit 587347E2)
    (at 124.5 100.9)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value hole_1.5mm (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0) (size 1.5 1.5) (drill 1.5) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 586E5461)
    (at 148.8 105.3)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -0.8 -1.1) (layer F.SilkS))
    (fp_text value 22u (at 1 -1.1 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C7-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 586E52DF)
    (at 152.6 108.8 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at 4.2 -0.4 270) (layer F.SilkS))
    (fp_text value 100n (at 2.45 -0.4 270) (layer F.SilkS))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C9-Pad2)"))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C9-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 586E52DA)
    (at 153.1 105.6)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at -1.6 -2.1 180) (layer F.SilkS))
    (fp_text value 1N4148 (at -0.85 -1.35) (layer F.SilkS))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C7-Pad1)"))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/SOD_Packages_SMD.3dshapes/SOD123.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Diodes_SMD:D_0603 (layer B.Cu) (tedit 586E517C)
    (at 130.5 102.15 180)
    (descr "Diode SMD in 0603 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D3 (at -0.9 1.05 180) (layer B.SilkS))
    (fp_text value Blue (at 0.6 1.05 180) (layer B.SilkS))
    (pad 2 smd rect (at 0.85 0 180) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -0.85 0 180) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_Packages_SMD.3dshapes/led_chip_0603_blue.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer B.Cu) (tedit 586E517F)
    (at 126.85 102.15)
    (descr "Diode SMD in 0603 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D4 (at 0.9 -1.05) (layer B.SilkS))
    (fp_text value Red (at -0.6 -1.05) (layer B.SilkS))
    (pad 1 smd rect (at -0.85 0) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 0.85 0) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/LED_Packages_SMD.3dshapes/led_chip_0603_red.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer B.Cu) (tedit 586E5177)
    (at 157.95 102.15 180)
    (descr "Diode SMD in 0603 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D5 (at -0.85 1.05 180) (layer B.SilkS))
    (fp_text value Red (at 0.65 1.05 180) (layer B.SilkS))
    (pad 1 smd rect (at -0.85 0 180) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(D5-Pad1)"))
    (pad 2 smd rect (at 0.85 0 180) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/LED_Packages_SMD.3dshapes/led_chip_0603_red.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_0603 (layer B.Cu) (tedit 586E5173)
    (at 154.6 102.15)
    (descr "Diode SMD in 0603 package")
    (tags "smd diode")
    (attr smd)
    (fp_text reference D6 (at 1 -1.05) (layer B.SilkS))
    (fp_text value Blue (at -0.6 -1.05) (layer B.SilkS))
    (pad 2 smd rect (at 0.85 0) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D6-Pad2)"))
    (pad 1 smd rect (at -0.85 0) (size 0.6 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/LED_Packages_SMD.3dshapes/led_chip_0603_blue.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 586E4F9D)
    (at 147.4 108.8 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.8 -0.2 90) (layer F.SilkS))
    (fp_text value 31K6 (at -2.8 0.5 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58933CFE)
    (at 154.2 103.4 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0.7 1.2 180) (layer F.SilkS))
    (fp_text value 1K* (at -0.7 1.2 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D6-Pad2)"))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 /S1_LEDs))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58933CF9)
    (at 158.3 103.4 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 1.2 1.2) (layer F.SilkS))
    (fp_text value 1K* (at -0.2 1.2) (layer F.SilkS))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 /S1_LEDs))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58933CDD)
    (at 130.7 103.4)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -0.6 -1.2) (layer F.SilkS))
    (fp_text value 1K* (at 0.8 -1.2) (layer F.SilkS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D3-Pad2)"))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /S2_LEDs))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58933CD7)
    (at 126.6 103.4)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -0.35 -1.2 -180) (layer F.SilkS))
    (fp_text value 1K* (at 1.15 -1.2 -180) (layer F.SilkS))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 /S2_LEDs))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5964812E)
    (at 146.1 104.9 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at -0.3 -1.2 180) (layer F.SilkS))
    (fp_text value BLM18HE152SN1D (at -0.1 0.9 90) (layer F.SilkS) hide)
    (fp_text user %R (at 0 -1.45 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x07_Pitch2.00mm locked (layer F.Cu) (tedit 597883A3)
    (at 131.65 109.55 90)
    (descr "Through hole straight pin header, 2x07, 2.00mm pitch, double rows")
    (tags "Through hole pin header THT 2x07 2.00mm double row")
    (fp_text reference P4 (at -2.65 -1.65 180) (layer F.SilkS))
    (fp_text value "Power Board" (at -2.65 2.15 180) (layer F.SilkS))
    (fp_text user %R (at 1 -2.06 90) (layer F.Fab) hide)
    (pad 14 thru_hole oval (at 2 12 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(P4-Pad14)"))
    (pad 13 thru_hole oval (at 0 12 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(J2-Pad1)"))
    (pad 12 thru_hole oval (at 2 10 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(P4-Pad12)"))
    (pad 11 thru_hole oval (at 0 10 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 10 thru_hole oval (at 2 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(P4-Pad10)"))
    (pad 9 thru_hole oval (at 0 8 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(P4-Pad9)"))
    (pad 8 thru_hole oval (at 2 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(P4-Pad8)"))
    (pad 7 thru_hole oval (at 0 6 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(P4-Pad7)"))
    (pad 6 thru_hole oval (at 2 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 /Relay1_Reset))
    (pad 5 thru_hole oval (at 0 4 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 /Relay2_Set))
    (pad 4 thru_hole oval (at 2 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 /Relay1_Set))
    (pad 3 thru_hole oval (at 0 2 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 /Relay2_Reset))
    (pad 2 thru_hole oval (at 2 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 /12Vcc))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(P4-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Female/female_header_2row_14pins_2mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-R_EIA-2012-12_Wave (layer F.Cu) (tedit 5947E736)
    (at 131.6 80.6 270)
    (descr "Tantalum capacitor, Case R, EIA 2012-12, 2.0x1.3x1.2mm, Wave soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C1 (at -3.2 0.4 270) (layer F.SilkS))
    (fp_text value 10u (at -3.3 -0.3 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.275 0 270) (size 1.75 1.26) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.275 0 270) (size 1.75 1.26) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeR_EIA-2012.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5948DA5E)
    (at 129.5 80.55 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 2.65 -0.4 90) (layer F.SilkS))
    (fp_text value 100n (at 2.65 0.4 90) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1206 (layer F.Cu) (tedit 5948FB67)
    (at 150.5 111.7)
    (descr "Capacitor SMD 1206, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C10 (at -2.6 1.4) (layer F.SilkS))
    (fp_text value 10u/25V (at 0.4 1.4) (layer F.SilkS))
    (fp_text user %R (at 0 -1.75) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.5 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /12Vcc))
    (model Capacitors_SMD.3dshapes/C_1206.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 596480D4)
    (at 137.1 105 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 2.5 0.5 180) (layer F.SilkS))
    (fp_text value 100n (at 2.6 -0.3 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 596480B5)
    (at 144.3 96.5 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at -2.5 0.3 180) (layer F.SilkS))
    (fp_text value 1uF (at -2.7 -0.4 180) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C4-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 596480AE)
    (at 139.6 94.7 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -2.8 0.6 270) (layer F.SilkS))
    (fp_text value 10K (at -2.8 -0.3 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 /TS1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 596480BC)
    (at 144.8 94.9 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at -2.5 0.3 180) (layer F.SilkS))
    (fp_text value 4K7 (at -2.5 -0.4 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 /MTSA))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 596480B9)
    (at 141.1 94.7 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at -2.8 0.4 270) (layer F.SilkS))
    (fp_text value 10K (at -2.9 -0.4 270) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 /TS2))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:SSOP-14_5.3x6.2mm_Pitch0.65mm (layer F.Cu) (tedit 596480C5)
    (at 141.6 101.6 90)
    (descr "SSOP14: plastic shrink small outline package; 14 leads; body width 5.3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot337-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U7 (at 1.35 -0.1 180) (layer F.SilkS))
    (fp_text value MTCH105 (at -0.15 -0.1 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 14 smd rect (at 3.45 -1.95 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 13 smd rect (at 3.45 -1.3 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 13 /TS1))
    (pad 12 smd rect (at 3.45 -0.65 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 11 /TS2))
    (pad 11 smd rect (at 3.45 0 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(C4-Pad2)"))
    (pad 10 smd rect (at 3.45 0.65 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 3.45 1.3 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(U7-Pad9)"))
    (pad 8 smd rect (at 3.45 1.95 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(U7-Pad8)"))
    (pad 7 smd rect (at -3.45 1.95 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(U7-Pad7)"))
    (pad 6 smd rect (at -3.45 1.3 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(U7-Pad6)"))
    (pad 5 smd rect (at -3.45 0.65 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(R3-Pad2)"))
    (pad 4 smd rect (at -3.45 0 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 /MTPM))
    (pad 3 smd rect (at -3.45 -0.65 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at -3.45 -1.3 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(R10-Pad2)"))
    (pad 1 smd rect (at -3.45 -1.95 90) (size 1.2 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/ssop_14_50x44_p065.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module myfootprints:livolo_ts_guard_cut_left (layer F.Cu) (tedit 59788286)
    (at 128.941992 92.575738)
    (fp_text reference U1 (at -1.123271 0.209684) (layer F.SilkS) hide)
    (fp_text value Touch (at -0.541992 -0.075738) (layer F.SilkS))
    (pad 1 smd circle (at -0.266992 0.024262) (size 15 15) (layers B.Cu)
      (net 29 "Net-(R10-Pad1)"))
    (pad 2 smd circle (at 4.008008 6.999262) (size 0.5 0.5) (layers F.Cu)
      (net 24 "Net-(R3-Pad1)"))
    (pad 2 smd circle (at 6.058008 5.324262) (size 0.5 0.5) (layers F.Cu)
      (net 24 "Net-(R3-Pad1)"))
  )
  (module myfootprints:livolo_ts_guard_cut_right (layer F.Cu) (tedit 5978827D)
    (at 155.958008 92.475738)
    (fp_text reference U6 (at 1.123271 0.209684) (layer F.SilkS) hide)
    (fp_text value Touch (at 0.341992 -0.075738) (layer F.SilkS))
    (pad 1 smd circle (at 0.266992 0.024262) (size 15 15) (layers B.Cu)
      (net 26 "Net-(R4-Pad2)"))
    (pad 2 smd circle (at -4.008008 6.999262) (size 0.5 0.5) (layers F.Cu)
      (net 27 "Net-(R9-Pad2)"))
    (pad 2 smd circle (at -6.058008 5.324262) (size 0.5 0.5) (layers F.Cu)
      (net 27 "Net-(R9-Pad2)"))
  )
  (module Connectors:GS2 (layer B.Cu) (tedit 59D25946)
    (at 146.7 108.6)
    (descr "2-pin solder bridge")
    (tags "solder bridge")
    (attr smd)
    (fp_text reference J2 (at 0.6 -2.4 -90) (layer B.SilkS))
    (fp_text value 3V_EN (at -0.3 -2.7 -90) (layer B.SilkS))
    (pad 2 smd rect (at 0 -0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at 0 0.64) (size 1.27 0.97) (layers B.Cu B.Paste B.Mask)
      (net 32 "Net-(J2-Pad1)"))
  )
  (gr_line (start 134.4 75.30098) (end 150 75.30098) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 150 75.30098) (end 150 70.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 134.4 75.30098) (end 134.4 70.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 150 70.2) (end 155.9 70.2) (layer Edge.Cuts) (width 0.1))
  (gr_text +3V (at 144 111.1) (layer B.SilkS))
  (gr_line (start 158.90064 111.60234) (end 162.91 107.59) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 157.89988 74.60216) (end 159.89886 76.60114) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.89842 111.60234) (end 128.9007 113.60132) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.2 105.60032) (end 164.2 78.60012) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 126.89918 74.60216) (end 125.40058 73.10102) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.9 70.2) (end 159.39848 73.10102) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.91 107.59) (end 164.2 105.6) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.7 105.60032) (end 120.7 78.60012) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 123.39906 75.1) (end 124.9002 76.60114) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 124.9002 76.60114) (end 126.89918 74.60216) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.40058 73.10102) (end 128.9 70.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.9 70.2) (end 134.4 70.2) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 159.89886 76.60114) (end 161.4 75.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 122.94 108.61) (end 125.89842 111.60234) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.89836 113.60132) (end 158.90064 111.60234) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.9007 113.60132) (end 155.89836 113.60132) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.7 105.6) (end 122.94 108.61) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 159.39848 73.10102) (end 157.89988 74.60216) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 120.7 78.6) (end 123.39906 75.1) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161.4 75.1) (end 164.2 78.6) (layer Edge.Cuts) (width 0.1))
  (gr_text REL1_SET (at 135.1 104.25 45) (layer B.SilkS))
  (gr_text REL1_RST (at 137.25 105.25 45) (layer B.SilkS))
  (gr_text REL2_RST (at 136.25 111.7 135) (layer B.SilkS))
  (gr_text REL2_SET (at 134.25 111.8 135) (layer B.SilkS))
  (gr_text "Rev. 0.3" (at 126.7 107.9 90) (layer F.SilkS))
  (gr_text SWDIO (at 155.5 81.6) (layer F.SilkS))
  (gr_text GND (at 161.3 81.6) (layer F.SilkS))
  (gr_text SWCLK (at 155.6 79.6) (layer F.SilkS))
  (gr_text 3V3 (at 161.2 79.7) (layer F.SilkS))
  (gr_text GND (at 141.65 111.1) (layer B.SilkS))
  (gr_text +12V (at 131.55 105.85) (layer B.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.45))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.45) (thermal_bridge_width 0.45) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 120.7 70.1) (xy 164.2 70.1) (xy 164.2 113.6) (xy 120.7 113.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.45))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 153.6 106.5) (xy 159.4 106.5) (xy 159.4 109.8) (xy 153.6 109.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.45))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.7 70.1) (xy 164.2 70.1) (xy 164.2 104.4) (xy 120.7 104.4)
      )
    )
  )
)
