(kicad_pcb (version 20170922) (host pcbnew no-vcs-found-47f37ef~60~ubuntu16.04.1)
(general
  (thickness 1.6)
  (drawings 29)
  (tracks 189)
  (zones 0)
  (modules 169)
  (nets 45)
)
(page A3)
(layers
  (0 F.Cu signal)
  (31 B.Cu signal)
  (32 B.Adhes user)
  (33 F.Adhes user)
  (34 B.Paste user)
  (35 F.Paste user)
  (36 B.SilkS user)
  (37 F.SilkS user)
  (38 B.Mask user)
  (39 F.Mask user)
  (40 Dwgs.User user)
  (41 Cmts.User user)
  (42 Eco1.User user)
  (43 Eco2.User user)
  (44 Edge.Cuts user)
)
(general
  (thickness 1.6)
  (drawings 29)
  (tracks 189)
  (zones 0)
  (modules 169)
  (nets 45)
)
(page A3)
(layers
  (0 F.Cu signal)
  (31 B.Cu signal)
  (32 B.Adhes user)
  (33 F.Adhes user)
  (34 B.Paste user)
  (35 F.Paste user)
  (36 B.SilkS user)
  (37 F.SilkS user)
  (38 B.Mask user)
  (39 F.Mask user)
  (40 Dwgs.User user)
  (41 Cmts.User user)
  (42 Eco1.User user)
  (43 Eco2.User user)
  (44 Edge.Cuts user)
)
(setup
  (last_trace_width 0.3)
  (user_trace_width 0.6)
  (trace_clearance 0.2)
  (zone_clearance 0.55)
  (zone_45_only no)
  (trace_min 0.2)
  (segment_width 0.2)
  (edge_width 0.15)
  (via_size 0.6)
  (via_drill 0.3)
  (via_min_size 0.3)
  (via_min_drill 0.3)
  (uvia_size 0.6)
  (uvia_drill 0.2)
  (uvias_allowed no)
  (uvia_min_size 0.508)
  (uvia_min_drill 0.127)
  (pcb_text_width 0.3)
  (pcb_text_size 1 1)
  (mod_edge_width 0.15)
  (mod_text_size 0.8 0.8)
  (mod_text_width 0.12)
  (pad_size 3.2 3.2)
  (pad_drill 3.2)
  (pad_to_mask_clearance 0)
  (aux_axis_origin 117.8687 84.2645)
  (grid_origin 117.91188 84.25942)
  (visible_elements FFFFFF7F)
  (pcbplotparams
    (layerselection 0x010f8_ffffffff)
    (usegerberextensions true)
    (usegerberattributes true)
    (usegerberadvancedattributes true)
    (creategerberjobfile true)
    (excludeedgelayer true)
    (linewidth 0.150000)
    (plotframeref false)
    (viasonmask false)
    (mode 1)
    (useauxorigin false)
    (hpglpennumber 1)
    (hpglpenspeed 20)
    (hpglpendiameter 15)
    (psnegative false)
    (psa4output false)
    (plotreference true)
    (plotvalue true)
    (plotinvisibletext false)
    (padsonsilk false)
    (subtractmaskfromsilk true)
    (outputformat 1)
    (mirror false)
    (drillshape 0)
    (scaleselection 1)
    (outputdirectory gerber/))
)
(net 0 "")
(net 1 GND)
(net 2 +3V3)
(net 3 +5V)
(net 4 /RFM69_CS)
(net 5 /RFM69_SCK)
(net 6 /RFM69_CE)
(net 7 /RFM69_MISO)
(net 8 /RFM69_MOSI)
(net 9 "Net-(J2-Pad1)")
(net 10 "Net-(BAR1-Pad9)")
(net 11 "Net-(BAR1-Pad8)")
(net 12 "Net-(BAR1-Pad7)")
(net 13 "Net-(BAR1-Pad6)")
(net 14 "Net-(BAR1-Pad5)")
(net 15 "Net-(BAR1-Pad4)")
(net 16 "Net-(BAR1-Pad3)")
(net 17 "Net-(BAR1-Pad2)")
(net 18 "Net-(BAR1-Pad1)")
(net 19 "Net-(J1-Pad7)")
(net 20 /SSD_SCL)
(net 21 /SSD_SDA)
(net 22 "Net-(BAR1-Pad20)")
(net 23 "Net-(BAR1-Pad19)")
(net 24 "Net-(BAR1-Pad18)")
(net 25 "Net-(BAR1-Pad17)")
(net 26 "Net-(BAR1-Pad11)")
(net 27 "Net-(BAR1-Pad12)")
(net 28 "Net-(BAR1-Pad16)")
(net 29 "Net-(BAR1-Pad15)")
(net 30 "Net-(BAR1-Pad14)")
(net 31 "Net-(BAR1-Pad13)")
(net 32 /SW1)
(net 33 /SW2)
(net 34 "Net-(J1-Pad26)")
(net 35 "Net-(J1-Pad18)")
(net 36 "Net-(J1-Pad17)")
(net 37 "Net-(J1-Pad16)")
(net 38 "Net-(J1-Pad15)")
(net 39 "Net-(J1-Pad13)")
(net 40 "Net-(J1-Pad12)")
(net 41 "Net-(J1-Pad11)")
(net 42 "Net-(J1-Pad10)")
(net 43 "Net-(J1-Pad8)")
(net 44 "Net-(J1-Pad1)")
(net_class Default "This is the default net class."
  (clearance 0.2)
  (trace_width 0.3)
  (via_dia 0.6)
  (via_drill 0.3)
  (uvia_dia 0.6)
  (uvia_drill 0.2)
  (diff_pair_gap 0.2)
  (diff_pair_width 0.3)
  (add_net +3V3)
  (add_net +5V)
  (add_net /RFM69_CE)
  (add_net /RFM69_CS)
  (add_net /RFM69_MISO)
  (add_net /RFM69_MOSI)
  (add_net /RFM69_SCK)
  (add_net /SSD_SCL)
  (add_net /SSD_SDA)
  (add_net /SW1)
  (add_net /SW2)
  (add_net GND)
  (add_net "Net-(BAR1-Pad1)")
  (add_net "Net-(BAR1-Pad11)")
  (add_net "Net-(BAR1-Pad12)")
  (add_net "Net-(BAR1-Pad13)")
  (add_net "Net-(BAR1-Pad14)")
  (add_net "Net-(BAR1-Pad15)")
  (add_net "Net-(BAR1-Pad16)")
  (add_net "Net-(BAR1-Pad17)")
  (add_net "Net-(BAR1-Pad18)")
  (add_net "Net-(BAR1-Pad19)")
  (add_net "Net-(BAR1-Pad2)")
  (add_net "Net-(BAR1-Pad20)")
  (add_net "Net-(BAR1-Pad3)")
  (add_net "Net-(BAR1-Pad4)")
  (add_net "Net-(BAR1-Pad5)")
  (add_net "Net-(BAR1-Pad6)")
  (add_net "Net-(BAR1-Pad7)")
  (add_net "Net-(BAR1-Pad8)")
  (add_net "Net-(BAR1-Pad9)")
  (add_net "Net-(J1-Pad1)")
  (add_net "Net-(J1-Pad10)")
  (add_net "Net-(J1-Pad11)")
  (add_net "Net-(J1-Pad12)")
  (add_net "Net-(J1-Pad13)")
  (add_net "Net-(J1-Pad15)")
  (add_net "Net-(J1-Pad16)")
  (add_net "Net-(J1-Pad17)")
  (add_net "Net-(J1-Pad18)")
  (add_net "Net-(J1-Pad26)")
  (add_net "Net-(J1-Pad7)")
  (add_net "Net-(J1-Pad8)")
  (add_net "Net-(J2-Pad1)")
)
  (module Displays:HDSP-4850 (layer F.Cu) (tedit 59DCAA63)
    (at 169.21188 87.35942 270)
    (descr "10-Element Green Bar Graph Array https://docs.broadcom.com/docs/AV02-1798EN")
    (tags "10-Element Green Bar Graph Array")
    (fp_text reference BAR1 (at 7.7 24.9 270) (layer F.SilkS))
    (fp_text value HDSP-4850_2 (at 2.76 25.21 270) (layer F.Fab))
    (fp_text user %R (at 4 12 270) (layer F.Fab))
    (pad 20 thru_hole oval (at 7.62 0 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 22 "Net-(BAR1-Pad20)"))
    (pad 19 thru_hole oval (at 7.62 2.54 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 23 "Net-(BAR1-Pad19)"))
    (pad 18 thru_hole oval (at 7.62 5.08 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 24 "Net-(BAR1-Pad18)"))
    (pad 17 thru_hole oval (at 7.62 7.62 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 25 "Net-(BAR1-Pad17)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 10 "Net-(BAR1-Pad9)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 11 thru_hole oval (at 7.62 22.86 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 26 "Net-(BAR1-Pad11)"))
    (pad 12 thru_hole oval (at 7.62 20.32 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 27 "Net-(BAR1-Pad12)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 11 "Net-(BAR1-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 12 "Net-(BAR1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 13 "Net-(BAR1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 14 "Net-(BAR1-Pad5)"))
    (pad 16 thru_hole oval (at 7.62 10.16 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 28 "Net-(BAR1-Pad16)"))
    (pad 15 thru_hole oval (at 7.62 12.7 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 29 "Net-(BAR1-Pad15)"))
    (pad 14 thru_hole oval (at 7.62 15.24 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 30 "Net-(BAR1-Pad14)"))
    (pad 13 thru_hole oval (at 7.62 17.78 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 31 "Net-(BAR1-Pad13)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 15 "Net-(BAR1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 16 "Net-(BAR1-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 17 "Net-(BAR1-Pad2)"))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.2 2.2) (drill 0.9144) (layers *.Cu *.Mask)
      (net 18 "Net-(BAR1-Pad1)"))
    (model /usr/share/kicad/modules/packages3d/Displays.3dshapes/HDSP-4850.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:KiCad-Logo2_6mm_SilkScreen locked (layer B.Cu) (tedit 0)
    (at 136.01188 98.35942)
    (descr "KiCad Logo")
    (tags "Logo KiCad")
    (attr virtual)
    (fp_text reference REF*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value KiCad-Logo2_6mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 59DC9685)
    (at 112.71188 82.65942)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 59DC9699)
    (at 112.71188 106.35942)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 59DC969F)
    (at 171.31188 106.35942)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 locked (layer F.Cu) (tedit 59DC96A5)
    (at 171.31188 82.65942)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm (layer F.Cu) (tedit 59650533)
    (at 117.91188 84.25942 90)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J1 (at 3.2 -2.5 90) (layer F.SilkS))
    (fp_text value RPI_Zero_W (at 1.27 50.59 90) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13 180) (layer F.Fab))
    (pad 40 thru_hole oval (at 2.54 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(BAR1-Pad3)"))
    (pad 39 thru_hole oval (at 0 48.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 38 thru_hole oval (at 2.54 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(BAR1-Pad1)"))
    (pad 37 thru_hole oval (at 0 45.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(BAR1-Pad4)"))
    (pad 36 thru_hole oval (at 2.54 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(BAR1-Pad2)"))
    (pad 35 thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(BAR1-Pad5)"))
    (pad 34 thru_hole oval (at 2.54 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 33 thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(BAR1-Pad6)"))
    (pad 32 thru_hole oval (at 2.54 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /SW1))
    (pad 31 thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(BAR1-Pad7)"))
    (pad 30 thru_hole oval (at 2.54 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 29 thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(BAR1-Pad8)"))
    (pad 28 thru_hole oval (at 2.54 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /SW2))
    (pad 27 thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(BAR1-Pad9)"))
    (pad 26 thru_hole oval (at 2.54 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J1-Pad26)"))
    (pad 25 thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole oval (at 2.54 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /RFM69_CS))
    (pad 23 thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /RFM69_SCK))
    (pad 22 thru_hole oval (at 2.54 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /RFM69_CE))
    (pad 21 thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /RFM69_MISO))
    (pad 20 thru_hole oval (at 2.54 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /RFM69_MOSI))
    (pad 18 thru_hole oval (at 2.54 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J1-Pad18)"))
    (pad 17 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J1-Pad17)"))
    (pad 16 thru_hole oval (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad16)"))
    (pad 15 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J1-Pad15)"))
    (pad 14 thru_hole oval (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J1-Pad13)"))
    (pad 12 thru_hole oval (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /SSD_SCL))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /SSD_SDA))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +5V))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Female/female_header_2row_40pins_2.54mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 -90))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-B_EIA-3528-21_Hand (layer F.Cu) (tedit 58CC8C08)
    (at 143.81188 105.15942 90)
    (descr "Tantalum capacitor, Case B, EIA 3528-21, 3.5x2.8x1.9mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C1 (at 4.9 -0.3 90) (layer F.SilkS))
    (fp_text value 22u (at 0 3.15 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2.15 0 90) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.15 0 90) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 146.61188 105.95942 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.3 -0.1 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 113.91188 87.55942)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -0.3 -1.6) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-B_EIA-3528-21_Hand (layer F.Cu) (tedit 58CC8C08)
    (at 114.71188 90.35942 180)
    (descr "Tantalum capacitor, Case B, EIA 3528-21, 3.5x2.8x1.9mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C4 (at 4.4 0 270) (layer F.SilkS))
    (fp_text value 22u (at 0 3.15 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 2.15 0 180) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.15 0 180) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (model ${KISYS3DMOD}/Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-B_EIA-3528-21_Hand (layer F.Cu) (tedit 58CC8C08)
    (at 120.71188 96.05942 270)
    (descr "Tantalum capacitor, Case B, EIA 3528-21, 3.5x2.8x1.9mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C5 (at 4.4 1.8 90) (layer F.SilkS))
    (fp_text value 22u (at 0 3.15 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0 270) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 2 smd rect (at 2.15 0 270) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitors_Tantalum_SMD.3dshapes/TantalC_SizeB_EIA-3528_HandSoldering.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 123.81188 95.45942 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 2.8 -0.7 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_radios:RFM69HW_SMD_Handsoldering (layer F.Cu) (tedit 558806AF)
    (at 126.31188 105.95942 90)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U1 (at 7.3 5.6 90) (layer F.SilkS))
    (fp_text value RFM69HW (at 8.382 7.112 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.4 0 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.4 2 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 6 /RFM69_CE))
    (pad 3 smd rect (at -1.4 4 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -1.4 6 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -1.4 8 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -1.4 10 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -1.4 12 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -1.4 14 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 9 smd rect (at 18.3 14 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 18.3 12 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J2-Pad1)"))
    (pad 11 smd rect (at 18.3 10 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 18.3 8 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 /RFM69_SCK))
    (pad 13 smd rect (at 18.3 6 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 /RFM69_MISO))
    (pad 14 smd rect (at 18.3 4 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 8 /RFM69_MOSI))
    (pad 15 smd rect (at 18.3 2 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 /RFM69_CS))
    (pad 16 smd rect (at 18.3 0 90) (size 3 1.2) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Radio_Modules.3dshapes/RFM69W.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 58CE4E7E)
    (at 114.21188 95.95942 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U2 (at -0.2 -0.3 180) (layer F.SilkS))
    (fp_text value AMS1117 (at 0 4.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (pad 4 smd rect (at 3.15 0 180) (size 2 3.8) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/SOT_Packages_SMD.3dshapes/SOT223-3.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 146.41188 98.25942 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.5 0.1 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(BAR1-Pad11)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 148.81188 98.25942 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.5 0.1 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(BAR1-Pad12)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 151.41188 98.25942 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.5 0.1 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 31 "Net-(BAR1-Pad13)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 154.01188 98.25942 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 2.5 0.1 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 30 "Net-(BAR1-Pad14)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 156.41188 98.25942 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 2.5 0.1 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 29 "Net-(BAR1-Pad15)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 159.01188 98.25942 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 2.5 0.1 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 28 "Net-(BAR1-Pad16)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 161.41188 98.25942 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 2.5 0.1 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(BAR1-Pad17)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 164.01188 98.25942 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 2.5 0.2 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(BAR1-Pad18)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 166.61188 98.25942 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 2.5 0.1 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(BAR1-Pad19)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 169.21188 98.25942 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 2.5 0.1 180) (layer B.SilkS))
    (fp_text value 220 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(BAR1-Pad20)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 122.01188 86.55942 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -3.1 0.1 180) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 122.11188 91.15942 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at -2.4 -0.1 90) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.55 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J1-Pad7)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Inline_Narrow_Oval (layer F.Cu) (tedit 58CE52AF)
    (at 120.71188 88.35942)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.6mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U3 (at 1.3 -1.7) (layer F.SilkS))
    (fp_text value DS18B20 (at 1.27 2.79) (layer F.Fab))
    (fp_text user %R (at 1.27 -3.56) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 0.9 1.5) (drill 0.6) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad7)"))
    (model ${KISYS3DMOD}/TO_Packages.3dshapes/TO92_inline.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.00mm (layer F.Cu) (tedit 59650533)
    (at 142.91188 91.65942)
    (descr "Through hole straight pin header, 1x01, 2.00mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.00mm single row")
    (fp_text reference J2 (at 0 -3.6) (layer F.SilkS))
    (fp_text value ANT (at 0 2.06) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(J2-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 123.71188 106.65942 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J3 (at 6.5 -2 180) (layer F.SilkS))
    (fp_text value SSD1306 (at 0 9.95 180) (layer F.Fab))
    (fp_text user %R (at 0 3.81 270) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /SSD_SDA))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /SSD_SCL))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +3V3))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Displays.3dshapes/OLED_0.91_128x32_sp.step
      (at (xyz 0 0 0.05118110236220473))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Female/female_header_1row_4pins_2.54mm.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 121.21188 100.15942 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 1.45 270) (layer B.SilkS))
    (fp_text value 4K7 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 21 /SSD_SDA))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 126.51188 102.65942 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at -0.2 -1.5 270) (layer B.SilkS))
    (fp_text value 4K7 (at 0 -1.55 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 20 /SSD_SCL))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers B.Cu B.Paste B.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 158.81188 102.35942)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at -3.1 0) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 /SW1))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 58724896)
    (at 164.71188 102.35942)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE7.pdf")
    (attr smd)
    (fp_text reference SW1 (at 0 0.2) (layer F.SilkS))
    (fp_text value BLE (at 0 3) (layer F.Fab))
    (fp_text user %R (at 0 -2.65) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 32 /SW1))
    (pad 2 smd rect (at 2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switches_SMD.3dshapes/SW_SPST_EVQPE1.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 158.81188 106.75942)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at -3.185001 0.1425) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 /SW2))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVQPE1 (layer F.Cu) (tedit 58724896)
    (at 164.71188 106.75942)
    (descr "Light Touch Switch, https://industrial.panasonic.com/cdbs/www-data/pdf/ATK0000/ATK0000CE7.pdf")
    (attr smd)
    (fp_text reference SW2 (at 0 0.2) (layer F.SilkS))
    (fp_text value BLE (at 0 3) (layer F.Fab))
    (fp_text user %R (at 0 -2.65) (layer F.Fab))
    (pad 1 smd rect (at -2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /SW2))
    (pad 2 smd rect (at 2.7 0) (size 2 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Button_Switches_SMD.3dshapes/SW_SPST_EVQPE1.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 114.966166 81.65342)
    (attr virtual)
    (fp_text reference V5_2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 168.966166 81.65342)
    (attr virtual)
    (fp_text reference V32_2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 168.966166 83.65342)
    (attr virtual)
    (fp_text reference V32_3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 110.966166 85.65342)
    (attr virtual)
    (fp_text reference V3_4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 112.966166 85.65342)
    (attr virtual)
    (fp_text reference V4_4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 170.966166 85.65342)
    (attr virtual)
    (fp_text reference V33_4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 172.966166 85.65342)
    (attr virtual)
    (fp_text reference V34_4 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 110.966166 87.65342)
    (attr virtual)
    (fp_text reference V3_5 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 116.966166 87.65342)
    (attr virtual)
    (fp_text reference V6_5 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 172.966166 87.65342)
    (attr virtual)
    (fp_text reference V34_5 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 148.966166 89.65342)
    (attr virtual)
    (fp_text reference V22_6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 150.966166 89.65342)
    (attr virtual)
    (fp_text reference V23_6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 152.966166 89.65342)
    (attr virtual)
    (fp_text reference V24_6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 154.966166 89.65342)
    (attr virtual)
    (fp_text reference V25_6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 158.966166 89.65342)
    (attr virtual)
    (fp_text reference V27_6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 160.966166 89.65342)
    (attr virtual)
    (fp_text reference V28_6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 162.966166 89.65342)
    (attr virtual)
    (fp_text reference V29_6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 164.966166 89.65342)
    (attr virtual)
    (fp_text reference V30_6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 166.966166 89.65342)
    (attr virtual)
    (fp_text reference V31_6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 168.966166 89.65342)
    (attr virtual)
    (fp_text reference V32_6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 170.966166 89.65342)
    (attr virtual)
    (fp_text reference V33_6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 172.966166 89.65342)
    (attr virtual)
    (fp_text reference V34_6 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 148.966166 91.65342)
    (attr virtual)
    (fp_text reference V22_7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 150.966166 91.65342)
    (attr virtual)
    (fp_text reference V23_7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 152.966166 91.65342)
    (attr virtual)
    (fp_text reference V24_7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 154.966166 91.65342)
    (attr virtual)
    (fp_text reference V25_7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 158.966166 91.65342)
    (attr virtual)
    (fp_text reference V27_7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 160.966166 91.65342)
    (attr virtual)
    (fp_text reference V28_7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 162.966166 91.65342)
    (attr virtual)
    (fp_text reference V29_7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 164.966166 91.65342)
    (attr virtual)
    (fp_text reference V30_7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 166.966166 91.65342)
    (attr virtual)
    (fp_text reference V31_7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 168.966166 91.65342)
    (attr virtual)
    (fp_text reference V32_7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 170.966166 91.65342)
    (attr virtual)
    (fp_text reference V33_7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 172.966166 91.65342)
    (attr virtual)
    (fp_text reference V34_7 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 112.966166 93.65342)
    (attr virtual)
    (fp_text reference V4_8 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 114.966166 93.65342)
    (attr virtual)
    (fp_text reference V5_8 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 162.966166 93.65342)
    (attr virtual)
    (fp_text reference V29_8 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 170.966166 93.65342)
    (attr virtual)
    (fp_text reference V33_8 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 172.966166 93.65342)
    (attr virtual)
    (fp_text reference V34_8 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 112.966166 95.65342)
    (attr virtual)
    (fp_text reference V4_9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 114.966166 95.65342)
    (attr virtual)
    (fp_text reference V5_9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 130.966166 95.65342)
    (attr virtual)
    (fp_text reference V13_9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 132.966166 95.65342)
    (attr virtual)
    (fp_text reference V14_9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 134.966166 95.65342)
    (attr virtual)
    (fp_text reference V15_9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 136.966166 95.65342)
    (attr virtual)
    (fp_text reference V16_9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 138.966166 95.65342)
    (attr virtual)
    (fp_text reference V17_9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 142.966166 95.65342)
    (attr virtual)
    (fp_text reference V19_9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 144.966166 95.65342)
    (attr virtual)
    (fp_text reference V20_9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 172.966166 95.65342)
    (attr virtual)
    (fp_text reference V34_9 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 112.966166 97.65342)
    (attr virtual)
    (fp_text reference V4_10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 114.966166 97.65342)
    (attr virtual)
    (fp_text reference V5_10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 130.966166 97.65342)
    (attr virtual)
    (fp_text reference V13_10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 132.966166 97.65342)
    (attr virtual)
    (fp_text reference V14_10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 134.966166 97.65342)
    (attr virtual)
    (fp_text reference V15_10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 136.966166 97.65342)
    (attr virtual)
    (fp_text reference V16_10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 138.966166 97.65342)
    (attr virtual)
    (fp_text reference V17_10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 142.966166 97.65342)
    (attr virtual)
    (fp_text reference V19_10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 144.966166 97.65342)
    (attr virtual)
    (fp_text reference V20_10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 152.966166 97.65342)
    (attr virtual)
    (fp_text reference V24_10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 162.966166 97.65342)
    (attr virtual)
    (fp_text reference V29_10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 170.966166 97.65342)
    (attr virtual)
    (fp_text reference V33_10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 172.966166 97.65342)
    (attr virtual)
    (fp_text reference V34_10 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 110.966166 99.65342)
    (attr virtual)
    (fp_text reference V3_11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 112.966166 99.65342)
    (attr virtual)
    (fp_text reference V4_11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 114.966166 99.65342)
    (attr virtual)
    (fp_text reference V5_11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 116.966166 99.65342)
    (attr virtual)
    (fp_text reference V6_11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 130.966166 99.65342)
    (attr virtual)
    (fp_text reference V13_11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 132.966166 99.65342)
    (attr virtual)
    (fp_text reference V14_11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 134.966166 99.65342)
    (attr virtual)
    (fp_text reference V15_11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 136.966166 99.65342)
    (attr virtual)
    (fp_text reference V16_11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 138.966166 99.65342)
    (attr virtual)
    (fp_text reference V17_11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 142.966166 99.65342)
    (attr virtual)
    (fp_text reference V19_11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 152.966166 99.65342)
    (attr virtual)
    (fp_text reference V24_11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 162.966166 99.65342)
    (attr virtual)
    (fp_text reference V29_11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 170.966166 99.65342)
    (attr virtual)
    (fp_text reference V33_11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 172.966166 99.65342)
    (attr virtual)
    (fp_text reference V34_11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 110.966166 101.65342)
    (attr virtual)
    (fp_text reference V3_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 112.966166 101.65342)
    (attr virtual)
    (fp_text reference V4_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 114.966166 101.65342)
    (attr virtual)
    (fp_text reference V5_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 116.966166 101.65342)
    (attr virtual)
    (fp_text reference V6_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 118.966166 101.65342)
    (attr virtual)
    (fp_text reference V7_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 130.966166 101.65342)
    (attr virtual)
    (fp_text reference V13_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 132.966166 101.65342)
    (attr virtual)
    (fp_text reference V14_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 134.966166 101.65342)
    (attr virtual)
    (fp_text reference V15_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 136.966166 101.65342)
    (attr virtual)
    (fp_text reference V16_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 138.966166 101.65342)
    (attr virtual)
    (fp_text reference V17_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 146.966166 101.65342)
    (attr virtual)
    (fp_text reference V21_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 148.966166 101.65342)
    (attr virtual)
    (fp_text reference V22_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 150.966166 101.65342)
    (attr virtual)
    (fp_text reference V23_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 152.966166 101.65342)
    (attr virtual)
    (fp_text reference V24_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 154.966166 101.65342)
    (attr virtual)
    (fp_text reference V25_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 164.966166 101.65342)
    (attr virtual)
    (fp_text reference V30_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 168.966166 101.65342)
    (attr virtual)
    (fp_text reference V32_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 170.966166 101.65342)
    (attr virtual)
    (fp_text reference V33_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 172.966166 101.65342)
    (attr virtual)
    (fp_text reference V34_12 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 110.966166 103.65342)
    (attr virtual)
    (fp_text reference V3_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 112.966166 103.65342)
    (attr virtual)
    (fp_text reference V4_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 114.966166 103.65342)
    (attr virtual)
    (fp_text reference V5_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 116.966166 103.65342)
    (attr virtual)
    (fp_text reference V6_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 118.966166 103.65342)
    (attr virtual)
    (fp_text reference V7_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 120.966166 103.65342)
    (attr virtual)
    (fp_text reference V8_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 130.966166 103.65342)
    (attr virtual)
    (fp_text reference V13_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 132.966166 103.65342)
    (attr virtual)
    (fp_text reference V14_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 134.966166 103.65342)
    (attr virtual)
    (fp_text reference V15_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 136.966166 103.65342)
    (attr virtual)
    (fp_text reference V16_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 138.966166 103.65342)
    (attr virtual)
    (fp_text reference V17_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 148.966166 103.65342)
    (attr virtual)
    (fp_text reference V22_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 150.966166 103.65342)
    (attr virtual)
    (fp_text reference V23_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 152.966166 103.65342)
    (attr virtual)
    (fp_text reference V24_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 154.966166 103.65342)
    (attr virtual)
    (fp_text reference V25_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 164.966166 103.65342)
    (attr virtual)
    (fp_text reference V30_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 168.966166 103.65342)
    (attr virtual)
    (fp_text reference V32_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 170.966166 103.65342)
    (attr virtual)
    (fp_text reference V33_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 172.966166 103.65342)
    (attr virtual)
    (fp_text reference V34_13 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 116.966166 105.65342)
    (attr virtual)
    (fp_text reference V6_14 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 118.966166 105.65342)
    (attr virtual)
    (fp_text reference V7_14 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 120.966166 105.65342)
    (attr virtual)
    (fp_text reference V8_14 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 148.966166 105.65342)
    (attr virtual)
    (fp_text reference V22_14 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 150.966166 105.65342)
    (attr virtual)
    (fp_text reference V23_14 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 152.966166 105.65342)
    (attr virtual)
    (fp_text reference V24_14 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 154.966166 105.65342)
    (attr virtual)
    (fp_text reference V25_14 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 158.966166 105.65342)
    (attr virtual)
    (fp_text reference V27_14 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 164.966166 105.65342)
    (attr virtual)
    (fp_text reference V30_14 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 168.966166 105.65342)
    (attr virtual)
    (fp_text reference V32_14 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 116.966166 107.65342)
    (attr virtual)
    (fp_text reference V6_15 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 118.966166 107.65342)
    (attr virtual)
    (fp_text reference V7_15 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 120.966166 107.65342)
    (attr virtual)
    (fp_text reference V8_15 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 148.966166 107.65342)
    (attr virtual)
    (fp_text reference V22_15 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 150.966166 107.65342)
    (attr virtual)
    (fp_text reference V23_15 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 152.966166 107.65342)
    (attr virtual)
    (fp_text reference V24_15 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 154.966166 107.65342)
    (attr virtual)
    (fp_text reference V25_15 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 164.966166 107.65342)
    (attr virtual)
    (fp_text reference V30_15 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (module VIA_MATRIX (layer F.Cu) (tedit 59DE0F43)
    (at 168.966166 107.65342)
    (attr virtual)
    (fp_text reference V32_15 (at 0 0) (layer F.SilkS) hide)
    (fp_text value AUTO_VIA (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 0.45 0.45) (drill 0.3) (layers *.Cu)
      (net 1 GND) (clearance 0.3) (zone_connect 2))
  )
  (gr_text ANT (at 142.91188 89.65942) (layer F.SilkS))
  (gr_text SDA (at 121.11188 102.25942) (layer F.SilkS))
  (gr_text SCL (at 121.11188 103.65942) (layer F.SilkS))
  (gr_text VCC (at 121.11188 105.25942) (layer F.SilkS))
  (gr_text GND (at 121.11188 106.85942) (layer F.SilkS))
  (gr_text SSD1306 (at 121.01188 108.65942) (layer F.SilkS))
  (gr_text "Rev. 0.1" (at 114.11188 102.65942) (layer F.SilkS))
  (gr_text "RaspberryPI Zero W MYSENSORS-BLE" (at 153.41188 104.75942) (layer B.SilkS))
  (gr_text BLE5 (at 159.11188 98.05942 90) (layer F.SilkS))
  (gr_text MYS_RX (at 156.51188 99.25942 90) (layer F.SilkS))
  (gr_text MYS_TX (at 154.11188 99.25942 90) (layer F.SilkS))
  (gr_text MYS_ERR (at 151.51188 99.25942 90) (layer F.SilkS))
  (gr_text PWR (at 146.31188 98.05942 90) (layer F.SilkS))
  (gr_text BLE4 (at 161.51188 98.05942 90) (layer F.SilkS))
  (gr_text BLE3 (at 164.11188 98.05942 90) (layer F.SilkS))
  (gr_text BLE2 (at 166.71188 98.05942 90) (layer F.SilkS))
  (gr_text BLE1 (at 169.31188 98.05942 90) (layer F.SilkS))
  (gr_line (start 171.5 109.5) (end 170.95 109.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.5 106.05) (end 174.5 106.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 174.5 82.5) (end 174.5 106.05) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.5 109.5) (end 170.95 109.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.5 98.5) (end 109.5 106.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.5 79.5) (end 171 79.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 109.5 98.5) (end 109.5 82.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 112.5 106.5) (end 112.5 109.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 171.5 106.5) (end 174.5 106.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 171.5 79.5) (end 171 79.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 171.5 82.5) (end 171.5 79.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 112.5 82.5) (end 109.5 82.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 109.51188 79.45942) (xy 174.51188 79.45942) (xy 174.51188 109.45942) (xy 109.51188 109.45942)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet))
    (polygon
      (pts
        (xy 109.51188 79.45942) (xy 174.51188 79.45942) (xy 174.51188 109.45942) (xy 109.51188 109.45942)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.55))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.71188 82.25942) (xy 139.21188 82.25942) (xy 139.21188 85.65942) (xy 120.71188 85.65942)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.55))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 123.760241 82.15942) (xy 147.01188 82.15942) (xy 149.31188 82.25942) (xy 149.31188 84.45942) (xy 147.01188 84.45942)
        (xy 147.01188 93.35942) (xy 146.11188 94.25942) (xy 123.659501 94.449692)
      )
    )
  )
)
