(kicad_pcb (version 4) (host pcbnew 4.0.4-stable)
  (general
    (links 105)
    (no_connects 0)
    (area 99.994999 25.395714 143.70743 81.605001)
    (thickness 1.6)
    (drawings 111)
    (tracks 719)
    (zones 0)
    (modules 50)
    (nets 32)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.2)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.1)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 1)
    (pad_drill 0)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (grid_origin 122.68 61.87)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory Gerber/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad2)")
  (net 4 "Net-(D3-Pad2)")
  (net 5 "Net-(D4-Pad2)")
  (net 6 RX)
  (net 7 SS)
  (net 8 TX)
  (net 9 MOSI)
  (net 10 MISO)
  (net 11 SCK)
  (net 12 "Net-(R3-Pad1)")
  (net 13 "Net-(Atmega1-Pad7)")
  (net 14 "Net-(Atmega1-Pad8)")
  (net 15 "Net-(Atmega1-Pad20)")
  (net 16 LEDJmp)
  (net 17 RST)
  (net 18 "Net-(Atmega1-Pad31)")
  (net 19 "Net-(D5-Pad2)")
  (net 20 CardS)
  (net 21 "Net-(D7-Pad2)")
  (net 22 BAT)
  (net 23 5V)
  (net 24 "Net-(P2-Pad7)")
  (net 25 Reg3.3V)
  (net 26 BTVCC)
  (net 27 BATVCC)
  (net 28 SDVCC)
  (net 29 FTDIRST)
  (net 30 RX_SD)
  (net 31 RX_BT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CardS)
    (add_net FTDIRST)
    (add_net MISO)
    (add_net MOSI)
    (add_net "Net-(Atmega1-Pad20)")
    (add_net "Net-(Atmega1-Pad31)")
    (add_net "Net-(Atmega1-Pad7)")
    (add_net "Net-(Atmega1-Pad8)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(P2-Pad7)")
    (add_net "Net-(R3-Pad1)")
    (add_net RST)
    (add_net RX)
    (add_net RX_BT)
    (add_net RX_SD)
    (add_net SCK)
    (add_net SS)
    (add_net TX)
  )
  (net_class Gnd ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.4)
    (uvia_drill 0.2)
    (add_net 5V)
    (add_net BAT)
    (add_net BATVCC)
    (add_net BTVCC)
    (add_net GND)
    (add_net LEDJmp)
    (add_net "Net-(D3-Pad2)")
    (add_net Reg3.3V)
    (add_net SDVCC)
  )
  (module Diodes_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 596118B2)
    (at 128.55 62.09)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D3 (at 0.09 -1.53) (layer F.SilkS))
    (fp_text value MBRA140? (at 0.1 1.9) (layer F.Fab))
    (fp_text user "" (at 0 -1.85) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 27 BATVCC))
    (pad 2 smd rect (at 1.25 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer B.Cu) (tedit 595DDD61)
    (at 134.85 34.5 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 2.36 0 270) (layer B.SilkS) hide)
    (fp_text value LED (at 0 -1.55 180) (layer B.Fab) hide)
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 16 LEDJmp))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Testpoint (layer F.Cu) (tedit 5A16D005)
    (at 122.48 63.18)
    (descr www.openhardware.io)
    (fp_text reference W5 (at 16.14 1.8) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0.2 -1.7) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 25 Reg3.3V))
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5A16D26F)
    (at 119.1 62.93)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 1.84 -1.41 180) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 Reg3.3V))
    (pad 2 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 RX))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P2-Pad7)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59DE7828)
    (at 121.99 43.39 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P3 (at 1.02 1.35 180) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at 0 4.87 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 30 RX_SD))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 18 "Net-(Atmega1-Pad31)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ASKicadLib:HC-06 (layer B.Cu) (tedit 58B814AB)
    (at 121.23 41.15)
    (fp_text reference U1 (at 5.43 12.51) (layer B.SilkS))
    (fp_text value HC-06_Bluetooth (at -3.64 12.43) (layer B.Fab) hide)
    (pad 1 smd rect (at -6.35 6) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(D5-Pad2)"))
    (pad 2 smd rect (at -6.35 4.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 31 RX_BT))
    (pad 3 smd rect (at -6.35 3) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at -6.35 1.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at -6.35 0) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at -6.35 -1.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 7 smd rect (at -6.35 -3) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 8 smd rect (at -6.35 -4.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 9 smd rect (at -6.35 -6) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 10 smd rect (at -6.35 -7.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 11 smd rect (at -6.35 -9) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 12 smd rect (at -6.35 -10.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 26 BTVCC))
    (pad 13 smd rect (at -6.35 -12) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -5.25 -13.5) (size 0.8 1.8) (layers B.Cu B.Paste B.Mask))
    (pad 15 smd rect (at -3.75 -13.5) (size 0.8 1.8) (layers B.Cu B.Paste B.Mask))
    (pad 16 smd rect (at -2.25 -13.5) (size 0.8 1.8) (layers B.Cu B.Paste B.Mask))
    (pad 17 smd rect (at -0.75 -13.5) (size 0.8 1.8) (layers B.Cu B.Paste B.Mask))
    (pad 18 smd rect (at 0.75 -13.5) (size 0.8 1.8) (layers B.Cu B.Paste B.Mask))
    (pad 19 smd rect (at 2.25 -13.5) (size 0.8 1.8) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd rect (at 3.75 -13.5) (size 0.8 1.8) (layers B.Cu B.Paste B.Mask))
    (pad 21 smd rect (at 5.25 -13.5) (size 0.8 1.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 22 smd rect (at 6.35 -12) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 23 smd rect (at 6.35 -10.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 24 smd rect (at 6.35 -9) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(R3-Pad1)"))
    (pad 25 smd rect (at 6.35 -7.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 26 smd rect (at 6.35 -6) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 27 smd rect (at 6.35 -4.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 28 smd rect (at 6.35 -3) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 29 smd rect (at 6.35 -1.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 30 smd rect (at 6.35 0) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 31 smd rect (at 6.35 1.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 32 smd rect (at 6.35 3) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 33 smd rect (at 6.35 4.5) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
    (pad 34 smd rect (at 6.35 6) (size 1.8 0.8) (layers B.Cu B.Paste B.Mask))
  )
  (module ASKicadLib:SOLDER-JUMPER_1-WAY (layer B.Cu) (tedit 59DE7872)
    (at 136.18 67.15 270)
    (fp_text reference LEDs1 (at 0.5 -2.67 450) (layer B.SilkS) hide)
    (fp_text value JUMPER (at -0.2 1.6 270) (layer B.SilkS) hide)
    (pad 1 smd rect (at -0.56 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 16 LEDJmp))
    (pad 2 smd rect (at 0.56 0 270) (size 1 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module ASKicadLib:Conn_uSDcard (layer F.Cu) (tedit 5718CF45)
    (at 109.52 35.32 270)
    (fp_text reference SD_CardModule1 (at 0 1 450) (layer F.Fab))
    (fp_text value MicroSD (at 0 0 450) (layer F.Fab))
    (fp_text user %R (at 2.1 -9.35 450) (layer Eco1.User))
    (pad 6 smd rect (at 7.75 -0.4 270) (size 1.2 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -7.75 -0.4 270) (size 1.2 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 6.85 -10 270) (size 1.6 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -7.75 -10 270) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -6.6 -10.5 270) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 20 CardS))
    (pad 7 smd rect (at -4.4 -10.5 270) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 10 MISO))
    (pad 8 smd rect (at -5.5 -10.5 270) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -3.3 -10.5 270) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -2.2 -10.5 270) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 SCK))
    (pad 4 smd rect (at -1.1 -10.5 270) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 28 SDVCC))
    (pad 1 smd rect (at 2.2 -10.5 270) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 1.1 -10.5 270) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 7 SS))
    (pad "" np_thru_hole circle (at 3.05 0 270) (size 1 1) (drill 1) (layers *.Cu))
    (pad "" np_thru_hole circle (at -4.93 0 270) (size 1 1) (drill 1) (layers *.Cu))
    (pad 3 smd rect (at 0 -10.5 270) (size 0.7 1.6) (layers F.Cu F.Paste F.Mask)
      (net 9 MOSI))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59DE78B6)
    (at 128.88 27.31 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P1 (at -0.73 -2.88 90) (layer F.SilkS) hide)
    (fp_text value ISCP (at 0 9.95 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 10 MISO))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 MOSI))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 11 SCK))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 RST))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_HC49-U_Vertical (layer F.Cu) (tedit 59DE77FD)
    (at 129.24 57.29)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (fp_text reference Crystal1 (at 11.196 0.168) (layer F.SilkS) hide)
    (fp_text value Crystal (at 2.44 3.525) (layer F.Fab))
    (fp_text user %R (at 10.99 0.24) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(Atmega1-Pad7)"))
    (pad 2 thru_hole circle (at 4.88 0) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(Atmega1-Pad8)"))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_HC49-U_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A16D07B)
    (at 112.84 46.36 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 2.96 -0.06 360) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user "" (at 0 -1.75 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 26 BTVCC))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A16D080)
    (at 110.6 46.39 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 2.93 -0.02 540) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user "" (at 0 -1.75 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 26 BTVCC))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59A90818)
    (at 136.12 70.81 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0.01 1.5 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user "" (at -1.12 -3.89 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 22 BAT))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A16D062)
    (at 122.5 33.12 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 2.82 0.43 180) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user "" (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 28 SDVCC))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59A9080F)
    (at 135.92 65.76 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -0.12 -1.32 270) (layer F.SilkS))
    (fp_text value 0,22pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user "" (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Atmega1-Pad7)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 595DBE0A)
    (at 134.8 44.24 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 2.88 0.07 450) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user "" (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 28 SDVCC))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 599F22B3)
    (at 135.92 61.08 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 2.95 -0.07 360) (layer F.SilkS))
    (fp_text value 0,22pF (at 0 1.75 90) (layer F.Fab))
    (fp_text user "" (at 1.36 -3.21 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Atmega1-Pad8)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A16D0C0)
    (at 130.52 54.09 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at -0.03 1.53 90) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75 90) (layer F.Fab))
    (fp_text user "" (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Atmega1-Pad20)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59E37600)
    (at 116.24 47.69 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -0.04 1.33 180) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user "" (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 17 RST))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 29 FTDIRST))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer B.Cu) (tedit 595DDD68)
    (at 134.88 30.82 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 2.33 0.05 270) (layer B.SilkS) hide)
    (fp_text value LED (at 0 -1.55 180) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 16 LEDJmp))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer B.Cu) (tedit 595DDD65)
    (at 134.86 38.21 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 2.35 0.04 270) (layer B.SilkS) hide)
    (fp_text value LED (at 0 -1.55 180) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 16 LEDJmp))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5A15D3F1)
    (at 118.75 67.04)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at -0.03 -1.49) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75) (layer F.Fab) hide)
    (fp_text user "" (at 0.41 4.53) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(P2-Pad7)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 5V))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5A16D089)
    (at 113.45 54.81 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -0.12 1.43 360) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user "" (at 0 -1.7 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 RX))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 25 Reg3.3V))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 599F23B2)
    (at 133 31.04)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 3.13 -0.01 90) (layer F.SilkS))
    (fp_text value 330 (at 0 1.75) (layer F.Fab) hide)
    (fp_text user "" (at -0.24 1.98) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 599F23B0)
    (at 132.98 29.19)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 3.1 -0.03 90) (layer F.SilkS))
    (fp_text value 330 (at 0 1.75) (layer F.Fab))
    (fp_text user "" (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 26 BTVCC))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 599F23A4)
    (at 133.02 37.94)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 3.1 0.02 90) (layer F.SilkS))
    (fp_text value 330 (at 0 1.75) (layer F.Fab))
    (fp_text user "" (at -1.09 -1.62) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 SDVCC))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D4-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 59E375F0)
    (at 116.24 45.06)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 -1.38) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75) (layer F.Fab))
    (fp_text user "" (at 0 -1.7) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 28 SDVCC))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 17 RST))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5_HandSoldering (layer F.Cu) (tedit 59E37592)
    (at 130 65.8)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (attr smd)
    (fp_text reference U2 (at 1.3 -2.01) (layer F.SilkS))
    (fp_text value NCP1402 (at 0 2.9) (layer F.Fab))
    (pad 1 smd rect (at -1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 27 BATVCC))
    (pad 2 smd rect (at -1.35 0) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 27 BATVCC))
    (pad 3 smd rect (at -1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 1.35 0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.35 -0.95) (size 1.56 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes\SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A16D27F)
    (at 123.81 66.48)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at -2.01 -1.49) (layer F.SilkS))
    (fp_text value 1,0uF (at 0 1.75) (layer F.Fab))
    (fp_text user "" (at -3.06 -1.82) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 5V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 59A803CB)
    (at 123.79 68.28)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 3.69 0.2 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75) (layer F.Fab))
    (fp_text user "" (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 5V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5A16D099)
    (at 112.03 60.72)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 1.7 1.56) (layer F.SilkS))
    (fp_text value 1,0uF (at 0 1.75) (layer F.Fab))
    (fp_text user "" (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 25 Reg3.3V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductors:Inductor_Wurth_HCI-7050 (layer B.Cu) (tedit 595DDE86)
    (at 130.21 63.6 180)
    (descr "Inductor, Wurth Elektronik, Wurth_HCI-7050, 6.9mmx6.9mm")
    (tags "inductor wurth hci smd")
    (attr smd)
    (fp_text reference L1 (at -2.52 2.68 180) (layer B.SilkS))
    (fp_text value 47uH (at 0 -4.95 180) (layer B.Fab))
    (pad 1 smd rect (at -2.55 0 180) (size 2.7 2.2) (layers B.Cu B.Paste B.Mask)
      (net 22 BAT))
    (pad 2 smd rect (at 2.55 0 180) (size 2.7 2.2) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(D3-Pad2)"))
    (model Inductors.3dshapes/Inductor_Wurth_HCI-7050.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 595DE7E9)
    (at 123.83 62.79 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U3 (at 0.59 -1.17 270) (layer F.SilkS) hide)
    (fp_text value XC6206 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 Reg3.3V))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 595DDD04)
    (at 124.2 49.72 90)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference Atmega1 (at 2.58 0.13 180) (layer F.SilkS) hide)
    (fp_text value ATMEGA328P-A (at 0 6.05 90) (layer F.Fab))
    (fp_text user "" (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at -4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at -4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 SDVCC))
    (pad 5 smd rect (at -4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 SDVCC))
    (pad 7 smd rect (at -4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(Atmega1-Pad7)"))
    (pad 8 smd rect (at -4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(Atmega1-Pad8)"))
    (pad 9 smd rect (at -2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at -2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at -1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 12 smd rect (at -0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 13 smd rect (at 0.4 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 1.2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 SS))
    (pad 15 smd rect (at 2 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 MOSI))
    (pad 16 smd rect (at 2.8 4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 MISO))
    (pad 17 smd rect (at 4.25 2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 SCK))
    (pad 18 smd rect (at 4.25 2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 28 SDVCC))
    (pad 19 smd rect (at 4.25 1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 4.25 0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(Atmega1-Pad20)"))
    (pad 21 smd rect (at 4.25 -0.4 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 22 smd rect (at 4.25 -1.2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at 4.25 -2 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 24 smd rect (at 4.25 -2.8 90) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 25 smd rect (at 2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 20 CardS))
    (pad 26 smd rect (at 2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 27 smd rect (at 1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 28 smd rect (at 0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (pad 29 smd rect (at -0.4 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 17 RST))
    (pad 30 smd rect (at -1.2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 RX_SD))
    (pad 31 smd rect (at -2 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Atmega1-Pad31)"))
    (pad 32 smd rect (at -2.8 -4.25 180) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 5A16D0A3)
    (at 113.46 65.64 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D5 (at -2.72 -0.1 180) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user "" (at 0 -1.85 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 TX))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323_HandSoldering (layer F.Cu) (tedit 5A16D0A0)
    (at 115.15 65.65 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D6 (at -2.72 0.16 180) (layer F.SilkS))
    (fp_text value D (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user "" (at 0 -1.85 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 8 TX))
    (pad 2 smd rect (at 1.25 0 90) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(Atmega1-Pad31)"))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer B.Cu) (tedit 599F19DD)
    (at 134.79 42.03 180)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D7 (at 2.19 -0.13 270) (layer B.SilkS) hide)
    (fp_text value LED (at 0 -1.55 180) (layer B.Fab))
    (fp_text user %R (at 0 1.25 180) (layer B.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(D7-Pad2)"))
    (pad 1 smd rect (at -1.1 0) (size 1.2 1.2) (layers B.Cu B.Paste B.Mask)
      (net 16 LEDJmp))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 599F2392)
    (at 132.99 40.18 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -3.13 -0.01 270) (layer F.SilkS))
    (fp_text value 330 (at 0 1.75 180) (layer F.Fab))
    (fp_text user "" (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(D7-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 SCK))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ASKicadLib:Slide_Switch_SPDT_3Pin_2Position_OnOFF_Angle (layer F.Cu) (tedit 59A94A76)
    (at 107.68 47.65 90)
    (descr https://learn.sparkfun.com/tutorials/switch-basics/poles-and-throws-open-and-closed)
    (tags "Slide Switch ")
    (fp_text reference SW1 (at 1.08 1.56 90) (layer F.SilkS))
    (fp_text value SWITCH_BTSD (at 1.03 -3.44 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -2 0 90) (size 1.4 1.4) (drill 0.75) (layers *.Cu *.Mask)
      (net 28 SDVCC))
    (pad 3 thru_hole circle (at 2 0 90) (size 1.4 1.4) (drill 0.75) (layers *.Cu *.Mask)
      (net 26 BTVCC))
    (pad 4 thru_hole circle (at 4.3 0 90) (size 1.8 1.8) (drill 1.25) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -4.3 0 90) (size 1.8 1.8) (drill 1.25) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.75) (layers *.Cu *.Mask)
      (net 25 Reg3.3V))
  )
  (module ASKicadLib:Slide_Switch_SPDT_3Pin_2Position_OnOFF_Angle (layer F.Cu) (tedit 59A94A70)
    (at 107.7 58.32 270)
    (descr https://learn.sparkfun.com/tutorials/switch-basics/poles-and-throws-open-and-closed)
    (tags "Slide Switch ")
    (fp_text reference SW2 (at -0.93 -1.49 270) (layer F.SilkS))
    (fp_text value SWITCH_BAT (at 1.03 -3.44 270) (layer F.Fab))
    (pad 1 thru_hole circle (at -2 0 270) (size 1.4 1.4) (drill 0.75) (layers *.Cu *.Mask)
      (net 25 Reg3.3V))
    (pad 3 thru_hole circle (at 2 0 270) (size 1.4 1.4) (drill 0.75) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at 4.3 0 270) (size 1.8 1.8) (drill 1.25) (layers *.Cu *.Mask))
    (pad 4 thru_hole circle (at -4.3 0 270) (size 1.8 1.8) (drill 1.25) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.75) (layers *.Cu *.Mask)
      (net 27 BATVCC))
  )
  (module Pin_Headers:Pin_Header_Angled_1x09_Pitch2.54mm (layer F.Cu) (tedit 59DE78CC)
    (at 131.46 70.83 270)
    (descr "Through hole angled pin header, 1x09, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x09 2.54mm single row")
    (fp_text reference P2 (at 5.33 1.2 270) (layer F.SilkS) hide)
    (fp_text value CONN_01X09 (at 4.385 22.59 270) (layer F.Fab))
    (fp_text user %R (at 2.77 10.16 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 BAT))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 Reg3.3V))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 5V))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(P2-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 TX))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 FTDIRST))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-363_SC-70-6_Handsoldering (layer F.Cu) (tedit 5A16D08E)
    (at 115.98 51.59 270)
    (descr "SOT-363, SC-70-6, Handsoldering")
    (tags "SOT-363 SC-70-6 Handsoldering")
    (attr smd)
    (fp_text reference U4 (at 0.05 1.81 450) (layer F.SilkS))
    (fp_text value SN74LVC1G3157DCKR (at 0 2 450) (layer F.Fab))
    (fp_text user %R (at 0 0 360) (layer F.Fab))
    (pad 1 smd rect (at -1.33 -0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 30 RX_SD))
    (pad 2 smd rect (at -1.33 0 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -1.33 0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 31 RX_BT))
    (pad 4 smd rect (at 1.33 0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 RX))
    (pad 5 smd rect (at 1.33 0 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 Reg3.3V))
    (pad 6 smd rect (at 1.33 -0.65 270) (size 1.5 0.4) (layers F.Cu F.Paste F.Mask)
      (net 28 SDVCC))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-C_EIA-6032-28_Reflow (layer F.Cu) (tedit 5A0B3CAB)
    (at 115.18 58.18 180)
    (descr "Tantalum capacitor, Case C, EIA 6032-28, 6.0x3.2x2.5mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C4 (at 0.01 -0.01 180) (layer F.SilkS))
    (fp_text value 68uF (at 0 3.35 180) (layer F.Fab))
    (fp_text user %R (at 12.3 3.19 180) (layer F.Fab) hide)
    (pad 1 smd rect (at -2.525 0 180) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.525 0 180) (size 2.55 2.5) (layers F.Cu F.Paste F.Mask)
      (net 27 BATVCC))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-C_EIA-6032-28.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad_Via (layer F.Cu) (tedit 5A15C679)
    (at 109.59 66.71)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference P4 (at -5.65 -0.3) (layer F.SilkS) hide)
    (fp_text value MountHole1 (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.5mm_Pad_Via (layer F.Cu) (tedit 5A15C677)
    (at 133.08 48.27)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (attr virtual)
    (fp_text reference P5 (at 5.95 0.21) (layer F.SilkS) hide)
    (fp_text value MountHole2 (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.325825 1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.875 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at -1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 0 -1.875) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
    (pad "" thru_hole circle (at 1.325825 -1.325825) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask))
  )
  (module ASKicadLib:Testpoint (layer F.Cu) (tedit 5A16D012)
    (at 123.85 38.09)
    (descr www.openhardware.io)
    (fp_text reference W1 (at 15.42 1.19) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0.2 -1.7) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 26 BTVCC))
  )
  (module ASKicadLib:Testpoint (layer F.Cu) (tedit 5A16D016)
    (at 123.99 36.38)
    (descr www.openhardware.io)
    (fp_text reference W2 (at 15.12 1.03) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0.2 -1.7) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 28 SDVCC))
  )
  (module ASKicadLib:Testpoint (layer F.Cu) (tedit 5A16CFFA)
    (at 110.52 58.57)
    (descr www.openhardware.io)
    (fp_text reference W3 (at -6.58 3.41) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0.2 -1.7) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 27 BATVCC))
  )
  (module ASKicadLib:Testpoint (layer F.Cu) (tedit 5A16D00A)
    (at 134.34 71.49)
    (descr www.openhardware.io)
    (fp_text reference W4 (at 5.06 -0.76) (layer F.SilkS) hide)
    (fp_text value TEST_1P (at 0.2 -1.7) (layer F.Fab) hide)
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 22 BAT))
  )
  (module graphicslogo:OpenSourceLogo_1000x1000_neg (layer B.Cu) (tedit 0)
    (at 121.31 61.46 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text "Serial #" (at 109.71 31.88) (layer B.SilkS))
  (gr_text "LEDs\n" (at 135.88 65.26) (layer B.SilkS))
  (gr_text X (at 123.27 43.71) (layer F.SilkS))
  (gr_text RT (at 123.32 42.21) (layer F.SilkS))
  (gr_text NO! (at 131.75 57.36) (layer F.SilkS))
  (gr_text "Logger Machine" (at 121.23 55.63) (layer B.SilkS))
  (gr_text ON<>OFF (at 110.95 62.24 90) (layer B.SilkS))
  (gr_text GND (at 131.67 69.12) (layer B.SilkS))
  (gr_text BAT (at 128.98 69.11) (layer B.SilkS))
  (gr_text 3,3 (at 126.23 69.12) (layer B.SilkS))
  (gr_line (start 105.45 74.9) (end 113.3 74.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 105.45 26.39) (end 105.45 74.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.79 26.39) (end 105.45 26.39) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text SDLink (at 134.95 40.18) (layer B.SilkS))
  (gr_text "GND\n" (at 122.52 69.09) (layer B.SilkS))
  (gr_text V+ (at 118.56 69.07) (layer B.SilkS))
  (gr_text RX (at 116.23 69.09) (layer B.SilkS))
  (gr_text TX (at 113.69 69.09) (layer B.SilkS))
  (gr_text RS (at 108.87 71 90) (layer B.SilkS))
  (gr_text "Licensed under CERN OHL V1.2" (at 133.35 73.57) (layer B.SilkS))
  (gr_text Power (at 135.59 68.93) (layer B.SilkS))
  (gr_text "+\n" (at 113.64 47.12) (layer B.SilkS))
  (gr_text "+\n" (at 113.65 45.61) (layer B.SilkS))
  (gr_text "+\n" (at 113.65 30.6) (layer B.SilkS))
  (gr_text "+\n" (at 113.65 29.1) (layer B.SilkS))
  (gr_text - (at 126.48 26.6) (layer B.SilkS))
  (gr_text + (at 128.8 32.1) (layer B.SilkS))
  (gr_text + (at 128.81 29.14) (layer B.SilkS))
  (gr_text BT<>SD (at 110.87 50.86 90) (layer B.SilkS))
  (gr_text "SD ON\n" (at 134.86 36.41) (layer B.SilkS))
  (gr_text "BTLink\n" (at 134.88 32.72) (layer B.SilkS))
  (gr_text "BT ON" (at 134.82 29.07) (layer B.SilkS))
  (gr_text "Rev 0.5" (at 109.56 28.27) (layer B.SilkS))
  (gr_text openhardware.io (at 121.34 57.15) (layer B.SilkS))
  (gr_text "by sundberg84" (at 121.26 67.07) (layer B.SilkS))
  (gr_line (start 137.44 74.9) (end 112.78 74.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.44 26.38) (end 137.44 74.9) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.78 26.38) (end 137.44 26.38) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 105.08 25.87) (xy 137.94 25.93) (xy 137.44 76.18) (xy 103.92 75.36) (xy 104.83 25.9)
      )
    )
  )
)
