(kicad_pcb (version 20171130) (host pcbnew 6.0.0-rc1-unknown-ebb74fc~66~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 116)
    (tracks 1004)
    (zones 0)
    (modules 56)
    (nets 74)
  )
  (page A4)
  (title_block
    (title "ESP32 MySensors Gateway")
    (rev v3)
    (company freynder)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.15)
    (trace_clearance 0.127)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.001)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.8796 1.8796)
    (pad_drill 1.016)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 D+)
  (net 4 D-)
  (net 5 RFMANT)
  (net 6 DTR)
  (net 7 IO0)
  (net 8 EN)
  (net 9 RTS)
  (net 10 SENSOR_VP)
  (net 11 SENSOR_VN)
  (net 12 IO34)
  (net 13 IO35)
  (net 14 IO32)
  (net 15 IO33)
  (net 16 IO25)
  (net 17 IO26)
  (net 18 IO27)
  (net 19 IO14)
  (net 20 IO12)
  (net 21 IO13)
  (net 22 IO15)
  (net 23 IO2)
  (net 24 IO4)
  (net 25 IO16)
  (net 26 CE-RST)
  (net 27 IO5)
  (net 28 IO18)
  (net 29 IO19)
  (net 30 IO21)
  (net 31 ESPRX)
  (net 32 ESPTX)
  (net 33 IO22)
  (net 34 IO23)
  (net 35 "Net-(Q1-Pad1)")
  (net 36 "Net-(Q2-Pad1)")
  (net 37 "Net-(D1-Pad2)")
  (net 38 "Net-(D2-Pad2)")
  (net 39 "Net-(D3-Pad2)")
  (net 40 "Net-(D4-Pad2)")
  (net 41 IO20)
  (net 42 "Net-(D5-Pad2)")
  (net 43 LEDB)
  (net 44 RFPOW)
  (net 45 "Net-(J1-Pad4)")
  (net 46 "Net-(U1-Pad16)")
  (net 47 "Net-(U1-Pad15)")
  (net 48 "Net-(U1-Pad12)")
  (net 49 "Net-(U1-Pad11)")
  (net 50 "Net-(U1-Pad7)")
  (net 51 "Net-(U2-Pad22)")
  (net 52 "Net-(U2-Pad21)")
  (net 53 "Net-(U2-Pad20)")
  (net 54 "Net-(U2-Pad19)")
  (net 55 "Net-(U2-Pad18)")
  (net 56 "Net-(U2-Pad17)")
  (net 57 "Net-(U5-Pad12)")
  (net 58 "Net-(U5-Pad11)")
  (net 59 "Net-(U5-Pad10)")
  (net 60 "Net-(U5-Pad4)")
  (net 61 "Net-(U7-Pad3)")
  (net 62 "Net-(U7-Pad4)")
  (net 63 "Net-(U7-Pad5)")
  (net 64 "Net-(U7-Pad6)")
  (net 65 "Net-(U7-Pad7)")
  (net 66 "Net-(U8-Pad15)")
  (net 67 "Net-(U8-Pad12)")
  (net 68 "Net-(U8-Pad11)")
  (net 69 "Net-(U8-Pad10)")
  (net 70 "Net-(U8-Pad9)")
  (net 71 "Net-(U8-Pad8)")
  (net 72 "Net-(U8-Pad7)")
  (net 73 "Net-(J8-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.15)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CE-RST)
    (add_net D+)
    (add_net D-)
    (add_net DTR)
    (add_net EN)
    (add_net ESPRX)
    (add_net ESPTX)
    (add_net IO0)
    (add_net IO12)
    (add_net IO13)
    (add_net IO14)
    (add_net IO15)
    (add_net IO16)
    (add_net IO18)
    (add_net IO19)
    (add_net IO2)
    (add_net IO20)
    (add_net IO21)
    (add_net IO22)
    (add_net IO23)
    (add_net IO25)
    (add_net IO26)
    (add_net IO27)
    (add_net IO32)
    (add_net IO33)
    (add_net IO34)
    (add_net IO35)
    (add_net IO4)
    (add_net IO5)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J8-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad18)")
    (add_net "Net-(U2-Pad19)")
    (add_net "Net-(U2-Pad20)")
    (add_net "Net-(U2-Pad21)")
    (add_net "Net-(U2-Pad22)")
    (add_net "Net-(U5-Pad10)")
    (add_net "Net-(U5-Pad11)")
    (add_net "Net-(U5-Pad12)")
    (add_net "Net-(U5-Pad4)")
    (add_net "Net-(U7-Pad3)")
    (add_net "Net-(U7-Pad4)")
    (add_net "Net-(U7-Pad5)")
    (add_net "Net-(U7-Pad6)")
    (add_net "Net-(U7-Pad7)")
    (add_net "Net-(U8-Pad10)")
    (add_net "Net-(U8-Pad11)")
    (add_net "Net-(U8-Pad12)")
    (add_net "Net-(U8-Pad15)")
    (add_net "Net-(U8-Pad7)")
    (add_net "Net-(U8-Pad8)")
    (add_net "Net-(U8-Pad9)")
    (add_net RTS)
    (add_net SENSOR_VN)
    (add_net SENSOR_VP)
  )
  (net_class ANT ""
    (clearance 0.127)
    (trace_width 0.3048)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net RFMANT)
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.3)
    (via_dia 0.9)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net LEDB)
    (add_net RFPOW)
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 146.482816 98.166936 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0.890016 -1.13284 180) (layer F.SilkS))
    (fp_text value 4.7K (at -0.004064 1.159256 180) (layer F.Fab))
    (fp_text user %R (at 0.01524 -1.13284 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 LEDB))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 IO21))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 143.135096 98.166936 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R9 (at 1.147064 -1.12268 180) (layer F.SilkS))
    (fp_text value 4.7K (at -0.041656 1.139952 180) (layer F.Fab))
    (fp_text user %R (at 0.00508 -1.152144 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 LEDB))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 IO22))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:CP_Elec_4x5.4 (layer F.Cu) (tedit 5A841F9D)
    (at 157.53 78.93 90)
    (descr "SMT capacitor, aluminium electrolytic, 4x5.4, Panasonic A5, Nichicon ")
    (tags "Capacitor Electrolytic")
    (attr smd)
    (fp_text reference C13 (at 2.89 -2.04 180) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 3.2 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.8 0 90) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.8 0 90) (size 2.6 1.6) (layers F.Cu F.Paste F.Mask)
      (net 43 LEDB))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/CP_Elec_4x5.4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Sparkfun Connectors:1X04_NO_SILK" (layer F.Cu) (tedit 5963D344)
    (at 163.75 81.39 90)
    (descr "PLATED THROUGH HOLE - 4 PIN NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - 4 PIN NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J8 (at -1.668 -0.174 180) (layer F.SilkS))
    (fp_text value "RXB6 Breakout" (at 9.32 -2.03 270) (layer F.SilkS))
    (fp_text user %R (at 9.62 -0.91 180) (layer F.Fab))
    (fp_text user "RXB6 Breakout" (at -1.78 0.1 180) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.62 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 IO15) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 73 "Net-(J8-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 LEDB) (solder_mask_margin 0.1016))
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B20DC38)
    (at 161.13 80.15 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C12 (at -3.93 1.51 180) (layer F.SilkS))
    (fp_text value 10uF (at -2.02 0.05 180) (layer F.Fab))
    (fp_text user %R (at 2.01 0.01 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 43 LEDB))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 138.48 147.22 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.43 180) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.84 -0.01 180) (layer F.Fab))
    (fp_text user %R (at 1.53 -0.01 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B20DC38)
    (at 137.88 149.3 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.82 180) (layer F.SilkS))
    (fp_text value 4.7uF (at -2.7 0.01 180) (layer F.Fab))
    (fp_text user %R (at 2.09 0.01 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Sparkfun Connectors:1X04_NO_SILK" (layer F.Cu) (tedit 5BA27885)
    (at 140.11 94.93)
    (descr "PLATED THROUGH HOLE - 4 PIN NO SILK OUTLINE")
    (tags "PLATED THROUGH HOLE - 4 PIN NO SILK OUTLINE")
    (attr virtual)
    (fp_text reference J7 (at -2.02 0.04) (layer F.SilkS))
    (fp_text value "I2C Breakout" (at 3.6 2.02) (layer F.SilkS))
    (fp_text user J7 (at -2.188 0.066) (layer F.Fab))
    (fp_text user "I2C Breakout" (at 0.86 2.098) (layer F.Fab))
    (pad 4 thru_hole circle (at 7.62 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 IO21) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 IO22) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016) (zone_connect 1) (thermal_width 0.508) (thermal_gap 0.381))
    (pad 1 thru_hole circle (at 0 0) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 LEDB) (solder_mask_margin 0.1016))
  )
  (module custom:connector-XH2.54-01x05 (layer F.Cu) (tedit 5B9CDD08)
    (at 151.49 129.15 270)
    (fp_text reference J2 (at 7.18 4.08) (layer F.SilkS))
    (fp_text value "Button Connector" (at 0.07 -4.73 270) (layer F.SilkS) hide)
    (fp_text user "Button Connector" (at 8.264 0.106) (layer F.Fab))
    (fp_text user %R (at 8.264 3.662) (layer F.Fab))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 IO27) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 IO35) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 7 IO0) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 EN) (solder_mask_margin 0.1016))
  )
  (module custom:connector-XH2.54-01x06 (layer F.Cu) (tedit 5B9CDDA8)
    (at 120.904 140.97 270)
    (fp_text reference J3 (at -8.05 -2.066) (layer F.SilkS))
    (fp_text value "Ext LED header" (at 0.07 -4.73 270) (layer F.SilkS) hide)
    (fp_text user "Ext LED header" (at 10.668 -0.254) (layer F.Fab))
    (fp_text user %R (at 10.668 2.794) (layer F.Fab))
    (pad 6 thru_hole circle (at 7.62 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 5.08 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 42 "Net-(D5-Pad2)") (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 40 "Net-(D4-Pad2)") (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 39 "Net-(D3-Pad2)") (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at -2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 38 "Net-(D2-Pad2)") (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 37 "Net-(D1-Pad2)") (solder_mask_margin 0.1016))
  )
  (module ESP_WROOM_32:MODULE_ESP-WROOM-32 (layer F.Cu) (tedit 0)
    (at 142.38 81.58)
    (attr smd)
    (fp_text reference U2 (at 8.13 10.49) (layer F.SilkS))
    (fp_text value ESP-WROOM-32 (at 0.41629 5.10227) (layer F.SilkS))
    (pad 1.1 smd rect (at 0.7 -0.845) (size 4 4) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 38 smd rect (at 9 -8.255 180) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 37 smd rect (at 9 -6.985 180) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 IO23))
    (pad 36 smd rect (at 9 -5.715 180) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 IO22))
    (pad 35 smd rect (at 9 -4.445 180) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 ESPTX))
    (pad 34 smd rect (at 9 -3.175 180) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 ESPRX))
    (pad 33 smd rect (at 9 -1.905 180) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 IO21))
    (pad 32 smd rect (at 9 -0.635 180) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 IO20))
    (pad 31 smd rect (at 9 0.635 180) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 IO19))
    (pad 30 smd rect (at 9 1.905 180) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 IO18))
    (pad 29 smd rect (at 9 3.175 180) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 27 IO5))
    (pad 28 smd rect (at 9 4.445 180) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 CE-RST))
    (pad 27 smd rect (at 9 5.715 180) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 IO16))
    (pad 26 smd rect (at 9 6.985 180) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 IO4))
    (pad 25 smd rect (at 9 8.255 180) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 IO0))
    (pad 24 smd rect (at 5.715 9.755 90) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 IO2))
    (pad 23 smd rect (at 4.445 9.755 90) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 IO15))
    (pad 22 smd rect (at 3.175 9.755 90) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(U2-Pad22)"))
    (pad 21 smd rect (at 1.905 9.755 90) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(U2-Pad21)"))
    (pad 20 smd rect (at 0.635 9.755 90) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(U2-Pad20)"))
    (pad 19 smd rect (at -0.635 9.755 90) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(U2-Pad19)"))
    (pad 18 smd rect (at -1.905 9.755 90) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U2-Pad18)"))
    (pad 17 smd rect (at -3.175 9.755 90) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U2-Pad17)"))
    (pad 16 smd rect (at -4.445 9.755 90) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 IO13))
    (pad 15 smd rect (at -5.715 9.755 90) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 14 smd rect (at -9 8.255) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 IO12))
    (pad 13 smd rect (at -9 6.985) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 IO14))
    (pad 12 smd rect (at -9 5.715) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 18 IO27))
    (pad 11 smd rect (at -9 4.445) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 IO26))
    (pad 10 smd rect (at -9 3.175) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 IO25))
    (pad 9 smd rect (at -9 1.905) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 IO33))
    (pad 8 smd rect (at -9 0.635) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 IO32))
    (pad 7 smd rect (at -9 -0.635) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 IO35))
    (pad 6 smd rect (at -9 -1.905) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 IO34))
    (pad 5 smd rect (at -9 -3.175) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 SENSOR_VN))
    (pad 4 smd rect (at -9 -4.445) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 10 SENSOR_VP))
    (pad 3 smd rect (at -9 -5.715) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 EN))
    (pad 2 smd rect (at -9 -6.985) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 LEDB))
    (pad 1 smd rect (at -9 -8.255) (size 1.7 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model /home/freynder/KiCad/KiCAD-ESP-WROOM-32.wrl
      (offset (xyz 0 2.9 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module RF_Module:nRF24L01_Breakout (layer F.Cu) (tedit 5A056C61)
    (at 133.64 103.61 270)
    (descr "nRF24L01 breakout board")
    (tags "nRF24L01 adapter breakout")
    (fp_text reference U6 (at -2.2 9.53) (layer F.SilkS))
    (fp_text value NRF24L01_Breakout (at -2.264 4.1) (layer F.Fab))
    (fp_text user %R (at -2.264 -0.472) (layer F.Fab))
    (pad 8 thru_hole circle (at 2.54 7.62 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 25 IO16))
    (pad 7 thru_hole circle (at 0 7.62 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 29 IO19))
    (pad 6 thru_hole circle (at 2.54 5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 34 IO23))
    (pad 5 thru_hole circle (at 0 5.08 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 28 IO18))
    (pad 4 thru_hole circle (at 2.54 2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 27 IO5))
    (pad 3 thru_hole circle (at 0 2.54 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 26 CE-RST))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 44 RFPOW))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/RF_Module.3dshapes/nRF24L01_Breakout.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:HOPERF_RFM69HW-MINPADS (layer F.Cu) (tedit 5B9CD89B)
    (at 146.636 110.058)
    (descr "Radio, RF, Module, http://www.hoperf.com/upload/rf/RFM69HW-V1.3.pdf")
    (tags "Radio RF Module")
    (attr smd)
    (fp_text reference U7 (at -9.016 -9.518) (layer F.SilkS))
    (fp_text value "RFM69(H)W" (at 0 2.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -9.1 -7) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 26 CE-RST))
    (pad 2 smd rect (at -9.1 -5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 25 IO16))
    (pad 3 smd rect (at -9.1 -3) (size 2.5 1) (layers Eco1.User)
      (net 61 "Net-(U7-Pad3)"))
    (pad 4 smd rect (at -9.1 -1) (size 2.5 1) (layers Eco1.User)
      (net 62 "Net-(U7-Pad4)"))
    (pad 5 smd rect (at -9.1 1) (size 2.5 1) (layers Eco1.User)
      (net 63 "Net-(U7-Pad5)"))
    (pad 6 smd rect (at -9.1 3) (size 2.5 1) (layers Eco1.User)
      (net 64 "Net-(U7-Pad6)"))
    (pad 7 smd rect (at -9.1 5) (size 2.5 1) (layers Eco1.User)
      (net 65 "Net-(U7-Pad7)"))
    (pad 8 smd rect (at -9.1 7) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 44 RFPOW))
    (pad 9 smd rect (at 9.1 7) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 9.1 5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 5 RFMANT))
    (pad 11 smd rect (at 9.1 3) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 12 smd rect (at 9.1 1) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 28 IO18))
    (pad 13 smd rect (at 9.1 -1) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 29 IO19))
    (pad 14 smd rect (at 9.1 -3) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 34 IO23))
    (pad 15 smd rect (at 9.1 -5) (size 2.5 1) (layers F.Cu F.Paste F.Mask)
      (net 27 IO5))
    (pad 16 smd rect (at 9.1 -7) (size 2.5 1) (layers Eco1.User))
    (model ${KISYS3DMOD}/RF_Module.3dshapes/HOPERF_RFM69HW.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:RFM69CW-XXXS2-MINPADS (layer F.Cu) (tedit 5B9CDB45)
    (at 155.68792 110.04004 180)
    (descr "HOPE RF RFM69CW RF TRANSCIEVER")
    (tags "HOPE RF RFM69CW RF TRANSCIEVER")
    (attr smd)
    (fp_text reference U5 (at 6.891805 9.47004 180) (layer F.SilkS))
    (fp_text value RFM69CW (at 5.73792 8.70004 180) (layer F.SilkS))
    (fp_text user 1 (at -4.84886 -5.98424 180) (layer Dwgs.User))
    (pad 14 smd rect (at 7.49808 -5.99948 180) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 13 smd rect (at 7.49808 -3.99796 180) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 26 CE-RST) (solder_mask_margin 0.1016))
    (pad 12 smd rect (at 7.49808 -1.99898 180) (size 2.99974 1.19888) (layers Eco1.User)
      (net 57 "Net-(U5-Pad12)") (solder_mask_margin 0.1016))
    (pad 11 smd rect (at 7.49808 0 180) (size 2.99974 1.19888) (layers Eco1.User)
      (net 58 "Net-(U5-Pad11)") (solder_mask_margin 0.1016))
    (pad 10 smd rect (at 7.49808 1.99898 180) (size 2.99974 1.19888) (layers Eco1.User)
      (net 59 "Net-(U5-Pad10)") (solder_mask_margin 0.1016))
    (pad 9 smd rect (at 7.49808 3.99796 180) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 25 IO16) (solder_mask_margin 0.1016))
    (pad 8 smd rect (at 7.49808 5.99948 180) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 29 IO19) (solder_mask_margin 0.1016))
    (pad 7 smd rect (at -7.49808 5.99948 180) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 27 IO5) (solder_mask_margin 0.1016))
    (pad 6 smd rect (at -7.49808 3.99796 180) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 28 IO18) (solder_mask_margin 0.1016))
    (pad 5 smd rect (at -7.49808 1.99898 180) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 34 IO23) (solder_mask_margin 0.1016))
    (pad 4 smd rect (at -7.49808 0 180) (size 2.99974 1.19888) (layers Eco1.User)
      (net 60 "Net-(U5-Pad4)") (solder_mask_margin 0.1016))
    (pad 3 smd rect (at -7.49808 -1.99898 180) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -7.49808 -3.99796 180) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 44 RFPOW) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -7.49808 -5.99948 180) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 RFMANT) (solder_mask_margin 0.1016))
  )
  (module custom:RFM69HCW-XXXS2-MINPADS (layer F.Cu) (tedit 5B9CD96E)
    (at 152.046 110.078)
    (descr "HOPE RF RFM69HCW RF TRANSCIEVER")
    (tags "HOPE RF RFM69HCW RF TRANSCIEVER")
    (attr smd)
    (fp_text reference U1 (at -7.576 -9.418) (layer F.SilkS))
    (fp_text value RFM69HCW (at -6.182629 -8.698 180) (layer F.SilkS))
    (fp_text user 1 (at -4.84886 -5.98424) (layer Dwgs.User))
    (pad 16 smd rect (at 7.49808 -6.9977) (size 2.99974 1.19888) (layers Eco1.User)
      (net 46 "Net-(U1-Pad16)") (solder_mask_margin 0.1016))
    (pad 15 smd rect (at 7.49808 -4.99872) (size 2.99974 1.19888) (layers Eco1.User)
      (net 47 "Net-(U1-Pad15)") (solder_mask_margin 0.1016))
    (pad 14 smd rect (at 7.49808 -2.99974) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 25 IO16) (solder_mask_margin 0.1016))
    (pad 13 smd rect (at 7.49808 -0.99822) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 44 RFPOW) (solder_mask_margin 0.1016))
    (pad 12 smd rect (at 7.49808 0.99822) (size 2.99974 1.19888) (layers Eco1.User)
      (net 48 "Net-(U1-Pad12)") (solder_mask_margin 0.1016))
    (pad 11 smd rect (at 7.49808 2.99974) (size 2.99974 1.19888) (layers Eco1.User)
      (net 49 "Net-(U1-Pad11)") (solder_mask_margin 0.1016))
    (pad 10 smd rect (at 7.49808 4.99872) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 9 smd rect (at 7.49808 6.9977) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 5 RFMANT) (solder_mask_margin 0.1016))
    (pad 8 smd rect (at -7.49808 6.9977) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 7 smd rect (at -7.49808 4.99872) (size 2.99974 1.19888) (layers Eco1.User)
      (net 50 "Net-(U1-Pad7)") (solder_mask_margin 0.1016))
    (pad 6 smd rect (at -7.49808 2.99974) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 26 CE-RST) (solder_mask_margin 0.1016))
    (pad 5 smd rect (at -7.49808 0.99822) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 27 IO5) (solder_mask_margin 0.1016))
    (pad 4 smd rect (at -7.49808 -0.99822) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 28 IO18) (solder_mask_margin 0.1016))
    (pad 3 smd rect (at -7.49808 -2.99974) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 34 IO23) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -7.49808 -4.99872) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 29 IO19) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -7.49808 -6.9977) (size 2.99974 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module custom:AMS1117-3.3 (layer F.Cu) (tedit 0)
    (at 142.55 132.4 270)
    (attr smd)
    (fp_text reference U4 (at 3.09 -2.7) (layer F.SilkS))
    (fp_text value AMS1117-3.3 (at 0.22 0.13 270) (layer F.SilkS))
    (fp_text user AMS1117-3.3 (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.345 270) (size 3.24 1.31) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 2.29 3.345 270) (size 0.93 1.31) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0 3.345 270) (size 0.93 1.31) (layers F.Cu F.Paste F.Mask)
      (net 44 RFPOW))
    (pad 1 smd rect (at -2.29 3.345 270) (size 0.93 1.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 144.37 120.73 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at -2.24 -0.03 180) (layer F.SilkS))
    (fp_text value 10uF (at -1.71 0 180) (layer F.Fab))
    (fp_text user %R (at 1.56 0.02 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 RFPOW))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B20DC38)
    (at 136.76 133.8 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0.01 1.76) (layer F.SilkS))
    (fp_text value 22uF (at -2.12 -0.03) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 44 RFPOW))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 161.16 84.27 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at -1.47 1.59) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.26 0.02) (layer F.Fab))
    (fp_text user %R (at 1.38 0.02) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 LEDB))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 144.34 122.76 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -2.04 -0.02 180) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.75 0.01 180) (layer F.Fab))
    (fp_text user %R (at 1.42 -0.03 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 RFPOW))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 126.47 151.158 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 1.999525 -0.01 180) (layer F.SilkS))
    (fp_text value 22 (at 1.238 0.04 180) (layer F.Fab))
    (fp_text user %R (at -1.282 -0.06 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 21 IO13))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 128.754999 78.385001 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 0.044999 1.494999) (layer F.SilkS))
    (fp_text value 10K (at 0.254999 1.204999) (layer F.Fab))
    (fp_text user %R (at -0.425001 1.174999) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 EN))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 LEDB))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 133.3 151.158 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 1.999525 0.03634 180) (layer F.SilkS))
    (fp_text value 22 (at 1.188 0.1 180) (layer F.Fab))
    (fp_text user %R (at -1.262 0.01 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 LEDB))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 131.5925 151.158 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 1.999525 0.024755 180) (layer F.SilkS))
    (fp_text value 22 (at 1.218 -0.0525 180) (layer F.Fab))
    (fp_text user %R (at -1.262 -0.0025 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 IO12))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 129.885 151.158 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 1.999525 0.01317 180) (layer F.SilkS))
    (fp_text value 120 (at 1.238 -0.025 180) (layer F.Fab))
    (fp_text user %R (at -1.262 0.025 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 IO33))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 128.1775 151.158 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 1.999525 0.001585 180) (layer F.SilkS))
    (fp_text value 120 (at 1.268 -0.0075) (layer F.Fab))
    (fp_text user %R (at -1.302 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 IO32))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 157.50536 146.459973 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R7 (at -0.02464 1.179973 180) (layer F.SilkS))
    (fp_text value 12K (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0.02536 0.819973 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 DTR))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 157.50536 148.237973 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R8 (at 0.02536 -1.252027 180) (layer F.SilkS))
    (fp_text value 12K (at -0.02464 -1.572027 180) (layer F.Fab))
    (fp_text user %R (at 0.00536 -0.932027) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 "Net-(Q1-Pad1)"))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 RTS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B20DC39)
    (at 126.0945 156.89 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D4 (at -1.99 0.0005) (layer F.SilkS))
    (fp_text value "LED RED" (at -1.3 -0.0045 180) (layer F.Fab))
    (fp_text user %R (at 1.49 -0.0345 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(D4-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B20DC39)
    (at 129.297 156.85 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D3 (at -2.03 0.013 180) (layer F.SilkS))
    (fp_text value "LED YELLOW" (at -1.34 -0.027 180) (layer F.Fab))
    (fp_text user %R (at 1.39 -0.047 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(D3-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B20DC39)
    (at 132.4995 156.85 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D2 (at -2.03 0.0255 180) (layer F.SilkS))
    (fp_text value "LED GREEN" (at -1.35 0.0005 180) (layer F.Fab))
    (fp_text user %R (at 1.44 -0.0295 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(D2-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B20DC39)
    (at 135.702 156.85 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D1 (at -2.03 0.038 180) (layer F.SilkS))
    (fp_text value "LED BLUE" (at -1.32 0.008 180) (layer F.Fab))
    (fp_text user %R (at 1.5 0.048 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(D1-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LED_SMD:LED_0603_1608Metric (layer F.Cu) (tedit 5B20DC39)
    (at 122.892 156.85 90)
    (descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags diode)
    (attr smd)
    (fp_text reference D5 (at -2.03 -0.012 180) (layer F.SilkS))
    (fp_text value "LED WHITE" (at -1.32 -0.002 180) (layer F.Fab))
    (fp_text user %R (at 1.44 0.068 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 128.754999 81.395001 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at 0.095001 -1.494999 180) (layer F.SilkS))
    (fp_text value 0.1uF (at -0.354999 -1.314999 180) (layer F.Fab))
    (fp_text user %R (at 0.395001 -1.194999 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 EN))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 134.44 109.36 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 2.08 -0.08 180) (layer F.SilkS))
    (fp_text value 10nF (at -0.11 0.83 180) (layer F.Fab))
    (fp_text user %R (at 1.4 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 RFPOW))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 134.45 111.05 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 2.09 -0.08 180) (layer F.SilkS))
    (fp_text value 1nF (at -0.02 -0.87 180) (layer F.Fab))
    (fp_text user %R (at 1.34 -0.09 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 RFPOW))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_CK_RS282G05A3 (layer F.Cu) (tedit 5A7A67D2)
    (at 163.83 136.343332)
    (descr https://www.mouser.com/ds/2/60/RS-282G05A-SM_RT-1159762.pdf)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SW2 (at 3.93 -1.573332) (layer F.SilkS))
    (fp_text value SW_INCLUSION (at 0 3) (layer F.SilkS) hide)
    (fp_text user %R (at 0.05 0.11) (layer F.Fab))
    (pad 2 smd rect (at 3.9 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.9 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 13 IO35))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_CK_RS282G05A3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_CK_RS282G05A3 (layer F.Cu) (tedit 5A7A67D2)
    (at 163.83 141.12)
    (descr https://www.mouser.com/ds/2/60/RS-282G05A-SM_RT-1159762.pdf)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SW3 (at 3.93 -1.61) (layer F.SilkS))
    (fp_text value SW_GEN1 (at 0 3) (layer F.SilkS) hide)
    (fp_text user %R (at 0.02 0.05) (layer F.Fab))
    (pad 2 smd rect (at 3.9 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.9 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 IO27))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_CK_RS282G05A3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Sparkfun Connectors:1X17_NO_SILK" (layer F.Cu) (tedit 5963DB92)
    (at 168.656 119.664 90)
    (descr "PLATED THROUGH HOLE -17 PIN NO SILK")
    (tags "PLATED THROUGH HOLE -17 PIN NO SILK")
    (attr virtual)
    (fp_text reference J6 (at 0 -1.524 90) (layer F.SilkS) hide)
    (fp_text value "Header Right" (at 0 1.651 90) (layer F.SilkS) hide)
    (pad 17 thru_hole circle (at 40.64 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 34 IO23) (solder_mask_margin 0.1016))
    (pad 16 thru_hole circle (at 38.1 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 33 IO22) (solder_mask_margin 0.1016))
    (pad 15 thru_hole circle (at 35.56 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 ESPTX) (solder_mask_margin 0.1016))
    (pad 14 thru_hole circle (at 33.02 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 31 ESPRX) (solder_mask_margin 0.1016))
    (pad 13 thru_hole circle (at 30.48 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 30 IO21) (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at 27.94 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 41 IO20) (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 25.4 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 29 IO19) (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 22.86 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 28 IO18) (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 20.32 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 IO5) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 17.78 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 CE-RST) (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 15.24 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 IO16) (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 24 IO4) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 23 IO2) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 22 IO15) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 LEDB) (solder_mask_margin 0.1016))
  )
  (module "Sparkfun Connectors:1X17_NO_SILK" (layer F.Cu) (tedit 5963DB92)
    (at 116.27 79.03 270)
    (descr "PLATED THROUGH HOLE -17 PIN NO SILK")
    (tags "PLATED THROUGH HOLE -17 PIN NO SILK")
    (attr virtual)
    (fp_text reference J5 (at 0 -1.524 270) (layer F.SilkS) hide)
    (fp_text value "Header Left" (at 0 1.651 270) (layer F.SilkS) hide)
    (pad 17 thru_hole circle (at 40.64 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 16 thru_hole circle (at 38.1 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 15 thru_hole circle (at 35.56 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (pad 14 thru_hole circle (at 33.02 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 +5V) (solder_mask_margin 0.1016))
    (pad 13 thru_hole circle (at 30.48 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 43 LEDB) (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at 27.94 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 21 IO13) (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 25.4 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 20 IO12) (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 22.86 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 19 IO14) (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 20.32 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 18 IO27) (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 17.78 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 17 IO26) (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 15.24 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 16 IO25) (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 15 IO33) (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 14 IO32) (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 13 IO35) (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 12 IO34) (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 11 SENSOR_VN) (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask)
      (net 10 SENSOR_VP) (solder_mask_margin 0.1016))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 166.4 68.61)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MK3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 166.4 156.4)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MK2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 118.6 68.61)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MK1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 118.6 156.4)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MK4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B20DC38)
    (at 136.64 143.84 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -0.01 1.71) (layer F.SilkS))
    (fp_text value 22uF (at -2.08 -0.08) (layer F.Fab))
    (fp_text user %R (at 1.37 1.45) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 43 LEDB))
    (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:AMS1117-3.3 (layer F.Cu) (tedit 0)
    (at 142.55 142.43 270)
    (attr smd)
    (fp_text reference U3 (at 3.02 -2.7) (layer F.SilkS))
    (fp_text value AMS1117-3.3 (at 0.14 -0.11 90) (layer F.SilkS))
    (fp_text user AMS1117-3.3 (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.345 270) (size 3.24 1.31) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 2.29 3.345 270) (size 0.93 1.31) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0 3.345 270) (size 0.93 1.31) (layers F.Cu F.Paste F.Mask)
      (net 43 LEDB))
    (pad 1 smd rect (at -2.29 3.345 270) (size 0.93 1.31) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 129.82 75.62 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 2.15 0.01 180) (layer F.SilkS))
    (fp_text value 0.1uF (at -1.76 0.01 180) (layer F.Fab))
    (fp_text user %R (at 1.46 0.04 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 LEDB))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B20DC38)
    (at 129.784153 73.873299 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 2.164153 0.011667 180) (layer F.SilkS))
    (fp_text value 10uF (at -1.685847 0.023299 180) (layer F.Fab))
    (fp_text user %R (at 1.344153 -0.026701 180) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 LEDB))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module custom:aliexpress_micro_USB_connector (layer F.Cu) (tedit 5B3F243E)
    (at 142.49 158.03 180)
    (fp_text reference J1 (at 3.17 3.79 180) (layer F.SilkS))
    (fp_text value USB_B_Micro (at -0.27 -3.34 180) (layer F.Fab) hide)
    (fp_text user "PCB edge" (at -0.375 -1.77 180) (layer F.Fab))
    (pad 6 smd rect (at 1.25 -1.35) (size 1.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2 -1.35) (size 1.3 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0.925 3.2) (size 0.4 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 0.275 3.2) (size 0.4 1.6) (layers F.Cu F.Paste F.Mask)
      (net 4 D-))
    (pad 3 smd rect (at -0.375 3.2) (size 0.4 1.6) (layers F.Cu F.Paste F.Mask)
      (net 3 D+))
    (pad 4 smd rect (at -1.025 3.2) (size 0.4 1.6) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at -1.675 3.2) (size 0.4 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 2.05 2.68) (size 1.35 1.35) (drill oval 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at -2.8 2.68) (size 1.35 1.35) (drill oval 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at -4 0) (size 1.35 1.8) (drill oval 0.7 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 3.25 0) (size 1.35 1.8) (drill oval 0.7 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Connector_Coaxial:U.FL_Molex_MCRF_73412-0110_Vertical (layer F.Cu) (tedit 5A1B5B59)
    (at 159.766 120.904 180)
    (descr "Molex Microcoaxial RF Connectors (MCRF), mates Hirose U.FL, (http://www.molex.com/pdm_docs/sd/734120110_sd.pdf)")
    (tags "mcrf hirose ufl u.fl microcoaxial")
    (attr smd)
    (fp_text reference J4 (at -2.694 0.054 180) (layer F.SilkS))
    (fp_text value u.FL (at 0 -3.302 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.044 180) (layer F.Fab))
    (pad 1 smd rect (at 0 1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 5 RFMANT))
    (pad 2 smd rect (at 0 -1.5 180) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.475 0 180) (size 1.05 2.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_Coaxial.3dshapes/U.FL_Molex_MCRF_73412-0110_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_CK_RS282G05A3 (layer F.Cu) (tedit 5A7A67D2)
    (at 163.83 126.79)
    (descr https://www.mouser.com/ds/2/60/RS-282G05A-SM_RT-1159762.pdf)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SW1 (at 3.93 -1.56) (layer F.SilkS))
    (fp_text value SW_RESET (at 0 3) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 3.9 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.9 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 8 EN))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_CK_RS282G05A3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_SMD:SW_SPST_CK_RS282G05A3 (layer F.Cu) (tedit 5A7A67D2)
    (at 163.83 131.566666)
    (descr https://www.mouser.com/ds/2/60/RS-282G05A-SM_RT-1159762.pdf)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SW4 (at 3.93 -1.586666) (layer F.SilkS))
    (fp_text value SW_BOOT (at 0 3) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 3.9 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.9 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask)
      (net 7 IO0))
    (model ${KISYS3DMOD}/Button_Switch_SMD.3dshapes/SW_SPST_CK_RS282G05A3.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "Sparkfun Silicon-Standard:SO16" (layer F.Cu) (tedit 5961E22B)
    (at 156.11 155.29 180)
    (descr "SOIC, 0.15 INCH WIDTH")
    (tags "SOIC, 0.15 INCH WIDTH")
    (attr smd)
    (fp_text reference U8 (at -6.1 -1.52) (layer F.SilkS))
    (fp_text value CH340C (at 5.969 0 270) (layer F.SilkS))
    (fp_text user CH340C (at 0 0 180) (layer F.Fab))
    (pad 16 smd rect (at -4.445 -2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 43 LEDB) (solder_mask_margin 0.1016))
    (pad 15 smd rect (at -3.175 -2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(U8-Pad15)") (solder_mask_margin 0.1016))
    (pad 14 smd rect (at -1.905 -2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 9 RTS) (solder_mask_margin 0.1016))
    (pad 13 smd rect (at -0.635 -2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 6 DTR) (solder_mask_margin 0.1016))
    (pad 12 smd rect (at 0.635 -2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(U8-Pad12)") (solder_mask_margin 0.1016))
    (pad 11 smd rect (at 1.905 -2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(U8-Pad11)") (solder_mask_margin 0.1016))
    (pad 10 smd rect (at 3.175 -2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(U8-Pad10)") (solder_mask_margin 0.1016))
    (pad 9 smd rect (at 4.445 -2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(U8-Pad9)") (solder_mask_margin 0.1016))
    (pad 8 smd rect (at 4.445 2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(U8-Pad8)") (solder_mask_margin 0.1016))
    (pad 7 smd rect (at 3.175 2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(U8-Pad7)") (solder_mask_margin 0.1016))
    (pad 6 smd rect (at 1.905 2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 4 D-) (solder_mask_margin 0.1016))
    (pad 5 smd rect (at 0.635 2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 3 D+) (solder_mask_margin 0.1016))
    (pad 4 smd rect (at -0.635 2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 43 LEDB) (solder_mask_margin 0.1016))
    (pad 3 smd rect (at -1.905 2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 32 ESPTX) (solder_mask_margin 0.1016))
    (pad 2 smd rect (at -3.175 2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 31 ESPRX) (solder_mask_margin 0.1016))
    (pad 1 smd rect (at -4.445 2.79908 180) (size 0.59944 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOP-16_4.4x10.4mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 154.26 147.34 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -0.01 -2.15 180) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 2.5 180) (layer F.Fab) hide)
    (fp_text user %R (at 0.11 -2.15) (layer F.Fab))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 IO0))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 DTR))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 160.74 147.38)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 0.11 2.11) (layer F.SilkS))
    (fp_text value Q_NPN_BEC (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0.08 2.14 180) (layer F.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 EN))
    (pad 2 smd rect (at -1 0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 RTS))
    (pad 1 smd rect (at -1 -0.95) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbol:OSHW-Logo2_24.3x20mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 141.06 133.75 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_24.3x20mm_SilkScreen (at 0.75 0 180) (layer B.Fab) hide)
  )
  (gr_text 23 (at 166.294858 78.96) (layer B.SilkS))
  (gr_text GND (at 166.054286 117.058125) (layer B.SilkS))
  (gr_text 3V3 (at 165.859429 119.63) (layer B.SilkS))
  (gr_text 18 (at 166.294858 96.753125) (layer B.SilkS))
  (gr_text 5 (at 166.778667 99.295) (layer B.SilkS))
  (gr_text 22 (at 166.294858 81.501875) (layer B.SilkS))
  (gr_text TX (at 166.39162 84.04375) (layer B.SilkS))
  (gr_text 15 (at 166.294858 112.004375) (layer B.SilkS))
  (gr_text GND (at 166.054286 114.51625) (layer B.SilkS))
  (gr_text 4 (at 166.778667 106.920625) (layer B.SilkS))
  (gr_text 2 (at 166.778667 109.4625) (layer B.SilkS))
  (gr_text 17 (at 166.294858 101.836875) (layer B.SilkS))
  (gr_text 16 (at 166.294858 104.37875) (layer B.SilkS))
  (gr_text 20 (at 166.294858 91.669375) (layer B.SilkS))
  (gr_text 19 (at 166.294858 94.21125) (layer B.SilkS))
  (gr_text RX (at 166.270667 86.585625) (layer B.SilkS))
  (gr_text 21 (at 166.294858 89.1275) (layer B.SilkS))
  (gr_text 27 (at 118.785619 99.43) (layer B.SilkS))
  (gr_text 14 (at 118.785619 101.96625) (layer B.SilkS))
  (gr_text GND (at 118.91 119.77) (layer B.SilkS))
  (gr_text GND (at 118.91 114.64) (layer B.SilkS))
  (gr_text GND (at 118.93 117.17) (layer B.SilkS))
  (gr_text 12 (at 118.785619 104.5025) (layer B.SilkS))
  (gr_text 13 (at 118.785619 107.03875) (layer B.SilkS))
  (gr_text 26 (at 118.785619 96.89375) (layer B.SilkS))
  (gr_text 3V3 (at 118.94 109.57) (layer B.SilkS))
  (gr_text 5V (at 118.737238 112.11125) (layer B.SilkS))
  (gr_text 25 (at 118.74 94.33) (layer B.SilkS))
  (gr_text 33 (at 118.74 91.77) (layer B.SilkS))
  (gr_text 32 (at 118.74 89.28) (layer B.SilkS))
  (gr_text 35 (at 118.74 86.73) (layer B.SilkS))
  (gr_text 34 (at 118.74 84.17) (layer B.SilkS))
  (gr_text 39 (at 118.74 81.62) (layer B.SilkS))
  (gr_text 36 (at 118.785619 79.14) (layer B.SilkS))
  (gr_text B (at 116.26 135.78) (layer F.SilkS))
  (gr_text G (at 116.26 138.3336) (layer F.SilkS))
  (gr_text Y (at 116.26 140.8872) (layer F.SilkS))
  (gr_text R (at 116.26 143.4408) (layer F.SilkS))
  (dimension 95 (width 0.15) (layer Cmts.User)
    (gr_text "95,000 mm" (at 111.53 112.5 270) (layer Cmts.User))
    (feature1 (pts (xy 115 160) (xy 112.243579 160)))
    (feature2 (pts (xy 115 65) (xy 112.243579 65)))
    (crossbar (pts (xy 112.83 65) (xy 112.83 160)))
    (arrow1a (pts (xy 112.83 160) (xy 112.243579 158.873496)))
    (arrow1b (pts (xy 112.83 160) (xy 113.416421 158.873496)))
    (arrow2a (pts (xy 112.83 65) (xy 112.243579 66.126504)))
    (arrow2b (pts (xy 112.83 65) (xy 113.416421 66.126504)))
  )
  (dimension 1.25 (width 0.15) (layer Cmts.User)
    (gr_text "1,250 mm" (at 172.27 159.375 270) (layer Cmts.User))
    (feature1 (pts (xy 170 160) (xy 171.556421 160)))
    (feature2 (pts (xy 170 158.75) (xy 171.556421 158.75)))
    (crossbar (pts (xy 170.97 158.75) (xy 170.97 160)))
    (arrow1a (pts (xy 170.97 160) (xy 170.383579 158.873496)))
    (arrow1b (pts (xy 170.97 160) (xy 171.556421 158.873496)))
    (arrow2a (pts (xy 170.97 158.75) (xy 170.383579 159.876504)))
    (arrow2b (pts (xy 170.97 158.75) (xy 171.556421 159.876504)))
  )
  (dimension 3.2 (width 0.15) (layer Cmts.User)
    (gr_text "3,200 mm" (at 166.4 162.79) (layer Cmts.User))
    (feature1 (pts (xy 168 156.4) (xy 168 162.076421)))
    (feature2 (pts (xy 164.8 156.4) (xy 164.8 162.076421)))
    (crossbar (pts (xy 164.8 161.49) (xy 168 161.49)))
    (arrow1a (pts (xy 168 161.49) (xy 166.873496 162.076421)))
    (arrow1b (pts (xy 168 161.49) (xy 166.873496 160.903579)))
    (arrow2a (pts (xy 164.8 161.49) (xy 165.926504 162.076421)))
    (arrow2b (pts (xy 164.8 161.49) (xy 165.926504 160.903579)))
  )
  (dimension 3.6 (width 0.15) (layer Cmts.User)
    (gr_text "3,600 mm" (at 116.8 162.36) (layer Cmts.User))
    (feature1 (pts (xy 118.6 156.4) (xy 118.6 161.646421)))
    (feature2 (pts (xy 115 156.4) (xy 115 161.646421)))
    (crossbar (pts (xy 115 161.06) (xy 118.6 161.06)))
    (arrow1a (pts (xy 118.6 161.06) (xy 117.473496 161.646421)))
    (arrow1b (pts (xy 118.6 161.06) (xy 117.473496 160.473579)))
    (arrow2a (pts (xy 115 161.06) (xy 116.126504 161.646421)))
    (arrow2b (pts (xy 115 161.06) (xy 116.126504 160.473579)))
  )
  (dimension 55.01 (width 0.15) (layer Cmts.User)
    (gr_text "55,010 mm" (at 142.495 60.24) (layer Cmts.User))
    (feature1 (pts (xy 170 65) (xy 170 60.953579)))
    (feature2 (pts (xy 114.99 65) (xy 114.99 60.953579)))
    (crossbar (pts (xy 114.99 61.54) (xy 170 61.54)))
    (arrow1a (pts (xy 170 61.54) (xy 168.873496 62.126421)))
    (arrow1b (pts (xy 170 61.54) (xy 168.873496 60.953579)))
    (arrow2a (pts (xy 114.99 61.54) (xy 116.116504 62.126421)))
    (arrow2b (pts (xy 114.99 61.54) (xy 116.116504 60.953579)))
  )
  (dimension 47.8 (width 0.15) (layer Cmts.User)
    (gr_text "47,800 mm" (at 142.5 62.99) (layer Cmts.User))
    (feature1 (pts (xy 166.4 68.61) (xy 166.4 63.703579)))
    (feature2 (pts (xy 118.6 68.61) (xy 118.6 63.703579)))
    (crossbar (pts (xy 118.6 64.29) (xy 166.4 64.29)))
    (arrow1a (pts (xy 166.4 64.29) (xy 165.273496 64.876421)))
    (arrow1b (pts (xy 166.4 64.29) (xy 165.273496 63.703579)))
    (arrow2a (pts (xy 118.6 64.29) (xy 119.726504 64.876421)))
    (arrow2b (pts (xy 118.6 64.29) (xy 119.726504 63.703579)))
  )
  (gr_arc (start 170 160) (end 170 158.75) (angle -90) (layer Edge.Cuts) (width 0.001))
  (gr_arc (start 115 160) (end 116.25 160) (angle -90) (layer Edge.Cuts) (width 0.001))
  (gr_arc (start 170 65) (end 168.75 65) (angle -90) (layer Edge.Cuts) (width 0.001))
  (gr_arc (start 115 65) (end 115 66.25) (angle -90) (layer Edge.Cuts) (width 0.001))
  (gr_text Inclusion (at 124.46 156.311619 90) (layer F.SilkS))
  (gr_text "MySensors ESP32\nGateway V4.0\nby freynder" (at 129.032 140.208 90) (layer F.SilkS))
  (gr_text "Ext. LED" (at 120.62 152.03) (layer F.SilkS))
  (gr_text "NRF24L01\nBreakout" (at 128.39 117.51) (layer F.SilkS))
  (gr_text CUSTOM (at 156.41 141.09) (layer F.SilkS))
  (gr_text INCLUS (at 156.685167 136.38) (layer F.SilkS))
  (gr_text FLASH (at 157.045 131.656666) (layer F.SilkS))
  (gr_text RESET (at 157.045 126.78) (layer F.SilkS))
  (gr_text U.FL (at 156.54 120.85) (layer F.SilkS))
  (gr_text "RFM69(H)W" (at 139.07 101.25) (layer F.SilkS))
  (gr_text Power (at 137.414 157.244953 90) (layer F.SilkS))
  (gr_text Receive (at 134.1755 156.749715 90) (layer F.SilkS))
  (gr_text Transmit (at 130.937 156.464 90) (layer F.SilkS))
  (gr_text Error (at 127.6985 157.549715 90) (layer F.SilkS))
  (gr_text 3V3 (at 165.859429 119.69) (layer F.SilkS))
  (gr_text GND (at 166.054286 117.118125) (layer F.SilkS))
  (gr_text GND (at 166.054286 114.57625) (layer F.SilkS))
  (gr_text 15 (at 166.294858 112.064375) (layer F.SilkS))
  (gr_text 2 (at 166.778667 109.5225) (layer F.SilkS))
  (gr_text 4 (at 166.778667 106.980625) (layer F.SilkS))
  (gr_text 16 (at 166.294858 104.43875) (layer F.SilkS))
  (gr_text 17 (at 166.294858 101.896875) (layer F.SilkS))
  (gr_text 5 (at 166.778667 99.355) (layer F.SilkS))
  (gr_text 18 (at 166.294858 96.813125) (layer F.SilkS))
  (gr_text 19 (at 166.294858 94.27125) (layer F.SilkS))
  (gr_text 20 (at 166.294858 91.729375) (layer F.SilkS))
  (gr_text 21 (at 166.294858 89.1875) (layer F.SilkS))
  (gr_text RX (at 166.270667 86.645625) (layer F.SilkS))
  (gr_text TX (at 166.39162 84.10375) (layer F.SilkS))
  (gr_text 22 (at 166.294858 81.561875) (layer F.SilkS))
  (gr_text 23 (at 166.294858 79.02) (layer F.SilkS))
  (gr_text W (at 116.26 145.9944) (layer F.SilkS))
  (gr_text GND (at 116.26 148.62) (layer F.SilkS))
  (gr_text GND (at 118.91 119.77) (layer F.SilkS))
  (gr_text GND (at 118.93 117.17) (layer F.SilkS))
  (gr_text GND (at 118.91 114.64) (layer F.SilkS))
  (gr_text 5V (at 118.737238 112.11125) (layer F.SilkS))
  (gr_text 3V3 (at 118.94 109.57) (layer F.SilkS))
  (gr_text 13 (at 118.785619 107.03875) (layer F.SilkS))
  (gr_text 12 (at 118.785619 104.5025) (layer F.SilkS))
  (gr_text 14 (at 118.785619 101.96625) (layer F.SilkS))
  (gr_text 27 (at 118.785619 99.43) (layer F.SilkS))
  (gr_text 26 (at 118.785619 96.89375) (layer F.SilkS))
  (gr_text 25 (at 118.785619 94.3575) (layer F.SilkS))
  (gr_text 33 (at 118.785619 91.82125) (layer F.SilkS))
  (gr_text 32 (at 118.785619 89.285) (layer F.SilkS))
  (gr_text 35 (at 118.785619 86.74875) (layer F.SilkS))
  (gr_text 34 (at 118.785619 84.2125) (layer F.SilkS))
  (gr_text 39 (at 118.785619 81.67625) (layer F.SilkS))
  (gr_text 36 (at 118.785619 79.14) (layer F.SilkS))
  (gr_line (start 160 65) (end 168.75 65) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 160 72.59) (end 160 65) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 125 72.59) (end 160 72.59) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 125 65) (end 125 72.59) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 115 158.75) (end 115 66.25) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 168.75 160) (end 116.25 160) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 170 66.25) (end 170 158.75) (layer Edge.Cuts) (width 0.001))
  (gr_line (start 116.25 65) (end 125 65) (layer Edge.Cuts) (width 0.001))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 169.49 65.51) (xy 169.49 159.49) (xy 115.51 159.49) (xy 115.51 65.51)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.1524)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.54 65.51) (xy 169.49 65.51) (xy 169.49 159.49) (xy 115.51 159.49) (xy 115.51 65.51)
      )
    )
  )
)
