(kicad_pcb (version 20171130) (host pcbnew 5.0.0)
  (general
    (thickness 1.6)
    (drawings 55)
    (tracks 125)
    (zones 0)
    (modules 36)
    (nets 36)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.4)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 +3V3)
  (net 4 "Net-(J1-Pad5)")
  (net 5 "Net-(J1-Pad6)")
  (net 6 "Net-(J1-Pad7)")
  (net 7 "Net-(J1-Pad8)")
  (net 8 SCL)
  (net 9 "Net-(J1-Pad10)")
  (net 10 23)
  (net 11 "Net-(J1-Pad12)")
  (net 12 "Net-(J1-Pad13)")
  (net 13 "Net-(J1-Pad14)")
  (net 14 2)
  (net 15 "Net-(J1-Pad16)")
  (net 16 17)
  (net 17 "Net-(J1-Pad18)")
  (net 18 36)
  (net 19 37)
  (net 20 38)
  (net 21 39)
  (net 22 34)
  (net 23 35)
  (net 24 "Net-(J2-Pad10)")
  (net 25 "Net-(J2-Pad11)")
  (net 26 DAC2)
  (net 27 "Net-(J2-Pad13)")
  (net 28 "Net-(J2-Pad14)")
  (net 29 "Net-(J2-Pad15)")
  (net 30 12)
  (net 31 DHT_D)
  (net 32 SDA)
  (net 33 "Net-(J7-Pad3)")
  (net 34 "Net-(BT1-Pad1)")
  (net 35 "Net-(BT1-Pad2)")
  (net_class Default "Dies ist die voreingestellte Netzklasse."
    (clearance 0.4)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 12)
    (add_net 17)
    (add_net 2)
    (add_net 23)
    (add_net 34)
    (add_net 35)
    (add_net 36)
    (add_net 37)
    (add_net 38)
    (add_net 39)
    (add_net DAC2)
    (add_net DHT_D)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J7-Pad3)")
    (add_net SCL)
    (add_net SDA)
  )
  (net_class POWER ""
    (clearance 0.4)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(BT1-Pad2)")
  )
  (module Libs:gl_2 (layer F.Cu) (tedit 0)
    (at 106.3 111 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Libs:gl_1 (layer F.Cu) (tedit 0)
    (at 136.3 91 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Libs:gl_1 (layer F.Cu) (tedit 0)
    (at 136.3 111 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Libs:gl_2 (layer F.Cu) (tedit 0)
    (at 136.3 91 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Libs:gl_1 (layer F.Cu) (tedit 0)
    (at 106.3 91 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Libs:gl_2 (layer F.Cu) (tedit 0)
    (at 106.3 91 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Libs:gl_1 (layer F.Cu) (tedit 0)
    (at 106.3 111 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Libs:gl_2 (layer F.Cu) (tedit 0)
    (at 136.3 111 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Libs:gl_2 (layer F.Cu) (tedit 0)
    (at 136.3 131 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Libs:gl_1 (layer F.Cu) (tedit 0)
    (at 136.3 131 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Libs:gl_2 (layer F.Cu) (tedit 0)
    (at 136.3 151 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Libs:gl_1 (layer F.Cu) (tedit 0)
    (at 136.3 151 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Libs:gl_2 (layer F.Cu) (tedit 0)
    (at 106.3 131 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Libs:gl_1 (layer F.Cu) (tedit 0)
    (at 106.3 131 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Libs:gl_2 (layer B.Cu) (tedit 0)
    (at 102.5 92.5 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Libs:gl_2 (layer B.Cu) (tedit 0)
    (at 102.5 112.5 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Libs:gl_2 (layer B.Cu) (tedit 0)
    (at 102.5 132.5 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Libs:gl_1 (layer B.Cu) (tedit 0)
    (at 102.5 92.5 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Libs:gl_1 (layer B.Cu) (tedit 0)
    (at 102.5 112.5 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Libs:gl_1 (layer B.Cu) (tedit 0)
    (at 102.5 132.5 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Socket_Strips:Socket_Strip_Straight_1x18_Pitch2.54mm (layer F.Cu) (tedit 58CD5446)
    (at 120.06 79.6)
    (descr "Through hole straight socket strip, 1x18, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x18 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x18_Female (at 0 45.51) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad5)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad7)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad8)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 SCL))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 23))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad12)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 2))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad16)"))
    (pad 17 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 17))
    (pad 18 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad18)"))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x18_Pitch2.54mm.wrl
      (offset (xyz 0 -21.58999967575073 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x18_Pitch2.54mm locked (layer F.Cu) (tedit 58CD5446)
    (at 142.92 79.6)
    (descr "Through hole straight socket strip, 1x18, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x18 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33) (layer F.SilkS))
    (fp_text value Conn_01x18_Female (at 0 45.51) (layer F.Fab))
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 36))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 37))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 38))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 39))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 34))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 35))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J2-Pad10)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J2-Pad11)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 DAC2))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J2-Pad13)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J2-Pad14)"))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J2-Pad15)"))
    (pad 16 thru_hole oval (at 0 38.1) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 12))
    (pad 17 thru_hole oval (at 0 40.64) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 DHT_D))
    (pad 18 thru_hole oval (at 0 43.18) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 SDA))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_1x18_Pitch2.54mm.wrl
      (offset (xyz 0 -21.58999967575073 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 121.92 144.78 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 0 20.11 90) (layer F.Fab))
    (fp_text user %R (at 0 8.89 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 2))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 17))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 34))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 35))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 36))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 37))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 38))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 39))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 121.92 147.32 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 0 20.11 90) (layer F.Fab))
    (fp_text user %R (at 0 8.89 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 121.92 149.86 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x08 (at 0 20.11 90) (layer F.Fab))
    (fp_text user %R (at 0 8.89 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x08_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 138 161 90)
    (descr "Through hole straight pin header, 2x02, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x02 2.54mm double row")
    (fp_text reference J6 (at 4.9 1.2) (layer F.SilkS))
    (fp_text value Conn_02x02_Top_Bottom (at 1.27 4.87 90) (layer F.Fab))
    (fp_text user %R (at 1.016 2.286 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 SDA))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 SCL))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 129.08 161 270)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J7 (at -2.2 8.03) (layer F.SilkS))
    (fp_text value Conn_01x04 (at 0 9.95 270) (layer F.Fab))
    (fp_text user %R (at 0 3.81) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 DHT_D))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J7-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Battery_Holders:Keystone_1042_1x18650 (layer F.Cu) (tedit 5A033499)
    (at 101 120.33 90)
    (descr "Battery holder for 18650 cylindrical cells http://www.keyelco.com/product.cfm/product_id/918")
    (tags "18650 Keystone 1042 Li-ion")
    (attr smd)
    (fp_text reference BT1 (at 0 -11.5 90) (layer F.SilkS))
    (fp_text value Battery_Cell (at 0 11.3 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -39.33 0 90) (size 7.34 6.35) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(BT1-Pad1)"))
    (pad 2 smd rect (at 39.33 0 90) (size 7.34 6.35) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(BT1-Pad2)"))
    (pad "" np_thru_hole circle (at 27.6 -8 90) (size 3.45 3.45) (drill 3.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -27.6 8 90) (size 3.45 3.45) (drill 3.45) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -35.93 -8 90) (size 2.39 2.39) (drill 2.39) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Battery_Holders.3dshapes/Keystone_1042_1x18650.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 130.81 90.17 90)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J8 (at 2.77 -2.51 90) (layer F.SilkS))
    (fp_text value Conn_01x02 (at 4.385 4.81 90) (layer F.Fab))
    (fp_text user %R (at 2.77 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(BT1-Pad2)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Symbols:OSHW-Logo2_14.6x12mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 137 132.9 90)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_14.6x12mm_SilkScreen (at 0.75 0 90) (layer B.Fab) hide)
  )
  (module Symbols:Symbol_KiCAD-Logo_CopperAndSilkScreenTop (layer B.Cu) (tedit 0)
    (at 131.1 111.55 90)
    (descr "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (tags "Symbol, KiCAD-Logo, Silk & Copper Top,")
    (fp_text reference REF** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value "KiCAD Logo" (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Libs:gl_1 (layer B.Cu) (tedit 0)
    (at 102.5 152.5 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Libs:gl_2 (layer B.Cu) (tedit 0)
    (at 102.5 152.5 90)
    (fp_text reference G*** (at 0 0 90) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer B.SilkS) hide)
  )
  (module Libs:gl_2 (layer F.Cu) (tedit 0)
    (at 106.3 151 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Libs:gl_1 (layer F.Cu) (tedit 0)
    (at 106.3 151 90)
    (fp_text reference G*** (at 0 0 90) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 90) (layer F.SilkS) hide)
  )
  (module Resistors_SMD:R_1210_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 133.75 157.55 90)
    (descr "Resistor SMD 1210, hand soldering")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference R1 (at 4.25 0.05 180) (layer F.SilkS))
    (fp_text value 5k1 (at 0 2.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 31 DHT_D))
    (pad 1 smd rect (at -2 0 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_arc (start 90.95 103.5) (end 90.95 103) (angle -180) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 91.5 117.5) (end 91.5 117) (angle -180) (layer Edge.Cuts) (width 0.2))
  (gr_text "... goes here" (at 152.4 153.924) (layer F.SilkS))
  (gr_text This... (at 104.902 110.236 90) (layer F.SilkS))
  (gr_text DHT (at 118.364 161.036 90) (layer F.SilkS))
  (gr_text "Shitty Addon\nConnector" (at 144.526 159.512 90) (layer F.SilkS))
  (gr_text "Designed in the Swiss Alps\n2018 @morgulbrut" (at 138.35 100.35 270) (layer B.SilkS))
  (gr_text "2 17 34 35 36 37 38 39" (at 131.2418 142.4051) (layer F.SilkS))
  (gr_arc (start 132 76) (end 140 76) (angle 180) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 89 104) (end 89 81) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 148 76) (end 140 76) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 148 133) (end 148 76) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 160 145) (end 148 133) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 160 155) (end 160 145) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 150 165) (end 160 155) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 95 165) (end 150 165) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 89 159) (end 95 165) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 89 117) (end 89 159) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 94 76) (end 89 81) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 124 76) (end 94 76) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 95 110) (end 98.6 110) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 155 149.5) (end 155 150.2) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 155.5 150.2) (end 155.5 150.7) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 155.5 149.5) (end 155 149.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 149 149.5) (end 149 150.2) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 148.5 150.2) (end 149 150.2) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 148.5 149.5) (end 148.5 149) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 145 149.5) (end 145 150.2) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 145.5 150.2) (end 145.5 150.7) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 145.5 149.5) (end 145 149.5) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 159 149.5) (end 159 150.2) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 158.5 150.2) (end 159 150.2) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 158.5 149.5) (end 158.5 149) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 145.5 150.7) (end 148.5 150.7) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 145.5 149) (end 148.5 149) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 155.5 150.7) (end 158.5 150.7) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 155.5 149) (end 158.5 149) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 110.373969 105.991801) (end 108.373969 105.991801) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 110.373969 114.991801) (end 108.373969 114.991801) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 110.373969 106.991801) (end 110.373969 105.991801) (angle 89.9) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 108.373969 106.991801) (end 107.373969 106.991801) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 108.373969 113.991801) (end 108.373969 114.991801) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 110.373969 113.991801) (end 111.373969 113.991801) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 89 104) (end 89 117) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 107.373969 113.991801) (end 107.373969 106.991801) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 111.373969 106.991801) (end 111.373969 113.991801) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 110.873969 116.999801) (end 110.373969 116.999801) (angle 180) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 110.873969 103.991801) (end 111.373969 103.991801) (angle 180) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 91.45 117) (end 110.373969 116.991801) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 110.373969 103.991801) (end 90.95 104) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 110.373969 103.991801) (end 110.373969 102.991801) (angle 89.9) (layer Edge.Cuts) (width 0.2))
  (gr_arc (start 110.373969 116.991801) (end 111.373969 116.991801) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 91.55 118) (end 110.373969 117.991801) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 90.95 103) (end 110.373969 102.991801) (layer Edge.Cuts) (width 0.2))
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145 147.5) (xy 149 147.5) (xy 149 152.5) (xy 145 152.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0.06) (thermal_bridge_width 0.06))
    (polygon
      (pts
        (xy 110.373969 107.491801) (xy 105.373969 107.491801) (xy 105.373969 103.991801) (xy 109.873969 103.991801) (xy 110.373969 103.991801)
        (xy 110.373969 105.991801)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (mode segment) (arc_segments 16) (thermal_gap 0.06) (thermal_bridge_width 0.06))
    (polygon
      (pts
        (xy 110.373969 116.991801) (xy 105.373969 116.991801) (xy 105.373969 113.491801) (xy 109.873969 113.491801) (xy 110.373969 113.491801)
        (xy 110.373969 115.491801)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0.06) (thermal_bridge_width 0.06))
    (polygon
      (pts
        (xy 110.401241 107.491801) (xy 105.401241 107.491801) (xy 105.401241 103.991801) (xy 109.901241 103.991801) (xy 110.401241 103.991801)
        (xy 110.401241 105.991801)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0.06) (thermal_bridge_width 0.06))
    (polygon
      (pts
        (xy 110.373969 116.991801) (xy 105.373969 116.991801) (xy 105.373969 113.491801) (xy 109.873969 113.491801) (xy 110.373969 113.491801)
        (xy 110.373969 115.491801)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0.06) (thermal_bridge_width 0.06))
    (polygon
      (pts
        (xy 110.373969 103.892519) (xy 110.373969 103.970226) (xy 110.373969 116.892519) (xy 105.373969 116.892519) (xy 105.373969 103.892519)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0.06) (thermal_bridge_width 0.06))
    (polygon
      (pts
        (xy 110.373969 103.991801) (xy 110.373969 116.991801) (xy 105.373969 116.991801) (xy 105.373969 103.991801)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0.06) (thermal_bridge_width 0.06))
    (polygon
      (pts
        (xy 149 147.5) (xy 149 152.5) (xy 145 152.5) (xy 145 147.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.05)
    (fill yes (arc_segments 16) (thermal_gap 0.06) (thermal_bridge_width 0.06))
    (polygon
      (pts
        (xy 159 147.5) (xy 159 152.5) (xy 155 152.5) (xy 155 147.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Mask) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155 147.5) (xy 159 147.5) (xy 159 152.5) (xy 155 152.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148 133) (xy 143 138) (xy 143 165) (xy 115 165) (xy 115 76)
        (xy 124 76) (xy 148 76)
      )
    )
  )
  (zone (net 3) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115 76) (xy 148 76) (xy 148 133) (xy 143 138) (xy 143 165)
        (xy 115 165)
      )
    )
  )
)
