(kicad_pcb (version 20171130) (host pcbnew 5.0.0-fee4fd1~66~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 28)
    (tracks 891)
    (zones 0)
    (modules 75)
    (nets 81)
  )
  (page A3)
  (title_block
    (date "15 nov 2012")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.2032)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.1)
    (edge_width 0.1)
    (via_size 0.9)
    (via_drill 0.6)
    (via_min_size 0.8)
    (via_min_drill 0.5)
    (uvia_size 0.5)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.5)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1 1)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2.5 2.5)
    (pad_drill 2.5)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 200 150)
    (grid_origin 200 150)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x01030_ffffffff)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Manufacturing"))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 +5V)
  (net 3 GND)
  (net 4 /ID_SD)
  (net 5 /ID_SC)
  (net 6 "/GPIO2(SDA1)")
  (net 7 "/GPIO3(SCL1)")
  (net 8 "/GPIO4(GCLK)")
  (net 9 "/GPIO14(TXD0)")
  (net 10 "/GPIO15(RXD0)")
  (net 11 "/GPIO24(GEN5)")
  (net 12 "/GPIO25(GEN6)")
  (net 13 "/GPIO10(SPI0_MOSI)")
  (net 14 "/GPIO9(SPI0_MISO)")
  (net 15 "/GPIO11(SPI0_SCK)")
  (net 16 "/GPIO8(SPI0_CE_N)")
  (net 17 "/GPIO7(SPI1_CE_N)")
  (net 18 "/GPIO12(PWM0)")
  (net 19 "/GPIO13(PWM1)")
  (net 20 "/GPIO19(SPI1_MISO)")
  (net 21 "/GPIO20(SPI1_MOSI)")
  (net 22 /DIN)
  (net 23 /BCLK)
  (net 24 "Net-(U1-Pad12)")
  (net 25 "Net-(U1-Pad14)")
  (net 26 "Net-(U1-Pad19)")
  (net 27 "Net-(U1-Pad32)")
  (net 28 +12V)
  (net 29 "Net-(J2-Pad2)")
  (net 30 /WS2812_DATA)
  (net 31 /PWM1)
  (net 32 /PWM2)
  (net 33 /PWM3)
  (net 34 /POWER)
  (net 35 "Net-(Q1-Pad1)")
  (net 36 "Net-(Q2-Pad1)")
  (net 37 "Net-(Q3-Pad1)")
  (net 38 "Net-(Q4-Pad1)")
  (net 39 /FAN)
  (net 40 "Net-(R9-Pad2)")
  (net 41 "Net-(R10-Pad2)")
  (net 42 /BUTTON1)
  (net 43 /BUTTON2)
  (net 44 /BUTTON3)
  (net 45 /BUTTON4)
  (net 46 /BTN_PWR)
  (net 47 "/GPIO17(GEN0)")
  (net 48 "/GPIO22(GEN3)")
  (net 49 "/GPIO27(GEN2)")
  (net 50 "/GPIO23(GEN4)")
  (net 51 "Net-(R21-Pad1)")
  (net 52 "Net-(J4-Pad2)")
  (net 53 "Net-(C14-Pad2)")
  (net 54 "Net-(C15-Pad2)")
  (net 55 "Net-(U2-Pad13)")
  (net 56 "Net-(U2-Pad12)")
  (net 57 "Net-(U2-Pad6)")
  (net 58 "Net-(U2-Pad5)")
  (net 59 "Net-(U2-Pad2)")
  (net 60 "Net-(U3-Pad2)")
  (net 61 "Net-(U3-Pad5)")
  (net 62 "Net-(U3-Pad6)")
  (net 63 "Net-(U3-Pad12)")
  (net 64 "Net-(U3-Pad13)")
  (net 65 "Net-(C16-Pad1)")
  (net 66 "Net-(C17-Pad1)")
  (net 67 "Net-(C18-Pad1)")
  (net 68 "Net-(C19-Pad1)")
  (net 69 "Net-(L1-Pad2)")
  (net 70 "Net-(L2-Pad2)")
  (net 71 "Net-(L3-Pad2)")
  (net 72 "Net-(L4-Pad2)")
  (net 73 /RESET_ATMEGA)
  (net 74 "Net-(U2-Pad17)")
  (net 75 "Net-(U3-Pad17)")
  (net 76 "Net-(D1-Pad1)")
  (net 77 "Net-(R19-Pad1)")
  (net 78 "Net-(LED1-Pad2)")
  (net 79 "Net-(LED2-Pad2)")
  (net 80 "Net-(LED3-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.9)
    (via_drill 0.6)
    (uvia_dia 0.5)
    (uvia_drill 0.1)
    (add_net /BCLK)
    (add_net /BTN_PWR)
    (add_net /BUTTON1)
    (add_net /BUTTON2)
    (add_net /BUTTON3)
    (add_net /BUTTON4)
    (add_net /DIN)
    (add_net /FAN)
    (add_net "/GPIO10(SPI0_MOSI)")
    (add_net "/GPIO11(SPI0_SCK)")
    (add_net "/GPIO12(PWM0)")
    (add_net "/GPIO13(PWM1)")
    (add_net "/GPIO14(TXD0)")
    (add_net "/GPIO15(RXD0)")
    (add_net "/GPIO17(GEN0)")
    (add_net "/GPIO19(SPI1_MISO)")
    (add_net "/GPIO2(SDA1)")
    (add_net "/GPIO20(SPI1_MOSI)")
    (add_net "/GPIO22(GEN3)")
    (add_net "/GPIO23(GEN4)")
    (add_net "/GPIO24(GEN5)")
    (add_net "/GPIO25(GEN6)")
    (add_net "/GPIO27(GEN2)")
    (add_net "/GPIO3(SCL1)")
    (add_net "/GPIO4(GCLK)")
    (add_net "/GPIO7(SPI1_CE_N)")
    (add_net "/GPIO8(SPI0_CE_N)")
    (add_net "/GPIO9(SPI0_MISO)")
    (add_net /ID_SC)
    (add_net /ID_SD)
    (add_net /POWER)
    (add_net /PWM1)
    (add_net /PWM2)
    (add_net /PWM3)
    (add_net /RESET_ATMEGA)
    (add_net /WS2812_DATA)
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(C15-Pad2)")
    (add_net "Net-(C16-Pad1)")
    (add_net "Net-(C17-Pad1)")
    (add_net "Net-(C18-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(L2-Pad2)")
    (add_net "Net-(L3-Pad2)")
    (add_net "Net-(L4-Pad2)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(LED2-Pad2)")
    (add_net "Net-(LED3-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
    (add_net "Net-(Q4-Pad1)")
    (add_net "Net-(R10-Pad2)")
    (add_net "Net-(R19-Pad1)")
    (add_net "Net-(R21-Pad1)")
    (add_net "Net-(R9-Pad2)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad32)")
    (add_net "Net-(U2-Pad12)")
    (add_net "Net-(U2-Pad13)")
    (add_net "Net-(U2-Pad17)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U2-Pad6)")
    (add_net "Net-(U3-Pad12)")
    (add_net "Net-(U3-Pad13)")
    (add_net "Net-(U3-Pad17)")
    (add_net "Net-(U3-Pad2)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
  )
  (net_class Power ""
    (clearance 0.2032)
    (trace_width 0.508)
    (via_dia 1)
    (via_drill 0.7)
    (uvia_dia 0.5)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
  )
  (module adafruit:FAN (layer F.Cu) (tedit 5BBEEE3E)
    (at 233.2454 119.6184)
    (fp_text reference REF** (at 0 0.5) (layer F.SilkS))
    (fp_text value FAN (at 0 -0.5) (layer F.Fab))
    (pad "" np_thru_hole circle (at -12.5 -12.5) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -12.5 12.5) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 12.5 12.5) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 12.5 -12.5) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (model /home/thomas/fan.wrl
      (offset (xyz 0 0 2.7))
      (scale (xyz 0.38 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 252.0954 120.3836 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R16 (at -3.036 0.0762 180) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 /ID_SD))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 55360473)
    (at 252.07 123.0252 90)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U5 (at 0.9906 2.7432 -180) (layer F.SilkS))
    (fp_text value 24AA02-OT (at -0.05 2.35 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 /ID_SC))
    (pad 2 smd rect (at -1.1 0 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at -1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 4 /ID_SD))
    (pad 4 smd rect (at 1.1 0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at 1.1 -0.95 90) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 252.8828 126.7336 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at -2.8956 -0.1016 180) (layer F.SilkS))
    (fp_text value 4k7 (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /ID_SC))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST_PH:Connectors_JST_B3B-PH-K (layer F.Cu) (tedit 5BBE5D38)
    (at 231.81858 146.08078)
    (descr "JST PH series connector, B3B-PH-K")
    (tags "connector jst ph")
    (fp_text reference J12 (at -2.826 0 90) (layer F.SilkS))
    (fp_text value "External relay" (at 1.86182 -2.25298) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 34 /POWER))
    (pad 3 thru_hole oval (at 4 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B3B-PH-K_1x03_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5415CDEB)
    (at 257.9374 120.9678)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R21 (at 2.01926 -0.0254 90) (layer F.SilkS))
    (fp_text value 100k (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R21-Pad1)"))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_obscurities:XTAL_3.2x1.5mm (layer B.Cu) (tedit 55B4F766)
    (at 255.46598 139.64188 315)
    (descr "XTAL 3.2 x 1.5mm footprint")
    (tags Xtal)
    (fp_text reference Y1 (at 0.3 1.5 315) (layer B.SilkS))
    (fp_text value Crystal (at 0 -1.8 315) (layer B.Fab))
    (pad 2 smd rect (at 1.5 0 315) (size 1.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(C15-Pad2)"))
    (pad 1 smd rect (at -1.5 0 315) (size 1.5 1.8) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(C14-Pad2)"))
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/crystal/crystal_smd_5x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.64 0.5 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 210.287 101.9686 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 3.2258 0.5842 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 210.3124 111.7222 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0.2954 1.5748 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 180) (layer F.Fab))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 261.3664 105.4992)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 2.1) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1) (layer B.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 42 /BUTTON1))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 261.30366 110.83066)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 2.1) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 43 /BUTTON2))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 254.56098 106.03006)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 2.1) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 44 /BUTTON3))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5415D6EA)
    (at 254.5592 111.138)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 2.1) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1) (layer B.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 45 /BUTTON4))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer B.Cu) (tedit 5BB10887)
    (at 261.33084 116.25102)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 2.1) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1) (layer B.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 46 /BTN_PWR))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 5415D6EA)
    (at 249.4792 144.4628 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 1.0922 -1.6764 270) (layer F.SilkS))
    (fp_text value 100nF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 73 /RESET_ATMEGA))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 229.6418 137.2746 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -2.2352 -0.0762 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 /FAN))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 229.6418 138.9002 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -2.2352 0.0254) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 /PWM1))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 55360473)
    (at 221.778 141.194 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U4 (at -2.3954 0.061) (layer F.SilkS))
    (fp_text value 74AUP1G34 (at -0.05 2.35 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 30 /WS2812_DATA))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(J4-Pad2)"))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST_PH:Connectors_JST_B2B-PH-K (layer F.Cu) (tedit 5BBE589B)
    (at 212.7 124.0158 270)
    (descr "JST PH series connector, B2B-PH-K")
    (tags "connector jst ph")
    (fp_text reference J2 (at 1.27 -2.7178 270) (layer F.SilkS))
    (fp_text value FAN (at 1 4 270) (layer F.SilkS))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(J2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 0)
    (at 203.6576 125.8446 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J1 (at -2.54 1.5748 180) (layer F.SilkS))
    (fp_text value Power (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 +12V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (offset (xyz 0 -2.539999961853027 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connectors_JST_PH:Connectors_JST_B2B-PH-K (layer F.Cu) (tedit 55F6C32A)
    (at 260.4266 114.5416)
    (descr "JST PH series connector, B2B-PH-K")
    (tags "connector jst ph")
    (fp_text reference J11 (at -2.794 0 90) (layer F.SilkS))
    (fp_text value BUTTON_PWR (at 1 4) (layer F.Fab))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 46 /BTN_PWR))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST_PH:Connectors_JST_B2B-PH-K (layer F.Cu) (tedit 55F6C32A)
    (at 253.4482 108.979)
    (descr "JST PH series connector, B2B-PH-K")
    (tags "connector jst ph")
    (fp_text reference J10 (at -2.794 0.254 90) (layer F.SilkS))
    (fp_text value BUTTON4 (at 1 4) (layer F.Fab))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 45 /BUTTON4))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST_PH:Connectors_JST_B2B-PH-K (layer F.Cu) (tedit 55F6C32A)
    (at 260.4266 103.4164)
    (descr "JST PH series connector, B2B-PH-K")
    (tags "connector jst ph")
    (fp_text reference J7 (at -2.794 0 90) (layer F.SilkS))
    (fp_text value BUTTON1 (at 1 4) (layer F.Fab))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 42 /BUTTON1))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03 (layer F.Cu) (tedit 5BBE5D08)
    (at 218.3134 145.555 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J4 (at 2.3876 -0.5588 180) (layer F.SilkS))
    (fp_text value WS2812 (at -2.5654 2.4892 180) (layer F.SilkS))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x03.wrl
      (offset (xyz 0 -2.539999961853027 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5415D631)
    (at 255.52133 136.68733 135)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at 0 1.9 135) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.9 135) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 135) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 53 "Net-(C14-Pad2)"))
    (pad 1 smd rect (at -0.75 0 135) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer B.Cu) (tedit 5415D631)
    (at 257.6326 138.7986 315)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at 0 1.9 315) (layer B.SilkS))
    (fp_text value 22pF (at 0 -1.9 315) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 315) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 54 "Net-(C15-Pad2)"))
    (pad 1 smd rect (at -0.75 0 315) (size 0.8 0.75) (layers B.Cu B.Paste B.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer F.Cu) (tedit 54130A77)
    (at 256.711954 134.769642 45)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference U1 (at 0 -6.05 45) (layer F.SilkS))
    (fp_text value ATmega328-AU (at 0 6.05 45) (layer F.Fab))
    (pad 1 smd rect (at -4.25 -2.8 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 32 /PWM2))
    (pad 2 smd rect (at -4.25 -2 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(R19-Pad1)"))
    (pad 3 smd rect (at -4.25 -1.2 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd rect (at -4.25 -0.4 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at -4.25 0.4 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 6 smd rect (at -4.25 1.2 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 7 smd rect (at -4.25 2 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(C14-Pad2)"))
    (pad 8 smd rect (at -4.25 2.8 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(C15-Pad2)"))
    (pad 9 smd rect (at -2.8 4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 31 /PWM1))
    (pad 10 smd rect (at -2 4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 33 /PWM3))
    (pad 11 smd rect (at -1.2 4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 30 /WS2812_DATA))
    (pad 12 smd rect (at -0.4 4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U1-Pad12)"))
    (pad 13 smd rect (at 0.4 4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 39 /FAN))
    (pad 14 smd rect (at 1.2 4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U1-Pad14)"))
    (pad 15 smd rect (at 2 4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 13 "/GPIO10(SPI0_MOSI)"))
    (pad 16 smd rect (at 2.8 4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "/GPIO9(SPI0_MISO)"))
    (pad 17 smd rect (at 4.25 2.8 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 15 "/GPIO11(SPI0_SCK)"))
    (pad 18 smd rect (at 4.25 2 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 19 smd rect (at 4.25 1.2 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U1-Pad19)"))
    (pad 20 smd rect (at 4.25 0.4 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 21 smd rect (at 4.25 -0.4 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 22 smd rect (at 4.25 -1.2 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(R21-Pad1)"))
    (pad 23 smd rect (at 4.25 -2 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 46 /BTN_PWR))
    (pad 24 smd rect (at 4.25 -2.8 45) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 34 /POWER))
    (pad 25 smd rect (at 2.8 -4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 50 "/GPIO23(GEN4)"))
    (pad 26 smd rect (at 2 -4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 "/GPIO24(GEN5)"))
    (pad 27 smd rect (at 1.2 -4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 4 /ID_SD))
    (pad 28 smd rect (at 0.4 -4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 5 /ID_SC))
    (pad 29 smd rect (at -0.4 -4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 73 /RESET_ATMEGA))
    (pad 30 smd rect (at -1.2 -4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 "/GPIO14(TXD0)"))
    (pad 31 smd rect (at -2 -4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 10 "/GPIO15(RXD0)"))
    (pad 32 smd rect (at -2.8 -4.25 135) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U1-Pad32)"))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5415CC62)
    (at 258.20664 104.43494 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0 1.9 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.9 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 42 /BUTTON1))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5415CC62)
    (at 251.38928 107.97316 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at 0 1.9 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.9 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 45 /BUTTON4))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 261.40958 130.24388 135)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0 -1.9 135) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 135) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 250.42207 138.24287 135)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at -0.197566 -1.257236 135) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.9 135) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0 135) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 209.525 144.0564)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at -2.54 0.254 90) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 0 2.3) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(Q3-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 0 -0.99822) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 80 "Net-(LED3-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5BBE5BFF)
    (at 203.5814 138.3922 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference LED3 (at -0.0508 5.6642 180) (layer F.SilkS))
    (fp_text value LED3 (at -0.0254 5.7912 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(LED3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 +12V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5BBE5BF3)
    (at 203.5814 131.2548 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference LED1 (at -0.0254 5.588 180) (layer F.SilkS))
    (fp_text value LED1 (at 0.0254 5.8928 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(LED1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 +12V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5BBE5BFA)
    (at 203.5814 134.8616 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference LED2 (at 0.0254 5.6134 180) (layer F.SilkS))
    (fp_text value LED2 (at -0.0254 5.842 180) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(LED2-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 28 +12V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 212.5984 134.9632 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at -2.54 0.254 180) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 78 "Net-(LED1-Pad2)"))
    (model Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 227.0136 142.2022 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.274 -0.0254) (layer F.SilkS))
    (fp_text value 0R (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(Q3-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 /PWM3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BABD547)
    (at 227.0002 138.9002 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.2352 -0.0762) (layer F.SilkS))
    (fp_text value 0R (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(Q1-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 /PWM1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 227.0002 140.5258 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.2352 -0.0254) (layer F.SilkS))
    (fp_text value 0R (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Q2-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 /PWM2))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 229.6418 140.5512 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2.2352 -0.0254) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 /PWM2))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 229.6672 142.2022 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -2.2352 -0.0254) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 /PWM3))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BABD53C)
    (at 227.0002 137.2746 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 2.3368 -0.0254 180) (layer F.SilkS))
    (fp_text value 0R (at 0 1.9 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(Q4-Pad1)"))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 /FAN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5BB956AC)
    (at 217.1704 104.3308 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0.33528 -1.60528 90) (layer F.SilkS))
    (fp_text value R (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R9-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 216.5354 114.1352 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0 -1.9 270) (layer F.SilkS))
    (fp_text value R (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R10-Pad2)"))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5415CC62)
    (at 258.20664 107.97824 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at 0 1.9 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.9 270) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 43 /BUTTON2))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5415CC62)
    (at 251.40198 104.45526 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at 0 1.9 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.9 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 44 /BUTTON3))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer B.Cu) (tedit 5415CC62)
    (at 258.04916 114.46724 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R15 (at 0 1.9 90) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.9 90) (layer B.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 46 /BTN_PWR))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 252.5272 143.1286 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R18 (at 1.8662 0.0254 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.9 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 +3V3))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 73 /RESET_ATMEGA))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical (layer B.Cu) (tedit 5A19A433)
    (at 208.37 98.77 270)
    (descr "Through hole straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x20 2.54mm double row")
    (fp_text reference P1 (at 2.208 1.512) (layer B.SilkS))
    (fp_text value Conn_02x20_Odd_Even (at -1.27 -51.03 270) (layer B.Fab))
    (fp_text user %R (at -1.27 -24.13 180) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/GPIO2(SDA1)"))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/GPIO3(SCL1)"))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/GPIO4(GCLK)"))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/GPIO14(TXD0)"))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/GPIO15(RXD0)"))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/GPIO17(GEN0)"))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /BCLK))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "/GPIO27(GEN2)"))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "/GPIO22(GEN3)"))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "/GPIO23(GEN4)"))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/GPIO24(GEN5)"))
    (pad 19 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/GPIO10(SPI0_MOSI)"))
    (pad 20 thru_hole oval (at -2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 21 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/GPIO9(SPI0_MISO)"))
    (pad 22 thru_hole oval (at -2.54 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/GPIO25(GEN6)"))
    (pad 23 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/GPIO11(SPI0_SCK)"))
    (pad 24 thru_hole oval (at -2.54 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/GPIO8(SPI0_CE_N)"))
    (pad 25 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 26 thru_hole oval (at -2.54 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/GPIO7(SPI1_CE_N)"))
    (pad 27 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /ID_SD))
    (pad 28 thru_hole oval (at -2.54 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /ID_SC))
    (pad 29 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 /BUTTON4))
    (pad 30 thru_hole oval (at -2.54 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 31 thru_hole oval (at 0 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 /BUTTON3))
    (pad 32 thru_hole oval (at -2.54 -38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/GPIO12(PWM0)"))
    (pad 33 thru_hole oval (at 0 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/GPIO13(PWM1)"))
    (pad 34 thru_hole oval (at -2.54 -40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 35 thru_hole oval (at 0 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/GPIO19(SPI1_MISO)"))
    (pad 36 thru_hole oval (at -2.54 -43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 /BUTTON2))
    (pad 37 thru_hole oval (at 0 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 /BUTTON1))
    (pad 38 thru_hole oval (at -2.54 -45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/GPIO20(SPI1_MOSI)"))
    (pad 39 thru_hole oval (at 0 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 GND))
    (pad 40 thru_hole oval (at -2.54 -48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /DIN))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 5BBE5D82)
    (at 261.5 146.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK4 (at 0 -3.7) (layer F.Fab))
    (fp_text value M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 5BBE5D8B)
    (at 203.5 146.5)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK3 (at 0 -3.7) (layer F.Fab))
    (fp_text value M2.5 (at 0 3.7) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 5BBE5D72)
    (at 261.5 97.5 180)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK2 (at 0 -3.7 180) (layer F.Fab))
    (fp_text value M2.5 (at 0 3.7 180) (layer F.Fab))
    (fp_text user %R (at 0.3 0 180) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.7mm_M2.5 (layer F.Cu) (tedit 5BBE5D79)
    (at 203.5 97.5 180)
    (descr "Mounting Hole 2.7mm, no annular, M2.5")
    (tags "mounting hole 2.7mm no annular m2.5")
    (attr virtual)
    (fp_text reference MK1 (at 0 -3.7 180) (layer F.Fab))
    (fp_text value M2.5 (at 0 3.7 180) (layer F.Fab))
    (fp_text user %R (at 0.3 0 180) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 541A9B8D)
    (at 214.478 111.7222)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 1.778 -1.7018) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5BBE3FD9)
    (at 214.4834 101.9686)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 2.99688 0.00508 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.1) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST_PH:Connectors_JST_B2B-PH-K (layer F.Cu) (tedit 55F6C32A)
    (at 260.4266 108.979)
    (descr "JST PH series connector, B2B-PH-K")
    (tags "connector jst ph")
    (fp_text reference J8 (at -2.794 0 90) (layer F.SilkS))
    (fp_text value BUTTON2 (at 1 4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 43 /BUTTON2))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_JST_PH:Connectors_JST_B2B-PH-K (layer F.Cu) (tedit 55F6C32A)
    (at 253.467 103.4164)
    (descr "JST PH series connector, B2B-PH-K")
    (tags "connector jst ph")
    (fp_text reference J9 (at -2.794 0 90) (layer F.SilkS))
    (fp_text value BUTTON3 (at 1 4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 44 /BUTTON3))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.7) (drill 0.7) (layers *.Cu *.Mask F.SilkS)
      (net 3 GND))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 5BBE5B08)
    (at 212.6238 138.6208 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at -2.54 0.254 180) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(Q2-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 79 "Net-(LED2-Pad2)"))
    (model Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 553634F8)
    (at 212.5984 130.2388 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at -2.54 -0.254 180) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(Q4-Pad1)"))
    (pad 2 smd rect (at 0.95 1.00076 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 3 smd rect (at 0 -0.99822 90) (size 0.8001 0.8001) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J2-Pad2)"))
    (model Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 254.483 114.85402)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference TH1 (at -2.4892 1.21158 90) (layer F.SilkS))
    (fp_text value 100k (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(R21-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 54130A77)
    (at 214.0716 106.2358 180)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (clearance 0.1524)
    (attr smd)
    (fp_text reference U2 (at -3.1496 -1.5748 180) (layer F.SilkS))
    (fp_text value MAX98357 (at 0 2.85 180) (layer F.Fab))
    (pad 17 smd rect (at -0.45 -0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U2-Pad17)") (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U2-Pad17)") (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 -0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U2-Pad17)") (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 74 "Net-(U2-Pad17)") (solder_paste_margin_ratio -0.2))
    (pad 16 smd oval (at -0.75 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /BCLK))
    (pad 15 smd oval (at -0.25 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 14 smd oval (at 0.25 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "/GPIO19(SPI1_MISO)"))
    (pad 13 smd oval (at 0.75 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(U2-Pad13)"))
    (pad 12 smd oval (at 1.475 -0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(U2-Pad12)"))
    (pad 11 smd oval (at 1.475 -0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 10 smd oval (at 1.475 0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(L1-Pad2)"))
    (pad 9 smd oval (at 1.475 0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(L3-Pad2)"))
    (pad 8 smd oval (at 0.75 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 7 smd oval (at 0.25 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 6 smd oval (at -0.25 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(U2-Pad6)"))
    (pad 5 smd oval (at -0.75 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(U2-Pad5)"))
    (pad 4 smd oval (at -1.475 0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(R9-Pad2)"))
    (pad 3 smd oval (at -1.475 0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 2 smd oval (at -1.475 -0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(U2-Pad2)"))
    (pad 1 smd oval (at -1.475 -0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /DIN))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DFN_QFN:QFN-16-1EP_3x3mm_Pitch0.5mm (layer F.Cu) (tedit 5BB7B713)
    (at 213.3604 115.6846 180)
    (descr "16-Lead Plastic Quad Flat, No Lead Package (NG) - 3x3x0.9 mm Body [QFN]; (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFN 0.5")
    (clearance 0.1524)
    (attr smd)
    (fp_text reference U3 (at 0 -2.85 180) (layer F.SilkS))
    (fp_text value MAX98357 (at 0 2.85 180) (layer F.Fab) hide)
    (pad 1 smd oval (at -1.475 -0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /DIN))
    (pad 2 smd oval (at -1.475 -0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(U3-Pad2)"))
    (pad 3 smd oval (at -1.475 0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 4 smd oval (at -1.475 0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(R10-Pad2)"))
    (pad 5 smd oval (at -0.75 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U3-Pad5)"))
    (pad 6 smd oval (at -0.25 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 62 "Net-(U3-Pad6)"))
    (pad 7 smd oval (at 0.25 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 8 smd oval (at 0.75 1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 9 smd oval (at 1.475 0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(L4-Pad2)"))
    (pad 10 smd oval (at 1.475 0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(L2-Pad2)"))
    (pad 11 smd oval (at 1.475 -0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 12 smd oval (at 1.475 -0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 63 "Net-(U3-Pad12)"))
    (pad 13 smd oval (at 0.75 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(U3-Pad13)"))
    (pad 14 smd oval (at 0.25 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 "/GPIO19(SPI1_MISO)"))
    (pad 15 smd oval (at -0.25 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 16 smd oval (at -0.75 -1.475 270) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /BCLK))
    (pad 17 smd rect (at 0.45 0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U3-Pad17)") (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at 0.45 -0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U3-Pad17)") (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U3-Pad17)") (solder_paste_margin_ratio -0.2))
    (pad 17 smd rect (at -0.45 -0.45 180) (size 0.9 0.9) (layers F.Cu F.Paste F.Mask)
      (net 75 "Net-(U3-Pad17)") (solder_paste_margin_ratio -0.2))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 207.6708 107.7732 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C16 (at 0.8756 1.778 90) (layer F.SilkS))
    (fp_text value 220nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(C16-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 207.6454 116.853 270)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C17 (at 0.9144 1.524 270) (layer F.SilkS))
    (fp_text value 220nF (at 0 1.9 270) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.75 0 270) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C17-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 207.6708 104.7746 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C18 (at 1.5868 -2.0574 180) (layer F.SilkS))
    (fp_text value 220nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C18-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5415D631)
    (at 207.6454 113.8558 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C19 (at 0 -1.9 90) (layer F.SilkS))
    (fp_text value 220nF (at 0 1.9 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 209.9314 107.1756)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L1 (at 0 1.5748) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(C16-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 69 "Net-(L1-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 209.779 116.2942)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L2 (at 0.3944 1.7526) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.9) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(C17-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 70 "Net-(L2-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 209.9314 105.5246)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L3 (at -0.127 -1.4732) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 71 "Net-(L3-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 67 "Net-(C18-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 209.779 114.6178)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference L4 (at -0.0388 -1.2954) (layer F.SilkS))
    (fp_text value Ferrite_Bead_Small (at 0 1.9) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 72 "Net-(L4-Pad2)"))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(C19-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_2pol (layer F.Cu) (tedit 0)
    (at 203.426319 105.491921 270)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J14 (at 1.27 -4.50088 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 4.50088 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(C18-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(C16-Pad1)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_2pol.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Terminal_Blocks:TerminalBlock_Pheonix_MPT-2.54mm_2pol (layer F.Cu) (tedit 0)
    (at 203.426319 111.541921 270)
    (descr "2-way 2.54mm pitch terminal block, Phoenix MPT series")
    (fp_text reference J15 (at -0.556321 -3.914281 270) (layer F.SilkS))
    (fp_text value Conn_01x02_Male (at 1.27 4.50088 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(C17-Pad1)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.99898 1.99898) (drill 1.09728) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(C19-Pad1)"))
    (model Terminal_Blocks.3dshapes/TerminalBlock_Pheonix_MPT-2.54mm_2pol.wrl
      (offset (xyz 1.269999980926514 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 54EA090C)
    (at 246.2534 145.174 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J13 (at 0.0254 -2.6162 180) (layer F.SilkS))
    (fp_text value "Reset disable" (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 73 /RESET_ATMEGA))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "/GPIO4(GCLK)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (offset (xyz 0 -1.269999980926514 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module LEDs:LED-0603 (layer F.Cu) (tedit 55BDE255)
    (at 240.96258 146.16206 270)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.5 270) (layer F.Fab))
    (pad 2 smd rect (at 0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 GND))
    (pad 1 smd rect (at -0.7493 0 90) (size 0.79756 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(D1-Pad1)"))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5415CC62)
    (at 241.6941 142.80926 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R19 (at -1.48336 -1.6256 180) (layer F.SilkS))
    (fp_text value 220R (at 0 1.9 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 77 "Net-(R19-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 76 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Nerdclub.dk\nRPI Arcade Sound \nand Light Extension" (at 240.6908 138.443) (layer F.SilkS))
  (gr_circle (center 233.2486 119.6216) (end 243.8404 128.7656) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200 113) (end 200 131) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200 97) (end 200 113) (layer Edge.Cuts) (width 0.1))
  (gr_text RJ45 (at 276.2 139.84) (layer Dwgs.User))
  (gr_text USB (at 277.724 121.552) (layer Dwgs.User))
  (gr_text USB (at 278.232 102.248) (layer Dwgs.User))
  (gr_arc (start 262 97) (end 262 94) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 262 147) (end 265 147) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 203 147) (end 203 150) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_arc (start 203 97) (end 200 97) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 262 94) (end 203 94) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 265 147) (end 265 97) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 203 150) (end 262 150) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 200 131) (end 200 147) (layer Edge.Cuts) (width 0.1))
  (gr_text "RASPBERRY-PI 40-PIN ADDON BOARD\nVIEW FROM TOP\nNOTE: P1 SHOULD BE FITTED ON THE REVERSE OF THE BOARD\n\nADD EDGE CUTS FROM CAMERA AND DISPLAY PORTS AS REQUIRED" (at 200 160.16) (layer Dwgs.User))
  (zone (net 3) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 199.8984 93.7644) (xy 265.3288 93.7644) (xy 265.3288 150.1524) (xy 199.746 150.1524) (xy 199.7968 93.7644)
      )
    )
  )
  (zone (net 3) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.254) (thermal_bridge_width 0.381))
    (polygon
      (pts
        (xy 199.7968 93.7644) (xy 265.3288 93.7644) (xy 265.3288 150.1524) (xy 199.746 150.1524)
      )
    )
  )
)
