(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)
  (general
    (thickness 1)
    (drawings 42)
    (tracks 459)
    (zones 0)
    (modules 38)
    (nets 55)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 +5V)
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(D3-Pad1)")
  (net 6 DTR)
  (net 7 GreenLED)
  (net 8 YellowLED)
  (net 9 RedLED)
  (net 10 IRQ)
  (net 11 Inclusion)
  (net 12 CE)
  (net 13 CS)
  (net 14 MOSI)
  (net 15 MISO)
  (net 16 SCK)
  (net 17 "Net-(AE1-Pad1)")
  (net 18 +3V3)
  (net 19 MISO_3v3)
  (net 20 MOSI_3v3)
  (net 21 SCK_3v3)
  (net 22 IRQ_3v3)
  (net 23 CS_3v3)
  (net 24 "Net-(U3-Pad16)")
  (net 25 "Net-(U3-Pad7)")
  (net 26 "Net-(U3-Pad6)")
  (net 27 "Net-(U3-Pad5)")
  (net 28 "Net-(U3-Pad4)")
  (net 29 "Net-(U3-Pad3)")
  (net 30 "Net-(U3-Pad1)")
  (net 31 "Net-(JP2-Pad2)")
  (net 32 A3)
  (net 33 "Net-(SHIELD1-PadAD5)")
  (net 34 "Net-(SHIELD1-PadAD4)")
  (net 35 "Net-(SHIELD1-PadV_IN)")
  (net 36 "Net-(SHIELD1-Pad3V3)")
  (net 37 "Net-(SHIELD1-Pad0)")
  (net 38 "Net-(SHIELD1-Pad1)")
  (net 39 "Net-(SHIELD1-Pad4)")
  (net 40 "Net-(SHIELD1-Pad10)")
  (net 41 "Net-(SHIELD1-Pad11)")
  (net 42 "Net-(SHIELD1-Pad12)")
  (net 43 "Net-(SHIELD1-Pad13)")
  (net 44 "Net-(SHIELD1-PadAREF)")
  (net 45 "Net-(SHIELD1-PadSDA)")
  (net 46 "Net-(SHIELD1-PadSCL)")
  (net 47 "Net-(SHIELD1-PadIO_R)")
  (net 48 "Net-(SHIELD1-PadNC)")
  (net 49 "Net-(SHIELD1-PadSP1)")
  (net 50 "Net-(SHIELD1-PadSP2)")
  (net 51 "Net-(SHIELD1-PadSP3)")
  (net 52 "Net-(SHIELD1-PadSP4)")
  (net 53 "Net-(SHIELD1-PadSP5)")
  (net 54 "Net-(SHIELD1-PadSP6)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A3)
    (add_net CE)
    (add_net CS)
    (add_net CS_3v3)
    (add_net DTR)
    (add_net GreenLED)
    (add_net IRQ)
    (add_net IRQ_3v3)
    (add_net Inclusion)
    (add_net MISO)
    (add_net MISO_3v3)
    (add_net MOSI)
    (add_net MOSI_3v3)
    (add_net "Net-(AE1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(JP2-Pad2)")
    (add_net "Net-(SHIELD1-Pad0)")
    (add_net "Net-(SHIELD1-Pad1)")
    (add_net "Net-(SHIELD1-Pad10)")
    (add_net "Net-(SHIELD1-Pad11)")
    (add_net "Net-(SHIELD1-Pad12)")
    (add_net "Net-(SHIELD1-Pad13)")
    (add_net "Net-(SHIELD1-Pad3V3)")
    (add_net "Net-(SHIELD1-Pad4)")
    (add_net "Net-(SHIELD1-PadAD4)")
    (add_net "Net-(SHIELD1-PadAD5)")
    (add_net "Net-(SHIELD1-PadAREF)")
    (add_net "Net-(SHIELD1-PadIO_R)")
    (add_net "Net-(SHIELD1-PadNC)")
    (add_net "Net-(SHIELD1-PadSCL)")
    (add_net "Net-(SHIELD1-PadSDA)")
    (add_net "Net-(SHIELD1-PadSP1)")
    (add_net "Net-(SHIELD1-PadSP2)")
    (add_net "Net-(SHIELD1-PadSP3)")
    (add_net "Net-(SHIELD1-PadSP4)")
    (add_net "Net-(SHIELD1-PadSP5)")
    (add_net "Net-(SHIELD1-PadSP6)")
    (add_net "Net-(SHIELD1-PadV_IN)")
    (add_net "Net-(U3-Pad1)")
    (add_net "Net-(U3-Pad16)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad4)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad6)")
    (add_net "Net-(U3-Pad7)")
    (add_net RedLED)
    (add_net SCK)
    (add_net SCK_3v3)
    (add_net YellowLED)
  )
  (net_class Big ""
    (clearance 0.2)
    (trace_width 0.6)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
  )
  (module freetronics_footprints:ARDUINO_SHIELD (layer F.Cu) (tedit 5C7C2D28)
    (at 138.53 117.54)
    (descr http://www.thingiverse.com/thing:9630)
    (fp_text reference SHIELD1 (at 5.715 -57.15) (layer F.SilkS) hide)
    (fp_text value ARDUINO_SHIELD (at 10.16 -54.61) (layer F.SilkS) hide)
    (pad AD5 thru_hole oval (at 63.5 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(SHIELD1-PadAD5)"))
    (pad AD4 thru_hole oval (at 60.96 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(SHIELD1-PadAD4)"))
    (pad AD3 thru_hole oval (at 58.42 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 A3))
    (pad AD0 thru_hole oval (at 50.8 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 SCK))
    (pad AD1 thru_hole oval (at 53.34 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 MOSI))
    (pad AD2 thru_hole oval (at 55.88 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 MISO))
    (pad V_IN thru_hole oval (at 45.72 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(SHIELD1-PadV_IN)"))
    (pad GND2 thru_hole oval (at 43.18 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad GND1 thru_hole oval (at 40.64 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3V3 thru_hole oval (at 35.56 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(SHIELD1-Pad3V3)"))
    (pad RST thru_hole oval (at 33.02 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 DTR))
    (pad 0 thru_hole oval (at 63.5 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(SHIELD1-Pad0)"))
    (pad 1 thru_hole oval (at 60.96 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(SHIELD1-Pad1)"))
    (pad 2 thru_hole oval (at 58.42 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 IRQ))
    (pad 3 thru_hole oval (at 55.88 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 Inclusion))
    (pad 4 thru_hole oval (at 53.34 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(SHIELD1-Pad4)"))
    (pad 5 thru_hole oval (at 50.8 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 CE))
    (pad 6 thru_hole oval (at 48.26 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 CS))
    (pad 7 thru_hole oval (at 45.72 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 RedLED))
    (pad 8 thru_hole oval (at 41.656 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 YellowLED))
    (pad 9 thru_hole oval (at 39.116 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GreenLED))
    (pad 10 thru_hole oval (at 36.576 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(SHIELD1-Pad10)"))
    (pad 11 thru_hole oval (at 34.036 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(SHIELD1-Pad11)"))
    (pad 12 thru_hole oval (at 31.496 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(SHIELD1-Pad12)"))
    (pad 13 thru_hole oval (at 28.956 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(SHIELD1-Pad13)"))
    (pad GND3 thru_hole oval (at 26.416 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad AREF thru_hole oval (at 23.876 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(SHIELD1-PadAREF)"))
    (pad 5V thru_hole oval (at 38.1 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 +5V))
    (pad "" np_thru_hole circle (at 66.04 -7.62 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 66.04 -35.56 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 15.24 -50.8 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 13.97 -2.54 90) (size 3.175 3.175) (drill 3.175) (layers *.Cu *.Mask F.SilkS))
    (pad SDA thru_hole oval (at 21.336 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(SHIELD1-PadSDA)"))
    (pad SCL thru_hole oval (at 18.796 -50.8 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(SHIELD1-PadSCL)"))
    (pad IO_R thru_hole oval (at 30.48 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(SHIELD1-PadIO_R)"))
    (pad NC thru_hole oval (at 27.94 -2.54 90) (size 2.54 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(SHIELD1-PadNC)"))
    (pad SP1 thru_hole circle (at 63.5 -30.48 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(SHIELD1-PadSP1)"))
    (pad SP2 thru_hole circle (at 66.04 -30.48 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(SHIELD1-PadSP2)"))
    (pad SP3 thru_hole circle (at 63.5 -27.94 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(SHIELD1-PadSP3)"))
    (pad SP4 thru_hole circle (at 66.04 -27.94 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(SHIELD1-PadSP4)"))
    (pad SP5 thru_hole circle (at 63.5 -25.4 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(SHIELD1-PadSP5)"))
    (pad SP6 thru_hole circle (at 66.04 -25.4 90) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 54 "Net-(SHIELD1-PadSP6)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5F280F67)
    (at 196.2 73.32 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at -4.18 0.03 -180) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 IRQ))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ASKicadLib:SMA_EDGE (layer F.Cu) (tedit 5C7845C9)
    (at 206.8576 96.5962 90)
    (fp_text reference AE1 (at 0 -6.35 90) (layer F.SilkS) hide)
    (fp_text value Antenna_Shield (at 4.0386 4.699 270) (layer F.SilkS) hide)
    (pad 2 smd rect (at -2.1463 -2.0955 90) (size 1.27 4.191) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.1463 -2.0955 90) (size 1.27 4.191) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 0 -1.8415 90) (size 1.27 3.683) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(AE1-Pad1)"))
    (pad 2 smd rect (at -2.1463 -2.0955 90) (size 1.27 4.191) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.1463 -2.0955 90) (size 1.27 4.191) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 5C99ED14)
    (at 205.71 96.61)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference AE2 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value Antenna (at 0 2.77) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(AE1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5C759D13)
    (at 161.4198 75.1708 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 1.3462 2.7804 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED-3MM.wrl
      (offset (xyz 1.5 0 0.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -85))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5C759D0F)
    (at 161.4198 81.026 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D2 (at 1.3462 2.7804 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +5V))
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 5C76C075)
    (at 161.4198 86.868 90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D3 (at 1.3462 2.7804 90) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 90) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 +5V))
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C76C193)
    (at 167.46 69.85)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 7.2008 0.5084) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GreenLED))
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C76C18F)
    (at 167.46 73.05)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 7.1654 0.5012) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 YellowLED))
  )
  (module Resistors_ThroughHole:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5C76C18A)
    (at 167.47 76.26)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R3 (at 7.2408 0.6404) (layer F.SilkS))
    (fp_text value R (at 5.08 2.31) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 RedLED))
  )
  (module ASKicadLib:SW_PUSH_AS (layer F.Cu) (tedit 588090BD)
    (at 145.2118 110.346 270)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 0 90) (layer F.SilkS))
    (fp_text value SW_PUSHBUTTON (at 0 3 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 3.5 0 270) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 6 DTR))
    (pad 1 smd rect (at -3.5 0 270) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module ASKicadLib:SW_PUSH_AS (layer F.Cu) (tedit 588090BD)
    (at 145.104 97.5354 270)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW2 (at 0 0 270) (layer F.SilkS))
    (fp_text value SW_PUSHBUTTON (at 0 3 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 3.5 0 270) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.5 0 270) (size 3 1.6) (layers F.Cu F.Paste F.Mask)
      (net 11 Inclusion))
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer F.Cu) (tedit 5C759A09)
    (at 153.7462 104.4702 90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at -1.0972 2.3224 180) (layer F.SilkS))
    (fp_text value LM1117-3.3 (at 0 4.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 4 smd rect (at 3.15 0 90) (size 2 3.8) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at -3.15 0 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 3 smd rect (at -3.15 2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -3.15 -2.3 90) (size 2 1.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module mysensors_radios:NRF24L01 (layer F.Cu) (tedit 5C7846A4)
    (at 170.446 83.546 90)
    (descr NRF24L01)
    (tags "nRF 24 NRF24L01 NRF24L01+")
    (fp_text reference U2 (at -1.016 -1.016 90) (layer F.SilkS) hide)
    (fp_text value NRF24L01 (at -8.382 7.112 90) (layer F.Fab) hide)
    (pad 7 thru_hole oval (at -9.144 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 MISO))
    (pad 8 thru_hole oval (at -9.144 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(JP2-Pad2)"))
    (pad 5 thru_hole oval (at -6.604 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 SCK))
    (pad 6 thru_hole oval (at -6.604 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 MOSI))
    (pad 3 thru_hole oval (at -4.064 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 CE))
    (pad 4 thru_hole oval (at -4.064 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 CS))
    (pad 1 thru_hole rect (at -1.524 1.524 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at -1.524 4.064 90) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 +3V3))
  )
  (module ASKicadLib:SOLDER-JUMPER_1-WAY (layer F.Cu) (tedit 0)
    (at 177.1142 92.0496 270)
    (fp_text reference JP2 (at 0 1.905 270) (layer F.SilkS))
    (fp_text value Jumper_NO_Small (at 0 0 270) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.65 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 10 IRQ))
    (pad 2 smd rect (at 0.65 0 270) (size 1 1) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(JP2-Pad2)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5F281712)
    (at 189.5 105.13 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 2.93 -0.06) (layer F.SilkS))
    (fp_text value R (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 19 MISO_3v3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5F281651)
    (at 192.32 105.13 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at -2.95 0 180) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 15 MISO))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5F281654)
    (at 195.02 105.12 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 2.95 -0.04) (layer F.SilkS))
    (fp_text value R (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 20 MOSI_3v3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5F281A42)
    (at 183.925 105.125 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 2.95 0) (layer F.SilkS))
    (fp_text value R (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 21 SCK_3v3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5F28140A)
    (at 197.7 105.1 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at -2.97 0 180) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 MOSI))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5F2819CD)
    (at 186.7 105.125 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at -2.935 0.04 180) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 16 SCK))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5C784735)
    (at 202.34 73.32 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at -4.18 -0.08 -180) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 22 IRQ_3v3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5F281A48)
    (at 178.075 105.125 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 2.925 -0.125) (layer F.SilkS))
    (fp_text value R (at 0.140199 1.908599 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 23 CS_3v3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5F281A39)
    (at 180.95 105.125 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at -2.95 0.05 180) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 CS))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_radios:RFM69HW_SMD_ThroughHole_Handsoldering (layer F.Cu) (tedit 55DEED2C)
    (at 197.5612 82.3976 270)
    (descr RFM69HW)
    (tags "RFM69HW, RF69")
    (fp_text reference U3 (at 0.254 -1.778 270) (layer F.SilkS))
    (fp_text value RFM69HW (at 8.382 7.112 270) (layer F.Fab) hide)
    (pad 16 thru_hole circle (at 17 0 270) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(U3-Pad16)"))
    (pad 15 thru_hole circle (at 17 2 270) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 CS_3v3))
    (pad 14 thru_hole circle (at 17 4 270) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 MOSI_3v3))
    (pad 13 thru_hole circle (at 17 6 270) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 MISO_3v3))
    (pad 12 thru_hole circle (at 17 8 270) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 SCK_3v3))
    (pad 11 thru_hole circle (at 17 10 270) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole circle (at 17 12 270) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(AE1-Pad1)"))
    (pad 9 thru_hole circle (at 17 14 270) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole circle (at -0.1 14 270) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 +3V3))
    (pad 7 thru_hole circle (at -0.1 12 270) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(U3-Pad7)"))
    (pad 6 thru_hole circle (at -0.1 10 270) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(U3-Pad6)"))
    (pad 5 thru_hole circle (at -0.1 8 270) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(U3-Pad5)"))
    (pad 4 thru_hole circle (at -0.1 6 270) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(U3-Pad4)"))
    (pad 3 thru_hole circle (at -0.1 4 270) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(U3-Pad3)"))
    (pad 2 thru_hole circle (at -0.1 2 270) (size 1.7272 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 IRQ_3v3))
    (pad 1 thru_hole rect (at -0.1 0 270) (size 2 1.7272) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(U3-Pad1)"))
    (pad 16 smd rect (at 18.3 0 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U3-Pad16)"))
    (pad 15 smd rect (at 18.3 2 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 23 CS_3v3))
    (pad 14 smd rect (at 18.3 4 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 20 MOSI_3v3))
    (pad 13 smd rect (at 18.3 6 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 19 MISO_3v3))
    (pad 12 smd rect (at 18.3 8 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 21 SCK_3v3))
    (pad 11 smd rect (at 18.3 10 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 10 smd rect (at 18.3 12 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(AE1-Pad1)"))
    (pad 9 smd rect (at 18.3 14 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at -1.4 14 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 7 smd rect (at -1.4 12 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(U3-Pad7)"))
    (pad 6 smd rect (at -1.4 10 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(U3-Pad6)"))
    (pad 5 smd rect (at -1.4 8 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(U3-Pad5)"))
    (pad 4 smd rect (at -1.4 6 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(U3-Pad4)"))
    (pad 3 smd rect (at -1.4 4 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(U3-Pad3)"))
    (pad 2 smd rect (at -1.4 2 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 22 IRQ_3v3))
    (pad 1 smd rect (at -1.4 0 270) (size 3 1.2) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(U3-Pad1)"))
    (model ${MYSLOCAL}/mysensors.3dshapes/mysensors_radios.3dshapes/rfm69hw.wrl
      (offset (xyz 8.458199872970582 -6.984999895095826 8.762999868392944))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model Crystals.3dshapes/Crystal_SMD_SeikoEpson_TSX3225-4pin_3.2x2.5mm.wrl
      (offset (xyz 8.432799873352051 -2.031999969482422 9.524999856948853))
      (scale (xyz 0.24 0.24 0.24))
      (rotate (xyz 0 0 90))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_strip_2mm_8.wrl
      (offset (xyz -0.1015999984741211 -7.010399894714356 7.873999881744385))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_strip_2mm_8.wrl
      (offset (xyz 16.99259974479675 -7.010399894714356 7.873999881744385))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_socket_2mm_8.wrl
      (offset (xyz -0.1015999984741211 -7.010399894714356 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model ${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/pin_strip/pin_socket_2mm_8.wrl
      (offset (xyz 16.99259974479675 -7.010399894714356 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model Housings_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_Pitch0.5mm.wrl
      (offset (xyz 5.206999921798706 -11.30299983024597 9.524999856948853))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 5F281235)
    (at 204.98 104.61 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 2.88 0.01 180) (layer F.SilkS))
    (fp_text value 0,1uF (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.9972 0 180) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 5F281304)
    (at 200.64 110.24 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 1.9 -2.16) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab) hide)
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 32 A3))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5F281301)
    (at 201.47 104.92 90)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U4 (at 3.21 -0.05 180) (layer F.SilkS))
    (fp_text value ATSHA204A (at 0 2.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab) hide)
    (pad 3 smd rect (at 1.5 0 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -1.5 0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 +5V))
    (pad 1 smd rect (at -1.5 -0.95 90) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 32 A3))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes\SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module mysensors_obscurities:MySensors-logo-sticker (layer F.Cu) (tedit 0)
    (at 165.6334 92.964 270)
    (fp_text reference G*** (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer F.SilkS) hide)
  )
  (module graphicslogo:OpenSourceLogo_1200x1200_Neg (layer F.Cu) (tedit 0)
    (at 185.8518 74.9046 270)
    (fp_text reference G*** (at 0 0 270) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 270) (layer F.SilkS) hide)
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5C99F21E)
    (at 159.76 107.52)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C1 (at 0.9 3.51) (layer F.SilkS))
    (fp_text value CP1 (at 1 3.75) (layer F.Fab) hide)
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 +5V))
    (pad 2 thru_hole circle (at 2 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5C99F220)
    (at 159.75 101.325)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C2 (at 1.17 3.46) (layer F.SilkS))
    (fp_text value CP1 (at 1 3.75) (layer F.Fab) hide)
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 2 thru_hole circle (at 2 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 +3V3))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_THT:CP_Radial_D5.0mm_P2.00mm (layer F.Cu) (tedit 5C99F223)
    (at 165.608 85.598)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (fp_text reference C3 (at 3.35 2.87) (layer F.SilkS))
    (fp_text value CP1 (at 1 3.75) (layer F.Fab) hide)
    (fp_text user %R (at 1 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 +3V3))
    (pad 2 thru_hole circle (at 2 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5F2816F4)
    (at 190.51 110.3)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 1.94 1.26) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 19 MISO_3v3))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 MISO))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5F2816FF)
    (at 195.91 110.29)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q2 (at 1.96 1.28 180) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 14 MOSI))
    (pad 2 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 MOSI_3v3))
    (pad 1 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5F281895)
    (at 185.1 110.3)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q3 (at 1.94 1.27) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 16 SCK))
    (pad 2 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 SCK_3v3))
    (pad 1 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5F280F64)
    (at 199.36 73.7 270)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q4 (at 3.8 -0.03) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -1.5 -0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at -1.5 0.95 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 IRQ_3v3))
    (pad 3 smd rect (at 1.5 0 270) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 10 IRQ))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 5F2819FA)
    (at 179.7 110.3)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q5 (at 1.925 1.25) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab) hide)
    (pad 1 smd rect (at -1.5 -0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 18 +3V3))
    (pad 2 smd rect (at -1.5 0.95) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 CS_3v3))
    (pad 3 smd rect (at 1.5 0) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 13 CS))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "ENC\n" (at 196.925 112.875) (layer F.SilkS))
  (gr_text "MI\n" (at 194.4 112.85) (layer F.SilkS))
  (gr_text V1.2 (at 190.8 91.35 270) (layer F.SilkS))
  (gr_text "Encryption\n" (at 202.32 100.29) (layer F.SilkS))
  (gr_text "G\n" (at 181.7 112.925) (layer F.SilkS))
  (gr_text G (at 179.125 112.9) (layer F.SilkS))
  (gr_text 5V (at 176.575 113) (layer F.SilkS))
  (gr_text "NSS\n" (at 186.17 69.6 270) (layer F.SilkS))
  (gr_text "CS\n" (at 187.29 69.55 270) (layer F.SilkS))
  (gr_text "CE\n" (at 189.28 69.6 270) (layer F.SilkS))
  (gr_text "IRQ\n" (at 196.88 69.47 270) (layer F.SilkS))
  (gr_text "MO\n\n" (at 191.8 113.55) (layer F.SilkS))
  (gr_text "SCK\n" (at 189.3 112.875) (layer F.SilkS))
  (gr_line (start 155.15 69.27) (end 152.5592 69.27) (layer Edge.Cuts) (width 0.15))
  (gr_text Gateway (at 160.7566 92.964 270) (layer F.SilkS))
  (gr_text "Licensed under CERN OHL  v.1.2" (at 181.525 90.275 270) (layer F.SilkS))
  (gr_text "Nrf24l01+ \n" (at 177.0126 86.4362 90) (layer F.SilkS))
  (gr_text "by sundberg84" (at 181.1528 75.1078 270) (layer F.SilkS))
  (gr_text "GW Shield" (at 190.627 75.057 270) (layer F.SilkS))
  (gr_line (start 156.43 89.25) (end 156.43 70.54) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 155.170029 70.5258) (end 155.160029 69.2658) (angle 89.85478498) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.5932 68.0058) (end 152.6032 69.2658) (angle 89.85478498) (layer Edge.Cuts) (width 0.15))
  (gr_text "Read  Write  Err" (at 158.242 79.502 270) (layer F.SilkS))
  (gr_text Reset (at 141.7828 110.346 270) (layer F.SilkS))
  (gr_text "Inclusion Mode" (at 141.3956 98.2974 270) (layer F.SilkS))
  (gr_arc (start 139.7762 116.2812) (end 139.7862 117.5412) (angle 89.85478498) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 138.5316 116.3066) (end 138.54 91.83) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 204.5716 117.5512) (end 139.7762 117.5512) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 204.5716 115.0112) (end 204.5716 117.5512) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 207.1116 112.4712) (end 204.5716 115.0112) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 207.1116 79.4512) (end 207.1116 112.4712) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 204.61 76.92) (end 207.12 79.45) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.3332 68.0466) (end 151.3332 65.4558) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 155.15 90.51) (end 139.71 90.5) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 155.17 89.250029) (end 156.43 89.240029) (angle 89.85478498) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 139.803193 91.759971) (end 138.543193 91.769971) (angle 89.85478498) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 204.6 65.45) (end 204.61 76.94) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.25 64.16) (end 204.6 65.45) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.527 64.1604) (end 203.25 64.16) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 152.590993 65.420371) (end 151.330993 65.430371) (angle 89.85478498) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 148.9814 63.0686) (xy 205.725 63.475) (xy 205.7758 76.3782) (xy 208.8238 79.8326) (xy 209.2302 119.2026)
        (xy 137.6022 118.7962) (xy 137.4854 89.5074) (xy 155.9854 89.1874)
      )
    )
  )
)
