(kicad_pcb (version 20171130) (host pcbnew 5.1.5-5.1.5)
  (general
    (thickness 1.6)
    (drawings 54)
    (tracks 109)
    (zones 0)
    (modules 9)
    (nets 13)
  )
  (page A4)
  (title_block
    (title "BME280 MySensor Node RFM95/96")
    (date 2019-12-09)
    (rev v0.3)
    (company JCW)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VCC)
  (net 3 SDA)
  (net 4 SCL)
  (net 5 DIO0)
  (net 6 ANT)
  (net 7 NSS)
  (net 8 SCK)
  (net 9 MOSI)
  (net 10 MISO)
  (net 11 VIN)
  (net 12 A0)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net A0)
    (add_net ANT)
    (add_net DIO0)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net NSS)
    (add_net "Net-(RFM9x1-Pad10)")
    (add_net "Net-(RFM9x1-Pad11)")
    (add_net "Net-(RFM9x1-Pad12)")
    (add_net "Net-(RFM9x1-Pad15)")
    (add_net "Net-(RFM9x1-Pad16)")
    (add_net "Net-(RFM9x1-Pad6)")
    (add_net "Net-(RFM9x1-Pad7)")
    (add_net "Net-(RFM9x1-Pad8)")
    (add_net "Net-(X1-Pad10D)")
    (add_net "Net-(X1-Pad11D)")
    (add_net "Net-(X1-Pad12D)")
    (add_net "Net-(X1-Pad1A)")
    (add_net "Net-(X1-Pad1B)")
    (add_net "Net-(X1-Pad1C)")
    (add_net "Net-(X1-Pad1D)")
    (add_net "Net-(X1-Pad2A)")
    (add_net "Net-(X1-Pad2B)")
    (add_net "Net-(X1-Pad2C)")
    (add_net "Net-(X1-Pad2D)")
    (add_net "Net-(X1-Pad3A)")
    (add_net "Net-(X1-Pad3B)")
    (add_net "Net-(X1-Pad3C)")
    (add_net "Net-(X1-Pad3D)")
    (add_net "Net-(X1-Pad4C)")
    (add_net "Net-(X1-Pad5A)")
    (add_net "Net-(X1-Pad5C)")
    (add_net "Net-(X1-Pad6A)")
    (add_net "Net-(X1-Pad6C)")
    (add_net "Net-(X1-Pad6D)")
    (add_net "Net-(X1-Pad7A)")
    (add_net "Net-(X1-Pad7D)")
    (add_net "Net-(X1-Pad8D)")
    (add_net "Net-(X1-Pad9D)")
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net VCC)
    (add_net VIN)
  )
  (net_class VCC ""
    (clearance 0.2)
    (trace_width 1)
    (via_dia 1)
    (via_drill 0.5)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 121.666 87.376)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference C1 (at 0 -2.032) (layer F.SilkS))
    (fp_text value C (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 A0))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 121.666 94.742 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R2 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value R (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 A0))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE5139B)
    (at 121.666 72.898 270)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 0 90) (layer F.SilkS))
    (fp_text value R (at 5.08 2.37 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 A0))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 VIN))
    (model ${KISYS3DMOD}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-92_Inline (layer F.Cu) (tedit 5A1DD157)
    (at 140.462 68.58)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference U1 (at 1.27 -3.56) (layer F.SilkS) hide)
    (fp_text value MCP1700-3302E_TO92 (at 1.27 2.79) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 2 VCC))
    (pad 2 thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers *.Cu *.Mask)
      (net 11 VIN))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 121.666 70.104 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value Conn_01x02_Male (at 0 4.87) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.27 90) (layer F.Fab))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 VIN))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module ArduinoJC:Arduino_Pro_Mini_JC (layer F.Cu) (tedit 5DEEC1E4)
    (at 132.240599 87.666599)
    (descr "Arduino Pro Mini")
    (tags "Arduino Pro Mini")
    (fp_text reference X1 (at 0.127 -22.987) (layer F.SilkS) hide)
    (fp_text value Arduino_Pro_Mini (at 0 -11.557 180) (layer F.Fab))
    (fp_text user DTR (at -6.223 -18.034 90) (layer F.SilkS))
    (fp_text user TXO (at -3.683 -18.034 90) (layer F.SilkS))
    (fp_text user RXI (at -1.143 -18.034 90) (layer F.SilkS))
    (fp_text user VCC (at 1.397 -18.034 90) (layer F.SilkS))
    (fp_text user GND (at 3.937 -18.161 90) (layer F.SilkS))
    (fp_text user GND (at 6.189401 -18.070599 90) (layer F.SilkS))
    (fp_text user GND (at 0 18.034 90) (layer F.SilkS))
    (fp_text user " A6" (at 2.633401 17.997401 90) (layer F.SilkS))
    (fp_text user " A7" (at 5.173401 17.997401 90) (layer F.SilkS))
    (fp_text user " 10" (at 9.906 15.24) (layer F.SilkS))
    (fp_text user " 11" (at 9.906 12.446) (layer F.SilkS))
    (fp_text user " 12" (at 9.906 9.906) (layer F.SilkS))
    (fp_text user " 13" (at 9.906 7.62) (layer F.SilkS))
    (fp_text user " A0" (at 9.906 5.08) (layer F.SilkS))
    (fp_text user " A1" (at 9.906 2.54) (layer F.SilkS))
    (fp_text user NC (at 10.414 -12.7 45) (layer F.SilkS))
    (fp_text user GND (at 10.414 -10.16 45) (layer F.SilkS))
    (fp_text user RST (at 10.16 -7.62 45) (layer F.SilkS))
    (fp_text user VCC (at 10.414 -5.08 45) (layer F.SilkS))
    (fp_text user " A3" (at 9.906 -2.54) (layer F.SilkS))
    (fp_text user " A2" (at 9.906 0) (layer F.SilkS))
    (fp_text user "  3" (at -5.748599 -0.036599) (layer F.SilkS))
    (fp_text user "  2" (at -5.748599 -2.576599 180) (layer F.SilkS))
    (fp_text user GND (at -4.478599 -5.116599 45) (layer F.SilkS))
    (fp_text user RST (at -4.478599 -7.656599 45) (layer F.SilkS))
    (fp_text user RXI (at -4.732599 -10.196599 45) (layer F.SilkS))
    (fp_text user TXO (at -4.732599 -12.482599 45) (layer F.SilkS))
    (fp_text user "  4" (at -6.002599 2.503401) (layer F.SilkS))
    (fp_text user "  5" (at -6.002599 5.043401) (layer F.SilkS))
    (fp_text user "  6" (at -6.002599 7.583401) (layer F.SilkS))
    (fp_text user "  7" (at -6.002599 10.123401) (layer F.SilkS))
    (fp_text user "  8" (at -6.002599 12.663401) (layer F.SilkS))
    (fp_text user "  9" (at -6.002599 15.203401) (layer F.SilkS))
    (fp_text user " A4" (at 2.125401 -1.306599) (layer F.SilkS))
    (fp_text user " A5" (at 2.125401 -3.846599) (layer F.SilkS))
    (pad 12A thru_hole circle (at 7.62 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 NSS))
    (pad 3B thru_hole circle (at 5.08 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2B thru_hole circle (at 2.54 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 1B thru_hole rect (at 0 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6C thru_hole circle (at 6.35 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5C thru_hole circle (at 3.81 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4C thru_hole circle (at 1.27 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3C thru_hole circle (at -1.27 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2C thru_hole circle (at -3.81 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 1C thru_hole rect (at -6.35 -15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11A thru_hole circle (at 7.62 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 MOSI))
    (pad 9A thru_hole circle (at 7.62 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 SCK))
    (pad 10A thru_hole circle (at 7.62 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 MISO))
    (pad 6A thru_hole circle (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5A thru_hole circle (at 7.62 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7A thru_hole circle (at 7.62 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 8A thru_hole circle (at 7.62 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 A0))
    (pad 4A thru_hole circle (at 7.62 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 VCC))
    (pad 3A thru_hole circle (at 7.62 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 1A thru_hole rect (at 7.62 -12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2A thru_hole circle (at 7.62 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2D thru_hole circle (at -7.62 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 1D thru_hole rect (at -7.62 -12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3D thru_hole circle (at -7.62 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 4D thru_hole circle (at -7.62 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8D thru_hole circle (at -7.62 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7D thru_hole circle (at -7.62 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5D thru_hole circle (at -7.62 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 DIO0))
    (pad 6D thru_hole circle (at -7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 10D thru_hole circle (at -7.62 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 9D thru_hole circle (at -7.62 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11D thru_hole circle (at -7.62 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 12D thru_hole circle (at -7.62 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 5B thru_hole circle (at 5.08 -3.81) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 SCL))
    (pad 4B thru_hole circle (at 5.08 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 SDA))
  )
  (module RF_Module:HOPERF_RFM9XW_SMD (layer F.Cu) (tedit 5C227243)
    (at 132.334 119.38 180)
    (descr "Low Power Long Range Transceiver Module SMD-16 (https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf)")
    (tags "LoRa Low Power Long Range Transceiver Module")
    (attr smd)
    (fp_text reference RFM9x1 (at -0.508 0.508) (layer F.SilkS))
    (fp_text value RFM95W-868S2 (at 0 9.5) (layer F.Fab) hide)
    (fp_text user %R (at -0.254 -1.778) (layer F.Fab))
    (pad 16 smd rect (at 8 -7 180) (size 2 1) (layers F.Cu F.Paste F.Mask))
    (pad 15 smd rect (at 8 -5 180) (size 2 1) (layers F.Cu F.Paste F.Mask))
    (pad 14 smd rect (at 8 -3 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 5 DIO0))
    (pad 13 smd rect (at 8 -1 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 2 VCC))
    (pad 12 smd rect (at 8 1 180) (size 2 1) (layers F.Cu F.Paste F.Mask))
    (pad 11 smd rect (at 8 3 180) (size 2 1) (layers F.Cu F.Paste F.Mask))
    (pad 10 smd rect (at 8 5 180) (size 2 1) (layers F.Cu F.Paste F.Mask))
    (pad 9 smd rect (at 8 7 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 6 ANT))
    (pad 8 smd rect (at -8 7 180) (size 2 1) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -8 5 180) (size 2 1) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -8 3 180) (size 2 1) (layers F.Cu F.Paste F.Mask))
    (pad 5 smd rect (at -8 1 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 7 NSS))
    (pad 4 smd rect (at -8 -1 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 8 SCK))
    (pad 3 smd rect (at -8 -3 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 9 MOSI))
    (pad 2 smd rect (at -8 -5 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 10 MISO))
    (pad 1 smd rect (at -8 -7 180) (size 2 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/RF_Module.3dshapes/HOPERF_RFM9XW_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A429)
    (at 132.334 108.966 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference BME1 (at 0.254 -2.54 90) (layer F.SilkS))
    (fp_text value "BME280 Connector" (at 0 10.39 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 3.81 180) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 SDA))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 SCL))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 VCC))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 124.46 108.966)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference ANT1 (at -2.794 -0.254 90) (layer F.SilkS))
    (fp_text value "Antenna THT" (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 ANT))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text A7 (at 137.16 105.41 90) (layer B.SilkS))
  (gr_text A6 (at 134.874 105.41 90) (layer B.SilkS))
  (gr_text GND (at 132.334 105.664 90) (layer B.SilkS))
  (gr_text GND (at 138.43 69.596 270) (layer B.SilkS))
  (gr_text GND (at 136.144 69.596 270) (layer B.SilkS))
  (gr_text VCC (at 133.604 69.596 270) (layer B.SilkS))
  (gr_text RXI (at 131.064 69.85 270) (layer B.SilkS))
  (gr_text TXO (at 128.27 69.596 270) (layer B.SilkS))
  (gr_text DTR (at 125.73 69.596 270) (layer B.SilkS))
  (gr_text 9 (at 127 102.87) (layer B.SilkS))
  (gr_text 8 (at 127 100.33) (layer B.SilkS))
  (gr_text 7 (at 127 97.79) (layer B.SilkS))
  (gr_text 6 (at 127 95.25) (layer B.SilkS))
  (gr_text 5 (at 127 92.71) (layer B.SilkS))
  (gr_text 4 (at 127 90.17) (layer B.SilkS))
  (gr_text 3 (at 127 87.63) (layer B.SilkS))
  (gr_text 2 (at 127 85.09) (layer B.SilkS))
  (gr_text GND (at 127.508 82.804) (layer B.SilkS))
  (gr_text RST (at 127.254 80.01) (layer B.SilkS))
  (gr_text RXI (at 127.254 77.724) (layer B.SilkS))
  (gr_text TX0 (at 127.254 75.184) (layer B.SilkS))
  (gr_text A4/SDA (at 133.096 86.36) (layer B.SilkS))
  (gr_text A5/SCL (at 133.096 83.82) (layer B.SilkS))
  (gr_text 10 (at 142.494 102.87) (layer B.SilkS))
  (gr_text 11 (at 142.494 100.33) (layer B.SilkS))
  (gr_text 12 (at 142.748 97.536) (layer B.SilkS))
  (gr_text 13 (at 142.748 95.25) (layer B.SilkS))
  (gr_text A0 (at 142.494 92.71) (layer B.SilkS))
  (gr_text A1 (at 142.494 90.17) (layer B.SilkS))
  (gr_text A2 (at 142.494 87.63) (layer B.SilkS))
  (gr_text A3 (at 142.748 85.09) (layer B.SilkS))
  (gr_text VCC (at 142.748 82.55) (layer B.SilkS))
  (gr_text RST (at 142.748 80.264) (layer B.SilkS))
  (gr_text GND (at 142.748 77.724) (layer B.SilkS))
  (gr_text "NC\n" (at 142.494 74.93) (layer B.SilkS))
  (gr_text DIO0 (at 121.666 122.428) (layer F.SilkS))
  (gr_text VCC (at 121.412 120.396) (layer F.SilkS))
  (gr_text GND (at 142.748 126.492) (layer F.SilkS))
  (gr_text MISO (at 143.002 124.46) (layer F.SilkS))
  (gr_text MOSI (at 143.002 122.428) (layer F.SilkS))
  (gr_text SCK (at 142.748 120.396) (layer F.SilkS))
  (gr_text NSS (at 142.748 118.364) (layer F.SilkS))
  (gr_text SDA (at 139.954 110.744) (layer F.SilkS))
  (gr_text SCL (at 137.414 110.744) (layer F.SilkS))
  (gr_text GND (at 134.874 110.744) (layer F.SilkS))
  (gr_text VCC (at 132.334 110.744) (layer F.SilkS))
  (gr_text + (at 123.952 70.104) (layer F.SilkS))
  (gr_text - (at 123.952 67.31 90) (layer F.SilkS))
  (gr_text 1700-33 (at 141.732 67.31) (layer F.SilkS))
  (gr_line (start 144.78 65.786) (end 144.78 128.016) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.888 65.786) (end 144.78 65.786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.888 128.016) (end 119.888 65.786) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 144.78 128.016) (end 119.888 128.016) (layer Edge.Cuts) (width 0.1))
  (gr_text "Arduino Pro Mini\n3.3V 8MHz" (at 130.81 94.488 90) (layer F.SilkS))
)
