(kicad_pcb (version 20171130) (host pcbnew 5.1.5-5.1.5)
  (general
    (thickness 1.6)
    (drawings 28)
    (tracks 105)
    (zones 0)
    (modules 8)
    (nets 28)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFEF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 DIO0)
  (net 2 3V3)
  (net 3 NSS)
  (net 4 SCK)
  (net 5 MOSI)
  (net 6 MISO)
  (net 7 GND)
  (net 8 "Net-(H1-Pad1)")
  (net 9 SDA)
  (net 10 SCL)
  (net 11 "Net-(U1-Pad16)")
  (net 12 "Net-(U1-Pad15)")
  (net 13 "Net-(U1-Pad12)")
  (net 14 "Net-(U1-Pad11)")
  (net 15 "Net-(U1-Pad10)")
  (net 16 "Net-(U1-Pad8)")
  (net 17 "Net-(U1-Pad7)")
  (net 18 "Net-(U1-Pad6)")
  (net 19 "Net-(X1-Pad6A)")
  (net 20 "Net-(X1-Pad5A)")
  (net 21 "Net-(X1-Pad7A)")
  (net 22 "Net-(X1-Pad3A)")
  (net 23 "Net-(X1-Pad2A)")
  (net 24 "Net-(X1-Pad2D)")
  (net 25 "Net-(X1-Pad3D)")
  (net 26 Vbat)
  (net 27 A0)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 3V3)
    (add_net A0)
    (add_net DIO0)
    (add_net GND)
    (add_net MISO)
    (add_net MOSI)
    (add_net NSS)
    (add_net "Net-(H1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(X1-Pad2A)")
    (add_net "Net-(X1-Pad2D)")
    (add_net "Net-(X1-Pad3A)")
    (add_net "Net-(X1-Pad3D)")
    (add_net "Net-(X1-Pad5A)")
    (add_net "Net-(X1-Pad6A)")
    (add_net "Net-(X1-Pad7A)")
    (add_net SCK)
    (add_net SCL)
    (add_net SDA)
    (add_net Vbat)
  )
  (module "JC KiCAD Addons:Molex_PicoBlade_2-Pin_1.25mm_PCB_Side_Pads" (layer B.Cu) (tedit 5E66B4A2)
    (at 208.8388 108.1532)
    (fp_text reference J2 (at 0.19 2.24) (layer B.SilkS) hide)
    (fp_text value Conn_01x02 (at 0.85 -2.17) (layer B.Fab))
    (pad 2 smd roundrect (at 0.625 0) (size 0.85 2.5) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (pad 1 smd roundrect (at -0.625 0) (size 0.85 2.5) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 26 Vbat))
  )
  (module RF_Module:HOPERF_RFM9XW_SMD (layer B.Cu) (tedit 5C227243)
    (at 201.93 128.016 270)
    (descr "Low Power Long Range Transceiver Module SMD-16 (https://www.hoperf.com/data/upload/portal/20181127/5bfcbea20e9ef.pdf)")
    (tags "LoRa Low Power Long Range Transceiver Module")
    (attr smd)
    (fp_text reference U1 (at 0 9.2 90) (layer B.SilkS) hide)
    (fp_text value RFM95W-868S2 (at 0 -9.5 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 16 smd rect (at 8 7 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(U1-Pad16)"))
    (pad 15 smd rect (at 8 5 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(U1-Pad15)"))
    (pad 14 smd rect (at 8 3 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 1 DIO0))
    (pad 13 smd rect (at 8 1 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3))
    (pad 12 smd rect (at 8 -1 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(U1-Pad12)"))
    (pad 11 smd rect (at 8 -3 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(U1-Pad11)"))
    (pad 10 smd rect (at 8 -5 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(U1-Pad10)"))
    (pad 9 smd rect (at 8 -7 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(H1-Pad1)"))
    (pad 8 smd rect (at -8 -7 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(U1-Pad8)"))
    (pad 7 smd rect (at -8 -5 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(U1-Pad7)"))
    (pad 6 smd rect (at -8 -3 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(U1-Pad6)"))
    (pad 5 smd rect (at -8 -1 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 3 NSS))
    (pad 4 smd rect (at -8 1 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 4 SCK))
    (pad 3 smd rect (at -8 3 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 5 MOSI))
    (pad 2 smd rect (at -8 5 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 6 MISO))
    (pad 1 smd rect (at -8 7 270) (size 2 1) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/RF_Module.3dshapes/HOPERF_RFM9XW_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 59FED5CC)
    (at 206.248 109.474)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at -4.826 3.556 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 SDA))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 SCL))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 3V3))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Wire:SolderWirePad_1x01_Drill1mm (layer F.Cu) (tedit 5AEE5EBE)
    (at 211.074 136.144)
    (descr "Wire solder connection")
    (tags connector)
    (attr virtual)
    (fp_text reference H1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 3.175) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 8 "Net-(H1-Pad1)"))
  )
  (module "KiCAD additional:Arduino_Pro_Mini_JC_modified_for_minimal_shield" (layer F.Cu) (tedit 5E2CAE8B)
    (at 203.752599 118.318599)
    (descr "Arduino Pro Mini")
    (tags "Arduino Pro Mini")
    (fp_text reference X1 (at 0.127 -22.987) (layer F.SilkS) hide)
    (fp_text value Arduino_Pro_Mini (at 0 -11.557 180) (layer F.Fab))
    (fp_text user " 10" (at 4.527401 15.24) (layer F.SilkS))
    (fp_text user " 11" (at 4.654401 12.7) (layer F.SilkS))
    (fp_text user " 12" (at 4.654401 10.078401) (layer F.SilkS))
    (fp_text user " 13" (at 4.654401 7.792401) (layer F.SilkS))
    (fp_text user " A0" (at 4.654401 5.125401) (layer F.SilkS))
    (fp_text user " A1" (at 4.908401 2.712401) (layer F.SilkS))
    (fp_text user "  2" (at -6.521599 -2.621599) (layer F.SilkS))
    (pad 12A thru_hole circle (at 7.62 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 NSS))
    (pad 11A thru_hole circle (at 7.62 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 MOSI))
    (pad 9A thru_hole circle (at 7.62 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 SCK))
    (pad 10A thru_hole circle (at 7.62 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 MISO))
    (pad 6A thru_hole circle (at 7.62 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(X1-Pad6A)"))
    (pad 5A thru_hole circle (at 7.62 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(X1-Pad5A)"))
    (pad 7A thru_hole circle (at 7.62 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(X1-Pad7A)"))
    (pad 8A thru_hole circle (at 7.62 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 27 A0))
    (pad 4A thru_hole circle (at 7.62 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 3V3))
    (pad 3A thru_hole circle (at 7.62 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(X1-Pad3A)"))
    (pad 2A thru_hole circle (at 7.62 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(X1-Pad2A)"))
    (pad 2D thru_hole circle (at -7.62 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(X1-Pad2D)"))
    (pad 3D thru_hole circle (at -7.62 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(X1-Pad3D)"))
    (pad 4D thru_hole circle (at -7.62 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 5D thru_hole circle (at -7.62 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 DIO0))
    (pad 5B thru_hole circle (at 5.08 -3.81) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 SCL))
    (pad 4B thru_hole circle (at 5.08 -1.27) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 SDA))
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer B.Cu) (tedit 5A02FF57)
    (at 200.66 109.22)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at 0 2.5) (layer B.SilkS) hide)
    (fp_text value MCP1700-3302E_SOT23 (at 0 -2.5) (layer B.Fab))
    (fp_text user %R (at 0 0 -90) (layer B.Fab))
    (pad 3 smd rect (at 1 0) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 26 Vbat))
    (pad 2 smd rect (at -1 -0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 3V3))
    (pad 1 smd rect (at -1 0.95) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 200.4425 113.03 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 1.82) (layer B.SilkS) hide)
    (fp_text value R_Small (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 27 A0))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 26 Vbat))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer B.Cu) (tedit 5B301BBD)
    (at 200.4425 116.84)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference 1M (at -0.0365 0 90) (layer B.SilkS))
    (fp_text value R_Small (at 0 -1.82) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 7 GND))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.175439)
      (net 27 A0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 470K (at 200.533 113.03 90) (layer B.SilkS))
  (gr_text GND (at 209.5246 110.617 90) (layer B.SilkS))
  (gr_text Vbat (at 208.3308 110.744 90) (layer B.SilkS))
  (gr_text GND (at 203.835 111.887) (layer B.SilkS))
  (gr_text 3V3 (at 204.089 109.601) (layer B.SilkS))
  (gr_text GND (at 203.454 112.014) (layer F.SilkS))
  (gr_text 3V3 (at 203.454 109.728) (layer F.SilkS))
  (gr_text SDA (at 203.962 117.094) (layer B.SilkS))
  (gr_text SCL (at 203.962 114.681) (layer B.SilkS))
  (gr_text VCC (at 209.55 113.284) (layer B.SilkS))
  (gr_text GND (at 198.882 113.284) (layer F.SilkS))
  (gr_text VCC (at 209.55 112.776) (layer F.SilkS))
  (gr_text SDA (at 203.454 117.094) (layer F.SilkS))
  (gr_text SCL (at 203.454 114.554) (layer F.SilkS))
  (gr_text NSS (at 202.946 122.936 270) (layer B.SilkS))
  (gr_text SCK (at 200.914 122.936 270) (layer B.SilkS))
  (gr_text MOSI (at 198.882 123.19 270) (layer B.SilkS))
  (gr_text MISO (at 196.85 123.19 270) (layer B.SilkS))
  (gr_text GND (at 194.818 122.936 270) (layer B.SilkS))
  (gr_text DIO0 (at 198.882 132.842 270) (layer B.SilkS))
  (gr_text 3V3 (at 200.914 133.096 270) (layer B.SilkS))
  (gr_text ANA (at 209.042 133.096 270) (layer B.SilkS))
  (gr_text RFM9x (at 206.502 128.016 270) (layer B.SilkS))
  (gr_text "Arduino Pro\nMini" (at 200.914 128.016 90) (layer F.SilkS))
  (gr_line (start 193.802 137.922) (end 193.802 106.934) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 212.598 137.922) (end 193.802 137.922) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 212.598 106.934) (end 212.598 137.922) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 193.802 106.934) (end 212.598 106.934) (layer Edge.Cuts) (width 0.05))
)
