(kicad_pcb (version 20171130) (host pcbnew 5.1.5+dfsg1-2build2)
  (general
    (thickness 1.6)
    (drawings 80)
    (tracks 1639)
    (zones 0)
    (modules 44)
    (nets 137)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.381)
    (user_trace_width 0.254)
    (user_trace_width 0.381)
    (user_trace_width 0.762)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 2)
    (pad_drill 1)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 26.5 25)
    (grid_origin 26.5 25)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "./GERBER"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /3V3)
  (net 3 "Net-(3V3_REGULATOR_1-Pad3)")
  (net 4 +5V)
  (net 5 /D_BTN1)
  (net 6 /D_BTN2)
  (net 7 /D_BTN3)
  (net 8 /5V_START)
  (net 9 "Net-(EXPANDER_1-Pad1)")
  (net 10 "Net-(EXPANDER_1-Pad2)")
  (net 11 "Net-(EXPANDER_1-Pad3)")
  (net 12 "Net-(EXPANDER_1-Pad4)")
  (net 13 "Net-(EXPANDER_1-Pad5)")
  (net 14 "Net-(EXPANDER_1-Pad19)")
  (net 15 "Net-(EXPANDER_1-Pad6)")
  (net 16 "Net-(EXPANDER_1-Pad20)")
  (net 17 "Net-(EXPANDER_1-Pad7)")
  (net 18 "Net-(EXPANDER_1-Pad21)")
  (net 19 "Net-(EXPANDER_1-Pad8)")
  (net 20 "Net-(EXPANDER_1-Pad22)")
  (net 21 "Net-(EXPANDER_1-Pad23)")
  (net 22 "Net-(EXPANDER_1-Pad24)")
  (net 23 "Net-(EXPANDER_1-Pad11)")
  (net 24 "Net-(EXPANDER_1-Pad25)")
  (net 25 "Net-(EXPANDER_1-Pad26)")
  (net 26 "Net-(EXPANDER_1-Pad27)")
  (net 27 "Net-(EXPANDER_1-Pad14)")
  (net 28 "Net-(EXPANDER_1-Pad28)")
  (net 29 "Net-(EXPANDER_2-Pad28)")
  (net 30 "Net-(EXPANDER_2-Pad14)")
  (net 31 "Net-(EXPANDER_2-Pad27)")
  (net 32 "Net-(EXPANDER_2-Pad26)")
  (net 33 "Net-(EXPANDER_2-Pad25)")
  (net 34 "Net-(EXPANDER_2-Pad11)")
  (net 35 "Net-(EXPANDER_2-Pad24)")
  (net 36 "Net-(EXPANDER_2-Pad23)")
  (net 37 "Net-(EXPANDER_2-Pad22)")
  (net 38 "Net-(EXPANDER_2-Pad8)")
  (net 39 "Net-(EXPANDER_2-Pad21)")
  (net 40 "Net-(EXPANDER_2-Pad7)")
  (net 41 "Net-(EXPANDER_2-Pad20)")
  (net 42 "Net-(EXPANDER_2-Pad6)")
  (net 43 "Net-(EXPANDER_2-Pad19)")
  (net 44 "Net-(EXPANDER_2-Pad5)")
  (net 45 "Net-(EXPANDER_2-Pad4)")
  (net 46 "Net-(EXPANDER_2-Pad3)")
  (net 47 "Net-(EXPANDER_2-Pad2)")
  (net 48 "Net-(EXPANDER_2-Pad1)")
  (net 49 "Net-(EXPANDER_3-Pad1)")
  (net 50 "Net-(EXPANDER_3-Pad2)")
  (net 51 "Net-(EXPANDER_3-Pad3)")
  (net 52 "Net-(EXPANDER_3-Pad4)")
  (net 53 "Net-(EXPANDER_3-Pad5)")
  (net 54 "Net-(EXPANDER_3-Pad19)")
  (net 55 "Net-(EXPANDER_3-Pad6)")
  (net 56 "Net-(EXPANDER_3-Pad20)")
  (net 57 "Net-(EXPANDER_3-Pad7)")
  (net 58 "Net-(EXPANDER_3-Pad21)")
  (net 59 "Net-(EXPANDER_3-Pad8)")
  (net 60 "Net-(EXPANDER_3-Pad22)")
  (net 61 "Net-(EXPANDER_3-Pad23)")
  (net 62 "Net-(EXPANDER_3-Pad24)")
  (net 63 "Net-(EXPANDER_3-Pad11)")
  (net 64 "Net-(EXPANDER_3-Pad25)")
  (net 65 "Net-(EXPANDER_3-Pad26)")
  (net 66 "Net-(EXPANDER_3-Pad27)")
  (net 67 "Net-(EXPANDER_3-Pad14)")
  (net 68 "Net-(EXPANDER_3-Pad28)")
  (net 69 "Net-(EXPANDER_4-Pad28)")
  (net 70 "Net-(EXPANDER_4-Pad14)")
  (net 71 "Net-(EXPANDER_4-Pad27)")
  (net 72 "Net-(EXPANDER_4-Pad26)")
  (net 73 "Net-(EXPANDER_4-Pad25)")
  (net 74 "Net-(EXPANDER_4-Pad11)")
  (net 75 "Net-(EXPANDER_4-Pad24)")
  (net 76 "Net-(EXPANDER_4-Pad23)")
  (net 77 "Net-(EXPANDER_4-Pad22)")
  (net 78 "Net-(EXPANDER_4-Pad8)")
  (net 79 "Net-(EXPANDER_4-Pad21)")
  (net 80 "Net-(EXPANDER_4-Pad7)")
  (net 81 "Net-(EXPANDER_4-Pad20)")
  (net 82 "Net-(EXPANDER_4-Pad6)")
  (net 83 "Net-(EXPANDER_4-Pad19)")
  (net 84 "Net-(EXPANDER_4-Pad5)")
  (net 85 "Net-(EXPANDER_4-Pad4)")
  (net 86 "Net-(EXPANDER_4-Pad3)")
  (net 87 "Net-(EXPANDER_4-Pad2)")
  (net 88 "Net-(EXPANDER_4-Pad1)")
  (net 89 /SDA1)
  (net 90 /SCL1)
  (net 91 /RX1)
  (net 92 /TX1)
  (net 93 /CLK0)
  (net 94 /MISO0)
  (net 95 /CS0)
  (net 96 /MOSI0)
  (net 97 /TX1_5V)
  (net 98 /RX1_5V)
  (net 99 "Net-(MAX485-PadJ1.1)")
  (net 100 /D_RS485)
  (net 101 "Net-(MAX485-PadJ1.4)")
  (net 102 "Net-(NanoPi_NEO_1-Pad17)")
  (net 103 /D_LED1)
  (net 104 /D_LED2)
  (net 105 "Net-(POWER_LED_1-Pad2)")
  (net 106 "Net-(R_LED0-Pad2)")
  (net 107 "Net-(R_LED0-Pad1)")
  (net 108 "Net-(R_LED1-Pad1)")
  (net 109 "Net-(R_LED2-Pad1)")
  (net 110 "Net-(RaspberryPi_1-Pad37)")
  (net 111 "Net-(RaspberryPi_1-Pad38)")
  (net 112 "Net-(RaspberryPi_1-Pad40)")
  (net 113 "Net-(RaspberryPi_1-Pad35)")
  (net 114 "Net-(RaspberryPi_1-Pad36)")
  (net 115 "Net-(RaspberryPi_1-Pad32)")
  (net 116 "Net-(RaspberryPi_1-Pad27)")
  (net 117 "Net-(RaspberryPi_1-Pad28)")
  (net 118 "Net-(RaspberryPi_1-Pad26)")
  (net 119 "Net-(RaspberryPi_1-Pad22)")
  (net 120 "Net-(RaspberryPi_1-Pad17)")
  (net 121 "Net-(RaspberryPi_1-Pad18)")
  (net 122 "Net-(RaspberryPi_1-Pad16)")
  (net 123 "Net-(RaspberryPi_1-Pad12)")
  (net 124 "Net-(RaspberryPi_1-Pad7)")
  (net 125 /LS_OUT_RX1)
  (net 126 /LS_OUT_TX1)
  (net 127 "Net-(NanoPi_NEO_1-Pad22)")
  (net 128 "Net-(NanoPi_NEO_1-Pad11)")
  (net 129 /3V3_PI)
  (net 130 /SDA1_HV)
  (net 131 "Net-(RaspberryPi_1-Pad34)")
  (net 132 "Net-(RaspberryPi_1-Pad30)")
  (net 133 "Net-(RaspberryPi_1-Pad25)")
  (net 134 "Net-(RaspberryPi_1-Pad20)")
  (net 135 "Net-(RaspberryPi_1-Pad14)")
  (net 136 /SCL1_HV)
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.381)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.254)
    (add_net /3V3)
    (add_net /CLK0)
    (add_net /CS0)
    (add_net /D_BTN1)
    (add_net /D_BTN2)
    (add_net /D_BTN3)
    (add_net /D_LED1)
    (add_net /D_LED2)
    (add_net /D_RS485)
    (add_net /LS_OUT_RX1)
    (add_net /LS_OUT_TX1)
    (add_net /MISO0)
    (add_net /MOSI0)
    (add_net "Net-(3V3_REGULATOR_1-Pad3)")
    (add_net "Net-(EXPANDER_1-Pad1)")
    (add_net "Net-(EXPANDER_1-Pad11)")
    (add_net "Net-(EXPANDER_1-Pad14)")
    (add_net "Net-(EXPANDER_1-Pad19)")
    (add_net "Net-(EXPANDER_1-Pad2)")
    (add_net "Net-(EXPANDER_1-Pad20)")
    (add_net "Net-(EXPANDER_1-Pad21)")
    (add_net "Net-(EXPANDER_1-Pad22)")
    (add_net "Net-(EXPANDER_1-Pad23)")
    (add_net "Net-(EXPANDER_1-Pad24)")
    (add_net "Net-(EXPANDER_1-Pad25)")
    (add_net "Net-(EXPANDER_1-Pad26)")
    (add_net "Net-(EXPANDER_1-Pad27)")
    (add_net "Net-(EXPANDER_1-Pad28)")
    (add_net "Net-(EXPANDER_1-Pad3)")
    (add_net "Net-(EXPANDER_1-Pad4)")
    (add_net "Net-(EXPANDER_1-Pad5)")
    (add_net "Net-(EXPANDER_1-Pad6)")
    (add_net "Net-(EXPANDER_1-Pad7)")
    (add_net "Net-(EXPANDER_1-Pad8)")
    (add_net "Net-(EXPANDER_2-Pad1)")
    (add_net "Net-(EXPANDER_2-Pad11)")
    (add_net "Net-(EXPANDER_2-Pad14)")
    (add_net "Net-(EXPANDER_2-Pad19)")
    (add_net "Net-(EXPANDER_2-Pad2)")
    (add_net "Net-(EXPANDER_2-Pad20)")
    (add_net "Net-(EXPANDER_2-Pad21)")
    (add_net "Net-(EXPANDER_2-Pad22)")
    (add_net "Net-(EXPANDER_2-Pad23)")
    (add_net "Net-(EXPANDER_2-Pad24)")
    (add_net "Net-(EXPANDER_2-Pad25)")
    (add_net "Net-(EXPANDER_2-Pad26)")
    (add_net "Net-(EXPANDER_2-Pad27)")
    (add_net "Net-(EXPANDER_2-Pad28)")
    (add_net "Net-(EXPANDER_2-Pad3)")
    (add_net "Net-(EXPANDER_2-Pad4)")
    (add_net "Net-(EXPANDER_2-Pad5)")
    (add_net "Net-(EXPANDER_2-Pad6)")
    (add_net "Net-(EXPANDER_2-Pad7)")
    (add_net "Net-(EXPANDER_2-Pad8)")
    (add_net "Net-(EXPANDER_3-Pad1)")
    (add_net "Net-(EXPANDER_3-Pad11)")
    (add_net "Net-(EXPANDER_3-Pad14)")
    (add_net "Net-(EXPANDER_3-Pad19)")
    (add_net "Net-(EXPANDER_3-Pad2)")
    (add_net "Net-(EXPANDER_3-Pad20)")
    (add_net "Net-(EXPANDER_3-Pad21)")
    (add_net "Net-(EXPANDER_3-Pad22)")
    (add_net "Net-(EXPANDER_3-Pad23)")
    (add_net "Net-(EXPANDER_3-Pad24)")
    (add_net "Net-(EXPANDER_3-Pad25)")
    (add_net "Net-(EXPANDER_3-Pad26)")
    (add_net "Net-(EXPANDER_3-Pad27)")
    (add_net "Net-(EXPANDER_3-Pad28)")
    (add_net "Net-(EXPANDER_3-Pad3)")
    (add_net "Net-(EXPANDER_3-Pad4)")
    (add_net "Net-(EXPANDER_3-Pad5)")
    (add_net "Net-(EXPANDER_3-Pad6)")
    (add_net "Net-(EXPANDER_3-Pad7)")
    (add_net "Net-(EXPANDER_3-Pad8)")
    (add_net "Net-(EXPANDER_4-Pad1)")
    (add_net "Net-(EXPANDER_4-Pad11)")
    (add_net "Net-(EXPANDER_4-Pad14)")
    (add_net "Net-(EXPANDER_4-Pad19)")
    (add_net "Net-(EXPANDER_4-Pad2)")
    (add_net "Net-(EXPANDER_4-Pad20)")
    (add_net "Net-(EXPANDER_4-Pad21)")
    (add_net "Net-(EXPANDER_4-Pad22)")
    (add_net "Net-(EXPANDER_4-Pad23)")
    (add_net "Net-(EXPANDER_4-Pad24)")
    (add_net "Net-(EXPANDER_4-Pad25)")
    (add_net "Net-(EXPANDER_4-Pad26)")
    (add_net "Net-(EXPANDER_4-Pad27)")
    (add_net "Net-(EXPANDER_4-Pad28)")
    (add_net "Net-(EXPANDER_4-Pad3)")
    (add_net "Net-(EXPANDER_4-Pad4)")
    (add_net "Net-(EXPANDER_4-Pad5)")
    (add_net "Net-(EXPANDER_4-Pad6)")
    (add_net "Net-(EXPANDER_4-Pad7)")
    (add_net "Net-(EXPANDER_4-Pad8)")
    (add_net "Net-(MAX485-PadJ1.1)")
    (add_net "Net-(MAX485-PadJ1.4)")
    (add_net "Net-(NanoPi_NEO_1-Pad11)")
    (add_net "Net-(NanoPi_NEO_1-Pad17)")
    (add_net "Net-(NanoPi_NEO_1-Pad22)")
    (add_net "Net-(POWER_LED_1-Pad2)")
    (add_net "Net-(R_LED0-Pad1)")
    (add_net "Net-(R_LED0-Pad2)")
    (add_net "Net-(R_LED1-Pad1)")
    (add_net "Net-(R_LED2-Pad1)")
    (add_net "Net-(RaspberryPi_1-Pad12)")
    (add_net "Net-(RaspberryPi_1-Pad14)")
    (add_net "Net-(RaspberryPi_1-Pad16)")
    (add_net "Net-(RaspberryPi_1-Pad17)")
    (add_net "Net-(RaspberryPi_1-Pad18)")
    (add_net "Net-(RaspberryPi_1-Pad20)")
    (add_net "Net-(RaspberryPi_1-Pad22)")
    (add_net "Net-(RaspberryPi_1-Pad25)")
    (add_net "Net-(RaspberryPi_1-Pad26)")
    (add_net "Net-(RaspberryPi_1-Pad27)")
    (add_net "Net-(RaspberryPi_1-Pad28)")
    (add_net "Net-(RaspberryPi_1-Pad30)")
    (add_net "Net-(RaspberryPi_1-Pad32)")
    (add_net "Net-(RaspberryPi_1-Pad34)")
    (add_net "Net-(RaspberryPi_1-Pad35)")
    (add_net "Net-(RaspberryPi_1-Pad36)")
    (add_net "Net-(RaspberryPi_1-Pad37)")
    (add_net "Net-(RaspberryPi_1-Pad38)")
    (add_net "Net-(RaspberryPi_1-Pad40)")
    (add_net "Net-(RaspberryPi_1-Pad7)")
  )
  (net_class I2C ""
    (clearance 0.381)
    (trace_width 0.762)
    (via_dia 1.143)
    (via_drill 0.889)
    (uvia_dia 0.889)
    (uvia_drill 0.381)
    (diff_pair_width 0.381)
    (diff_pair_gap 0.4572)
    (add_net /SCL1)
    (add_net /SCL1_HV)
    (add_net /SDA1)
    (add_net /SDA1_HV)
  )
  (net_class PowerWide ""
    (clearance 0.381)
    (trace_width 0.762)
    (via_dia 1.143)
    (via_drill 0.889)
    (uvia_dia 0.889)
    (uvia_drill 0.381)
    (diff_pair_width 0.381)
    (diff_pair_gap 0.4572)
    (add_net +5V)
    (add_net /3V3_PI)
    (add_net /5V_START)
    (add_net GND)
  )
  (net_class Serial ""
    (clearance 0.381)
    (trace_width 0.762)
    (via_dia 1.143)
    (via_drill 0.889)
    (uvia_dia 0.889)
    (uvia_drill 0.381)
    (diff_pair_width 0.381)
    (diff_pair_gap 0.4572)
    (add_net /RX1)
    (add_net /RX1_5V)
    (add_net /TX1)
    (add_net /TX1_5V)
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 5CB7A7D7)
    (at 39.348 35.284)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference "" (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm_Pad (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 5CB7A7D7)
    (at 147.044 87.608)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference "" (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm_Pad (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 5CB7A7D7)
    (at 43.942 71.628)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference "" (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm_Pad (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 5CB7A7D7)
    (at 211.814 126.216)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference "" (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm_Pad (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 5CB7A7D7)
    (at 214.884 41.656)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference "" (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm_Pad (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 5CB7A7D7)
    (at 126.238 40.386)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference "" (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm_Pad (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 5CB7A7D7)
    (at 50.038 115.062)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference "" (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm_Pad (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.5mm_Pad (layer F.Cu) (tedit 5CB7A7D7)
    (at 208.28 94.234)
    (descr "Mounting Hole 3.5mm")
    (tags "mounting hole 3.5mm")
    (attr virtual)
    (fp_text reference "" (at 0 -4.5) (layer F.SilkS))
    (fp_text value MountingHole_3.5mm_Pad (at 0 4.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 7 7) (drill 3.5) (layers *.Cu *.Mask))
  )
  (module w_conn_strip:vasch_strip_20x2 (layer F.Cu) (tedit 5FAB39D4)
    (at 56.4 49.4 180)
    (descr "Box header 20x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference RaspberryPi_1 (at -2.4 -5.5 180) (layer F.SilkS) hide)
    (fp_text value "Raspberry Socket" (at -33.2 0.1 270) (layer F.SilkS))
    (fp_text user 3V3 (at -26.48 6.6 90) (layer F.SilkS))
    (fp_text user 5V (at -26.58 -5.87 90) (layer F.SilkS))
    (fp_text user GND (at -21.48 -6.27 90) (layer F.SilkS))
    (fp_text user TX (at -18.98 -5.77 90) (layer F.SilkS))
    (fp_text user RX (at -16.38 -5.77 90) (layer F.SilkS))
    (fp_text user SDA (at -23.98 6.6 90) (layer F.SilkS))
    (fp_text user SCL (at -21.48 6.6 90) (layer F.SilkS))
    (fp_text user 5V (at -24.08 -5.87 90) (layer F.SilkS))
    (fp_text user GND (at 21.7 6.8 270) (layer F.SilkS))
    (fp_text user D_BTN1 (at 11.6 7.9 270) (layer F.SilkS))
    (fp_text user D_BTN2 (at 14.1 7.9 270) (layer F.SilkS))
    (fp_text user D_BTN3 (at 9.1 7.9 270) (layer F.SilkS))
    (fp_text user CLK (at 1.4 6.7 270) (layer F.SilkS))
    (fp_text user MISO (at -1.1 7 270) (layer F.SilkS))
    (fp_text user MOSI (at -3.6 7 270) (layer F.SilkS))
    (fp_text user CS0 (at 1.4 -6.2 270) (layer F.SilkS))
    (fp_text user GND (at -16.4 6.8 270) (layer F.SilkS))
    (fp_text user D_LED2 (at -11.5 7.2 270) (layer F.SilkS))
    (fp_text user D_LED4 (at -8.9 7.2 270) (layer F.SilkS))
    (fp_text user D_RS485 (at -13.8 7.3 270) (layer F.SilkS))
    (pad 37 thru_hole oval (at 19.19 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 110 "Net-(RaspberryPi_1-Pad37)"))
    (pad 38 thru_hole oval (at 19.19 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 111 "Net-(RaspberryPi_1-Pad38)"))
    (pad 40 thru_hole oval (at 21.73 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 112 "Net-(RaspberryPi_1-Pad40)"))
    (pad 39 thru_hole oval (at 21.73 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 35 thru_hole oval (at 16.65 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 113 "Net-(RaspberryPi_1-Pad35)"))
    (pad 36 thru_hole oval (at 16.65 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(RaspberryPi_1-Pad36)"))
    (pad 34 thru_hole oval (at 14.11 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 131 "Net-(RaspberryPi_1-Pad34)"))
    (pad 33 thru_hole oval (at 14.11 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D_BTN2))
    (pad 31 thru_hole oval (at 11.57 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 5 /D_BTN1))
    (pad 32 thru_hole oval (at 11.57 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(RaspberryPi_1-Pad32)"))
    (pad 27 thru_hole oval (at 6.49 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(RaspberryPi_1-Pad27)"))
    (pad 28 thru_hole oval (at 6.49 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 117 "Net-(RaspberryPi_1-Pad28)"))
    (pad 30 thru_hole oval (at 9.03 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 132 "Net-(RaspberryPi_1-Pad30)"))
    (pad 29 thru_hole oval (at 9.03 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 7 /D_BTN3))
    (pad 25 thru_hole oval (at 3.95 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 133 "Net-(RaspberryPi_1-Pad25)"))
    (pad 26 thru_hole oval (at 3.95 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 118 "Net-(RaspberryPi_1-Pad26)"))
    (pad 24 thru_hole oval (at 1.41 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 95 /CS0))
    (pad 23 thru_hole oval (at 1.41 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 93 /CLK0))
    (pad 21 thru_hole oval (at -1.13 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 94 /MISO0))
    (pad 22 thru_hole oval (at -1.13 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 119 "Net-(RaspberryPi_1-Pad22)"))
    (pad 20 thru_hole oval (at -3.67 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 134 "Net-(RaspberryPi_1-Pad20)"))
    (pad 19 thru_hole oval (at -3.67 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 96 /MOSI0))
    (pad 17 thru_hole oval (at -6.21 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 120 "Net-(RaspberryPi_1-Pad17)"))
    (pad 18 thru_hole oval (at -6.21 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 121 "Net-(RaspberryPi_1-Pad18)"))
    (pad 16 thru_hole oval (at -8.75 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 122 "Net-(RaspberryPi_1-Pad16)"))
    (pad 15 thru_hole oval (at -8.75 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 103 /D_LED1))
    (pad 13 thru_hole oval (at -11.29 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 104 /D_LED2))
    (pad 14 thru_hole oval (at -11.29 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 135 "Net-(RaspberryPi_1-Pad14)"))
    (pad 12 thru_hole oval (at -13.83 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 123 "Net-(RaspberryPi_1-Pad12)"))
    (pad 11 thru_hole oval (at -13.83 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 100 /D_RS485))
    (pad 9 thru_hole oval (at -16.37 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole oval (at -16.37 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 91 /RX1))
    (pad 8 thru_hole oval (at -18.91 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 92 /TX1))
    (pad 7 thru_hole oval (at -18.91 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 124 "Net-(RaspberryPi_1-Pad7)"))
    (pad 1 thru_hole rect (at -26.53 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 129 /3V3_PI))
    (pad 2 thru_hole oval (at -26.53 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 3 thru_hole oval (at -23.99 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 89 /SDA1))
    (pad 4 thru_hole oval (at -23.99 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 5 thru_hole oval (at -21.45 1.47 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 90 /SCL1))
    (pad 6 thru_hole oval (at -21.45 -1.07 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model walter/conn_strip/vasch_strip_20x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole (layer F.Cu) (tedit 55217C7B)
    (at 32.448 62.198 90)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005 90) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole (layer F.Cu) (tedit 55217CCB)
    (at 81.448 62.198 90)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005 90) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole (layer F.Cu) (tedit 55217CB9)
    (at 81.448 120.198 90)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005 90) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module RPi_Hat:RPi_Hat_Mounting_Hole (layer F.Cu) (tedit 55217CA2)
    (at 32.448 120.198 90)
    (descr "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 2,7mm, No Annular, Kein Restring,")
    (fp_text reference "" (at 0 -4.0005 90) (layer F.SilkS) hide)
    (fp_text value "" (at 0.09906 3.59918 90) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 0 90) (size 2.75 2.75) (drill 2.75) (layers *.Cu *.Mask)
      (solder_mask_margin 1.725) (clearance 1.725))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5C63A16B)
    (at 82.658 141.464)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (solder_mask_margin 1)
    (attr virtual)
    (fp_text reference H2 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5C63A15C)
    (at 82.658 106.064)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (solder_mask_margin 1)
    (attr virtual)
    (fp_text reference H3 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5C63A165)
    (at 47.258 141.464)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (solder_mask_margin 1)
    (attr virtual)
    (fp_text reference H1 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3mm (layer F.Cu) (tedit 5C63A154)
    (at 47.258 106.064)
    (descr "Mounting Hole 3mm, no annular")
    (tags "mounting hole 3mm no annular")
    (solder_mask_margin 1)
    (attr virtual)
    (fp_text reference H4 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module Socket_Strips:Socket_Strip_Straight_2x12_Pitch2.54mm (layer F.Cu) (tedit 5FA9AC00)
    (at 58.742 84.91 90)
    (descr "Through hole straight socket strip, 2x12, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x12 2.54mm double row")
    (fp_text reference NanoPi_NEO_1 (at -0.18 -14.59 90) (layer F.SilkS) hide)
    (fp_text value "NanoPi NEO Socket" (at -0.69 -16.642 270) (layer F.SilkS))
    (fp_text user %R (at -0.18 -14.59 90) (layer F.Fab) hide)
    (fp_text user RX (at 4.61 -1.942 270) (layer F.SilkS))
    (fp_text user TX (at 4.71 -4.542 90) (layer F.SilkS))
    (fp_text user 5V (at 3.91 -12.242 90) (layer F.SilkS))
    (fp_text user 5V (at 4.71 -9.642 90) (layer F.SilkS))
    (fp_text user GND (at 5.21 -7.342 90) (layer F.SilkS))
    (fp_text user 3v3 (at -5.39 -12.242 90) (layer F.SilkS))
    (fp_text user SDA (at -5.49 -9.742 90) (layer F.SilkS))
    (fp_text user SCL (at -5.39 -7.242 90) (layer F.SilkS))
    (fp_text user GND (at -5.49 -2.142 90) (layer F.SilkS))
    (fp_text user D_RS485 (at -6.19 -4.642 90) (layer F.SilkS))
    (fp_text user D_LED4 (at -6.09 5.458 90) (layer F.SilkS))
    (fp_text user D_LED2 (at -6.19 2.958 90) (layer F.SilkS))
    (fp_text user MOSI (at -5.69 10.558 90) (layer F.SilkS))
    (fp_text user MISO (at -5.69 13.158 90) (layer F.SilkS))
    (fp_text user CLK (at -5.39 15.658 90) (layer F.SilkS))
    (fp_text user CS0 (at 5.11 15.758 90) (layer F.SilkS))
    (fp_text user D_BTN2 (at 6.31 7.958 90) (layer F.SilkS))
    (fp_text user D_BTN1 (at 6.31 5.458 90) (layer F.SilkS))
    (fp_text user D_BTN3 (at 6.21 0.358 90) (layer F.SilkS))
    (fp_text user GND (at 5.21 10.558 90) (layer F.SilkS))
    (pad 24 thru_hole oval (at 1.09 15.68 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 95 /CS0))
    (pad 23 thru_hole oval (at -1.45 15.68 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 93 /CLK0))
    (pad 22 thru_hole oval (at 1.09 13.14 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 127 "Net-(NanoPi_NEO_1-Pad22)"))
    (pad 21 thru_hole oval (at -1.45 13.14 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 94 /MISO0))
    (pad 20 thru_hole oval (at 1.09 10.6 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 19 thru_hole oval (at -1.45 10.6 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 /MOSI0))
    (pad 18 thru_hole oval (at 1.09 8.06 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /D_BTN2))
    (pad 17 thru_hole oval (at -1.45 8.06 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "Net-(NanoPi_NEO_1-Pad17)"))
    (pad 16 thru_hole oval (at 1.09 5.52 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /D_BTN1))
    (pad 15 thru_hole oval (at -1.45 5.52 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 103 /D_LED1))
    (pad 14 thru_hole oval (at 1.09 2.98 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole oval (at -1.45 2.98 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 104 /D_LED2))
    (pad 12 thru_hole oval (at 1.09 0.44 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /D_BTN3))
    (pad 11 thru_hole oval (at -1.45 0.44 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 128 "Net-(NanoPi_NEO_1-Pad11)"))
    (pad 10 thru_hole oval (at 1.09 -2.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 91 /RX1))
    (pad 9 thru_hole oval (at -1.45 -2.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at 1.09 -4.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 /TX1))
    (pad 7 thru_hole oval (at -1.45 -4.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 100 /D_RS485))
    (pad 6 thru_hole oval (at 1.09 -7.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at -1.45 -7.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 /SCL1))
    (pad 4 thru_hole oval (at 1.09 -9.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 3 thru_hole oval (at -1.45 -9.72 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 /SDA1))
    (pad 2 thru_hole oval (at 1.09 -12.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 1 thru_hole rect (at -1.45 -12.26 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 129 /3V3_PI))
    (model ${KISYS3DMOD}/Socket_Strips.3dshapes/Socket_Strip_Straight_2x12_Pitch2.54mm.wrl
      (offset (xyz -1.269999980926514 -13.96999979019165 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module w_conn_screw:mors_2p (layer F.Cu) (tedit 0)
    (at 217.1 113.4)
    (descr "Terminal block 2 pins")
    (tags DEV)
    (fp_text reference POWER_SWITCH_1 (at 0 -5.842) (layer F.SilkS) hide)
    (fp_text value "Power switch" (at -0.5 -5.9) (layer F.SilkS))
    (pad 1 thru_hole rect (at -2.54 0) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 2 thru_hole circle (at 2.54 0) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 8 /5V_START))
    (model walter/conn_screw/mors_2p.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aetas_kicad:8p8c_2x8_roomhub (layer F.Cu) (tedit 5CC938AE)
    (at 147.955 136.525)
    (descr "8p8c socket")
    (fp_text reference RJ45x16_1 (at 14.05 -18.83) (layer F.SilkS) hide)
    (fp_text value "RJ45 x16" (at -0.255 -18.325 -180) (layer F.SilkS))
    (pad 4.7 thru_hole circle (at -38.35678 -15.28) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 4.5 thru_hole circle (at -35.81678 -15.28) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(EXPANDER_1-Pad7)"))
    (pad 16.4 thru_hole circle (at 49.4745 -12.72) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(EXPANDER_4-Pad6)"))
    (pad 6.4 thru_hole circle (at -20.54655 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(EXPANDER_2-Pad26)"))
    (pad 14.8 thru_hole circle (at 30.3945 -12.72) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 6.6 thru_hole circle (at -23.08655 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(EXPANDER_2-Pad28)"))
    (pad 16.8 thru_hole circle (at 44.3945 -12.72) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 16.5 thru_hole circle (at 48.2045 -15.26) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(EXPANDER_4-Pad7)"))
    (pad 14.4 thru_hole circle (at 35.4745 -12.72) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(EXPANDER_4-Pad26)"))
    (pad 14.1 thru_hole circle (at 39.2845 -15.26) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 14.7 thru_hole circle (at 31.6645 -15.26) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 12.4 thru_hole circle (at 21.4641 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(EXPANDER_3-Pad6)"))
    (pad 14.2 thru_hole circle (at 38.0145 -12.72) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 12.1 thru_hole circle (at 25.2741 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 12.6 thru_hole circle (at 18.9241 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(EXPANDER_3-Pad8)"))
    (pad 16.3 thru_hole circle (at 50.7445 -15.26) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(EXPANDER_4-Pad5)"))
    (pad 12.3 thru_hole circle (at 22.7341 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 53 "Net-(EXPANDER_3-Pad5)"))
    (pad 12.7 thru_hole circle (at 17.6541 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 4.1 thru_hole circle (at -30.73678 -15.28) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2.8 thru_hole circle (at -53.627 -12.75) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 12.5 thru_hole circle (at 20.1941 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(EXPANDER_3-Pad7)"))
    (pad 4.3 thru_hole circle (at -33.27678 -15.28) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(EXPANDER_1-Pad5)"))
    (pad 14.3 thru_hole circle (at 36.7445 -15.26) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(EXPANDER_4-Pad25)"))
    (pad 2.3 thru_hole circle (at -47.277 -15.29) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(EXPANDER_1-Pad25)"))
    (pad 4.8 thru_hole circle (at -39.62678 -12.74) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 16.7 thru_hole circle (at 45.6645 -15.26) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 12.8 thru_hole circle (at 16.3841 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 8.8 thru_hole circle (at -11.626385 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 8.1 thru_hole circle (at -2.736385 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 8.7 thru_hole circle (at -10.356385 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 6.3 thru_hole circle (at -19.27655 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(EXPANDER_2-Pad25)"))
    (pad 4.6 thru_hole circle (at -37.08678 -12.74) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(EXPANDER_1-Pad8)"))
    (pad 10.6 thru_hole circle (at 4.9239 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(EXPANDER_3-Pad28)"))
    (pad 16.1 thru_hole circle (at 53.2845 -15.26) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 16.6 thru_hole circle (at 46.9345 -12.72) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 78 "Net-(EXPANDER_4-Pad8)"))
    (pad 2.1 thru_hole circle (at -44.737 -15.29) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10.3 thru_hole circle (at 8.7339 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(EXPANDER_3-Pad25)"))
    (pad 6.8 thru_hole circle (at -25.62655 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 16.2 thru_hole circle (at 52.0145 -12.72) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 10.8 thru_hole circle (at 2.3839 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 10.4 thru_hole circle (at 7.4639 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(EXPANDER_3-Pad26)"))
    (pad 2.6 thru_hole circle (at -51.087 -12.75) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(EXPANDER_1-Pad28)"))
    (pad 4.2 thru_hole circle (at -32.00678 -12.74) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 8.5 thru_hole circle (at -7.816385 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(EXPANDER_2-Pad7)"))
    (pad 8.6 thru_hole circle (at -9.086385 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(EXPANDER_2-Pad8)"))
    (pad 8.3 thru_hole circle (at -5.276385 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 44 "Net-(EXPANDER_2-Pad5)"))
    (pad 10.2 thru_hole circle (at 10.0039 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 10.5 thru_hole circle (at 6.1939 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(EXPANDER_3-Pad27)"))
    (pad 6.2 thru_hole circle (at -18.00655 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 2.5 thru_hole circle (at -49.817 -15.29) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(EXPANDER_1-Pad27)"))
    (pad 14.5 thru_hole circle (at 34.2045 -15.26) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(EXPANDER_4-Pad27)"))
    (pad 2.4 thru_hole circle (at -48.547 -12.75) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(EXPANDER_1-Pad26)"))
    (pad 6.1 thru_hole circle (at -16.73655 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4.4 thru_hole circle (at -34.54678 -12.74) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(EXPANDER_1-Pad6)"))
    (pad 8.4 thru_hole circle (at -6.546385 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(EXPANDER_2-Pad6)"))
    (pad 2.7 thru_hole circle (at -52.357 -15.29) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 10.1 thru_hole circle (at 11.2739 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10.7 thru_hole circle (at 3.6539 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 12.2 thru_hole circle (at 24.0041 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 2.2 thru_hole circle (at -46.007 -12.75) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 14.6 thru_hole circle (at 32.9345 -12.72) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(EXPANDER_4-Pad28)"))
    (pad 8.2 thru_hole circle (at -4.006385 -12.73) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 6.5 thru_hole circle (at -21.81655 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(EXPANDER_2-Pad27)"))
    (pad 6.7 thru_hole circle (at -24.35655 -15.27) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 1.2 thru_hole circle (at -52.357 -8.54) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 1.4 thru_hole circle (at -49.817 -8.54) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(EXPANDER_1-Pad22)"))
    (pad 1.8 thru_hole circle (at -44.737 -8.54) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 1.6 thru_hole circle (at -47.277 -8.54) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(EXPANDER_1-Pad24)"))
    (pad 1.1 thru_hole circle (at -53.627 -6) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1.3 thru_hole circle (at -51.087 -6) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(EXPANDER_1-Pad21)"))
    (pad "" np_thru_hole circle (at -54.97 0.39) (size 3.2004 3.2004) (drill 3.2004) (layers *.Cu *.Mask F.SilkS))
    (pad 1.7 thru_hole circle (at -46.007 -6) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 1.5 thru_hole circle (at -48.547 -6) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(EXPANDER_1-Pad23)"))
    (pad 3.5 thru_hole circle (at -34.54678 -5.99) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(EXPANDER_1-Pad3)"))
    (pad 3.3 thru_hole circle (at -37.08678 -5.99) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(EXPANDER_1-Pad1)"))
    (pad 3.6 thru_hole circle (at -33.27678 -8.53) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(EXPANDER_1-Pad4)"))
    (pad 3.1 thru_hole circle (at -39.62678 -5.99) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3.7 thru_hole circle (at -32.00678 -5.99) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 3.8 thru_hole circle (at -30.73678 -8.53) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 3.4 thru_hole circle (at -35.81678 -8.53) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(EXPANDER_1-Pad2)"))
    (pad 3.2 thru_hole circle (at -38.35678 -8.53) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 5.1 thru_hole circle (at -25.62655 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5.8 thru_hole circle (at -16.73655 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 5.2 thru_hole circle (at -24.35655 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 5.4 thru_hole circle (at -21.81655 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(EXPANDER_2-Pad22)"))
    (pad 5.3 thru_hole circle (at -23.08655 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(EXPANDER_2-Pad21)"))
    (pad 5.6 thru_hole circle (at -19.27655 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(EXPANDER_2-Pad24)"))
    (pad 5.5 thru_hole circle (at -20.54655 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(EXPANDER_2-Pad23)"))
    (pad 5.7 thru_hole circle (at -18.00655 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 7.5 thru_hole circle (at -6.546385 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 46 "Net-(EXPANDER_2-Pad3)"))
    (pad 7.1 thru_hole circle (at -11.626385 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 7.4 thru_hole circle (at -7.816385 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 47 "Net-(EXPANDER_2-Pad2)"))
    (pad 7.6 thru_hole circle (at -5.276385 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 45 "Net-(EXPANDER_2-Pad4)"))
    (pad 7.2 thru_hole circle (at -10.356385 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 7.8 thru_hole circle (at -2.736385 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 7.3 thru_hole circle (at -9.086385 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 48 "Net-(EXPANDER_2-Pad1)"))
    (pad 7.7 thru_hole circle (at -4.006385 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 15.1 thru_hole circle (at 44.3945 -5.97) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 15.5 thru_hole circle (at 49.4745 -5.97) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(EXPANDER_4-Pad3)"))
    (pad 15.8 thru_hole circle (at 53.2845 -8.51) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 15.2 thru_hole circle (at 45.6645 -8.51) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 15.7 thru_hole circle (at 52.0145 -5.97) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad "" np_thru_hole circle (at 55.03 0.39) (size 3.2004 3.2004) (drill 3.2004) (layers *.Cu *.Mask F.SilkS))
    (pad 15.6 thru_hole circle (at 50.7445 -8.51) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(EXPANDER_4-Pad4)"))
    (pad 15.4 thru_hole circle (at 48.2045 -8.51) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(EXPANDER_4-Pad2)"))
    (pad 15.3 thru_hole circle (at 46.9345 -5.97) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(EXPANDER_4-Pad1)"))
    (pad 13.5 thru_hole circle (at 35.4745 -5.97) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(EXPANDER_4-Pad23)"))
    (pad 13.8 thru_hole circle (at 39.2845 -8.51) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 13.3 thru_hole circle (at 32.9345 -5.97) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 79 "Net-(EXPANDER_4-Pad21)"))
    (pad 13.6 thru_hole circle (at 36.7445 -8.51) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(EXPANDER_4-Pad24)"))
    (pad 13.2 thru_hole circle (at 31.6645 -8.51) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 13.4 thru_hole circle (at 34.2045 -8.51) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(EXPANDER_4-Pad22)"))
    (pad 13.1 thru_hole circle (at 30.3945 -5.97) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 13.7 thru_hole circle (at 38.0145 -5.97) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 11.3 thru_hole circle (at 18.9241 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 49 "Net-(EXPANDER_3-Pad1)"))
    (pad 11.6 thru_hole circle (at 22.7341 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 52 "Net-(EXPANDER_3-Pad4)"))
    (pad 11.1 thru_hole circle (at 16.3841 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 11.5 thru_hole circle (at 21.4641 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 51 "Net-(EXPANDER_3-Pad3)"))
    (pad 11.7 thru_hole circle (at 24.0041 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 11.4 thru_hole circle (at 20.1941 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 50 "Net-(EXPANDER_3-Pad2)"))
    (pad 11.8 thru_hole circle (at 25.2741 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 11.2 thru_hole circle (at 17.6541 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 9.1 thru_hole circle (at 2.3839 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 9.2 thru_hole circle (at 3.6539 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 9.3 thru_hole circle (at 4.9239 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(EXPANDER_3-Pad21)"))
    (pad 9.4 thru_hole circle (at 6.1939 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(EXPANDER_3-Pad22)"))
    (pad 9.5 thru_hole circle (at 7.4639 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(EXPANDER_3-Pad23)"))
    (pad 9.6 thru_hole circle (at 8.7339 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(EXPANDER_3-Pad24)"))
    (pad 9.7 thru_hole circle (at 10.0039 -5.98) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 9.8 thru_hole circle (at 11.2739 -8.52) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (model walter/conn_misc/8p8c.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 179.717 44.176 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R_LED_POWER_1 (at 3.81 -1.86 90) (layer F.SilkS) hide)
    (fp_text value R_POWER_LED (at 3.81 1.86 90) (layer F.SilkS))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 105 "Net-(POWER_LED_1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 189.877 44.176 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R_LED2 (at 3.81 -1.86 90) (layer F.SilkS) hide)
    (fp_text value R_LED2 (at 3.81 1.86 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 109 "Net-(R_LED2-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 104 /D_LED2))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 200.037 44.176 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R_LED1 (at 3.81 -1.86 90) (layer F.SilkS) hide)
    (fp_text value R_LED4 (at 3.81 1.86 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 108 "Net-(R_LED1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 103 /D_LED1))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 194.957 44.176 270)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R_LED0 (at 3.81 -1.86 90) (layer F.SilkS) hide)
    (fp_text value R_LED3 (at 3.81 1.86 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 107 "Net-(R_LED0-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 106 "Net-(R_LED0-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-28_W7.62mm_LongPads (layer F.Cu) (tedit 59C78D6B)
    (at 193.04 104.775 180)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference EXPANDER_4 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value MCP23017_SP (at 3.81 35.35) (layer F.Fab))
    (fp_text user %R (at 3.81 16.51) (layer F.Fab) hide)
    (fp_text user 011 (at 3.84 36.075 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 88 "Net-(EXPANDER_4-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 33.02 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 87 "Net-(EXPANDER_4-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 30.48 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 86 "Net-(EXPANDER_4-Pad3)"))
    (pad 17 thru_hole oval (at 7.62 27.94 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 85 "Net-(EXPANDER_4-Pad4)"))
    (pad 18 thru_hole oval (at 7.62 25.4 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 84 "Net-(EXPANDER_4-Pad5)"))
    (pad 19 thru_hole oval (at 7.62 22.86 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 83 "Net-(EXPANDER_4-Pad19)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 82 "Net-(EXPANDER_4-Pad6)"))
    (pad 20 thru_hole oval (at 7.62 20.32 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 81 "Net-(EXPANDER_4-Pad20)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 80 "Net-(EXPANDER_4-Pad7)"))
    (pad 21 thru_hole oval (at 7.62 17.78 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 79 "Net-(EXPANDER_4-Pad21)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 "Net-(EXPANDER_4-Pad8)"))
    (pad 22 thru_hole oval (at 7.62 15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 77 "Net-(EXPANDER_4-Pad22)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 23 thru_hole oval (at 7.62 12.7 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(EXPANDER_4-Pad23)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole oval (at 7.62 10.16 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(EXPANDER_4-Pad24)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(EXPANDER_4-Pad11)"))
    (pad 25 thru_hole oval (at 7.62 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(EXPANDER_4-Pad25)"))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 136 /SCL1_HV))
    (pad 26 thru_hole oval (at 7.62 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 72 "Net-(EXPANDER_4-Pad26)"))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 130 /SDA1_HV))
    (pad 27 thru_hole oval (at 7.62 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 71 "Net-(EXPANDER_4-Pad27)"))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 70 "Net-(EXPANDER_4-Pad14)"))
    (pad 28 thru_hole oval (at 7.62 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 69 "Net-(EXPANDER_4-Pad28)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-28_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-28_W7.62mm_LongPads (layer F.Cu) (tedit 59C78D6B)
    (at 165.1 104.775 180)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference EXPANDER_3 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value MCP23017_SP (at 3.81 35.35) (layer F.Fab))
    (fp_text user %R (at 3.81 16.51) (layer F.Fab) hide)
    (fp_text user 010 (at 4 36.075 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "Net-(EXPANDER_3-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 33.02 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(EXPANDER_3-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 30.48 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(EXPANDER_3-Pad3)"))
    (pad 17 thru_hole oval (at 7.62 27.94 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 52 "Net-(EXPANDER_3-Pad4)"))
    (pad 18 thru_hole oval (at 7.62 25.4 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 53 "Net-(EXPANDER_3-Pad5)"))
    (pad 19 thru_hole oval (at 7.62 22.86 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 54 "Net-(EXPANDER_3-Pad19)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 55 "Net-(EXPANDER_3-Pad6)"))
    (pad 20 thru_hole oval (at 7.62 20.32 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 56 "Net-(EXPANDER_3-Pad20)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 57 "Net-(EXPANDER_3-Pad7)"))
    (pad 21 thru_hole oval (at 7.62 17.78 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "Net-(EXPANDER_3-Pad21)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 59 "Net-(EXPANDER_3-Pad8)"))
    (pad 22 thru_hole oval (at 7.62 15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "Net-(EXPANDER_3-Pad22)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 23 thru_hole oval (at 7.62 12.7 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 61 "Net-(EXPANDER_3-Pad23)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole oval (at 7.62 10.16 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "Net-(EXPANDER_3-Pad24)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "Net-(EXPANDER_3-Pad11)"))
    (pad 25 thru_hole oval (at 7.62 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(EXPANDER_3-Pad25)"))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 136 /SCL1_HV))
    (pad 26 thru_hole oval (at 7.62 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 65 "Net-(EXPANDER_3-Pad26)"))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 130 /SDA1_HV))
    (pad 27 thru_hole oval (at 7.62 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "Net-(EXPANDER_3-Pad27)"))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "Net-(EXPANDER_3-Pad14)"))
    (pad 28 thru_hole oval (at 7.62 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 68 "Net-(EXPANDER_3-Pad28)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-28_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-28_W7.62mm_LongPads (layer F.Cu) (tedit 59C78D6B)
    (at 137.16 104.775 180)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference EXPANDER_2 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value MCP23017_SP (at 3.81 35.35) (layer F.Fab))
    (fp_text user %R (at 3.81 16.51) (layer F.Fab) hide)
    (fp_text user 001 (at 3.76 36.175 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(EXPANDER_2-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 33.02 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 47 "Net-(EXPANDER_2-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 30.48 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(EXPANDER_2-Pad3)"))
    (pad 17 thru_hole oval (at 7.62 27.94 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(EXPANDER_2-Pad4)"))
    (pad 18 thru_hole oval (at 7.62 25.4 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(EXPANDER_2-Pad5)"))
    (pad 19 thru_hole oval (at 7.62 22.86 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(EXPANDER_2-Pad19)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 42 "Net-(EXPANDER_2-Pad6)"))
    (pad 20 thru_hole oval (at 7.62 20.32 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 41 "Net-(EXPANDER_2-Pad20)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 40 "Net-(EXPANDER_2-Pad7)"))
    (pad 21 thru_hole oval (at 7.62 17.78 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 39 "Net-(EXPANDER_2-Pad21)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 38 "Net-(EXPANDER_2-Pad8)"))
    (pad 22 thru_hole oval (at 7.62 15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(EXPANDER_2-Pad22)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 23 thru_hole oval (at 7.62 12.7 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 36 "Net-(EXPANDER_2-Pad23)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole oval (at 7.62 10.16 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(EXPANDER_2-Pad24)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 34 "Net-(EXPANDER_2-Pad11)"))
    (pad 25 thru_hole oval (at 7.62 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 33 "Net-(EXPANDER_2-Pad25)"))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 136 /SCL1_HV))
    (pad 26 thru_hole oval (at 7.62 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 32 "Net-(EXPANDER_2-Pad26)"))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 130 /SDA1_HV))
    (pad 27 thru_hole oval (at 7.62 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(EXPANDER_2-Pad27)"))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 30 "Net-(EXPANDER_2-Pad14)"))
    (pad 28 thru_hole oval (at 7.62 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(EXPANDER_2-Pad28)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-28_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-28_W7.62mm_LongPads (layer F.Cu) (tedit 59C78D6B)
    (at 109.22 104.775 180)
    (descr "28-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference EXPANDER_1 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value MCP23017_SP (at 3.81 35.35) (layer F.Fab))
    (fp_text user %R (at 3.81 16.51) (layer F.Fab) hide)
    (fp_text user 000 (at 4.02 36.175 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(EXPANDER_1-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 33.02 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(EXPANDER_1-Pad2)"))
    (pad 16 thru_hole oval (at 7.62 30.48 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(EXPANDER_1-Pad3)"))
    (pad 17 thru_hole oval (at 7.62 27.94 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(EXPANDER_1-Pad4)"))
    (pad 18 thru_hole oval (at 7.62 25.4 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(EXPANDER_1-Pad5)"))
    (pad 19 thru_hole oval (at 7.62 22.86 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(EXPANDER_1-Pad19)"))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(EXPANDER_1-Pad6)"))
    (pad 20 thru_hole oval (at 7.62 20.32 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(EXPANDER_1-Pad20)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(EXPANDER_1-Pad7)"))
    (pad 21 thru_hole oval (at 7.62 17.78 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(EXPANDER_1-Pad21)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(EXPANDER_1-Pad8)"))
    (pad 22 thru_hole oval (at 7.62 15.24 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(EXPANDER_1-Pad22)"))
    (pad 9 thru_hole oval (at 0 20.32 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad 23 thru_hole oval (at 7.62 12.7 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(EXPANDER_1-Pad23)"))
    (pad 10 thru_hole oval (at 0 22.86 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 24 thru_hole oval (at 7.62 10.16 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(EXPANDER_1-Pad24)"))
    (pad 11 thru_hole oval (at 0 25.4 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(EXPANDER_1-Pad11)"))
    (pad 25 thru_hole oval (at 7.62 7.62 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(EXPANDER_1-Pad25)"))
    (pad 12 thru_hole oval (at 0 27.94 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 136 /SCL1_HV))
    (pad 26 thru_hole oval (at 7.62 5.08 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(EXPANDER_1-Pad26)"))
    (pad 13 thru_hole oval (at 0 30.48 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 130 /SDA1_HV))
    (pad 27 thru_hole oval (at 7.62 2.54 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(EXPANDER_1-Pad27)"))
    (pad 14 thru_hole oval (at 0 33.02 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(EXPANDER_1-Pad14)"))
    (pad 28 thru_hole oval (at 7.62 0 180) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(EXPANDER_1-Pad28)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-28_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_2x2 (layer F.Cu) (tedit 0)
    (at 217.6 72.2 180)
    (descr "Pin strip 2x2pin")
    (tags "CONN DEV")
    (fp_text reference 3V3_ADD_1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "3.3V ADD" (at 0.076 -3.952) (layer F.SilkS))
    (fp_text user 3V3 (at -3.424 -0.152 90) (layer F.SilkS))
    (fp_text user GND (at 3.376 -0.252 90) (layer F.SilkS))
    (pad 4 thru_hole oval (at 1.27 -1.27 180) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 1.27 1.27 180) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at -1.27 -1.27 180) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 2 /3V3))
    (pad 1 thru_hole rect (at -1.27 1.27 180) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 2 /3V3))
    (model walter/pin_strip/pin_strip_2x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Power_Integrations:TO-220 (layer F.Cu) (tedit 0)
    (at 205.994 72.136 180)
    (descr "Non Isolated JEDEC TO-220 Package")
    (tags "Power Integration YN Package")
    (fp_text reference 3V3_REGULATOR_1 (at 0 -4.318) (layer F.SilkS) hide)
    (fp_text value "3.3V REGULATOR" (at 0.294 2.936) (layer F.SilkS))
    (pad 1 thru_hole oval (at -2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 3 "Net-(3V3_REGULATOR_1-Pad3)"))
    (pad 2 thru_hole oval (at 0 0 180) (size 2.032 2.54) (drill 1.143) (layers *.Cu *.Mask)
      (net 2 /3V3))
  )
  (module w_pin_strip:pin_strip_2x2 (layer F.Cu) (tedit 0)
    (at 217.424 81.788 180)
    (descr "Pin strip 2x2pin")
    (tags "CONN DEV")
    (fp_text reference 5V_ADD_1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value "5V ADD" (at -0.076 -4.212) (layer F.SilkS))
    (fp_text user 5V (at -3.476 -0.012 270) (layer F.SilkS))
    (fp_text user GND (at 3.424 0.088 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 1.27 180) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 2 thru_hole oval (at -1.27 -1.27 180) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 3 thru_hole oval (at 1.27 1.27 180) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole oval (at 1.27 -1.27 180) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (model walter/pin_strip/pin_strip_2x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_2 (layer F.Cu) (tedit 0)
    (at 204.724 82.55 180)
    (descr "Pin strip 2pin")
    (tags "CONN DEV")
    (fp_text reference 5V_TO_DL33CV_JUMPER_1 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value Jumper (at -0.176 -2.65) (layer F.SilkS) hide)
    (pad 1 thru_hole rect (at -1.27 0 180) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 2 thru_hole oval (at 1.27 0 180) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(3V3_REGULATOR_1-Pad3)"))
    (model walter/pin_strip/pin_strip_2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5923F252)
    (at 68.326 34.29)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference BUTTON_2 (at 3.25 -2) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /D_BTN2))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 6 /D_BTN2))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz 0.1269999980926514 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_PUSH_6mm (layer F.Cu) (tedit 5923F252)
    (at 57.658 34.29)
    (descr https://www.omron.com/ecb/products/pdf/en-b3f.pdf)
    (tags "tact sw push 6mm")
    (fp_text reference BUTTON_1 (at 3.25 -2) (layer F.SilkS))
    (fp_text value SW_Push (at 3.75 6.7) (layer F.Fab))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 2 thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /D_BTN1))
    (pad 1 thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 5 /D_BTN1))
    (pad 1 thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_PUSH_6mm.wrl
      (offset (xyz 0.1269999980926514 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_screw:mors_2p (layer F.Cu) (tedit 0)
    (at 213.372 51.796 180)
    (descr "Terminal block 2 pins")
    (tags DEV)
    (fp_text reference BUTTON_3 (at 0 -5.842) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x02 (at 0 5.842) (layer F.SilkS) hide)
    (pad 2 thru_hole circle (at 2.54 0 180) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 1 thru_hole rect (at -2.54 0 180) (size 2.99974 2.99974) (drill 1.24968) (layers *.Cu *.Mask F.SilkS)
      (net 7 /D_BTN3))
    (model walter/conn_screw/mors_2p.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_misc:dc_socket (layer F.Cu) (tedit 0)
    (at 216.8 140.3)
    (descr "Socket, DC power supply")
    (fp_text reference DC_JACK_1 (at 0 8.6995) (layer F.SilkS) hide)
    (fp_text value "DC 5V" (at 0.2 -9) (layer F.SilkS))
    (fp_text user GND (at 7.7 -3.4 90) (layer F.SilkS))
    (pad 1 thru_hole oval (at 5.30098 -3.50012) (size 1.99898 4.0005) (drill oval 1.00076 2.99974) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 -0.24892) (size 4.0005 1.99898) (drill oval 2.99974 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 -6.25094) (size 4.50088 1.99898) (drill oval 3.50012 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 8 /5V_START))
    (model walter/conn_misc/dc_socket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_conn_strip:vasch_strip_5x2 (layer F.Cu) (tedit 0)
    (at 151.384 39.624 180)
    (descr "Box header 5x2pin 2.54mm")
    (tags "CONN DEV")
    (fp_text reference EXTRA_IO_CONNECTOR_1 (at 0 -5.7) (layer F.SilkS) hide)
    (fp_text value "Extra IO Connector" (at 11.684 0.324 90) (layer F.SilkS))
    (pad 9 thru_hole oval (at 5.08 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 10 thru_hole oval (at 5.08 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 8 thru_hole oval (at 2.54 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 93 /CLK0))
    (pad 7 thru_hole oval (at 2.54 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 94 /MISO0))
    (pad 1 thru_hole rect (at -5.08 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 130 /SDA1_HV))
    (pad 2 thru_hole oval (at -5.08 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 136 /SCL1_HV))
    (pad 3 thru_hole oval (at -2.54 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 4 thru_hole oval (at -2.54 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 5 thru_hole oval (at 0 1.27 180) (size 1.5 2) (drill 1 (offset 0 0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 96 /MOSI0))
    (pad 6 thru_hole oval (at 0 -1.27 180) (size 1.5 2) (drill 1 (offset 0 -0.25)) (layers *.Cu *.Mask F.SilkS)
      (net 95 /CS0))
    (model walter/conn_strip/vasch_strip_5x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module aetas_kicad:LEVEL-SHIFTER-4CH (layer F.Cu) (tedit 5CB24CDF)
    (at 101.6 44.958)
    (descr "<b>4-Channel Bi-Directional  Logic Level Converter</b> based on <b>BSS128</b> transistors")
    (fp_text reference LEVEL_SHIFTER_1 (at 0 -9.525) (layer F.SilkS) hide)
    (fp_text value "LEVEL SHIFTER" (at 0 9.525) (layer F.SilkS))
    (fp_text user HV1 (at 3.175 -6.35) (layer F.SilkS))
    (fp_text user HV2 (at 3.175 -3.81) (layer F.SilkS))
    (fp_text user HV (at 3.175 -1.27) (layer F.SilkS))
    (fp_text user GND (at 0 1.27) (layer F.SilkS))
    (fp_text user HV3 (at 3.175 3.81) (layer F.SilkS))
    (fp_text user HV4 (at 3.175 6.35) (layer F.SilkS))
    (fp_text user LV1 (at -3.175 -6.35) (layer F.SilkS))
    (fp_text user LV2 (at -3.175 -3.81) (layer F.SilkS))
    (fp_text user LV (at -3.175 -1.27) (layer F.SilkS))
    (fp_text user LV3 (at -3.175 3.81) (layer F.SilkS))
    (fp_text user LV4 (at -3.175 6.35) (layer F.SilkS))
    (pad C1 thru_hole rect (at 5.08 -6.35) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 130 /SDA1_HV))
    (pad C2 thru_hole circle (at 5.08 -3.81) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 136 /SCL1_HV))
    (pad B1 thru_hole circle (at 5.08 -1.27) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V))
    (pad B3 thru_hole circle (at 5.08 1.27) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad C3 thru_hole circle (at 5.08 3.81) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 125 /LS_OUT_RX1))
    (pad C4 thru_hole circle (at 5.08 6.35) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 126 /LS_OUT_TX1))
    (pad A1 thru_hole rect (at -5.08 -6.35) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 89 /SDA1))
    (pad A2 thru_hole circle (at -5.08 -3.81) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 90 /SCL1))
    (pad B2 thru_hole circle (at -5.08 -1.27) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 129 /3V3_PI))
    (pad B4 thru_hole circle (at -5.08 1.27) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad A3 thru_hole circle (at -5.08 3.81) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 91 /RX1))
    (pad A4 thru_hole circle (at -5.08 6.35) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 92 /TX1))
  )
  (module "DIY Library:RS485-TTL-CONVERTER" (layer F.Cu) (tedit 0)
    (at 147.066 55.626)
    (descr "<b>RS485 to TTL converter</b> based on <b>MAX485</b> chip")
    (fp_text reference MAX485 (at 0 -8.255) (layer F.SilkS) hide)
    (fp_text value MAX485 (at 0.134 7.774) (layer F.SilkS))
    (pad J1.1 thru_hole rect (at -20.32 3.81) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 99 "Net-(MAX485-PadJ1.1)") (solder_mask_margin 0.1016))
    (pad J1.2 thru_hole circle (at -20.32 1.27) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 100 /D_RS485) (solder_mask_margin 0.1016))
    (pad J1.3 thru_hole circle (at -20.32 -1.27) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 100 /D_RS485) (solder_mask_margin 0.1016))
    (pad J1.4 thru_hole circle (at -20.32 -3.81) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 101 "Net-(MAX485-PadJ1.4)") (solder_mask_margin 0.1016))
    (pad J2.1 thru_hole rect (at 20.32 -3.81 180) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 4 +5V) (solder_mask_margin 0.1016))
    (pad J2.2 thru_hole circle (at 20.32 -1.27 180) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 98 /RX1_5V) (solder_mask_margin 0.1016))
    (pad J2.3 thru_hole circle (at 20.32 1.27 180) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 97 /TX1_5V) (solder_mask_margin 0.1016))
    (pad J2.4 thru_hole circle (at 20.32 3.81 180) (size 1.508 1.508) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND) (solder_mask_margin 0.1016))
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 587A3A7B)
    (at 177.177 32.258)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference POWER_LED_1 (at 1.27 -2.96) (layer F.SilkS) hide)
    (fp_text value "POWER LED" (at 1.523 -2.958) (layer F.SilkS))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 105 "Net-(POWER_LED_1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_2x2 (layer F.Cu) (tedit 0)
    (at 110.998 61.468 180)
    (descr "Pin strip 2x2pin")
    (tags "CONN DEV")
    (fp_text reference RS485_Jumpers_1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value UART_JUMPERS (at 3.398 1.568 90) (layer F.SilkS))
    (pad 4 thru_hole oval (at 1.27 -1.27 180) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 98 /RX1_5V))
    (pad 3 thru_hole oval (at 1.27 1.27 180) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 125 /LS_OUT_RX1))
    (pad 2 thru_hole oval (at -1.27 -1.27 180) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 97 /TX1_5V))
    (pad 1 thru_hole rect (at -1.27 1.27 180) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 126 /LS_OUT_TX1))
    (model walter/pin_strip/pin_strip_2x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_2x2 (layer F.Cu) (tedit 0)
    (at 119.634 53.848 270)
    (descr "Pin strip 2x2pin")
    (tags "CONN DEV")
    (fp_text reference RS485_MAX_Jumpers_1 (at 0 -3.81 90) (layer F.SilkS) hide)
    (fp_text value "MAX485 JUMPERS" (at 2.252 3.534 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at -1.27 1.27 270) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 125 /LS_OUT_RX1))
    (pad 2 thru_hole oval (at -1.27 -1.27 270) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(MAX485-PadJ1.4)"))
    (pad 3 thru_hole oval (at 1.27 1.27 270) (size 1.524 1.99898) (drill 1.00076 (offset 0 0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 126 /LS_OUT_TX1))
    (pad 4 thru_hole oval (at 1.27 -1.27 270) (size 1.524 1.99898) (drill 1.00076 (offset 0 -0.24892)) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(MAX485-PadJ1.1)"))
    (model walter/pin_strip/pin_strip_2x2.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_socket_1 (layer F.Cu) (tedit 0)
    (at 194.957 59.416)
    (descr "Pin socket 1pin")
    (tags "CONN DEV")
    (fp_text reference STATUS_RGB_LED1_1 (at 0 -2.159) (layer F.SilkS) hide)
    (fp_text value LED3_IN (at -0.057 -2.316) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask F.SilkS)
      (net 106 "Net-(R_LED0-Pad2)"))
    (model walter/pin_strip/pin_socket_1.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_BL-FL7680RGB (layer F.Cu) (tedit 59F6ACD6)
    (at 189.877 32.111)
    (descr "'Piranha' RGB LED, through hole, common anode, 7.62x7.62mm, BGRA pin order, https://cdn-shop.adafruit.com/datasheets/BL-FL7680RGB.pdf")
    (tags "RGB LED Piranha Super-Flux BetLux")
    (fp_text reference STATUS_RGB_LED_1 (at 2.54 -2.27) (layer F.SilkS) hide)
    (fp_text value LED_ABRG (at 2.123 -2.711) (layer F.SilkS))
    (fp_text user %R (at 2.54 2.54) (layer F.Fab) hide)
    (pad 3 thru_hole circle (at 5.08 5.08) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 107 "Net-(R_LED0-Pad1)"))
    (pad 4 thru_hole circle (at 5.08 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 108 "Net-(R_LED1-Pad1)"))
    (pad 2 thru_hole circle (at 0 5.08) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 109 "Net-(R_LED2-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_BL-FL7680RGB.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text mqgateway.com (at 32.004 89.408 90) (layer B.SilkS))
  (gr_text NanoPi (at 46.101 128.0668 90) (layer F.SilkS))
  (gr_text NanoPi (at 83.947 127.7112 270) (layer F.SilkS))
  (gr_text NanoPi (at 64.2112 105.029) (layer F.SilkS))
  (gr_text Raspberry (at 30.226 109.22 90) (layer F.SilkS))
  (gr_text Raspberry (at 30.226 76.962 90) (layer F.SilkS))
  (gr_text Raspberry (at 83.82 77.724 270) (layer F.SilkS))
  (gr_text Raspberry (at 57.658 60.198) (layer F.SilkS))
  (gr_text GND (at 210.9 54.9) (layer F.SilkS))
  (gr_text GND (at 174.3 32.2) (layer F.SilkS))
  (gr_text optional (at 142.7 39.6 90) (layer F.SilkS))
  (gr_text optional (at 144.5 56) (layer F.SilkS))
  (gr_text "MIT License\nCopyright (c) 2020 Mariusz Jozala" (at 223.2 29.7) (layer B.SilkS))
  (gr_text RPi (at 81.2 66.7) (layer B.SilkS))
  (gr_text RPi (at 32.3 66.6) (layer B.SilkS))
  (gr_text RPi (at 81.4 115.5) (layer B.SilkS))
  (gr_text RPi (at 32.4 115.4) (layer B.SilkS))
  (gr_text NanoPi (at 47.1 101.8) (layer B.SilkS))
  (gr_text NanoPi (at 82.7 102) (layer B.SilkS))
  (gr_text NanoPi (at 82.6 137.4) (layer B.SilkS))
  (gr_text NanoPi (at 47 137.4) (layer B.SilkS))
  (gr_text "MIT License\nCopyright (c) 2020 Mariusz Jozala" (at 28.7 28.3) (layer F.SilkS))
  (gr_text mqgateway.com (at 222.5 33.6 270) (layer F.SilkS))
  (gr_text Aetas (at 72.1 115) (layer B.SilkS))
  (gr_text "rev. 1.0" (at 44.196 126.746) (layer B.SilkS))
  (gr_text MqGateway (at 58.3 120.8) (layer B.SilkS))
  (gr_text "rev 1.0" (at 218.238 35.744) (layer F.SilkS))
  (gr_text MqGateway (at 204.738 33.144) (layer F.SilkS))
  (gr_text Aetas (at 205.038 30.944) (layer F.SilkS))
  (gr_text "Connect vertically\nto enable UART" (at 113.2 65.7) (layer F.SilkS))
  (gr_text "Connect horizontally\nto enable MAX485" (at 117.5 49.6) (layer F.SilkS))
  (gr_text TX5V (at 153.9 32.9 90) (layer F.SilkS))
  (gr_text MOSI (at 151.4 32.9 90) (layer F.SilkS))
  (gr_text MISO (at 148.9 32.9 90) (layer F.SilkS))
  (gr_text CLK0 (at 148.9 46.3 90) (layer F.SilkS))
  (gr_text CS0 (at 151.4 46 90) (layer F.SilkS))
  (gr_text RX5V (at 154 46.5 90) (layer F.SilkS))
  (gr_text SDA_5V (at 162.2 38.1) (layer F.SilkS))
  (gr_text SCL_5V (at 162.3 41.1) (layer F.SilkS))
  (gr_text 5V (at 146.3 45.6 90) (layer F.SilkS))
  (gr_text GND (at 146.3 33.2 90) (layer F.SilkS))
  (gr_text GND (at 186.6 32) (layer F.SilkS))
  (gr_text 4 (at 197.2 32) (layer F.SilkS))
  (gr_text 3 (at 197.2 37.1) (layer F.SilkS))
  (gr_text 2 (at 187.6 37.1) (layer F.SilkS))
  (gr_text "CONNECT TO\nENABLE 3.3V\nREGULATOR" (at 204.6 86.9) (layer F.SilkS))
  (gr_text 2 (at 98.2 114.7) (layer F.SilkS))
  (gr_text 1 (at 98.2 118) (layer F.SilkS))
  (gr_text 3 (at 112.8 118) (layer F.SilkS))
  (gr_text 4 (at 112.8 114.7) (layer F.SilkS))
  (gr_text 6 (at 127 114.9) (layer F.SilkS))
  (gr_text 5 (at 127 118.2) (layer F.SilkS))
  (gr_text 8 (at 140.3 114.7) (layer F.SilkS))
  (gr_text 7 (at 140.3 118) (layer F.SilkS))
  (gr_text 10 (at 155.3 114.9) (layer F.SilkS))
  (gr_text 9 (at 155.3 118.2) (layer F.SilkS))
  (gr_text 12 (at 168.5 114.5) (layer F.SilkS))
  (gr_text 11 (at 168.5 117.8) (layer F.SilkS))
  (gr_text 14 (at 182.6 114.6) (layer F.SilkS))
  (gr_text 13 (at 182.6 117.9) (layer F.SilkS))
  (gr_text 16 (at 196.5 114.6) (layer F.SilkS))
  (gr_text 15 (at 196.5 117.9) (layer F.SilkS))
  (dimension 120 (width 0.15) (layer Dwgs.User)
    (gr_text "120,000 mm" (at 233.3 85 270) (layer Dwgs.User))
    (feature1 (pts (xy 226.6 145) (xy 232.586421 145)))
    (feature2 (pts (xy 226.6 25) (xy 232.586421 25)))
    (crossbar (pts (xy 232 25) (xy 232 145)))
    (arrow1a (pts (xy 232 145) (xy 231.413579 143.873496)))
    (arrow1b (pts (xy 232 145) (xy 232.586421 143.873496)))
    (arrow2a (pts (xy 232 25) (xy 231.413579 26.126504)))
    (arrow2b (pts (xy 232 25) (xy 232.586421 26.126504)))
  )
  (dimension 200 (width 0.15) (layer Dwgs.User)
    (gr_text "200,000 mm" (at 126.5 18.7) (layer Dwgs.User))
    (feature1 (pts (xy 226.5 25) (xy 226.5 19.413579)))
    (feature2 (pts (xy 26.5 25) (xy 26.5 19.413579)))
    (crossbar (pts (xy 26.5 20) (xy 226.5 20)))
    (arrow1a (pts (xy 226.5 20) (xy 225.373496 20.586421)))
    (arrow1b (pts (xy 226.5 20) (xy 225.373496 19.413579)))
    (arrow2a (pts (xy 26.5 20) (xy 27.626504 20.586421)))
    (arrow2b (pts (xy 26.5 20) (xy 27.626504 19.413579)))
  )
  (gr_line (start 226.5 25) (end 226.5 145) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 26.5 25) (end 226.5 25) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 26.5 145) (end 26.5 25) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 82.658 141.464) (end 84.158 141.464) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 82.658 106.064) (end 84.158 106.064) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 47.258 141.464) (end 48.758 141.464) (layer Edge.Cuts) (width 0.2))
  (gr_circle (center 47.258 106.064) (end 48.758 106.064) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 26.5 145) (end 226.5 145) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 226.5 145) (xy 26.5 145) (xy 26.5 25) (xy 226.5 25)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 226.5 145) (xy 26.6 145) (xy 26.6 25) (xy 226.5 25)
      )
    )
  )
)
