(kicad_pcb (version 20171130) (host pcbnew 5.1.9-73d0e3b20d~88~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 111)
    (tracks 252)
    (zones 0)
    (modules 15)
    (nets 49)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 /C39)
  (net 2 /C38)
  (net 3 /C37)
  (net 4 /C36)
  (net 5 /C35)
  (net 6 /C34)
  (net 7 /C32)
  (net 8 /C31)
  (net 9 /C30)
  (net 10 /C28)
  (net 11 /C27)
  (net 12 /C25)
  (net 13 /C24)
  (net 14 /C23)
  (net 15 /C22)
  (net 16 /C21)
  (net 17 /C20)
  (net 18 /C17)
  (net 19 /C16)
  (net 20 /C15)
  (net 21 /C14)
  (net 22 /C12)
  (net 23 /C11)
  (net 24 /C9)
  (net 25 /C8)
  (net 26 /C7)
  (net 27 /C6)
  (net 28 /C4)
  (net 29 /C2)
  (net 30 GND)
  (net 31 +5V)
  (net 32 +3V3)
  (net 33 "Net-(J107-Pad11)")
  (net 34 "Net-(J107-Pad10)")
  (net 35 "Net-(J107-Pad9)")
  (net 36 "Net-(J107-Pad8)")
  (net 37 "Net-(J107-Pad7)")
  (net 38 "Net-(J107-Pad6)")
  (net 39 "Net-(J107-Pad5)")
  (net 40 "Net-(J107-Pad4)")
  (net 41 "Net-(J107-Pad3)")
  (net 42 "Net-(J107-Pad2)")
  (net 43 "Net-(J107-Pad1)")
  (net 44 "Net-(J107-Pad15)")
  (net 45 "Net-(J107-Pad14)")
  (net 46 "Net-(J107-Pad13)")
  (net 47 "Net-(J107-Pad12)")
  (net 48 "Net-(J102-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /C11)
    (add_net /C12)
    (add_net /C14)
    (add_net /C15)
    (add_net /C16)
    (add_net /C17)
    (add_net /C2)
    (add_net /C20)
    (add_net /C21)
    (add_net /C22)
    (add_net /C23)
    (add_net /C24)
    (add_net /C25)
    (add_net /C27)
    (add_net /C28)
    (add_net /C30)
    (add_net /C31)
    (add_net /C32)
    (add_net /C34)
    (add_net /C35)
    (add_net /C36)
    (add_net /C37)
    (add_net /C38)
    (add_net /C39)
    (add_net /C4)
    (add_net /C6)
    (add_net /C7)
    (add_net /C8)
    (add_net /C9)
    (add_net GND)
    (add_net "Net-(J102-Pad1)")
    (add_net "Net-(J107-Pad1)")
    (add_net "Net-(J107-Pad10)")
    (add_net "Net-(J107-Pad11)")
    (add_net "Net-(J107-Pad12)")
    (add_net "Net-(J107-Pad13)")
    (add_net "Net-(J107-Pad14)")
    (add_net "Net-(J107-Pad15)")
    (add_net "Net-(J107-Pad2)")
    (add_net "Net-(J107-Pad3)")
    (add_net "Net-(J107-Pad4)")
    (add_net "Net-(J107-Pad5)")
    (add_net "Net-(J107-Pad6)")
    (add_net "Net-(J107-Pad7)")
    (add_net "Net-(J107-Pad8)")
    (add_net "Net-(J107-Pad9)")
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_SilkScreen (layer B.Cu) (tedit 0)
    (at 121.9 118.9 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module Symbol:OSHW-Logo2_7.3x6mm_SilkScreen (layer F.Cu) (tedit 0)
    (at 121.9 118.9)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer F.SilkS) hide)
    (fp_text value OSHW-Logo2_7.3x6mm_SilkScreen (at 0.75 0) (layer F.Fab) hide)
  )
  (module Button_Switch_THT:SW_DIP_SPSTx01_Slide_9.78x4.72mm_W7.62mm_P2.54mm (layer F.Cu) (tedit 5A4E1404)
    (at 119.5 88)
    (descr "1x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 9.78x4.72mm (see e.g. https://www.ctscorp.com/wp-content/uploads/206-208.pdf)")
    (tags "DIP Switch SPST Slide 7.62mm 300mil")
    (fp_text reference Fan (at -0.3 -3.7) (layer F.SilkS))
    (fp_text value SW_SPST (at 3.81 3.42) (layer F.Fab) hide)
    (fp_text user on (at 5.365 -1.4975) (layer F.Fab) hide)
    (fp_text user %R (at 7.27 0 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 48 "Net-(J102-Pad1)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 +5V))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx01_Slide_9.78x4.72mm_W7.62mm_P2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A41D)
    (at 175.7 92.4)
    (descr "Through hole straight socket strip, 1x15, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x15 2.54mm single row")
    (fp_text reference J108 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value Conn_01x11_Female (at 0 38.33) (layer F.Fab) hide)
    (fp_text user %R (at 0 17.78 90) (layer F.Fab) hide)
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J107-Pad15)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J107-Pad14)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J107-Pad13)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J107-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J107-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J107-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J107-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J107-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J107-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J107-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J107-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J107-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J107-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J107-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J107-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x15_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x15_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A41D)
    (at 169.7 92.4)
    (descr "Through hole straight socket strip, 1x15, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x15 2.54mm single row")
    (fp_text reference J107 (at 0 -2.77) (layer F.SilkS) hide)
    (fp_text value Conn_01x11_Female (at 0 38.33) (layer F.Fab) hide)
    (fp_text user %R (at 0 17.78 90) (layer F.Fab) hide)
    (pad 15 thru_hole oval (at 0 35.56) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "Net-(J107-Pad15)"))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "Net-(J107-Pad14)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J107-Pad13)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "Net-(J107-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J107-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J107-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J107-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J107-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J107-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J107-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J107-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(J107-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J107-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J107-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "Net-(J107-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x15_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical_SMD locked (layer B.Cu) (tedit 5A19A428)
    (at 147.7 80.25 270)
    (descr "surface-mounted straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Surface mounted socket strip SMD 2x20 2.54mm double row")
    (attr smd)
    (fp_text reference J105 (at 0 26.9 270) (layer B.SilkS) hide)
    (fp_text value "Rpi Connector" (at 0 -26.9 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab) hide)
    (pad 40 smd rect (at -2.52 -24.13 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 1 /C39))
    (pad 39 smd rect (at 2.52 -24.13 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 30 GND))
    (pad 38 smd rect (at -2.52 -21.59 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 3 /C37))
    (pad 37 smd rect (at 2.52 -21.59 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 2 /C38))
    (pad 36 smd rect (at -2.52 -19.05 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 5 /C35))
    (pad 35 smd rect (at 2.52 -19.05 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 4 /C36))
    (pad 34 smd rect (at -2.52 -16.51 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 30 GND))
    (pad 33 smd rect (at 2.52 -16.51 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 6 /C34))
    (pad 32 smd rect (at -2.52 -13.97 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 8 /C31))
    (pad 31 smd rect (at 2.52 -13.97 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 7 /C32))
    (pad 30 smd rect (at -2.52 -11.43 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 30 GND))
    (pad 29 smd rect (at 2.52 -11.43 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 9 /C30))
    (pad 28 smd rect (at -2.52 -8.89 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 11 /C27))
    (pad 27 smd rect (at 2.52 -8.89 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 10 /C28))
    (pad 26 smd rect (at -2.52 -6.35 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 12 /C25))
    (pad 25 smd rect (at 2.52 -6.35 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 30 GND))
    (pad 24 smd rect (at -2.52 -3.81 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 14 /C23))
    (pad 23 smd rect (at 2.52 -3.81 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 13 /C24))
    (pad 22 smd rect (at -2.52 -1.27 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 16 /C21))
    (pad 21 smd rect (at 2.52 -1.27 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 15 /C22))
    (pad 20 smd rect (at -2.52 1.27 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 30 GND))
    (pad 19 smd rect (at 2.52 1.27 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 17 /C20))
    (pad 18 smd rect (at -2.52 3.81 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 18 /C17))
    (pad 17 smd rect (at 2.52 3.81 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 32 +3V3))
    (pad 16 smd rect (at -2.52 6.35 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 20 /C15))
    (pad 15 smd rect (at 2.52 6.35 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 19 /C16))
    (pad 14 smd rect (at -2.52 8.89 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 30 GND))
    (pad 13 smd rect (at 2.52 8.89 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 21 /C14))
    (pad 12 smd rect (at -2.52 11.43 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 23 /C11))
    (pad 11 smd rect (at 2.52 11.43 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 22 /C12))
    (pad 10 smd rect (at -2.52 13.97 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 24 /C9))
    (pad 9 smd rect (at 2.52 13.97 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 30 GND))
    (pad 8 smd rect (at -2.52 16.51 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 26 /C7))
    (pad 7 smd rect (at 2.52 16.51 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 25 /C8))
    (pad 6 smd rect (at -2.52 19.05 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 30 GND))
    (pad 5 smd rect (at 2.52 19.05 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 27 /C6))
    (pad 4 smd rect (at -2.52 21.59 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 31 +5V))
    (pad 3 smd rect (at 2.52 21.59 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 28 /C4))
    (pad 2 smd rect (at -2.52 24.13 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 31 +5V))
    (pad 1 smd rect (at 2.52 24.13 270) (size 3 1) (layers B.Cu B.Paste B.Mask)
      (net 29 /C2))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_2x20_P2.54mm_Vertical_SMD locked (layer F.Cu) (tedit 5A19A428)
    (at 147.7 80.25 90)
    (descr "surface-mounted straight socket strip, 2x20, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Surface mounted socket strip SMD 2x20 2.54mm double row")
    (attr smd)
    (fp_text reference J101 (at 0 -26.9 90) (layer F.SilkS) hide)
    (fp_text value "Upper Connector" (at 0 26.9 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab) hide)
    (pad 40 smd rect (at -2.52 24.13 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 39 smd rect (at 2.52 24.13 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 1 /C39))
    (pad 38 smd rect (at -2.52 21.59 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /C38))
    (pad 37 smd rect (at 2.52 21.59 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /C37))
    (pad 36 smd rect (at -2.52 19.05 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /C36))
    (pad 35 smd rect (at 2.52 19.05 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /C35))
    (pad 34 smd rect (at -2.52 16.51 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /C34))
    (pad 33 smd rect (at 2.52 16.51 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 32 smd rect (at -2.52 13.97 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 7 /C32))
    (pad 31 smd rect (at 2.52 13.97 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /C31))
    (pad 30 smd rect (at -2.52 11.43 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 9 /C30))
    (pad 29 smd rect (at 2.52 11.43 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 28 smd rect (at -2.52 8.89 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 10 /C28))
    (pad 27 smd rect (at 2.52 8.89 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 11 /C27))
    (pad 26 smd rect (at -2.52 6.35 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 25 smd rect (at 2.52 6.35 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 12 /C25))
    (pad 24 smd rect (at -2.52 3.81 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 13 /C24))
    (pad 23 smd rect (at 2.52 3.81 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 14 /C23))
    (pad 22 smd rect (at -2.52 1.27 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 15 /C22))
    (pad 21 smd rect (at 2.52 1.27 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 16 /C21))
    (pad 20 smd rect (at -2.52 -1.27 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 17 /C20))
    (pad 19 smd rect (at 2.52 -1.27 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 18 smd rect (at -2.52 -3.81 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 32 +3V3))
    (pad 17 smd rect (at 2.52 -3.81 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 18 /C17))
    (pad 16 smd rect (at -2.52 -6.35 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 19 /C16))
    (pad 15 smd rect (at 2.52 -6.35 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 20 /C15))
    (pad 14 smd rect (at -2.52 -8.89 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 21 /C14))
    (pad 13 smd rect (at 2.52 -8.89 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 12 smd rect (at -2.52 -11.43 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 22 /C12))
    (pad 11 smd rect (at 2.52 -11.43 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 23 /C11))
    (pad 10 smd rect (at -2.52 -13.97 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 9 smd rect (at 2.52 -13.97 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 24 /C9))
    (pad 8 smd rect (at -2.52 -16.51 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 25 /C8))
    (pad 7 smd rect (at 2.52 -16.51 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 26 /C7))
    (pad 6 smd rect (at -2.52 -19.05 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 27 /C6))
    (pad 5 smd rect (at 2.52 -19.05 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 30 GND))
    (pad 4 smd rect (at -2.52 -21.59 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 28 /C4))
    (pad 3 smd rect (at 2.52 -21.59 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 31 +5V))
    (pad 2 smd rect (at -2.52 -24.13 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 29 /C2))
    (pad 1 smd rect (at 2.52 -24.13 90) (size 3 1) (layers F.Cu F.Paste F.Mask)
      (net 31 +5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x20_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad locked (layer B.Cu) (tedit 56D1B4CB)
    (at 157.2 126.5 180)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 3.8) (layer B.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 -3.8) (layer B.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad locked (layer B.Cu) (tedit 56D1B4CB)
    (at 125.2 126.5 90)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 3.8 90) (layer B.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 -3.8 90) (layer B.Fab) hide)
    (fp_text user %R (at 0.3 0 90) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad locked (layer B.Cu) (tedit 56D1B4CB)
    (at 157.2 94.5 270)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 3.8 90) (layer B.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 -3.8 90) (layer B.Fab) hide)
    (fp_text user %R (at 0.3 0 90) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 270) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3_DIN965_Pad locked (layer B.Cu) (tedit 56D1B4CB)
    (at 125.3 94.35)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (attr virtual)
    (fp_text reference REF** (at 0 3.8) (layer B.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_DIN965_Pad (at 0 -3.8) (layer B.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer B.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A430)
    (at 143.4 88.2 270)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference J106 (at 0 -2.77 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Female (at 0 15.47 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 6.35) (layer F.Fab) hide)
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 +5V))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 +5V))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 +5V))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 +5V))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 +5V))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 +5V))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A430)
    (at 177.1 88.2 270)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference J104 (at 0 -2.77 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Female (at 0 15.47 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 6.35) (layer F.Fab) hide)
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 +3V3))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 +3V3))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 +3V3))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 +3V3))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 +3V3))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x06_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A430)
    (at 160.3 88.2 270)
    (descr "Through hole straight socket strip, 1x06, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x06 2.54mm single row")
    (fp_text reference J103 (at 0 -2.77 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x06_Female (at 0 15.47 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 6.35) (layer F.Fab) hide)
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 GND))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x06_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical (layer F.Cu) (tedit 5C28146C)
    (at 176.5 81.6 90)
    (descr "JST XH series connector, B2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST XH vertical")
    (fp_text reference J102 (at 1.25 -3.55 90) (layer F.SilkS) hide)
    (fp_text value Fan (at 1.25 4.6 90) (layer F.Fab) hide)
    (fp_text user %R (at 1.25 2.7 90) (layer F.Fab) hide)
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask)
      (net 30 GND))
    (pad 1 thru_hole roundrect (at 0 0 90) (size 1.7 2) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235294118)
      (net 48 "Net-(J102-Pad1)"))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_XH_B2B-XH-A_1x02_P2.50mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Copyright © 2021 Spyridakis Christos" (at 166.9 113.4 90) (layer B.SilkS))
  (gr_text 5V (at 130.6 90.6) (layer B.SilkS))
  (gr_text Gnd (at 148.1 90.6) (layer B.SilkS))
  (gr_text 3v3 (at 164.9 90.7) (layer B.SilkS))
  (gr_text "Raspberry Pi breakout" (at 141.6 129.2) (layer B.SilkS))
  (gr_text 3 (at 167 97.5) (layer F.SilkS))
  (gr_text 12 (at 167 120.2) (layer F.SilkS))
  (gr_text 10 (at 167 115.1) (layer F.SilkS))
  (gr_text 5 (at 167 102.6) (layer F.SilkS))
  (gr_text 14 (at 167 125.4) (layer F.SilkS))
  (gr_text 6 (at 167 105.2) (layer F.SilkS))
  (gr_text 13 (at 167 123) (layer F.SilkS))
  (gr_text 11 (at 167 117.6) (layer F.SilkS))
  (gr_text 4 (at 167 100.1) (layer F.SilkS))
  (gr_text 15 (at 167 128) (layer F.SilkS))
  (gr_text 9 (at 166.9 112.7) (layer F.SilkS))
  (gr_text 2 (at 167 94.9) (layer F.SilkS))
  (gr_text 7 (at 166.9 107.6) (layer F.SilkS))
  (gr_text 8 (at 166.9 110.1) (layer F.SilkS))
  (gr_text 1 (at 167 92.4) (layer F.SilkS))
  (gr_text JLCJLCJLCJLC (at 178.3 124.5 90) (layer B.SilkS))
  (gr_text 15 (at 178.3 128) (layer F.SilkS))
  (gr_text 14 (at 178.3 125.4) (layer F.SilkS))
  (gr_text 13 (at 178.3 123) (layer F.SilkS))
  (gr_text 12 (at 178.3 120.2) (layer F.SilkS))
  (gr_text 11 (at 178.3 117.6) (layer F.SilkS))
  (gr_text 10 (at 178.3 115.1) (layer F.SilkS))
  (gr_text 9 (at 178.2 112.7) (layer F.SilkS))
  (gr_text 8 (at 178.2 110.1) (layer F.SilkS))
  (gr_text 7 (at 178.2 107.6) (layer F.SilkS))
  (gr_text 6 (at 178.3 105.2) (layer F.SilkS))
  (gr_text 5 (at 178.3 102.6) (layer F.SilkS))
  (gr_text 4 (at 178.3 100.1) (layer F.SilkS))
  (gr_text 3 (at 178.3 97.5) (layer F.SilkS))
  (gr_text 2 (at 178.3 94.9) (layer F.SilkS))
  (gr_text 1 (at 178.3 92.4) (layer F.SilkS))
  (dimension 55.8 (width 0.15) (layer Dwgs.User)
    (gr_text "55,800 mm" (at 112.7 102.8 270) (layer Dwgs.User))
    (feature1 (pts (xy 117.4 130.7) (xy 113.413579 130.7)))
    (feature2 (pts (xy 117.4 74.9) (xy 113.413579 74.9)))
    (crossbar (pts (xy 114 74.9) (xy 114 130.7)))
    (arrow1a (pts (xy 114 130.7) (xy 113.413579 129.573496)))
    (arrow1b (pts (xy 114 130.7) (xy 114.586421 129.573496)))
    (arrow2a (pts (xy 114 74.9) (xy 113.413579 76.026504)))
    (arrow2b (pts (xy 114 74.9) (xy 114.586421 76.026504)))
  )
  (dimension 5.7 (width 0.15) (layer Dwgs.User)
    (gr_text "5,700 mm" (at 120.25 67) (layer Dwgs.User))
    (feature1 (pts (xy 117.4 76.5) (xy 117.4 67.713579)))
    (feature2 (pts (xy 123.1 76.5) (xy 123.1 67.713579)))
    (crossbar (pts (xy 123.1 68.3) (xy 117.4 68.3)))
    (arrow1a (pts (xy 117.4 68.3) (xy 118.526504 67.713579)))
    (arrow1b (pts (xy 117.4 68.3) (xy 118.526504 68.886421)))
    (arrow2a (pts (xy 123.1 68.3) (xy 121.973496 67.713579)))
    (arrow2b (pts (xy 123.1 68.3) (xy 121.973496 68.886421)))
  )
  (dimension 62.5 (width 0.15) (layer Dwgs.User)
    (gr_text "62,500 mm" (at 148.65 61.7) (layer Dwgs.User))
    (feature1 (pts (xy 179.9 74.9) (xy 179.9 62.413579)))
    (feature2 (pts (xy 117.4 74.9) (xy 117.4 62.413579)))
    (crossbar (pts (xy 117.4 63) (xy 179.9 63)))
    (arrow1a (pts (xy 179.9 63) (xy 178.773496 63.586421)))
    (arrow1b (pts (xy 179.9 63) (xy 178.773496 62.413579)))
    (arrow2a (pts (xy 117.4 63) (xy 118.526504 63.586421)))
    (arrow2b (pts (xy 117.4 63) (xy 118.526504 62.413579)))
  )
  (gr_text "Raspberry Pi breakout" (at 163.1 116.4 90) (layer F.SilkS))
  (gr_text Fan (at 177 85.7) (layer F.SilkS))
  (gr_text 3v3 (at 165 91.6 90) (layer F.SilkS))
  (gr_text Gnd (at 161.8 91.9 90) (layer F.SilkS))
  (gr_text 5V (at 130.3 91.1 90) (layer F.SilkS))
  (gr_text 19 (at 166.8 85) (layer F.SilkS))
  (gr_text Gnd (at 171.8 85) (layer F.SilkS))
  (gr_text 13 (at 164.2 85) (layer F.SilkS))
  (gr_text 6 (at 161.7 85) (layer F.SilkS))
  (gr_text Sd (at 156.7 85) (layer F.SilkS))
  (gr_text Gnd (at 154.1 85) (layer F.SilkS))
  (gr_text 26 (at 169.3 85) (layer F.SilkS))
  (gr_text 5 (at 159.2 85) (layer F.SilkS))
  (gr_text Sc (at 156.6 75.6) (layer F.SilkS))
  (gr_text 7 (at 154.1 75.6) (layer F.SilkS))
  (gr_text 12 (at 161.7 75.6) (layer F.SilkS))
  (gr_text 16 (at 166.8 75.6) (layer F.SilkS))
  (gr_text 21 (at 171.9 75.6) (layer F.SilkS))
  (gr_text Gnd (at 164.2 75.6) (layer F.SilkS))
  (gr_text 20 (at 169.25 75.6) (layer F.SilkS))
  (gr_text Gnd (at 159.1 75.6) (layer F.SilkS))
  (gr_text Sda (at 126.1 85) (layer F.SilkS))
  (gr_text 3v3 (at 123.55 85) (layer F.SilkS))
  (gr_text 3v3 (at 143.95 85) (layer F.SilkS))
  (gr_text 4 (at 131.15 85.1) (layer F.SilkS))
  (gr_text 17 (at 136.3 85) (layer F.SilkS))
  (gr_text 22 (at 141.35 85) (layer F.SilkS))
  (gr_text Gnd (at 133.75 85) (layer F.SilkS))
  (gr_text Mis (at 149.05 85) (layer F.SilkS))
  (gr_text 27 (at 138.85 85) (layer F.SilkS))
  (gr_text Scl (at 128.65 85) (layer F.SilkS))
  (gr_text Clk (at 151.55 85) (layer F.SilkS))
  (gr_text Mos (at 146.5 85) (layer F.SilkS))
  (gr_text Gnd (at 146.5 75.6) (layer F.SilkS))
  (gr_text 24 (at 143.95 75.6) (layer F.SilkS))
  (gr_text 8 (at 151.55 75.6) (layer F.SilkS))
  (gr_text 25 (at 149.05 75.6) (layer F.SilkS))
  (gr_text 18 (at 136.3 75.6) (layer F.SilkS))
  (gr_text Rx (at 133.75 75.6) (layer F.SilkS))
  (gr_text 23 (at 141.35 75.6) (layer F.SilkS))
  (gr_text Gnd (at 138.85 75.6) (layer F.SilkS))
  (gr_text Tx (at 131.15 75.6) (layer F.SilkS))
  (gr_text Gnd (at 128.65 75.6) (layer F.SilkS))
  (gr_text 5V (at 126.1 75.6) (layer F.SilkS))
  (gr_text 5V (at 123.55 75.6) (layer F.SilkS))
  (gr_circle (center 141.2 110.5) (end 155.2 101.5) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 118.2 129.9) (end 117.4 129.9) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 179.1 129.9) (end 179.1 130.7) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 179.1 75.7) (end 179.9 75.7) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 118.2 75.7) (end 118.2 74.9) (angle -90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 117.4 129.9) (end 117.4 75.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.1 130.7) (end 118.2 130.7) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 179.9 75.7) (end 179.9 129.9) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 118.2 74.9) (end 179.1 74.9) (layer Edge.Cuts) (width 0.15))
  (zone (net 30) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 179.9 131.592935) (xy 117.3 131.6) (xy 117.3 74.6) (xy 179.9 74.592935)
      )
    )
  )
  (zone (net 30) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.5 131.5) (xy 179.9 131.574654) (xy 179.9 74.574654) (xy 117.5 74.5)
      )
    )
  )
)
