(kicad_pcb (version 4) (host pcbnew 4.0.7)
  (general
    (links 185)
    (no_connects 0)
    (area 92.190477 80.845 170.85 143.700001)
    (thickness 1.6)
    (drawings 88)
    (tracks 327)
    (zones 0)
    (modules 50)
    (nets 56)
  )
  (page A4)
  (title_block
    (title "USB Host Shield for M5Stack")
    (date 2018-09-06)
    (rev "ver 0.2")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (trace_clearance 0.18)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 104 133)
    (grid_origin 104 133)
    (visible_elements 7FFEFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerver/))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /+5V)
  (net 3 "Net-(J1-Pad2)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad8)")
  (net 6 "Net-(J1-Pad10)")
  (net 7 "Net-(J1-Pad13)")
  (net 8 "Net-(J1-Pad14)")
  (net 9 "Net-(J1-Pad25)")
  (net 10 "Net-(J1-Pad26)")
  (net 11 "Net-(J1-Pad30)")
  (net 12 "Net-(J1-Pad11)")
  (net 13 "Net-(J1-Pad9)")
  (net 14 "Net-(J1-Pad7)")
  (net 15 "Net-(J1-Pad6)")
  (net 16 "Net-(J1-Pad16)")
  (net 17 "Net-(J1-Pad20)")
  (net 18 VCC)
  (net 19 VDD)
  (net 20 "Net-(J1-Pad15)")
  (net 21 SDA)
  (net 22 SCL)
  (net 23 "Net-(J1-Pad19)")
  (net 24 "Net-(J1-Pad21)")
  (net 25 "Net-(J1-Pad22)")
  (net 26 "Net-(J1-Pad23)")
  (net 27 "Net-(J1-Pad24)")
  (net 28 "Net-(J20-Pad1)")
  (net 29 "Net-(J31-Pad5)")
  (net 30 "Net-(J31-Pad6)")
  (net 31 "Net-(J32-Pad5)")
  (net 32 "Net-(J32-Pad6)")
  (net 33 "Net-(J33-Pad5)")
  (net 34 "Net-(J33-Pad6)")
  (net 35 "Net-(J34-Pad5)")
  (net 36 "Net-(J34-Pad6)")
  (net 37 "Net-(J35-Pad5)")
  (net 38 "Net-(J35-Pad6)")
  (net 39 A0)
  (net 40 A1)
  (net 41 A2)
  (net 42 A3)
  (net 43 A4)
  (net 44 A5)
  (net 45 PWM0)
  (net 46 PWM1)
  (net 47 PWM2)
  (net 48 PWM3)
  (net 49 PWM4)
  (net 50 PWM5)
  (net 51 PWM6)
  (net 52 PWM7)
  (net 53 PWM8)
  (net 54 PWM9)
  (net 55 "Net-(R23-Pad1)")
  (net_class Default "これは標準のネット クラスです。"
    (clearance 0.18)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+5V)
    (add_net A0)
    (add_net A1)
    (add_net A2)
    (add_net A3)
    (add_net A4)
    (add_net A5)
    (add_net GND)
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad13)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad15)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad24)")
    (add_net "Net-(J1-Pad25)")
    (add_net "Net-(J1-Pad26)")
    (add_net "Net-(J1-Pad30)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J20-Pad1)")
    (add_net "Net-(J31-Pad5)")
    (add_net "Net-(J31-Pad6)")
    (add_net "Net-(J32-Pad5)")
    (add_net "Net-(J32-Pad6)")
    (add_net "Net-(J33-Pad5)")
    (add_net "Net-(J33-Pad6)")
    (add_net "Net-(J34-Pad5)")
    (add_net "Net-(J34-Pad6)")
    (add_net "Net-(J35-Pad5)")
    (add_net "Net-(J35-Pad6)")
    (add_net "Net-(R23-Pad1)")
    (add_net PWM0)
    (add_net PWM1)
    (add_net PWM2)
    (add_net PWM3)
    (add_net PWM4)
    (add_net PWM5)
    (add_net PWM6)
    (add_net PWM7)
    (add_net PWM8)
    (add_net PWM9)
    (add_net SCL)
    (add_net SDA)
    (add_net VCC)
    (add_net VDD)
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B61DD55)
    (at 107 130)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MK1 (at -5.54 -0.302) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B32D20E)
    (at 143.624 123.348 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at 2.413 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-323 (layer F.Cu) (tedit 5B3722B8)
    (at 145.529 123.348 90)
    (descr SOD-323)
    (tags SOD-323)
    (attr smd)
    (fp_text reference D1 (at 2.7305 0.127 90) (layer F.SilkS))
    (fp_text value 1N4148 (at 0.1 1.9 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.85 90) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 18 VCC))
    (pad 2 smd rect (at 1.05 0 90) (size 0.6 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-323.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B61DD4A)
    (at 107 86)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MK2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B61DD71)
    (at 151 86)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MK3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 5B61DD62)
    (at 151 130)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference MK4 (at 5 -1) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5B61DD59)
    (at 111 130)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference MK5 (at 0.112 4.016) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5B61DD45)
    (at 111 86)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference MK6 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5B61DD6D)
    (at 147 86)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference MK7 (at 0 -4) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_2.2mm_M2 (layer F.Cu) (tedit 5B61DD5D)
    (at 147 130)
    (descr "Mounting Hole 2.2mm, no annular, M2")
    (tags "mounting hole 2.2mm no annular m2")
    (attr virtual)
    (fp_text reference MK8 (at 0 5) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
  )
  (module footprint:OSHW-logo_silkscreen-front_3mm (layer B.Cu) (tedit 0)
    (at 142.354 86.7085 180)
    (fp_text reference LOGO1 (at 0 -1.59004 180) (layer B.SilkS) hide)
    (fp_text value OPEN_HARDWARE_1 (at 0 1.59004 180) (layer B.SilkS) hide)
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B5F2AC4)
    (at 124 122.5 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 1.5 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 /+5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B37235C)
    (at 121.78 102.52)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C100 (at -1.905 1.397) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B372573)
    (at 139.052 113.696 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C101 (at 1.4224 -1.3208 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 138.925 104.425 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C102 (at 0 -1.5 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 90) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 138.29 98.075 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C103 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 59958EE7)
    (at 128.765 98.075 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C104 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 5B372382)
    (at 119.24 98.075 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C105 (at 0.254 -1.0795 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 18 VCC))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B5F299F)
    (at 140 125.5 270)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J11 (at -2.763 -0.068 360) (layer F.SilkS))
    (fp_text value VCC_SEL (at 4.385 4.81 270) (layer F.Fab))
    (fp_text user %R (at 2.77 1.27 360) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /+5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B5F29BC)
    (at 148 122)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J12 (at 0.704 5.031 90) (layer F.SilkS))
    (fp_text value SRV_VCC (at 4.385 4.81) (layer F.Fab))
    (fp_text user %R (at 2.77 1.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 VCC))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_1x02_Pitch2.54mm (layer F.Cu) (tedit 5B370726)
    (at 117.97 130.968 90)
    (descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x02 2.54mm single row")
    (fp_text reference J20 (at 0.508 5.08 90) (layer F.SilkS))
    (fp_text value Battery (at 4.385 4.81 90) (layer F.Fab))
    (fp_text user %R (at 2.77 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "Net-(J20-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x02_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x03_Pitch2.54mm (layer F.Cu) (tedit 5B61DC85)
    (at 141.465 112.68)
    (descr "Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x03 2.54mm double row")
    (fp_text reference J31 (at 3.429 -1.905) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 5.655 7.35) (layer F.Fab))
    (fp_text user %R (at 5.31 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 VCC))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 VCC))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "Net-(J31-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(J31-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x03_Pitch2.54mm (layer F.Cu) (tedit 5B61DC7D)
    (at 141.465 103.155)
    (descr "Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x03 2.54mm double row")
    (fp_text reference J32 (at 3.683 -2.159) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 5.655 7.35) (layer F.Fab))
    (fp_text user %R (at 5.31 2.54 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 VCC))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 VCC))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J32-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J32-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x03_Pitch2.54mm (layer F.Cu) (tedit 5B61DC6F)
    (at 137.02 95.535 90)
    (descr "Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x03 2.54mm double row")
    (fp_text reference J33 (at 1.016 6.858 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 5.655 7.35 90) (layer F.Fab))
    (fp_text user %R (at 5.31 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 VCC))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 VCC))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J33-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J33-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x03_Pitch2.54mm (layer F.Cu) (tedit 5B61DC6B)
    (at 127.495 95.535 90)
    (descr "Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x03 2.54mm double row")
    (fp_text reference J34 (at 1.143 6.858 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 5.655 7.35 90) (layer F.Fab))
    (fp_text user %R (at 5.31 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 VCC))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 VCC))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(J34-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J34-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Angled_2x03_Pitch2.54mm (layer F.Cu) (tedit 5B61DC66)
    (at 117.97 95.535 90)
    (descr "Through hole angled pin header, 2x03, 2.54mm pitch, 6mm pin length, double rows")
    (tags "Through hole angled pin header THT 2x03 2.54mm double row")
    (fp_text reference J35 (at 1.143 6.985 90) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 5.655 7.35 90) (layer F.Fab))
    (fp_text user %R (at 5.31 2.54 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 VCC))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 VCC))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J35-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J35-Pad6)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprint:SOLDERJUMPER_REFLOW (layer F.Cu) (tedit 5B372343)
    (at 119.875 112.68)
    (fp_text reference JP105 (at -0.3175 2.0955) (layer F.SilkS))
    (fp_text value SOLDERJUMPER (at 0 1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.762 0) (size 1.1684 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (pad 2 smd rect (at 0.762 0) (size 1.1684 1.6002) (layers F.Cu F.Paste F.Mask)
      (net 39 A0))
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B370741)
    (at 138.29 118.395 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 220 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(J31-Pad5)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 45 PWM0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B37073D)
    (at 138.29 116.49)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.54 0) (layer F.SilkS))
    (fp_text value 220 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 46 PWM1))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J31-Pad6)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B37076E)
    (at 138.29 108.87 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.54 0 180) (layer F.SilkS))
    (fp_text value 220 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(J32-Pad5)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 47 PWM2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B37077F)
    (at 138.29 106.965)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at -2.54 0) (layer F.SilkS))
    (fp_text value 220 (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 48 PWM3))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(J32-Pad6)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B372301)
    (at 142.735 98.71 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 2.286 -0.127 270) (layer F.SilkS))
    (fp_text value 220 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(J33-Pad5)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 PWM4))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B3722FC)
    (at 140.83 98.71 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -2.2225 0.0635 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 50 PWM5))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(J33-Pad6)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B3707D8)
    (at 133.21 98.71 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 2.54 0 270) (layer F.SilkS))
    (fp_text value 220 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(J34-Pad5)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 51 PWM6))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B3707E4)
    (at 131.305 98.71 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 52 PWM7))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(J34-Pad6)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B372390)
    (at 123.685 98.71 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 -1.3335 270) (layer F.SilkS))
    (fp_text value 220 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(J35-Pad5)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 53 PWM8))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B372385)
    (at 121.78 98.71 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at -1.905 -1.0795 90) (layer F.SilkS))
    (fp_text value 220 (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 54 PWM9))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(J35-Pad6)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B370D09)
    (at 114.922 128.936 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R17 (at 0 1.524 270) (layer F.SilkS))
    (fp_text value 0 (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad30)"))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J20-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B372350)
    (at 117.97 109.505 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R21 (at -2.794 -0.0635 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 SCL))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B37234C)
    (at 119.24 109.505 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R22 (at -2.794 0 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 SDA))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58E0A804)
    (at 127.495 102.52)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R23 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R23-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B3723A5)
    (at 124.955 102.52 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R100 (at 0.0635 -1.2065 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 44 A5))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B3722EB)
    (at 128.13 113.315 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R101 (at 0.127 -1.397 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 43 A4))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B37092B)
    (at 127.0505 115.9185 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R102 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 42 A3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B37093D)
    (at 125.463 115.9185 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R103 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 41 A2))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B3722E6)
    (at 123.685 113.315 270)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R104 (at -0.3175 1.2065 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 40 A1))
    (pad 2 smd rect (at 0.75 0 270) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 5B370979)
    (at 123.685 115.855 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R105 (at -3.175 0 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0.75 0 90) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 39 A0))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprint:slide_switch_angled (layer F.Cu) (tedit 5B61DD77)
    (at 150 92)
    (descr "slide switch angled")
    (tags "slide switch angled")
    (fp_text reference SW1 (at -3.328 1.884 90) (layer F.SilkS))
    (fp_text value Sliede_SW_01 (at 2.5 9) (layer F.Fab))
    (pad GND thru_hole rect (at 0 6.5 90) (size 2.8 3.5) (drill oval 0.8 1.5) (layers *.Cu *.Mask))
    (pad 1 thru_hole rect (at 0 0) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad30)"))
    (pad 2 thru_hole oval (at 0 2) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(J20-Pad1)"))
    (pad 3 thru_hole oval (at 0 4) (size 1.35 1.35) (drill 0.8) (layers *.Cu *.Mask))
    (pad GND thru_hole rect (at 0 -2.5 90) (size 2.8 3.5) (drill oval 0.8 1.5) (layers *.Cu *.Mask))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x03_Pitch2.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprint:PCA9685_TSSOP28 (layer F.Cu) (tedit 593273C1)
    (at 126.86 107.6)
    (fp_text reference U1 (at -5.5 0 90) (layer F.Fab))
    (fp_text value PCA9685 (at 6 0 90) (layer F.Fab))
    (pad 1 smd rect (at -4.22402 2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 39 A0))
    (pad 2 smd rect (at -3.57378 2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 40 A1))
    (pad 3 smd rect (at -2.92354 2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 41 A2))
    (pad 4 smd rect (at -2.2733 2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 42 A3))
    (pad 5 smd rect (at -1.62306 2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 43 A4))
    (pad 6 smd rect (at -0.97282 2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 45 PWM0))
    (pad 7 smd rect (at -0.32258 2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 46 PWM1))
    (pad 8 smd rect (at 0.32258 2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 47 PWM2))
    (pad 9 smd rect (at 0.97282 2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 48 PWM3))
    (pad 10 smd rect (at 1.62306 2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 49 PWM4))
    (pad 11 smd rect (at 2.2733 2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 50 PWM5))
    (pad 12 smd rect (at 2.92354 2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 51 PWM6))
    (pad 13 smd rect (at 3.57378 2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 52 PWM7))
    (pad 14 smd rect (at 4.22402 2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 15 smd rect (at 4.22402 -2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 53 PWM8))
    (pad 16 smd rect (at 3.57378 -2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 54 PWM9))
    (pad 17 smd rect (at 2.92354 -2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask))
    (pad 18 smd rect (at 2.2733 -2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask))
    (pad 19 smd rect (at 1.62306 -2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask))
    (pad 20 smd rect (at 0.97282 -2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask))
    (pad 21 smd rect (at 0.32258 -2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask))
    (pad 22 smd rect (at -0.32258 -2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask))
    (pad 23 smd rect (at -0.97282 -2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(R23-Pad1)"))
    (pad 24 smd rect (at -1.62306 -2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 44 A5))
    (pad 25 smd rect (at -2.2733 -2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 26 smd rect (at -2.92354 -2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 22 SCL))
    (pad 27 smd rect (at -3.57378 -2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 21 SDA))
    (pad 28 smd rect (at -4.22402 -2.91592) (size 0.3048 0.9906) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
  )
  (module footprint:Pin_Header_MBUS_SMD_TH (layer F.Cu) (tedit 5B58717A)
    (at 110 108)
    (descr "surface-mounted straight pin header, 2x15, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x15 2.54mm double row")
    (attr smd)
    (fp_text reference J1 (at -7.9 0.2 270) (layer F.SilkS))
    (fp_text value M-BUS (at 0 20.11) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 13.97) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 16.51) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -13.97) (size 0.8 0.8) (drill 0.8) (layers *.Cu *.Mask))
    (pad 1 smd rect (at -2.525 -17.78) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.525 -17.78) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at -2.525 -5.08) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J1-Pad11)"))
    (pad 9 smd rect (at -2.525 -7.62) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J1-Pad9)"))
    (pad 7 smd rect (at -2.525 -10.16) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(J1-Pad7)"))
    (pad 5 smd rect (at -2.525 -12.7) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.525 -15.24) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 thru_hole circle (at -3.175 -17.78) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.525 -17.78) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 4 smd rect (at 2.525 -15.24) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 6 smd rect (at 2.525 -12.7) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(J1-Pad6)"))
    (pad 8 smd rect (at 2.525 -10.16) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 10 smd rect (at 2.525 -7.62) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 12 smd rect (at 2.525 -5.08) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 19 VDD))
    (pad 13 smd rect (at -2.525 -2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(J1-Pad13)"))
    (pad 14 smd rect (at 2.525 -2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(J1-Pad14)"))
    (pad 15 smd rect (at -2.525 0) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J1-Pad15)"))
    (pad 16 smd rect (at 2.525 0) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J1-Pad16)"))
    (pad 17 smd rect (at -2.525 2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 21 SDA))
    (pad 18 smd rect (at 2.525 2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 22 SCL))
    (pad 19 smd rect (at -2.525 5.08) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(J1-Pad19)"))
    (pad 20 smd rect (at 2.525 5.08) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad20)"))
    (pad 21 smd rect (at -2.525 7.62) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J1-Pad21)"))
    (pad 22 smd rect (at 2.525 7.62) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(J1-Pad22)"))
    (pad 23 smd rect (at -2.525 10.16) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J1-Pad23)"))
    (pad 24 smd rect (at 2.525 10.16) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(J1-Pad24)"))
    (pad 25 smd rect (at -2.525 12.7) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad25)"))
    (pad 26 smd rect (at 2.525 12.7) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad26)"))
    (pad 27 smd rect (at -2.525 15.24) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad25)"))
    (pad 28 smd rect (at 2.525 15.24) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 2 /+5V))
    (pad 29 smd rect (at -2.525 17.78) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(J1-Pad25)"))
    (pad 30 smd rect (at 2.525 17.78) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J1-Pad30)"))
    (pad 2 smd rect (at 2.555 -17.78) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 smd rect (at -2.525 -15.24) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 2.555 -15.24) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 smd rect (at -2.525 -12.7) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 6 smd rect (at 2.555 -12.7) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(J1-Pad6)"))
    (pad 7 smd rect (at -2.525 -10.16) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(J1-Pad7)"))
    (pad 8 smd rect (at 2.555 -10.16) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 9 smd rect (at -2.525 -7.62) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(J1-Pad9)"))
    (pad 10 smd rect (at 2.555 -7.62) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 11 smd rect (at -2.525 -5.08) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(J1-Pad11)"))
    (pad 12 smd rect (at 2.555 -5.08) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 19 VDD))
    (pad 13 smd rect (at -2.525 -2.54) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(J1-Pad13)"))
    (pad 14 smd rect (at 2.555 -2.54) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(J1-Pad14)"))
    (pad 15 smd rect (at -2.525 0) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(J1-Pad15)"))
    (pad 16 smd rect (at 2.555 0) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(J1-Pad16)"))
    (pad 17 smd rect (at -2.525 2.54) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 21 SDA))
    (pad 18 smd rect (at 2.555 2.54) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 22 SCL))
    (pad 19 smd rect (at -2.525 5.08) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(J1-Pad19)"))
    (pad 20 smd rect (at 2.555 5.08) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(J1-Pad20)"))
    (pad 21 smd rect (at -2.525 7.62) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(J1-Pad21)"))
    (pad 22 smd rect (at 2.555 7.62) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(J1-Pad22)"))
    (pad 23 smd rect (at -2.525 10.16) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(J1-Pad23)"))
    (pad 24 smd rect (at 2.555 10.16) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(J1-Pad24)"))
    (pad 25 smd rect (at -2.525 12.7) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad25)"))
    (pad 26 smd rect (at 2.555 12.7) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(J1-Pad26)"))
    (pad 27 smd rect (at -2.525 15.24) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad25)"))
    (pad 28 smd rect (at 2.555 15.24) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 2 /+5V))
    (pad 29 smd rect (at -2.525 17.78) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(J1-Pad25)"))
    (pad 30 smd rect (at 2.555 17.78) (size 3.15 1) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(J1-Pad30)"))
    (pad 3 thru_hole circle (at -3.175 -15.24) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole circle (at -3.175 -12.7) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -3.175 -10.16) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad7)"))
    (pad 9 thru_hole circle (at -3.175 -7.62) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad9)"))
    (pad 11 thru_hole circle (at -3.175 -5.08) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad11)"))
    (pad 13 thru_hole circle (at -3.175 -2.54) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad13)"))
    (pad 15 thru_hole circle (at -3.175 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad15)"))
    (pad 17 thru_hole circle (at -3.175 2.54) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 21 SDA))
    (pad 19 thru_hole circle (at -3.175 5.08) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad19)"))
    (pad 21 thru_hole circle (at -3.175 7.62) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad21)"))
    (pad 23 thru_hole circle (at -3.175 10.16) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad23)"))
    (pad 25 thru_hole circle (at -3.175 12.7) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad25)"))
    (pad 27 thru_hole circle (at -3.175 15.24) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad25)"))
    (pad 29 thru_hole circle (at -3.175 17.78) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad25)"))
    (pad 2 thru_hole circle (at 3.175 -17.78) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 4 thru_hole circle (at 3.175 -15.24) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 6 thru_hole circle (at 3.175 -12.7) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad6)"))
    (pad 8 thru_hole circle (at 3.175 -10.16) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 10 thru_hole circle (at 3.175 -7.62) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 12 thru_hole circle (at 3.175 -5.08) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 19 VDD))
    (pad 14 thru_hole circle (at 3.175 -2.54) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad14)"))
    (pad 16 thru_hole circle (at 3.175 0) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)"))
    (pad 18 thru_hole circle (at 3.175 2.54) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 22 SCL))
    (pad 20 thru_hole circle (at 3.175 5.08) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad20)"))
    (pad 22 thru_hole circle (at 3.175 7.62) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad22)"))
    (pad 24 thru_hole circle (at 3.175 10.16) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad24)"))
    (pad 26 thru_hole circle (at 3.175 12.7) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad26)"))
    (pad 28 thru_hole circle (at 3.175 15.24) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 2 /+5V))
    (pad 30 thru_hole circle (at 3.175 17.78) (size 0.8 0.8) (drill 0.4) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad30)"))
    (pad "" np_thru_hole circle (at 0 -16.51) (size 1 1) (drill 1) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -1.27 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole circle (at 1.27 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -1.27 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at 1.27 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -1.27 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 6 thru_hole circle (at 1.27 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -1.27 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at 1.27 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -1.27 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at 1.27 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at -1.27 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad11)"))
    (pad 12 thru_hole circle (at 1.27 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 VDD))
    (pad 13 thru_hole circle (at -1.27 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad13)"))
    (pad 14 thru_hole circle (at 1.27 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad14)"))
    (pad 15 thru_hole circle (at -1.27 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "Net-(J1-Pad15)"))
    (pad 16 thru_hole circle (at 1.27 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad16)"))
    (pad 17 thru_hole circle (at -1.27 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 SDA))
    (pad 18 thru_hole circle (at 1.27 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 SCL))
    (pad 19 thru_hole circle (at -1.27 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(J1-Pad19)"))
    (pad 20 thru_hole circle (at 1.27 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad20)"))
    (pad 21 thru_hole circle (at -1.27 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad21)"))
    (pad 22 thru_hole circle (at 1.27 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad22)"))
    (pad 23 thru_hole circle (at -1.27 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad23)"))
    (pad 24 thru_hole circle (at 1.27 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad24)"))
    (pad 25 thru_hole circle (at -1.27 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad25)"))
    (pad 26 thru_hole circle (at 1.27 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad26)"))
    (pad 27 thru_hole circle (at -1.27 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad25)"))
    (pad 28 thru_hole circle (at 1.27 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /+5V))
    (pad 29 thru_hole circle (at -1.27 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad25)"))
    (pad 30 thru_hole circle (at 1.27 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad30)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x15_Pitch2.54mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 116.954 86.518 90) (layer F.SilkS))
  (gr_text GND (at 126.352 84.74 90) (layer F.SilkS))
  (gr_text GND (at 135.75 84.486 90) (layer F.SilkS))
  (gr_text GND (at 151.244 102.012) (layer F.SilkS))
  (gr_text GND (at 151.244 111.41) (layer F.SilkS))
  (gr_line (start 143.7 133) (end 114.3 133) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154 125.7) (end 154 116.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144 132.7) (end 143.7 133) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151 132.7) (end 144 132.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.7 126) (end 154 125.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.7 130) (end 153.7 126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154 90.3) (end 154 99.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.7 90) (end 154 90.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.7 86) (end 153.7 90) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.7 83) (end 117 83) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144 83.3) (end 143.7 83) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151 83.3) (end 144 83.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 151 86) (end 151 83.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 151 130) (end 153.7 130) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104 125.7) (end 104 90.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 114 132.7) (end 114.3 133) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107 132.7) (end 114 132.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.3 126) (end 104 125.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.3 130) (end 104.3 126) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 107 130) (end 107 132.7) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.3 90) (end 104 90.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 104.3 86) (end 104.3 90) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.3 83.3) (end 112.5 83.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 107 83.3) (end 112.3 83.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 107 86) (end 104.3 86) (angle 90) (layer Edge.Cuts) (width 0.15))
  (target plus (at 104 133) (size 5) (width 0.15) (layer Edge.Cuts))
  (gr_text ON (at 153.022 90.074 90) (layer F.SilkS))
  (gr_text "SHORT=Int\nOpen=Ext" (at 143.624 128.936 90) (layer F.SilkS))
  (gr_text GND (at 120.51 119.03 270) (layer F.SilkS))
  (gr_text BAT (at 117.97 118.903 270) (layer F.SilkS))
  (gr_text Vcc (at 152.26 126.65) (layer F.SilkS))
  (gr_text GND (at 152.26 119.792) (layer F.SilkS))
  (gr_line (start 153 115.5) (end 154 116.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153 100.5) (end 153 115.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 154 99.5) (end 153 100.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_text hardware (at 142.608 89.1596) (layer B.SilkS))
  (gr_text "open source" (at 142.4556 88.6008) (layer B.SilkS))
  (gr_text "v 1.0" (at 121.78 86.3275) (layer B.SilkS))
  (gr_text M-BUS (at 116.6365 102.2025 270) (layer F.SilkS))
  (gr_text "SERVO DRIVER for M5Stack" (at 132.1305 84.4225) (layer B.SilkS))
  (dimension 3 (width 0.2) (layer Eco1.User)
    (gr_text 3mm (at 94 132 90) (layer Eco1.User))
    (feature1 (pts (xy 107 130) (xy 95.3 130)))
    (feature2 (pts (xy 107 133) (xy 95.3 133)))
    (crossbar (pts (xy 98 133) (xy 98 130)))
    (arrow1a (pts (xy 98 130) (xy 98.586421 131.126504)))
    (arrow1b (pts (xy 98 130) (xy 97.413579 131.126504)))
    (arrow2a (pts (xy 98 133) (xy 98.586421 131.873496)))
    (arrow2b (pts (xy 98 133) (xy 97.413579 131.873496)))
  )
  (dimension 4 (width 0.2) (layer Eco1.User)
    (gr_text 4mm (at 113 136) (layer Eco1.User))
    (feature1 (pts (xy 111 130) (xy 111 138.7)))
    (feature2 (pts (xy 107 130) (xy 107 138.7)))
    (crossbar (pts (xy 107 136) (xy 111 136)))
    (arrow1a (pts (xy 111 136) (xy 109.873496 136.586421)))
    (arrow1b (pts (xy 111 136) (xy 109.873496 135.413579)))
    (arrow2a (pts (xy 107 136) (xy 108.126504 136.586421)))
    (arrow2b (pts (xy 107 136) (xy 108.126504 135.413579)))
  )
  (dimension 3 (width 0.2) (layer Eco1.User)
    (gr_text 3mm (at 102 136) (layer Eco1.User))
    (feature1 (pts (xy 107 130) (xy 107 138.7)))
    (feature2 (pts (xy 104 130) (xy 104 138.7)))
    (crossbar (pts (xy 104 136) (xy 107 136)))
    (arrow1a (pts (xy 107 136) (xy 105.873496 136.586421)))
    (arrow1b (pts (xy 107 136) (xy 105.873496 135.413579)))
    (arrow2a (pts (xy 104 136) (xy 105.126504 136.586421)))
    (arrow2b (pts (xy 104 136) (xy 105.126504 135.413579)))
  )
  (gr_text BAT (at 115.176 125.888 270) (layer F.SilkS))
  (gr_text 5V (at 115.176 123.348 270) (layer F.SilkS))
  (gr_text 34 (at 115.176 120.808 270) (layer F.SilkS))
  (gr_text 0 (at 115.176 118.268 270) (layer F.SilkS))
  (gr_text 13 (at 115.176 115.728 270) (layer F.SilkS))
  (gr_text 5 (at 115.176 113.188 270) (layer F.SilkS))
  (gr_text 22 (at 115.176 110.648 270) (layer F.SilkS))
  (gr_text 17 (at 115.176 108.108 270) (layer F.SilkS))
  (gr_text 1 (at 115.176 105.568 270) (layer F.SilkS))
  (gr_text 3V3 (at 115.176 103.028 270) (layer F.SilkS))
  (gr_text 26 (at 115.176 100.488 270) (layer F.SilkS))
  (gr_text 25 (at 115.176 97.948 270) (layer F.SilkS))
  (gr_text EN (at 115.176 95.408 270) (layer F.SilkS))
  (gr_text 36 (at 115.176 92.868 270) (layer F.SilkS))
  (gr_text 35 (at 115.176 90.328 270) (layer F.SilkS))
  (gr_text HPWR (at 105.016 123.348 90) (layer F.SilkS))
  (gr_text 15 (at 105.016 118.268 90) (layer F.SilkS))
  (gr_text 12 (at 105.016 115.728 90) (layer F.SilkS))
  (gr_text 2 (at 105.016 113.188 90) (layer F.SilkS))
  (gr_text 21 (at 105.016 110.648 90) (layer F.SilkS))
  (gr_text 16 (at 105.016 108.108 90) (layer F.SilkS))
  (gr_text 3 (at 105.016 105.568 90) (layer F.SilkS))
  (gr_text 18 (at 105.016 103.028 90) (layer F.SilkS))
  (gr_text 19 (at 105.016 100.488 90) (layer F.SilkS))
  (gr_text 23 (at 105.016 97.948 90) (layer F.SilkS))
  (gr_text GND (at 105.016 92.868 90) (layer F.SilkS))
  (gr_line (start 116 85.5) (end 116.5 85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.5 85) (end 113 85.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.5 85) (end 116.5 83.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 113 85.5) (end 116 85.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 112.5 83.5) (end 112.5 85) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.5 83.5) (end 117 83) (angle 90) (layer Edge.Cuts) (width 0.15))
  (dimension 50 (width 0.3) (layer Eco1.User)
    (gr_text "50.000 mm" (at 164.35 108 90) (layer Eco1.User))
    (feature1 (pts (xy 152 83) (xy 165.7 83)))
    (feature2 (pts (xy 152 133) (xy 165.7 133)))
    (crossbar (pts (xy 163 133) (xy 163 83)))
    (arrow1a (pts (xy 163 83) (xy 163.586421 84.126504)))
    (arrow1b (pts (xy 163 83) (xy 162.413579 84.126504)))
    (arrow2a (pts (xy 163 133) (xy 163.586421 131.873496)))
    (arrow2b (pts (xy 163 133) (xy 162.413579 131.873496)))
  )
  (dimension 50 (width 0.3) (layer Eco1.User)
    (gr_text "50.000 mm" (at 129 142.35) (layer Eco1.User))
    (feature1 (pts (xy 154 131) (xy 154 143.7)))
    (feature2 (pts (xy 104 131) (xy 104 143.7)))
    (crossbar (pts (xy 104 141) (xy 154 141)))
    (arrow1a (pts (xy 154 141) (xy 152.873496 141.586421)))
    (arrow1b (pts (xy 154 141) (xy 152.873496 140.413579)))
    (arrow2a (pts (xy 104 141) (xy 105.126504 141.586421)))
    (arrow2b (pts (xy 104 141) (xy 105.126504 140.413579)))
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154 133) (xy 104 133) (xy 104 83) (xy 154 83)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 154 133) (xy 104 133) (xy 104 83) (xy 154 83)
      )
    )
  )
)
