(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" mixed)
    (31 "B.Cu" mixed)
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "VCC")
  (net 2 "GND")
  (net 3 "Net-(D1-Pad2)")
  (net 4 "D4")
  (net 5 "D3")
  (net 6 "D13{slash}SCK")
  (net 7 "D12{slash}MISO")
  (net 8 "D2{slash}INT0")
  (net 9 "A5{slash}SCL")
  (net 10 "D5")
  (net 11 "D7")
  (net 12 "D9")
  (net 13 "D10{slash}SS")
  (net 14 "D11{slash}MOSI")
  (net 15 "D6")
  (footprint "MyGlobalLibrary:2X4_nRF24L01" (layer "F.Cu")
    (tedit 0)
    (at 153.9 80.6 180)
    (property "Sheetfile" "nRF24L01_shield_v001.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -5.08 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "2x4_nRF24L01" (at 0 -3.81 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.81 1.27 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "bidirectional"))
    (pad "2" thru_hole circle (at -1.27 1.27 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 12 "D9") (pinfunction "CE") (pintype "bidirectional"))
    (pad "3" thru_hole circle (at 1.27 1.27 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 6 "D13{slash}SCK") (pinfunction "SCK") (pintype "bidirectional"))
    (pad "4" thru_hole circle (at 3.81 1.27 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 "D12{slash}MISO") (pinfunction "MISO") (pintype "bidirectional"))
    (pad "5" thru_hole circle (at 3.81 -1.27 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 8 "D2{slash}INT0") (pinfunction "IRQ") (pintype "bidirectional"))
    (pad "6" thru_hole circle (at 1.27 -1.27 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 14 "D11{slash}MOSI") (pinfunction "MOSI") (pintype "bidirectional"))
    (pad "7" thru_hole circle (at -1.27 -1.27 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 13 "D10{slash}SS") (pinfunction "CSN") (pintype "bidirectional"))
    (pad "8" thru_hole circle (at -3.81 -1.27 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 1 "VCC") (pinfunction "VCC") (pintype "bidirectional"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 160.1 80.6 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "nRF24L01_shield_v001.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "0.1uF" (at 3.3 0.2 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 162.2 80.6 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "nRF24L01_shield_v001.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 3.35 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MyGlobalLibrary:nRF24L01_smd" (layer "F.Cu")
    (tedit 0)
    (at 153.9 86.6 180)
    (property "Sheetfile" "nRF24L01_shield_v001.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 -5.08 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "nRF24L01_smd_1" (at 0 -3.175 180 unlocked) (layer "F.Fab") hide)
    (fp_text user "Antenna" (at 0 -20.32 180 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 2.54 180 unlocked) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -4.445 0 180) (size 0.9 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "VCC") (pinfunction "3.3V") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -3.175 0 180) (size 0.9 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -1.905 0 180) (size 0.9 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "D9") (pinfunction "CE") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -0.635 0 180) (size 0.9 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "D10{slash}SS") (pinfunction "CSN") (pintype "bidirectional"))
    (pad "5" smd roundrect (at 0.635 0 180) (size 0.9 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "D13{slash}SCK") (pinfunction "SCK") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 1.905 0 180) (size 0.9 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "D11{slash}MOSI") (pinfunction "MOSI") (pintype "bidirectional"))
    (pad "7" smd roundrect (at 3.175 0 180) (size 0.9 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "D12{slash}MISO") (pinfunction "MISO") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 4.445 0 180) (size 0.9 3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "D2{slash}INT0") (pinfunction "IRQ") (pintype "bidirectional"))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 139.7 78.3)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (property "Sheetfile" "nRF24L01_shield_v001.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x07_Male" (at 0 17.57) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 7.62 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "D4") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "D3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "D13{slash}SCK") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "D12{slash}MISO") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "D2{slash}INT0") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "A5{slash}SCL") (pinfunction "Pin_7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x07_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 167.64 78.6)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (property "Sheetfile" "nRF24L01_shield_v001.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x07_Male" (at 0 17.57) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 7.62 90) (layer "F.Fab") hide)
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "D5") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "D7") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "D9") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "D10{slash}SS") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "D11{slash}MOSI") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "D6") (pinfunction "Pin_7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x07_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 164.840196 94.381022 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (property "Sheetfile" "nRF24L01_shield_v001.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "330R" (at -2.325 0 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 15 "D6") (pintype "passive"))
    (pad "2" smd roundrect (at 1 0 90) (size 1.2 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2083333333)
      (net 3 "Net-(D1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 162.300196 94.381022 90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "Sheetfile" "nRF24L01_shield_v001.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "LED" (at -2.315 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 3 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 137.35 75.77) (end 170 97.6) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "D7 ()" (at 166.624 83.82) (layer "B.SilkS"))
  (gr_text "VCC (VCC)" (at 140.716 78.486) (layer "B.SilkS"))
  (gr_text "GND (GND)" (at 166.624 78.74) (layer "B.SilkS"))
  (gr_text "D10/SS (NSS)" (at 166.624 88.9) (layer "B.SilkS"))
  (gr_text "A5/SCL ()" (at 140.716 93.726) (layer "B.SilkS"))
  (gr_text "D12/MISO (MISO)" (at 140.716 88.646) (layer "B.SilkS"))
  (gr_text "D3 ()" (at 140.716 83.566) (layer "B.SilkS"))
  (gr_text "nRF24L01\nVersion 001a\n" (at 153.9 92.5) (layer "B.SilkS"))
  (gr_text "D6 (LED1)" (at 166.624 93.98) (layer "B.SilkS"))
  (gr_text "D4 (SW)" (at 140.716 81.026) (layer "B.SilkS"))
  (gr_text "D13/SCK (SCK)\n" (at 140.716 86.106) (layer "B.SilkS"))
  (gr_text "D9 (NRESET)" (at 166.624 86.36) (layer "B.SilkS"))
  (gr_text "D2/INT0 ()" (at 140.716 91.186) (layer "B.SilkS"))
  (gr_text "D11/MOSI (MOSI)" (at 166.624 91.44) (layer "B.SilkS"))
  (gr_text "D5 ()" (at 166.624 81.28) (layer "B.SilkS"))
  (gr_text "-" (at 160.936196 95.385152) (layer "F.SilkS"))
  (gr_text "D3" (at 141.224 83.566) (layer "F.SilkS"))
  (gr_text "D7" (at 166.116 83.566) (layer "F.SilkS"))
  (gr_text "D5" (at 166.116 81.026) (layer "F.SilkS"))
  (gr_text "CSN" (at 154.55 88.4 90) (layer "F.SilkS"))
  (gr_text "D11/MOSI" (at 166.116 91.186) (layer "F.SilkS"))
  (gr_text "VCC" (at 141.224 78.486) (layer "F.SilkS"))
  (gr_text "D9" (at 166.116 86.106) (layer "F.SilkS"))
  (gr_text "IRQ" (at 149.45 88.4 90) (layer "F.SilkS"))
  (gr_text "CE" (at 155.825 88.4 90) (layer "F.SilkS"))
  (gr_text "D13/SCK\n" (at 141.224 85.852) (layer "F.SilkS"))
  (gr_text "A5/SCL" (at 141.224 93.726) (layer "F.SilkS"))
  (gr_text "D2/INT0" (at 141.224 91.186) (layer "F.SilkS"))
  (gr_text "SCK" (at 153.275 88.4 90) (layer "F.SilkS"))
  (gr_text "nRF24L01\nVersion 001a\n" (at 153.924 94.488) (layer "F.SilkS"))
  (gr_text "D4" (at 141.224 81.026) (layer "F.SilkS"))
  (gr_text "D12/MISO" (at 141.224 88.646) (layer "F.SilkS"))
  (gr_text "GND" (at 166.116 78.486) (layer "F.SilkS"))
  (gr_text "VCC" (at 158.375 88.4 90) (layer "F.SilkS"))
  (gr_text "MISO" (at 150.725 88.4 90) (layer "F.SilkS"))
  (gr_text "GND" (at 157.1 88.4 90) (layer "F.SilkS"))
  (gr_text "D10/SS" (at 166.116 88.646) (layer "F.SilkS"))
  (gr_text "MOSI" (at 152 88.4 90) (layer "F.SilkS"))
  (gr_text "+" (at 160.936196 93.293143) (layer "F.SilkS"))
  (zone (net 1) (net_name "VCC") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.5))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.116 88.105869)
        (xy 155.956 88.105869)
        (xy 155.956 82.296)
        (xy 137.668 82.296)
        (xy 137.668 76.2)
        (xy 166.116 76.2)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.4))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 170.18 97.536)
        (xy 137.16 97.536)
        (xy 137.16 75.692)
        (xy 170.18 75.692)
      )
    )
  )
)
