(footprint "pro_mini_rfmshield" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 62D16557)
  (descr "IC, ARDUINO_PRO_MINI x 0,6\"")
  (tags "DIL ARDUINO PRO MINI")
  (attr through_hole)
  (fp_text reference "REF**" (at 10.16 13.97 90) (layer "F.SilkS"))
  (fp_text value "ArduinoProMini" (at 0 0 90) (layer "F.Fab") hide)
  (fp_text user "Pro Mini 3v3" (at 0 -7.62 unlocked) (layer "F.SilkS"))
  (fp_text user "Headers" (at 0 15.24 unlocked) (layer "F.SilkS"))
  (pad "1" thru_hole circle (at 7.62 13.97 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "2" thru_hole circle (at 7.62 11.43 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "3" thru_hole circle (at 7.62 8.89 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "18" thru_hole circle (at -7.62 -1.27 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "19" thru_hole circle (at -7.62 1.27 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "20" thru_hole circle (at -7.62 3.81 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "22" thru_hole circle (at -7.62 8.89 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "DI00" thru_hole circle (at 7.62 3.81 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "GND1" thru_hole circle (at 7.62 6.35 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "GND2" thru_hole circle (at -7.62 11.43 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "MISO" thru_hole circle (at -7.62 -8.89 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "MOSI" thru_hole circle (at -7.62 -11.43 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "NSS" thru_hole circle (at -7.62 -13.97 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "RAW" thru_hole circle (at -7.62 13.97 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "SCK" thru_hole circle (at -7.62 -6.35 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "SCL" thru_hole circle (at -5.08 5.08 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "SDA" thru_hole circle (at -5.08 2.54 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "VCC" thru_hole circle (at -7.62 6.35 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (pad "VolDiv" thru_hole circle (at -7.62 -3.81 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS"))
  (model "Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl"
    (offset (xyz -3.809999943 5.079999924 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl"
    (offset (xyz 13.96999979 2.539999962 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
  (model "Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl"
    (offset (xyz 0 7.619999886 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl"
    (offset (xyz 0 -7.619999886 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl"
    (offset (xyz 6.349999905 5.079999924 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "${MYSLOCAL}/mysensors.3dshapes/mysensors_arduino.3dshapes/arduino_pro_mini.wrl"
    (offset (xyz -1.269999981 0 12.19199982))
    (scale (xyz 0.395 0.395 0.395))
    (rotate (xyz 0 0 180))
  )
  (model "SMD_Packages.3dshapes/TQFP-32.wrl"
    (offset (xyz 1.269999981 0 13.0174998))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 315))
  )
  (model "Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl"
    (offset (xyz 13.96999979 -7.619999886 11.30299983))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 180 90))
  )
  (model "Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl"
    (offset (xyz 13.96999979 7.619999886 11.30299983))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 180 90))
  )
  (model "Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl"
    (offset (xyz 13.96999979 5.079999924 11.30299983))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 180 0))
  )
  (model "Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl"
    (offset (xyz 7.619999886 5.079999924 11.30299983))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 180 90))
  )
  (model "Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl"
    (offset (xyz -2.539999962 5.079999924 11.30299983))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 180 90))
  )
  (model "${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl"
    (offset (xyz -7.619999886 0 13.0174998))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl"
    (offset (xyz 13.96999979 -4.444999933 13.0174998))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "Pin_Headers.3dshapes/Pin_Header_Angled_1x06_Pitch2.54mm.wrl"
    (offset (xyz -16.50999975 -6.349999905 13.0174998))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 180))
  )
  (model "Resistors_SMD.3dshapes/R_0603.wrl"
    (offset (xyz -7.619999886 -1.269999981 13.0174998))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "Resistors_SMD.3dshapes/R_0603.wrl"
    (offset (xyz 13.96999979 -3.174999952 13.0174998))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "Capacitors_SMD.3dshapes/C_0603.wrl"
    (offset (xyz -7.619999886 1.269999981 13.0174998))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-S_EIA-3216-12.wrl"
    (offset (xyz -8.889999866 3.809999943 13.0174998))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-S_EIA-3216-12.wrl"
    (offset (xyz -8.889999866 -3.809999943 13.0174998))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl"
    (offset (xyz -10.15999985 0 13.0174998))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
  (model "Capacitors_SMD.3dshapes/C_1210.wrl"
    (offset (xyz -12.69999981 0 13.0174998))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
  (model "${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/switch/smd_push.wrl"
    (offset (xyz 10.15999985 0 13.0174998))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
