(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (date "sam. 04 avril 2015")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (color "Green") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (color "Green") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (aux_axis_origin 137.16 114.3)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/")
    )
  )
  (net 0 "")
  (net 1 "Net-(Booster1-Pad1)")
  (net 2 "GND")
  (net 3 "Net-(C1-Pad1)")
  (net 4 "+3V3")
  (net 5 "unconnected-(RFM69HW1-Pad1)")
  (net 6 "unconnected-(RFM69HW1-Pad3)")
  (net 7 "unconnected-(RFM69HW1-Pad4)")
  (net 8 "unconnected-(RFM69HW1-Pad5)")
  (net 9 "unconnected-(RFM69HW1-Pad6)")
  (net 10 "unconnected-(RFM69HW1-Pad7)")
  (net 11 "unconnected-(RFM69HW1-Pad10)")
  (net 12 "unconnected-(RFM69HW1-Pad16)")
  (net 13 "unconnected-(ProMini1-Pad18)")
  (net 14 "unconnected-(ProMini1-Pad19)")
  (net 15 "unconnected-(ProMini1-Pad20)")
  (net 16 "unconnected-(ProMini1-Pad22)")
  (net 17 "Net-(ProMini1-PadDI00)")
  (net 18 "unconnected-(ProMini1-PadRAW)")
  (net 19 "Net-(ProMini1-PadMISO)")
  (net 20 "Net-(ProMini1-PadMOSI)")
  (net 21 "Net-(ProMini1-PadNSS)")
  (net 22 "Net-(ProMini1-PadSCK)")
  (net 23 "Net-(HDC1080-Pad3)")
  (net 24 "Net-(HDC1080-Pad4)")
  (net 25 "Net-(ExtraGND1-Pad1)")
  (net 26 "unconnected-(ProMini1-Pad1)")
  (net 27 "unconnected-(ProMini1-Pad2)")
  (net 28 "unconnected-(ProMini1-Pad3)")
  (footprint "RF_Module:HOPERF_RFM69HW" (layer "F.Cu")
    (tedit 5A030172)
    (at 104.775 66.04 90)
    (descr "Radio, RF, Module, http://www.hoperf.com/upload/rf/RFM69HW-V1.3.pdf")
    (tags "Radio RF Module")
    (property "Sheetfile" "shield.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RFM69HW1" (at 0 -0.127 90) (layer "F.SilkS") hide)
    (fp_text value "RFM69HW" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -9.1 -7 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "unconnected-(RFM69HW1-Pad1)") (pinfunction "RESET") (pintype "input"))
    (pad "2" smd rect (at -9.1 -5 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(ProMini1-PadDI00)") (pinfunction "DIO0") (pintype "bidirectional"))
    (pad "3" smd rect (at -9.1 -3 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "unconnected-(RFM69HW1-Pad3)") (pinfunction "DIO1") (pintype "bidirectional"))
    (pad "4" smd rect (at -9.1 -1 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "unconnected-(RFM69HW1-Pad4)") (pinfunction "DIO2") (pintype "bidirectional"))
    (pad "5" smd rect (at -9.1 1 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "unconnected-(RFM69HW1-Pad5)") (pinfunction "DIO3") (pintype "bidirectional"))
    (pad "6" smd rect (at -9.1 3 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "unconnected-(RFM69HW1-Pad6)") (pinfunction "DIO4") (pintype "bidirectional"))
    (pad "7" smd rect (at -9.1 5 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "unconnected-(RFM69HW1-Pad7)") (pinfunction "DIO5") (pintype "bidirectional"))
    (pad "8" smd rect (at -9.1 7 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "Net-(Booster1-Pad1)") (pinfunction "3.3V") (pintype "power_in"))
    (pad "9" smd rect (at 9.1 7 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "10" smd rect (at 9.1 5 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "unconnected-(RFM69HW1-Pad10)") (pinfunction "ANA") (pintype "output"))
    (pad "11" smd rect (at 9.1 3 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "12" smd rect (at 9.1 1 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(ProMini1-PadSCK)") (pinfunction "SCK") (pintype "input"))
    (pad "13" smd rect (at 9.1 -1 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(ProMini1-PadMISO)") (pinfunction "MISO") (pintype "output"))
    (pad "14" smd rect (at 9.1 -3 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(ProMini1-PadMOSI)") (pinfunction "MOSI") (pintype "input"))
    (pad "15" smd rect (at 9.1 -5 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(ProMini1-PadNSS)") (pinfunction "NSS") (pintype "input"))
    (pad "16" smd rect (at 9.1 -7 90) (size 2.5 1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "unconnected-(RFM69HW1-Pad16)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/RF_Module.3dshapes/HOPERF_RFM69HW.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 109.922 98.891 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Sheetfile" "shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at 4.572 -2.54 90) (layer "F.SilkS"))
    (fp_text value "C Booster" (at 1.758 3.892 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 4.573754 -2.553832 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(Booster1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 62D150FC)
    (at 103.318 97.89)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Booster1" (at -2.032 2.525 90) (layer "F.SilkS") hide)
    (fp_text value "Booster Pins" (at 0 6.14) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.508 3.033 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(Booster1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "+3V3") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 97.73 98.891)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at -3.048 1.27 90) (layer "F.SilkS") hide)
    (fp_text value "Battery" (at 0 4.87) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 94.488 111.098)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 5.08 0) (layer "F.SilkS"))
    (fp_text value "R1" (at 5.08 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "+3V3") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 105.156 83.82)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Extra3v3" (at 2.032 2.54 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Female" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(Booster1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(Booster1-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(Booster1-Pad1)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 109.22 52.832 -90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "HDC1080" (at 0 -2.33 -90) (layer "F.SilkS"))
    (fp_text value "HDC1080" (at 0 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(Booster1-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "Net-(HDC1080-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(HDC1080-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 94.488 108.05)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 5.08 0) (layer "F.SilkS"))
    (fp_text value "R2" (at 5.08 0) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.112 -2.779) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 109.728 110.59 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Sheetfile" "shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at -1.524 -3.556 90) (layer "F.SilkS"))
    (fp_text value "C Voltage Divider" (at 1.25 4.4 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:pro_mini_rfmshield" (layer "F.Cu")
    (tedit 66F27A26)
    (at 102.87 75.565)
    (descr "IC, ARDUINO_PRO_MINI x 0,6\"")
    (tags "DIL ARDUINO PRO MINI")
    (property "Sheetfile" "shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "ProMini1" (at 11.938 13.97 90) (layer "F.SilkS"))
    (fp_text value "rfmshield_pro_mini_pins" (at 0 0 90) (layer "F.Fab") hide)
    (fp_text user "Pro Mini 3v3" (at 1.27 3.175 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 7.62 13.97 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 26 "unconnected-(ProMini1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 7.62 11.43 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 27 "unconnected-(ProMini1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 7.62 8.89 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 28 "unconnected-(ProMini1-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "18" thru_hole circle (at -7.62 -1.27 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 13 "unconnected-(ProMini1-Pad18)") (pinfunction "18") (pintype "passive"))
    (pad "19" thru_hole circle (at -7.62 1.27 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 14 "unconnected-(ProMini1-Pad19)") (pinfunction "19") (pintype "passive"))
    (pad "20" thru_hole circle (at -7.62 3.81 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 15 "unconnected-(ProMini1-Pad20)") (pinfunction "20") (pintype "passive"))
    (pad "22" thru_hole circle (at -7.62 8.89 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 16 "unconnected-(ProMini1-Pad22)") (pinfunction "22") (pintype "passive"))
    (pad "DI00" thru_hole circle (at 7.62 3.81 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 17 "Net-(ProMini1-PadDI00)") (pinfunction "DI00") (pintype "passive"))
    (pad "GND1" thru_hole circle (at 7.62 6.35 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 2 "GND") (pinfunction "GND1") (pintype "passive"))
    (pad "GND2" thru_hole circle (at -7.62 11.43 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 25 "Net-(ExtraGND1-Pad1)") (pinfunction "GND2") (pintype "passive"))
    (pad "MISO" thru_hole circle (at -7.62 -8.89 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 19 "Net-(ProMini1-PadMISO)") (pinfunction "MISO") (pintype "passive"))
    (pad "MOSI" thru_hole circle (at -7.62 -11.43 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 20 "Net-(ProMini1-PadMOSI)") (pinfunction "MOSI") (pintype "passive"))
    (pad "NSS" thru_hole circle (at -7.62 -13.97 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 21 "Net-(ProMini1-PadNSS)") (pinfunction "NSS") (pintype "passive"))
    (pad "RAW" thru_hole circle (at -7.62 13.97 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 18 "unconnected-(ProMini1-PadRAW)") (pinfunction "RAW") (pintype "passive"))
    (pad "SCK" thru_hole circle (at -7.62 -6.35 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 22 "Net-(ProMini1-PadSCK)") (pinfunction "SCK") (pintype "passive"))
    (pad "SCL" thru_hole circle (at -5.08 5.08 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 24 "Net-(HDC1080-Pad4)") (pinfunction "SCL") (pintype "passive"))
    (pad "SDA" thru_hole circle (at -5.08 2.54 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 23 "Net-(HDC1080-Pad3)") (pinfunction "SDA") (pintype "passive"))
    (pad "VCC" thru_hole circle (at -7.62 6.35 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 1 "Net-(Booster1-Pad1)") (pinfunction "VCC") (pintype "passive"))
    (pad "VolDiv" thru_hole circle (at -7.62 -3.81 90) (size 1.50114 1.50114) (drill 0.8001) (layers *.Cu *.Mask "F.SilkS")
      (net 3 "Net-(C1-Pad1)") (pinfunction "VolDiv") (pintype "passive"))
    (model "Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl"
      (offset (xyz -3.809999943 5.079999924 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl"
      (offset (xyz 13.96999979 2.539999962 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl"
      (offset (xyz 0 7.619999886 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "Socket_Strips.3dshapes/Socket_Strip_Straight_1x12_Pitch2.54mm.wrl"
      (offset (xyz 0 -7.619999886 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl"
      (offset (xyz 6.349999905 5.079999924 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${MYSLOCAL}/mysensors.3dshapes/mysensors_arduino.3dshapes/arduino_pro_mini.wrl"
      (offset (xyz -1.269999981 0 12.19199982))
      (scale (xyz 0.395 0.395 0.395))
      (rotate (xyz 0 0 180))
    )
    (model "SMD_Packages.3dshapes/TQFP-32.wrl"
      (offset (xyz 1.269999981 0 13.0174998))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 315))
    )
    (model "Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl"
      (offset (xyz 13.96999979 -7.619999886 11.30299983))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model "Pin_Headers.3dshapes/Pin_Header_Straight_1x12_Pitch2.54mm.wrl"
      (offset (xyz 13.96999979 7.619999886 11.30299983))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model "Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl"
      (offset (xyz 13.96999979 5.079999924 11.30299983))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model "Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl"
      (offset (xyz 7.619999886 5.079999924 11.30299983))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model "Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl"
      (offset (xyz -2.539999962 5.079999924 11.30299983))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 90))
    )
    (model "${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl"
      (offset (xyz -7.619999886 0 13.0174998))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/smd_leds/led_0603.wrl"
      (offset (xyz 13.96999979 -4.444999933 13.0174998))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "Pin_Headers.3dshapes/Pin_Header_Angled_1x06_Pitch2.54mm.wrl"
      (offset (xyz -16.50999975 -6.349999905 13.0174998))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
    (model "Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz -7.619999886 -1.269999981 13.0174998))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "Resistors_SMD.3dshapes/R_0603.wrl"
      (offset (xyz 13.96999979 -3.174999952 13.0174998))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz -7.619999886 1.269999981 13.0174998))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-S_EIA-3216-12.wrl"
      (offset (xyz -8.889999866 3.809999943 13.0174998))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-S_EIA-3216-12.wrl"
      (offset (xyz -8.889999866 -3.809999943 13.0174998))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz -10.15999985 0 13.0174998))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "Capacitors_SMD.3dshapes/C_1210.wrl"
      (offset (xyz -12.69999981 0 13.0174998))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
    (model "${MYSLOCAL}/mysensors.3dshapes/w.lain.3dshapes/switch/smd_push.wrl"
      (offset (xyz 10.15999985 0 13.0174998))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 99.568 83.82)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "shield.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "ExtraGND1" (at 2.54 2.54 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x03_Female" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(ExtraGND1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(ExtraGND1-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(ExtraGND1-Pad1)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 93.472 50.8) (end 113.284 50.8) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 93.472 114.3) (end 93.472 50.8) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 113.284 50.8) (end 113.284 114.3) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 113.284 114.3) (end 93.472 114.3) (layer "Edge.Cuts") (width 0.1))
  (gr_text "v1alpha\n" (at 104.14 93.98) (layer "F.SilkS"))
  (gr_text "Booster" (at 101.286 100.415 -270) (layer "F.SilkS"))
  (gr_text "Pro Mini Headers here" (at 103.632 91.948) (layer "F.SilkS"))
  (gr_text "GND\n" (at 105.35 100.415 -270) (layer "F.SilkS"))
  (gr_text "2" (at 112.776 79.248 90) (layer "F.SilkS"))
  (gr_text "TX0" (at 112.776 89.408 90) (layer "F.SilkS"))
  (gr_text "Battery" (at 94.682 100.415 -270) (layer "F.SilkS"))
  (gr_text "+" (at 95.698 98.803379 -90) (layer "F.SilkS"))
  (gr_text "10" (at 96.52 61.468 90) (layer "F.SilkS"))
  (gr_text "Vin" (at 105.35 102.955 -270) (layer "F.SilkS"))
  (gr_text "RAW" (at 96.52 89.408 90) (layer "F.SilkS"))
  (gr_text "-" (at 95.698 101.343379 -90) (layer "F.SilkS"))
  (gr_text "GND\n" (at 105.664 54.864) (layer "F.SilkS"))
  (gr_text "SCL" (at 98.044 54.864) (layer "F.SilkS"))
  (gr_text "Vout" (at 105.35 97.875 -270) (layer "F.SilkS"))
  (gr_text "Voltage Divider" (at 101.6 105.525) (layer "F.SilkS"))
  (gr_text "RFM69HW" (at 104.14 65.532 90) (layer "F.SilkS"))
  (gr_text "Extra GND" (at 101.6 86.36 90) (layer "F.SilkS"))
  (gr_text "NSS" (at 100.076 59.944 90) (layer "F.SilkS"))
)
