(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A5")
  (title_block
    (title "Epi")
    (date "2022-10-27")
    (rev "1,1")
    (company "Rasmus L.")
  )
  (layers
    (0 "F.Cu" mixed)
    (31 "B.Cu" mixed)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 109.69 54.65)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/prod")
    )
  )
  (net 0 "")
  (net 1 "+5V")
  (net 2 "GND")
  (net 3 "Net-(C2-Pad2)")
  (net 4 "Net-(C5-Pad2)")
  (net 5 "Net-(C6-Pad2)")
  (net 6 "Net-(C7-Pad1)")
  (net 7 "Net-(C8-Pad2)")
  (net 8 "RST")
  (net 9 "D1{slash}TX")
  (net 10 "D0{slash}RX")
  (net 11 "A4")
  (net 12 "IO11")
  (net 13 "IO12")
  (net 14 "Net-(J4-PadA5)")
  (net 15 "Net-(J4-PadA6)")
  (net 16 "Net-(J4-PadA7)")
  (net 17 "unconnected-(J4-PadA8)")
  (net 18 "Net-(J4-PadB5)")
  (net 19 "unconnected-(J4-PadB8)")
  (net 20 "unconnected-(U1-Pad8)")
  (net 21 "D+")
  (net 22 "D-")
  (net 23 "D7")
  (net 24 "Net-(D2-Pad2)")
  (net 25 "D15{slash}SCK")
  (net 26 "D16{slash}MOSI")
  (net 27 "D14{slash}MISO")
  (net 28 "D3{slash}SCL")
  (net 29 "D2{slash}SDA")
  (net 30 "unconnected-(U1-Pad22)")
  (net 31 "D4")
  (net 32 "D6")
  (net 33 "IO8")
  (net 34 "IO9")
  (net 35 "IO10")
  (net 36 "D5")
  (net 37 "IO13")
  (net 38 "Net-(R7-Pad1)")
  (net 39 "A0")
  (net 40 "A1")
  (net 41 "A2")
  (net 42 "A3")
  (net 43 "A5")
  (net 44 "Net-(F1-Pad1)")
  (net 45 "unconnected-(J4-PadS1)")
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.6 61.6 180)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.16) (layer "F.SilkS") hide)
    (fp_text value "1µf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 180) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 105.34 60.0365 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RV1" (at 0 -1.17 90) (layer "F.SilkS") hide)
    (fp_text value "ESD protection varistor" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(J4-PadA7)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_2016-4Pin_2.0x1.6mm" (layer "F.Cu")
    (tedit 5A0FD1B2)
    (at 104.33 71.92)
    (descr "SMD Crystal SERIES SMD2016/4 http://www.q-crystal.com/upload/5/2015552223166229.pdf, 2.0x1.6mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Y1" (at 0 -2) (layer "F.SilkS") hide)
    (fp_text value "Crystal_GND24_Small" (at 0 2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.7 0.55) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "Net-(C6-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 0.7 0.55) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 0.7 -0.55) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(C5-Pad2)") (pinfunction "3") (pintype "passive"))
    (pad "4" smd roundrect (at -0.7 -0.55) (size 0.9 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
      (chamfer_ratio 0.3) (chamfer bottom_right)
      (net 2 "GND") (pinfunction "4") (pintype "passive"))
    (model "${KIPRJMOD}/extra/crystal.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 105.14 58.6365 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.17) (layer "F.SilkS") hide)
    (fp_text value "5,1kΩ" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(J4-PadB5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107.08 60.5365)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.16) (layer "F.SilkS") hide)
    (fp_text value "100nf" (at 0 1.16) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm" (layer "F.Cu")
    (tedit 5DC5F6A5)
    (at 104.34 66.1865 -90)
    (descr "QFN, 44 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/2512S.pdf#page=17), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -4.82 90) (layer "F.SilkS") hide)
    (fp_text value "ATmega32U4-M" (at 0 4.82 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -3.3375 -2.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "D7") (pinfunction "PE6") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -3.3375 -2 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "UVCC") (pintype "power_in"))
    (pad "3" smd roundrect (at -3.3375 -1.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "D-") (pinfunction "D-") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -3.3375 -1 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "D+") (pinfunction "D+") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -3.3375 -0.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "UGND") (pintype "passive"))
    (pad "6" smd roundrect (at -3.3375 0 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C8-Pad2)") (pinfunction "UCAP") (pintype "passive"))
    (pad "7" smd roundrect (at -3.3375 0.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VBUS") (pintype "input"))
    (pad "8" smd roundrect (at -3.3375 1 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "unconnected-(U1-Pad8)") (pinfunction "PB0") (pintype "bidirectional+no_connect"))
    (pad "9" smd roundrect (at -3.3375 1.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "D15{slash}SCK") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -3.3375 2 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "D16{slash}MOSI") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "11" smd roundrect (at -3.3375 2.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "D14{slash}MISO") (pinfunction "PB3") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -2.5 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "IO11") (pinfunction "PB7") (pintype "bidirectional"))
    (pad "13" smd roundrect (at -2 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "RST") (pinfunction "~{RESET}") (pintype "input"))
    (pad "14" smd roundrect (at -1.5 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "15" smd roundrect (at -1 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "16" smd roundrect (at -0.5 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C6-Pad2)") (pinfunction "XTAL2") (pintype "output"))
    (pad "17" smd roundrect (at 0 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C5-Pad2)") (pinfunction "XTAL1") (pintype "input"))
    (pad "18" smd roundrect (at 0.5 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "D3{slash}SCL") (pinfunction "PD0") (pintype "bidirectional"))
    (pad "19" smd roundrect (at 1 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "D2{slash}SDA") (pinfunction "PD1") (pintype "bidirectional"))
    (pad "20" smd roundrect (at 1.5 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "D0{slash}RX") (pinfunction "PD2") (pintype "bidirectional"))
    (pad "21" smd roundrect (at 2 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "D1{slash}TX") (pinfunction "PD3") (pintype "bidirectional"))
    (pad "22" smd roundrect (at 2.5 3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "unconnected-(U1-Pad22)") (pinfunction "PD5") (pintype "bidirectional"))
    (pad "23" smd roundrect (at 3.3375 2.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "24" smd roundrect (at 3.3375 2 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad2)") (pinfunction "AVCC") (pintype "power_in"))
    (pad "25" smd roundrect (at 3.3375 1.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "D4") (pinfunction "PD4") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 3.3375 1 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "IO12") (pinfunction "PD6") (pintype "bidirectional"))
    (pad "27" smd roundrect (at 3.3375 0.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "D6") (pinfunction "PD7") (pintype "bidirectional"))
    (pad "28" smd roundrect (at 3.3375 0 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "IO8") (pinfunction "PB4") (pintype "bidirectional"))
    (pad "29" smd roundrect (at 3.3375 -0.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "IO9") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "30" smd roundrect (at 3.3375 -1 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "IO10") (pinfunction "PB6") (pintype "bidirectional"))
    (pad "31" smd roundrect (at 3.3375 -1.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "D5") (pinfunction "PC6") (pintype "bidirectional"))
    (pad "32" smd roundrect (at 3.3375 -2 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "IO13") (pinfunction "PC7") (pintype "bidirectional"))
    (pad "33" smd roundrect (at 3.3375 -2.5 270) (size 1.075 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(R7-Pad1)") (pinfunction "~{HWB}/PE2") (pintype "bidirectional"))
    (pad "34" smd roundrect (at 2.5 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "VCC") (pintype "passive"))
    (pad "35" smd roundrect (at 2 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "36" smd roundrect (at 1.5 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "A0") (pinfunction "PF7") (pintype "bidirectional"))
    (pad "37" smd roundrect (at 1 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "A1") (pinfunction "PF6") (pintype "bidirectional"))
    (pad "38" smd roundrect (at 0.5 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "A2") (pinfunction "PF5") (pintype "bidirectional"))
    (pad "39" smd roundrect (at 0 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "A3") (pinfunction "PF4") (pintype "bidirectional"))
    (pad "40" smd roundrect (at -0.5 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "A4") (pinfunction "PF1") (pintype "bidirectional"))
    (pad "41" smd roundrect (at -1 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "A5") (pinfunction "PF0") (pintype "bidirectional"))
    (pad "42" smd roundrect (at -1.5 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C7-Pad1)") (pinfunction "AREF") (pintype "passive"))
    (pad "43" smd roundrect (at -2 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "44" smd roundrect (at -2.5 -3.3375 270) (size 0.25 1.075) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad2)") (pinfunction "AVCC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 107.19 71.95 -90)
    (descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 0 -1.17 90) (layer "F.SilkS") hide)
    (fp_text value "LED" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 104.39 60.0365 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.17 90) (layer "F.SilkS") hide)
    (fp_text value "22Ω" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(J4-PadA7)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "D-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.34 61.5865 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.17) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "RST") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.94 70.02 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.17 90) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 102.115 59.0865 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.17 90) (layer "F.SilkS") hide)
    (fp_text value "22Ω" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(J4-PadA6)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "D+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 101.64 60.6365 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "FB1" (at 0 -1.17) (layer "F.SilkS") hide)
    (fp_text value "Ferrite bead low-pass filter" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 104.34 66.1865)
    (fp_text reference "" (at 0 0) (layer "F.SilkS"))
    (fp_text value "" (at 0 0) (layer "F.SilkS"))
    (pad "1" smd roundrect (at 0 0 90) (size 1.25 1.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 101.165 59.0865 90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RV2" (at 0 -1.17 90) (layer "F.SilkS") hide)
    (fp_text value "ESD protection varistor" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(J4-PadA6)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 90) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107.09 59.5865 180)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.17) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 180) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 106.44 61.5865)
    (descr "Diode SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.17) (layer "F.SilkS") hide)
    (fp_text value "Diode" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.485 0) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "RST") (pinfunction "A") (pintype "passive"))
    (model "${KIPRJMOD}/extra/diode.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 102.4 72.1 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "22pf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x12_P1.27mm_Vertical" locked (layer "F.Cu")
    (tedit 59FED6E3)
    (at 97.99 58.92)
    (descr "Through hole straight pin header, 1x12, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x12 1.27mm single row")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -1.695) (layer "F.SilkS") hide)
    (fp_text value "Connector 1x12" (at 0 15.665) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.985 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 9 "D1{slash}TX") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole roundrect locked (at 0 1.27) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 "D0{slash}RX") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole roundrect locked (at 0 2.54) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole roundrect locked (at 0 3.81) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole roundrect locked (at 0 5.08) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 29 "D2{slash}SDA") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole roundrect locked (at 0 6.35) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 28 "D3{slash}SCL") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole roundrect locked (at 0 7.62) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 31 "D4") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole roundrect locked (at 0 8.89) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 36 "D5") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole roundrect locked (at 0 10.16) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 32 "D6") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole roundrect locked (at 0 11.43) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 23 "D7") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole roundrect locked (at 0 12.7) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 33 "IO8") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole roundrect locked (at 0 13.97) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 34 "IO9") (pinfunction "Pin_12") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x12_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x05_P1.27mm_Vertical" locked (layer "F.Cu")
    (tedit 59FED6E3)
    (at 106.88 74.16 -90)
    (descr "Through hole straight pin header, 1x05, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x05 1.27mm single row")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -1.695 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x05" (at 0 6.775 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 270) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 12 "IO11") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole roundrect locked (at 0 1.27 270) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 13 "IO12") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole roundrect locked (at 0 2.54 270) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 37 "IO13") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole roundrect locked (at 0 3.81 270) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 43 "A5") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole roundrect locked (at 0 5.08 270) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x05_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.49 60.1365 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "22pf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.95 63.7065 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "1µf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.29 71.95 -90)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.17 -270) (layer "F.SilkS") hide)
    (fp_text value "1kΩ" (at 0 1.17 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(D2-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0 270) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "IO13") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "USB-C-Connectors-master:USB-C MC-314C-4P16" (layer "F.Cu")
    (tedit 0)
    (at 104.34 53.3415 180)
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J4" (at 0 -5.4 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "USB-C 2.0 mid-mount female connector" (at 0 -7.4 180 unlocked) (layer "F.Fab"))
    (pad "A1" smd rect (at -3.2 -4 270) (size 1 0.6155) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "A1" smd rect (at 3.2 -4 270) (size 1 0.6155) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "A4" smd rect (at -2.4 -4 270) (size 1 0.6155) (layers "F.Cu" "F.Mask")
      (net 44 "Net-(F1-Pad1)") (pinfunction "VBUS") (pintype "passive"))
    (pad "A5" smd rect (at -1.250923 -4 270) (size 1 0.30775) (layers "F.Cu" "F.Mask")
      (net 14 "Net-(J4-PadA5)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd rect (at -0.24997 -4 270) (size 1 0.30775) (layers "F.Cu" "F.Mask")
      (net 15 "Net-(J4-PadA6)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" smd rect (at 0.248831 -4.00086 270) (size 1 0.30775) (layers "F.Cu" "F.Mask")
      (net 16 "Net-(J4-PadA7)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" smd rect (at 1.249411 -4 270) (size 1 0.30775) (layers "F.Cu" "F.Mask")
      (net 17 "unconnected-(J4-PadA8)") (pinfunction "SBU1") (pintype "bidirectional+no_connect"))
    (pad "A9" smd rect (at 2.4 -4 270) (size 1 0.6155) (layers "F.Cu" "F.Mask")
      (net 44 "Net-(F1-Pad1)") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" smd rect (at 1.752189 -4 270) (size 1 0.30775) (layers "F.Cu" "F.Mask")
      (net 18 "Net-(J4-PadB5)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" smd rect (at 0.749308 -4.00086 270) (size 1 0.30775) (layers "F.Cu" "F.Mask")
      (net 15 "Net-(J4-PadA6)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" smd rect (at -0.750447 -4 270) (size 1 0.30775) (layers "F.Cu" "F.Mask")
      (net 16 "Net-(J4-PadA7)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" smd rect (at -1.75 -4 270) (size 1 0.30775) (layers "F.Cu" "F.Mask")
      (net 19 "unconnected-(J4-PadB8)") (pinfunction "SBU2") (pintype "bidirectional+no_connect"))
    (pad "B12" smd rect (at -3.2 -4.4 270) (size 0.3 0.60775) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B12" smd rect (at 3.2 -4.4 270) (size 0.3 0.60775) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole oval (at 5.6 0.75 270) (size 2.3 1.2) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 45 "unconnected-(J4-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at -5.6 0.75 270) (size 2.3 1.2) (drill oval 1.7 0.6) (layers *.Cu *.Mask)
      (net 45 "unconnected-(J4-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at -5.6 -3.25 270) (size 2 1.2) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 45 "unconnected-(J4-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 5.6 -3.25 270) (size 2 1.2) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 45 "unconnected-(J4-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/DIY/USB-C.stp"
      (offset (xyz 0 0.4 -1.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.14 58.3365 -90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "22pf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 270) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.25 72.1 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "22pf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 107.04 58.6365)
    (descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.17) (layer "F.SilkS") hide)
    (fp_text value "5,1kΩ" (at 0 1.17) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(J4-PadA5)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.51 0) (size 0.54 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.14 60.1865 90)
    (descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.16 90) (layer "F.SilkS") hide)
    (fp_text value "100nf" (at 0 1.16 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.48 0 90) (size 0.56 0.62) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_0402_1005Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 108.49 58.2865 -90)
    (descr "Fuse SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F1" (at 0 -1.17 90) (layer "F.SilkS") hide)
    (fp_text value "Polyfuse 500mA HC" (at 0 1.17 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(F1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.485 0 270) (size 0.59 0.64) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+5V") (pintype "passive"))
    (model "${KIPRJMOD}/extra/1005_polyfuse.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_1.27mm:PinHeader_1x12_P1.27mm_Vertical" locked (layer "F.Cu")
    (tedit 59FED6E3)
    (at 110.69 58.92)
    (descr "Through hole straight pin header, 1x12, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x12 1.27mm single row")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -1.695) (layer "F.SilkS") hide)
    (fp_text value "Connector 1x12" (at 0 15.665) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.985 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole roundrect locked (at 0 1.27) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole roundrect locked (at 0 2.54) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 8 "RST") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole roundrect locked (at 0 3.81) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 11 "A4") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole roundrect locked (at 0 5.08) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 42 "A3") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole roundrect locked (at 0 6.35) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 41 "A2") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole roundrect locked (at 0 7.62) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 40 "A1") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole roundrect locked (at 0 8.89) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 39 "A0") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole roundrect locked (at 0 10.16) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 25 "D15{slash}SCK") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole roundrect locked (at 0 11.43) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 27 "D14{slash}MISO") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole roundrect locked (at 0 12.7) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 26 "D16{slash}MOSI") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole roundrect locked (at 0 13.97) (size 1.5 1) (drill 0.65) (property pad_prop_castellated) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 35 "IO10") (pinfunction "Pin_12") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x12_P1.27mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "B.Cu")
    (tedit 5A0F774F)
    (at 106.135 58.7 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "D-" (at 0.635 1.2) (layer "B.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -1.55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.45) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 16 "Net-(J4-PadA7)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Pad_D1.0mm" (layer "B.Cu")
    (tedit 5A0F774F)
    (at 102.545 58.75 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "File: epi.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "D+" (at 0.295 1) (layer "B.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -1.55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.45) (layer "B.Fab"))
    (pad "1" smd circle (at 0 0 180) (size 1 1) (layers "B.Cu" "B.Mask")
      (net 15 "Net-(J4-PadA6)") (pinfunction "1") (pintype "passive"))
  )
  (gr_line (start 110.69 51.4) (end 110.69 53.65) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 97.99 51.4) (end 97.99 53.65) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.64 57.3365) (end 100.84 56.8365) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 100.84 56.8365) (end 107.84 56.8365) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 110.69 55.65) (mid 109.69 54.65) (end 110.69 53.65) (layer "Edge.Cuts") (width 0.1))
  (gr_arc (start 97.99 53.65) (mid 98.99 54.65) (end 97.99 55.65) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 109.04 51.4) (end 110.69 51.4) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 109.04 57.3365) (end 109.04 51.4) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 110.69 74.16) (end 110.69 55.65) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 97.99 74.16) (end 110.69 74.16) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 97.99 55.65) (end 97.99 74.16) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 97.99 51.4) (end 99.64 51.4) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 99.64 51.4) (end 99.64 57.3365) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 107.84 56.8365) (end 109.04 57.3365) (layer "Edge.Cuts") (width 0.1))
  (gr_text "A1" (at 109.09 66.613) (layer "B.SilkS"))
  (gr_text "Epi v1,4" (at 104.240187 60.404121) (layer "B.SilkS"))
  (gr_text "5V" (at 109.09 58.993) (layer "B.SilkS"))
  (gr_text "~13" (at 104.365 72.24619 90) (layer "B.SilkS"))
  (gr_text "A0" (at 109.09 67.883) (layer "B.SilkS"))
  (gr_text "12" (at 105.6525 72.531904 90) (layer "B.SilkS"))
  (gr_text "~3" (at 99.525714 65.34) (layer "B.SilkS"))
  (gr_text "7" (at 99.24 70.42) (layer "B.SilkS"))
  (gr_text "1" (at 99.24 58.99) (layer "B.SilkS"))
  (gr_text "8" (at 99.24 71.69) (layer "B.SilkS"))
  (gr_text "16" (at 109.051905 71.693) (layer "B.SilkS"))
  (gr_text "-D+" (at 104.34 57.75) (layer "B.SilkS"))
  (gr_text "15" (at 109.051905 69.153) (layer "B.SilkS"))
  (gr_text "~11" (at 106.94 72.24619 90) (layer "B.SilkS"))
  (gr_text "~6" (at 99.525714 69.15) (layer "B.SilkS"))
  (gr_text "2" (at 99.24 60.26) (layer "B.SilkS"))
  (gr_text "R" (at 109.41381 61.47) (layer "B.SilkS"))
  (gr_text "10~" (at 108.766191 72.963) (layer "B.SilkS"))
  (gr_text "~5" (at 99.525714 67.88) (layer "B.SilkS"))
  (gr_text "A2" (at 109.09 65.343) (layer "B.SilkS"))
  (gr_text "4" (at 99.24 66.61) (layer "B.SilkS"))
  (gr_text "2" (at 99.24 64.07) (layer "B.SilkS"))
  (gr_text "CERN\nOHL-P" (at 104.3 69.25) (layer "B.SilkS"))
  (gr_text "A4" (at 109.09 62.803) (layer "B.SilkS"))
  (gr_text "A5" (at 103.0775 72.57 90) (layer "B.SilkS"))
  (gr_text "A3" (at 109.09 64.073) (layer "B.SilkS"))
  (gr_text "~9" (at 99.525714 72.96) (layer "B.SilkS"))
  (gr_text "14" (at 109.051905 70.423) (layer "B.SilkS"))
  (gr_text "RoHS" (at 118.99 68.92) (layer "Dwgs.User"))
  (gr_text "Made in\nthe EU" (at 118.94 65.37) (layer "Dwgs.User"))
  (gr_text "JLCJLCJLCJLC" (at 118.79 61.3365) (layer "Dwgs.User"))
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 110.84 74.3865)
        (xy 97.84 74.3865)
        (xy 97.84 50.6365)
        (xy 110.84 50.6365)
      )
    )
  )
)
