(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "VCC")
  (net 2 "GND")
  (net 3 "+5V")
  (net 4 "Net-(D1-Pad1)")
  (net 5 "Net-(D1-Pad2)")
  (net 6 "Net-(J2-Pad1)")
  (net 7 "Net-(J2-Pad2)")
  (net 8 "Net-(J3-Pad6)")
  (net 9 "Net-(R2-Pad1)")
  (net 10 "Net-(R3-Pad2)")
  (net 11 "Net-(R7-Pad1)")
  (net 12 "Net-(R4-Pad2)")
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 144.75 87.25 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C2" (at 4.75 0) (layer "F.SilkS"))
    (fp_text value "10nf" (at 1.25 2.5 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 -270) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 178.025 73.225 -90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 1.275 -2.475 180) (layer "F.SilkS"))
    (fp_text value "Conn_02x03_M" (at 1.27 7.41 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+5V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad1)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad2)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 152.06 84 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R8" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "10kΩ" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad6)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Wide" (layer "F.Cu")
    (tedit 5A2795B7)
    (at 139.48 84.46 -90)
    (descr "TO-92 leads molded, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at 2.79 -0.25 180) (layer "F.SilkS"))
    (fp_text value "L78L05_TO92" (at 2.54 2.79 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+5V") (pinfunction "VO") (pintype "power_out"))
    (pad "2" thru_hole circle (at 2.54 -2.54 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle (at 5.08 0 270) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "VCC") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H4.3mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 154.75 90.5 90)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=4.3mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW3" (at 3.25 2.15 180) (layer "F.SilkS"))
    (fp_text value "SW_MEC_5E" (at 3.75 6.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 6.5 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad6)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad6)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 180) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H4.3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5A19A429)
    (at 135.5 73.7)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 2.5 3.8) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_F" (at 0 10.39) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+5V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KIPRJMOD}/OLED.stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 148.28 91.5)
    (descr "Resistor, Axial_DIN0204 series, Axial, Vertical, pin pitch=2.54mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Vertical pin pitch 2.54mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "TH1" (at 1.27 -1.92) (layer "F.SilkS"))
    (fp_text value "10kΩ" (at 1.27 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -1.92) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 9 "Net-(R2-Pad1)") (pintype "passive"))
    (model "${KIPRJMOD}/weirdthermistor.stp"
      (offset (xyz 0 0 -2.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 165.75 78.44 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R4" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R3-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 131.81 82.75 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R1" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "10kΩ" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 162.5 86.06 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R6" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text value "2,2kΩ" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(R4-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (tedit 587A3A7B)
    (at 125 77 -90)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "D1" (at 1.25 -3.25 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 2.96 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0 270) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "" (layer "F.Cu")
    (tedit 0)
    (at 149.5 103.65)
    (fp_text reference "" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "" (at 0 0) (layer "F.SilkS") hide)
    (pad "1" thru_hole circle (at 0 0 180) (size 2 2) (drill 1.5) (layers *.Cu *.Mask)
      (pinfunction "1") (pintype "passive"))
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (tedit 5A02E8C5)
    (at 149.8 80.8 180)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 4.05) (layer "F.SilkS"))
    (fp_text value "ATtiny85" (at 6.81 10.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(J3-Pad6)") (pinfunction "~{RESET}/PB5") (pintype "bidirectional"))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R2-Pad1)") (pinfunction "XTAL1/PB3") (pintype "bidirectional"))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R7-Pad1)") (pinfunction "XTAL2/PB4") (pintype "bidirectional"))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-Pad1)") (pinfunction "AREF/PB0") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-Pad2)") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220F-3_Vertical" (layer "F.Cu")
    (tedit 5AC8BA0D)
    (at 131.29 88.805 180)
    (descr "TO-220F-3, Vertical, RM 2.54mm, see http://www.st.com/resource/en/datasheet/stp20nm60.pdf")
    (tags "TO-220F-3 Vertical RM 2.54mm")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Q1" (at 2.54 -2.195) (layer "F.SilkS"))
    (fp_text value "Q_NMOS_GDS" (at 2.54 2.9025) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.1675) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.905 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 5 "Net-(D1-Pad2)") (pinfunction "G") (pintype "input"))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.905 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "VCC") (pinfunction "D") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0 180) (size 1.905 2) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "S") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220F-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H4.3mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 180.25 84 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=4.3mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 3.25 2.25) (layer "F.SilkS"))
    (fp_text value "SW_MEC_5E" (at 3.75 6.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(R7-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(R7-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(R3-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 10 "Net-(R3-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H4.3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 114.5 88.817621 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=6.3mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 6.3mm Electrolytic Capacitor")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C3" (at 1.25 -4.5 180) (layer "F.SilkS"))
    (fp_text value "100µf" (at 1.25 4.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D6.3mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_BarrelJack:BarrelJack_Horizontal" (layer "F.Cu")
    (tedit 5A1DBF6A)
    (at 117.5 84.5 -90)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -3 0 180) (layer "F.SilkS"))
    (fp_text value "Barrel_Jack_MountingPin" (at -6.2 -5.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3 -2.95 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" thru_hole roundrect (at -6 0 270) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "3" thru_hole roundrect (at -3 4.7 270) (size 3.5 3.5) (drill 2.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25))
    (model "${KIPRJMOD}/barrel_jack.stp"
      (offset (xyz -5.75 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 169 86.06 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R3" (at 3.81 0 90) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "+5V") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 132.31 73.5 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R5" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "1kΩ" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm_H4.3mm" (layer "F.Cu")
    (tedit 5A02FE31)
    (at 180.25 91.5 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=4.3mm")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at 3.25 2.25) (layer "F.SilkS"))
    (fp_text value "SW_MEC_5E" (at 3.75 6.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(R7-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 11 "Net-(R7-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(R4-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 12 "Net-(R4-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H4.3mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 155.19 75.75)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R7" (at 3.81 0.048683) (layer "F.SilkS"))
    (fp_text value "10kΩ" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Disc_D5.0mm_W2.5mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 135.75 86 -90)
    (descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 2.50mm  diameter 5mm width 2.5mm Capacitor")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "C1" (at 4.75 0 180) (layer "F.SilkS"))
    (fp_text value "330nf" (at 1.25 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "VCC") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 162.69 89.25)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "File: 50x70_tiny.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "R2" (at 3.81 0) (layer "F.SilkS"))
    (fp_text value "10kΩ" (at 3.81 2.37) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 106.75 72.75) (end 106.75 70) (layer "Edge.Cuts") (width 0.2))
  (gr_arc (start 183.45 145.75) (mid 181.95 144.25) (end 183.45 142.75) (layer "Edge.Cuts") (width 0.2))
  (gr_arc (start 183.5 75.75) (mid 182 74.25) (end 183.5 72.75) (layer "Edge.Cuts") (width 0.2))
  (gr_circle (center 152.375 95.5) (end 154.125 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_line (start 183.5 75.75) (end 185 75.75) (layer "Edge.Cuts") (width 0.2))
  (gr_circle (center 118.666666 95.5) (end 120.416666 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_circle (center 135.875 95.5) (end 137.625 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_circle (center 131.75 95.5) (end 133.5 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_line (start 183.5 72.75) (end 185 72.75) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 184.95 145.75) (end 184.95 148.5) (layer "Edge.Cuts") (width 0.2))
  (gr_arc (start 108.25 72.75) (mid 109.75 74.25) (end 108.25 75.75) (layer "Edge.Cuts") (width 0.2))
  (gr_circle (center 144.125 95.5) (end 145.875 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_circle (center 148.25 95.5) (end 150 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_line (start 106.75 70) (end 185 70) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 183.45 142.75) (end 184.95 142.75) (layer "Edge.Cuts") (width 0.2))
  (gr_circle (center 114.583333 95.5) (end 116.333333 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_line (start 106.75 142.75) (end 106.75 75.75) (layer "Edge.Cuts") (width 0.2))
  (gr_circle (center 177.125 95.5) (end 178.875 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_arc (start 108.25 142.75) (mid 109.75 144.25) (end 108.25 145.75) (layer "Edge.Cuts") (width 0.2))
  (gr_circle (center 181.25 95.5) (end 183 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_line (start 108.25 75.75) (end 106.75 75.75) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 183.45 145.75) (end 184.95 145.75) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 108.25 142.75) (end 106.75 142.75) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 185 70) (end 185 72.75) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 184.95 148.5) (end 106.75 148.5) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 185 75.75) (end 184.95 142.75) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 106.75 148.5) (end 106.75 145.75) (layer "Edge.Cuts") (width 0.2))
  (gr_line (start 108.25 145.75) (end 106.75 145.75) (layer "Edge.Cuts") (width 0.2))
  (gr_circle (center 160.625 95.5) (end 162.375 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_circle (center 110.5 95.5) (end 112.25 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_circle (center 168.875 95.5) (end 170.625 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_circle (center 140 95.5) (end 141.75 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_circle (center 173 95.5) (end 174.75 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_circle (center 122.75 95.5) (end 124.5 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_circle (center 164.75 95.5) (end 166.5 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_line (start 108.25 72.75) (end 106.75 72.75) (layer "Edge.Cuts") (width 0.2))
  (gr_circle (center 156.5 95.5) (end 158.25 95.5) (layer "Edge.Cuts") (width 0.15) (fill none))
  (gr_text "RESET" (at 157 92.75) (layer "F.SilkS"))
  (gr_text "JLCJLCJLCJLC" (at 183.35 84.4 90) (layer "F.SilkS"))
  (gr_text "70x50mm TinyReflow V1,2 CERN-OHL-P v2" (at 108.5 119.5 270) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.5))
    (min_thickness 0.5) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (island_removal_mode 2) (island_area_min 1))
    (polygon
      (pts
        (xy 186 94)
        (xy 105.75 94)
        (xy 105.75 69.25)
        (xy 186 69.25)
      )
    )
  )
)
