(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "Hammar32")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 109.315 72.142756)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "Net-(C5-Pad1)")
  (net 3 "Net-(C7-Pad2)")
  (net 4 "+3.3V")
  (net 5 "Net-(C6-Pad1)")
  (net 6 "Net-(C7-Pad1)")
  (net 7 "Net-(C18-Pad1)")
  (net 8 "Net-(C8-Pad1)")
  (net 9 "Net-(C9-Pad1)")
  (net 10 "Net-(C9-Pad2)")
  (net 11 "RST")
  (net 12 "Net-(C10-Pad1)")
  (net 13 "Net-(C10-Pad2)")
  (net 14 "Net-(C11-Pad1)")
  (net 15 "Net-(C12-Pad1)")
  (net 16 "T-END")
  (net 17 "T-BED")
  (net 18 "Net-(C12-Pad2)")
  (net 19 "Net-(C15-Pad1)")
  (net 20 "Net-(C16-Pad1)")
  (net 21 "Net-(C17-Pad1)")
  (net 22 "Net-(D1-Pad2)")
  (net 23 "Net-(D2-Pad2)")
  (net 24 "Net-(D4-Pad2)")
  (net 25 "Net-(D5-Pad1)")
  (net 26 "Net-(D6-Pad2)")
  (net 27 "Net-(F3-Pad1)")
  (net 28 "Net-(C22-Pad2)")
  (net 29 "Net-(J3-PadA5)")
  (net 30 "unconnected-(J3-PadA8)")
  (net 31 "Net-(J3-PadB5)")
  (net 32 "TX")
  (net 33 "unconnected-(J3-PadB8)")
  (net 34 "unconnected-(J3-PadS1)")
  (net 35 "RX")
  (net 36 "IO0")
  (net 37 "SS")
  (net 38 "SCK")
  (net 39 "MISO")
  (net 40 "SDA")
  (net 41 "SCL")
  (net 42 "MOSI")
  (net 43 "Net-(U7-Pad7)")
  (net 44 "Net-(U7-Pad8)")
  (net 45 "unconnected-(U7-Pad9)")
  (net 46 "Net-(J12-Pad2)")
  (net 47 "D+")
  (net 48 "D-")
  (net 49 "Net-(J15-Pad3)")
  (net 50 "Net-(Q1-Pad1)")
  (net 51 "Net-(Q2-Pad1)")
  (net 52 "Net-(R1-Pad1)")
  (net 53 "X-MIN")
  (net 54 "Y-MIN")
  (net 55 "Z-MIN")
  (net 56 "END")
  (net 57 "BED")
  (net 58 "FAN")
  (net 59 "Net-(R4-Pad2)")
  (net 60 "Net-(R2-Pad2)")
  (net 61 "Net-(R3-Pad1)")
  (net 62 "E-EN")
  (net 63 "Net-(R5-Pad1)")
  (net 64 "Net-(R6-Pad2)")
  (net 65 "Net-(R7-Pad1)")
  (net 66 "Net-(R8-Pad2)")
  (net 67 "Net-(R9-Pad1)")
  (net 68 "Net-(R12-Pad1)")
  (net 69 "Net-(R16-Pad2)")
  (net 70 "Net-(R17-Pad2)")
  (net 71 "Net-(R18-Pad2)")
  (net 72 "Net-(R10-Pad1)")
  (net 73 "Net-(R11-Pad1)")
  (net 74 "Net-(R13-Pad2)")
  (net 75 "Net-(R14-Pad2)")
  (net 76 "Net-(R15-Pad2)")
  (net 77 "Net-(R19-Pad2)")
  (net 78 "Net-(R20-Pad2)")
  (net 79 "Net-(R38-Pad2)")
  (net 80 "Net-(RV1-Pad2)")
  (net 81 "Net-(RV2-Pad2)")
  (net 82 "Net-(RV3-Pad2)")
  (net 83 "Net-(RV4-Pad2)")
  (net 84 "X-2B")
  (net 85 "unconnected-(U1-Pad7)")
  (net 86 "X-STP")
  (net 87 "X-DIR")
  (net 88 "unconnected-(U1-Pad20)")
  (net 89 "X-1B")
  (net 90 "X-1A")
  (net 91 "unconnected-(U1-Pad25)")
  (net 92 "X-2A")
  (net 93 "Y-STP")
  (net 94 "Y-DIR")
  (net 95 "Z-STP")
  (net 96 "Z-DIR")
  (net 97 "E-STP")
  (net 98 "E-DIR")
  (net 99 "unconnected-(U7-Pad10)")
  (net 100 "unconnected-(U7-Pad11)")
  (net 101 "unconnected-(U7-Pad12)")
  (net 102 "Y-2B")
  (net 103 "unconnected-(U3-Pad7)")
  (net 104 "unconnected-(U3-Pad20)")
  (net 105 "Y-1B")
  (net 106 "Y-1A")
  (net 107 "unconnected-(U3-Pad25)")
  (net 108 "Y-2A")
  (net 109 "Z-2B")
  (net 110 "unconnected-(U4-Pad7)")
  (net 111 "unconnected-(U4-Pad20)")
  (net 112 "Z-1B")
  (net 113 "Z-1A")
  (net 114 "unconnected-(U4-Pad25)")
  (net 115 "Z-2A")
  (net 116 "E-2B")
  (net 117 "Net-(R39-Pad1)")
  (net 118 "Net-(R41-Pad1)")
  (net 119 "E-1B")
  (net 120 "E-1A")
  (net 121 "Net-(R42-Pad2)")
  (net 122 "E-2A")
  (net 123 "ENDCONN")
  (net 124 "BEDCONN-F")
  (net 125 "Net-(J1-Pad8)")
  (net 126 "VIN")
  (net 127 "unconnected-(U7-Pad15)")
  (net 128 "unconnected-(U2-Pad7)")
  (net 129 "unconnected-(U2-Pad25)")
  (net 130 "unconnected-(U6-Pad17)")
  (net 131 "unconnected-(U2-Pad20)")
  (net 132 "unconnected-(U6-Pad18)")
  (net 133 "unconnected-(U6-Pad19)")
  (net 134 "unconnected-(U6-Pad20)")
  (net 135 "unconnected-(J2-Pad1)")
  (net 136 "unconnected-(J2-Pad8)")
  (net 137 "unconnected-(U6-Pad21)")
  (net 138 "+VDC")
  (net 139 "BEDCONN")
  (net 140 "unconnected-(U6-Pad22)")
  (net 141 "RTS")
  (net 142 "unconnected-(U6-Pad32)")
  (net 143 "DTR")
  (net 144 "unconnected-(J2-Pad9)")
  (footprint "Potentiometer_SMD:Potentiometer_Bourns_3314J_Vertical" (layer "F.Cu")
    (tedit 5A81E1D7)
    (at 139.405 83.112874 180)
    (descr "Potentiometer, vertical, Bourns 3314J, http://www.bourns.com/docs/Product-Datasheets/3314.pdf")
    (tags "Potentiometer vertical Bourns 3314J")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RV1" (at 0 -4.25) (layer "F.SilkS") hide)
    (fp_text value "Potentiometer_10kΩ" (at 0 -7.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.7) (layer "F.Fab"))
    (pad "1" smd rect (at 1.15 -2 180) (size 1.3 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "Net-(R13-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 0 2 180) (size 2 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "Net-(RV1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at -1.15 -2 180) (size 1.3 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3314J_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 104.965 91.722756 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C21" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "10µF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "T-END") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 112.965 77.722756 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "68mΩ" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.805 100.972756 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R33" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "680Ω" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "Net-(J15-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Z-MIN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 131.605 76.972756 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "68mΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(R3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 170.155 102.472756 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q5" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "PMV40UN2R or equivalent" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "FAN") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "Net-(J1-Pad8)") (pinfunction "D") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "S") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 177.805 112.512874 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R40" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "5,1kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "Net-(J3-PadB5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 101.865 87.162874)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "20kΩ" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(R14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 128.055 81.762874 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "+VDC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 149.555 87.362874 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100kΩ" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(R16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm" (layer "F.Cu")
    (tedit 5DC5F6A4)
    (at 133.655 81.612874)
    (descr "QFN, 28 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=283), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "A4988" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect (at 0 1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.12 -1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.12 0) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.12 1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.12 1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.12 0) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 0) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.12 -1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 -1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -2.45 -1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "Y-2B") (pinfunction "OUT2B") (pintype "power_out"))
    (pad "2" smd roundrect (at -2.45 -1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "E-EN") (pinfunction "EN") (pintype "input"))
    (pad "3" smd roundrect (at -2.45 -0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "4" smd roundrect (at -2.45 0) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C7-Pad1)") (pinfunction "CP1") (pintype "input"))
    (pad "5" smd roundrect (at -2.45 0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C7-Pad2)") (pinfunction "CP2") (pintype "input"))
    (pad "6" smd roundrect (at -2.45 1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C6-Pad1)") (pinfunction "VCP") (pintype "input"))
    (pad "7" smd roundrect (at -2.45 1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "unconnected-(U1-Pad7)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "8" smd roundrect (at -1.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(C15-Pad1)") (pinfunction "VREG") (pintype "input"))
    (pad "9" smd roundrect (at -1 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "MS1") (pintype "input"))
    (pad "10" smd roundrect (at -0.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "MS2") (pintype "input"))
    (pad "11" smd roundrect (at 0 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "MS3") (pintype "input"))
    (pad "12" smd roundrect (at 0.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(R20-Pad2)") (pinfunction "RESET") (pintype "input"))
    (pad "13" smd roundrect (at 1 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(R9-Pad1)") (pinfunction "ROSC") (pintype "input"))
    (pad "14" smd roundrect (at 1.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(R20-Pad2)") (pinfunction "SLEEP") (pintype "input"))
    (pad "15" smd roundrect (at 2.45 1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "VDD") (pintype "input"))
    (pad "16" smd roundrect (at 2.45 1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Y-STP") (pinfunction "STEP") (pintype "input"))
    (pad "17" smd roundrect (at 2.45 0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(RV1-Pad2)") (pinfunction "VREF") (pintype "input"))
    (pad "18" smd roundrect (at 2.45 0) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "19" smd roundrect (at 2.45 -0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Y-DIR") (pinfunction "DIR") (pintype "input"))
    (pad "20" smd roundrect (at 2.45 -1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "unconnected-(U1-Pad20)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "21" smd roundrect (at 2.45 -1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "Y-1B") (pinfunction "OUT1B") (pintype "power_out"))
    (pad "22" smd roundrect (at 1.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "+VDC") (pinfunction "VBB1") (pintype "input"))
    (pad "23" smd roundrect (at 1 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(R4-Pad2)") (pinfunction "SENSE1") (pintype "input"))
    (pad "24" smd roundrect (at 0.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 106 "Y-1A") (pinfunction "OUT1A") (pintype "power_out"))
    (pad "25" smd roundrect (at 0 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "unconnected-(U1-Pad25)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "26" smd roundrect (at -0.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "Y-2A") (pinfunction "OUT2A") (pintype "power_out"))
    (pad "27" smd roundrect (at -1 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(R3-Pad1)") (pinfunction "SENSE2") (pintype "input"))
    (pad "28" smd roundrect (at -1.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "+VDC") (pinfunction "VBB2") (pintype "input"))
    (pad "29" smd rect (at 0 0) (size 3.35 3.35) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 149.605 76.972756 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "68mΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(R5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 134.855 86.222756 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(R9-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.465 102.222756 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R34" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "SCL") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DIY:8-VSONP (5x6)" (layer "F.Cu")
    (tedit 0)
    (at 171.215 93.472756 90)
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q3" (at -0.425 9.585 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TI CSD17310Q5A or equivalent" (at -0.375 8.835 -90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at 2.75 -2 90) (size 0.75 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "BED") (pinfunction "G") (pintype "input"))
    (pad "2" smd rect (at -3 2 90) (size 0.75 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S") (pintype "passive"))
    (pad "2" smd rect (at -3 -0.666667 90) (size 0.75 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S") (pintype "passive"))
    (pad "2" smd rect (at -0.375 0 90) (size 4.5 4.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S") (pintype "passive"))
    (pad "2" smd rect (at -3 0.666666 90) (size 0.75 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S") (pintype "passive"))
    (pad "2" smd rect (at -3 -2 90) (size 0.75 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd rect (at 2.75 -0.666667 90) (size 0.75 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "BEDCONN-F") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect (at 2.75 0.666666 90) (size 0.75 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "BEDCONN-F") (pinfunction "D") (pintype "passive"))
    (pad "3" smd rect (at 2.75 2 90) (size 0.75 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 124 "BEDCONN-F") (pinfunction "D") (pintype "passive"))
    (model "${KIPRJMOD}/FET.stp"
      (offset (xyz -0.125 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_6.3x4.9" (layer "F.Cu")
    (tedit 5BCA39CF)
    (at 105.215 76.222756)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic C5, 6.3x4.9mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -4.35) (layer "F.SilkS") hide)
    (fp_text value "100µF" (at -10.13 -0.15) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8 0) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 138 "+VDC") (pintype "passive"))
    (pad "2" smd roundrect (at 2.8 0) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x4.9.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 158.215 112.972756 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R41" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1kΩ" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "Net-(R41-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "RX") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 149.755 85.612874)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C16" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "220nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(C16-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 152.465 93.012874 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R24" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "BED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(D1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.715 92.222756 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R23" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(Q2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "DTR") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.465 96.722756 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C22" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(C22-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 173.215 104.582638 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R35" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "FAN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 171.965 113.722756 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R42" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "22Ω" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "D-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "Net-(R42-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.465 99.722756 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R32" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "SDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_6.3x4.9" (layer "F.Cu")
    (tedit 5BCA39CF)
    (at 158.965 75.422756 -90)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic C5, 6.3x4.9mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0 -4.35 90) (layer "F.SilkS") hide)
    (fp_text value "100µF" (at 0 4.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8 0 270) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 138 "+VDC") (pintype "passive"))
    (pad "2" smd roundrect (at 2.8 0 270) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x4.9.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 104.965 96.972756 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C23" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "10µF" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "T-BED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145.715 91.722756)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R21" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Z-DIR") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 175.215 96.222756 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R27" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "END") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.155 85.612874)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "220nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "Net-(C15-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 102.305 96.962874 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R31" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "4,7kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "T-BED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 151.915 88.972756 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C20" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "220nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 102.305 93.512874 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R26" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "4,7kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "T-END") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 101.555 88.662874 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R19" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100kΩ" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(R19-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323" (layer "F.Cu")
    (tedit 58641739)
    (at 173.965 109.722756)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D6" (at 0 -1.85) (layer "F.SilkS") hide)
    (fp_text value "USB protection diode, >500mA >24V. Silicon fine" (at -0.25 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.85) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "+VDC") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(D6-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm" (layer "F.Cu")
    (tedit 5DC5F6A4)
    (at 97.655 81.662874)
    (descr "QFN, 28 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=283), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "A4988" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect (at 1.12 1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.12 -1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 -1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 0) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.12 1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.12 -1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.12 0) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.12 0) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -2.45 -1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "E-2B") (pinfunction "OUT2B") (pintype "power_out"))
    (pad "2" smd roundrect (at -2.45 -1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "E-EN") (pinfunction "EN") (pintype "input"))
    (pad "3" smd roundrect (at -2.45 -0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "4" smd roundrect (at -2.45 0) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C10-Pad1)") (pinfunction "CP1") (pintype "input"))
    (pad "5" smd roundrect (at -2.45 0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C10-Pad2)") (pinfunction "CP2") (pintype "input"))
    (pad "6" smd roundrect (at -2.45 1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C5-Pad1)") (pinfunction "VCP") (pintype "input"))
    (pad "7" smd roundrect (at -2.45 1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "unconnected-(U3-Pad7)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "8" smd roundrect (at -1.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C17-Pad1)") (pinfunction "VREG") (pintype "input"))
    (pad "9" smd roundrect (at -1 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "MS1") (pintype "input"))
    (pad "10" smd roundrect (at -0.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "MS2") (pintype "input"))
    (pad "11" smd roundrect (at 0 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "MS3") (pintype "input"))
    (pad "12" smd roundrect (at 0.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(R19-Pad2)") (pinfunction "RESET") (pintype "input"))
    (pad "13" smd roundrect (at 1 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(R11-Pad1)") (pinfunction "ROSC") (pintype "input"))
    (pad "14" smd roundrect (at 1.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(R19-Pad2)") (pinfunction "SLEEP") (pintype "input"))
    (pad "15" smd roundrect (at 2.45 1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "VDD") (pintype "input"))
    (pad "16" smd roundrect (at 2.45 1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "E-STP") (pinfunction "STEP") (pintype "input"))
    (pad "17" smd roundrect (at 2.45 0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(RV2-Pad2)") (pinfunction "VREF") (pintype "input"))
    (pad "18" smd roundrect (at 2.45 0) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "19" smd roundrect (at 2.45 -0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "E-DIR") (pinfunction "DIR") (pintype "input"))
    (pad "20" smd roundrect (at 2.45 -1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "unconnected-(U3-Pad20)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "21" smd roundrect (at 2.45 -1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "E-1B") (pinfunction "OUT1B") (pintype "power_out"))
    (pad "22" smd roundrect (at 1.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "+VDC") (pinfunction "VBB1") (pintype "input"))
    (pad "23" smd roundrect (at 1 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(R2-Pad2)") (pinfunction "SENSE1") (pintype "input"))
    (pad "24" smd roundrect (at 0.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "E-1A") (pinfunction "OUT1A") (pintype "power_out"))
    (pad "25" smd roundrect (at 0 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "unconnected-(U3-Pad25)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "26" smd roundrect (at -0.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 122 "E-2A") (pinfunction "OUT2A") (pintype "power_out"))
    (pad "27" smd roundrect (at -1 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(R1-Pad1)") (pinfunction "SENSE2") (pintype "input"))
    (pad "28" smd roundrect (at -1.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "+VDC") (pinfunction "VBB2") (pintype "input"))
    (pad "29" smd rect (at 0 0) (size 3.35 3.35) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 99.165 76.972756 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "68mΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "Net-(R2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DIY:LED 0603 reverse mount" (layer "F.Cu")
    (tedit 0)
    (at 176.965 94.372756 180)
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 0.15 -1.45 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "LED_Small" (at 0.2 1.85 180 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 1.3 1.3) (drill 1.3) (layers *.Mask "B.Cu"))
    (pad "1" smd rect (at -0.95 0 180) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 0.95 0 180) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 98.755 86.262874 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(R11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 96.155 85.662874)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C17" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "220nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(C17-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 147.605 81.812874 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 152.715 86.222756 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(R10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_SMD:Potentiometer_Bourns_3314J_Vertical" (layer "F.Cu")
    (tedit 5A81E1D7)
    (at 103.355 83.162874 180)
    (descr "Potentiometer, vertical, Bourns 3314J, http://www.bourns.com/docs/Product-Datasheets/3314.pdf")
    (tags "Potentiometer vertical Bourns 3314J")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RV2" (at 0 -4.25) (layer "F.SilkS") hide)
    (fp_text value "Potentiometer_10kΩ" (at 0 4.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.7) (layer "F.Fab"))
    (pad "1" smd rect (at 1.15 -2 180) (size 1.3 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "Net-(R14-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 0 2 180) (size 2 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "Net-(RV2-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at -1.15 -2 180) (size 1.3 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3314J_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_6.3x4.9" (layer "F.Cu")
    (tedit 5BCA39CF)
    (at 124.465 76.222756)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic C5, 6.3x4.9mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -4.35) (layer "F.SilkS") hide)
    (fp_text value "100µF" (at 0 4.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8 0) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 138 "+VDC") (pintype "passive"))
    (pad "2" smd roundrect (at 2.8 0) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x4.9.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 130.715 92.222756 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R22" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 141 "RTS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(Q1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 165.465 117.722756 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C28" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 159.25 100.5 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C25" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "330nF" (at -0.08 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "+VDC") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.655 76.972756 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "68mΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.055 81.862874 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "+VDC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm" (layer "F.Cu")
    (tedit 5DC5F6A4)
    (at 151.605 81.612874)
    (descr "QFN, 28 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=283), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "A4988" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect (at 1.12 0) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.12 -1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.12 -1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 -1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.12 1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.12 1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 0) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.12 0) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -2.45 -1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "X-2B") (pinfunction "OUT2B") (pintype "power_out"))
    (pad "2" smd roundrect (at -2.45 -1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "E-EN") (pinfunction "EN") (pintype "input"))
    (pad "3" smd roundrect (at -2.45 -0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "4" smd roundrect (at -2.45 0) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C9-Pad1)") (pinfunction "CP1") (pintype "input"))
    (pad "5" smd roundrect (at -2.45 0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C9-Pad2)") (pinfunction "CP2") (pintype "input"))
    (pad "6" smd roundrect (at -2.45 1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C8-Pad1)") (pinfunction "VCP") (pintype "input"))
    (pad "7" smd roundrect (at -2.45 1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "unconnected-(U2-Pad7)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "8" smd roundrect (at -1.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(C16-Pad1)") (pinfunction "VREG") (pintype "input"))
    (pad "9" smd roundrect (at -1 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "MS1") (pintype "input"))
    (pad "10" smd roundrect (at -0.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "MS2") (pintype "input"))
    (pad "11" smd roundrect (at 0 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "MS3") (pintype "input"))
    (pad "12" smd roundrect (at 0.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(R16-Pad2)") (pinfunction "RESET") (pintype "input"))
    (pad "13" smd roundrect (at 1 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(R10-Pad1)") (pinfunction "ROSC") (pintype "input"))
    (pad "14" smd roundrect (at 1.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(R16-Pad2)") (pinfunction "SLEEP") (pintype "input"))
    (pad "15" smd roundrect (at 2.45 1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "VDD") (pintype "input"))
    (pad "16" smd roundrect (at 2.45 1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "X-STP") (pinfunction "STEP") (pintype "input"))
    (pad "17" smd roundrect (at 2.45 0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(RV4-Pad2)") (pinfunction "VREF") (pintype "input"))
    (pad "18" smd roundrect (at 2.45 0) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "19" smd roundrect (at 2.45 -0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "X-DIR") (pinfunction "DIR") (pintype "input"))
    (pad "20" smd roundrect (at 2.45 -1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "unconnected-(U2-Pad20)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "21" smd roundrect (at 2.45 -1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "X-1B") (pinfunction "OUT1B") (pintype "power_out"))
    (pad "22" smd roundrect (at 1.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "+VDC") (pinfunction "VBB1") (pintype "input"))
    (pad "23" smd roundrect (at 1 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(R6-Pad2)") (pinfunction "SENSE1") (pintype "input"))
    (pad "24" smd roundrect (at 0.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "X-1A") (pinfunction "OUT1A") (pintype "power_out"))
    (pad "25" smd roundrect (at 0 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 129 "unconnected-(U2-Pad25)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "26" smd roundrect (at -0.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "X-2A") (pinfunction "OUT2A") (pintype "power_out"))
    (pad "27" smd roundrect (at -1 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "Net-(R5-Pad1)") (pinfunction "SENSE2") (pintype "input"))
    (pad "28" smd roundrect (at -1.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "+VDC") (pinfunction "VBB2") (pintype "input"))
    (pad "29" smd rect (at 0 0) (size 3.35 3.35) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DIY:LED 0603 reverse mount" (layer "F.Cu")
    (tedit 0)
    (at 171.715 106.972756 -90)
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D5" (at 0.15 -1.45 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "LED_Small" (at 0.2 1.85 -90 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0 270) (size 1.3 1.3) (drill 1.3) (layers *.Mask "B.Cu"))
    (pad "1" smd rect (at -0.95 0 270) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(D5-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 0.95 0 270) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3.3V") (pinfunction "A") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 135.215 76.972756 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "68mΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "Net-(R4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DIY:mini BUCK" (layer "F.Cu")
    (tedit 0)
    (at 161.965 97.722756)
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U5" (at 0 -10.25 unlocked) (layer "F.SilkS") hide)
    (fp_text value "DPAK 3,3v linear regulator + caps OR mini buck converter" (at 0 -12 unlocked) (layer "F.Fab"))
    (fp_text user "VIN" (at -2.95 -7.8 unlocked) (layer "F.SilkS"))
    (pad "" smd rect (at 0.585 -4.775) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 3.935 -4.775) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 3.935 -1.725) (size 3.05 2.75) (layers "F.Paste"))
    (pad "" smd rect (at 0.585 -1.725) (size 3.05 2.75) (layers "F.Paste"))
    (pad "1" smd rect (at -4.04 -5.53) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "+VDC") (pinfunction "IN") (pintype "power_in"))
    (pad "1" smd roundrect (at -5.45 -8.45) (size 2.1 2.1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "+VDC") (pinfunction "IN") (pintype "power_in"))
    (pad "2" smd rect (at 2.26 -3.25) (size 6.4 5.8) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at 5.45 8.45) (size 2.1 2.1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at 5.45 -8.45) (size 2.1 2.1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at -5.45 8.45) (size 2.1 2.1) (layers "F.Cu" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "OUT") (pintype "power_out"))
    (pad "3" smd rect (at -4.04 -0.97) (size 2.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3.3V") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-2.step"
      (offset (xyz 0.25 3.25 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 179.305 117.512874 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RV6" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "ESD varistor, optional" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "D-") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323" (layer "F.Cu")
    (tedit 58641739)
    (at 108.555 101.012874 90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D3" (at 0 -1.85 90) (layer "F.SilkS") hide)
    (fp_text value "Zener_~3,3v" (at 0.1 1.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.85 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.05 0 90) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Z-MIN") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.05 0 90) (size 0.6 0.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122.965 96.722756 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R29" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "RST") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(C22-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 177.805 117.512874 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R43" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "5,1kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(J3-PadA5)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 151.215 112.222756)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C27" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 153.965 93.012874 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R25" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "BED") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_C_Receptacle_HRO_TYPE-C-31-M-12" (layer "F.Cu")
    (tedit 5D3C0721)
    (at 185.615 114.972756 90)
    (descr "USB Type-C receptacle for USB 2.0 and PD, http://www.krhro.com/uploads/soft/180320/1-1P320120243.pdf")
    (tags "usb usb-c 2.0 pd")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J3" (at 0 -5.645 90) (layer "F.SilkS") hide)
    (fp_text value "USB_C_Receptacle_USB2.0" (at 0 5.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 2.89 -2.6 90) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -2.89 -2.6 90) (size 0.65 0.65) (drill 0.65) (layers *.Cu *.Mask))
    (pad "A1" smd roundrect (at -3.25 -4.045 90) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
      (chamfer_ratio 0.5) (chamfer bottom_left)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "A4" smd rect (at -2.45 -4.045 90) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(F3-Pad1)") (pinfunction "VBUS") (pintype "passive"))
    (pad "A5" smd rect (at -1.25 -4.045 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(J3-PadA5)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A6" smd rect (at -0.25 -4.045 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "D+") (pinfunction "D+") (pintype "bidirectional"))
    (pad "A7" smd rect (at 0.25 -4.045 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "D-") (pinfunction "D-") (pintype "bidirectional"))
    (pad "A8" smd rect (at 1.25 -4.045 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "unconnected-(J3-PadA8)") (pinfunction "SBU1") (pintype "bidirectional+no_connect"))
    (pad "A9" smd rect (at 2.45 -4.045 90) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(F3-Pad1)") (pinfunction "VBUS") (pintype "passive"))
    (pad "A12" smd roundrect (at 3.25 -4.045 90) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
      (chamfer_ratio 0.5) (chamfer bottom_right)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B1" smd roundrect (at 3.25 -4.045 90) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
      (chamfer_ratio 0.5) (chamfer bottom_right)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B4" smd rect (at 2.45 -4.045 90) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(F3-Pad1)") (pinfunction "VBUS") (pintype "passive"))
    (pad "B5" smd rect (at 1.75 -4.045 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(J3-PadB5)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B6" smd rect (at 0.75 -4.045 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "D+") (pinfunction "D+") (pintype "bidirectional"))
    (pad "B7" smd rect (at -0.75 -4.045 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "D-") (pinfunction "D-") (pintype "bidirectional"))
    (pad "B8" smd rect (at -1.75 -4.045 90) (size 0.3 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "unconnected-(J3-PadB8)") (pinfunction "SBU2") (pintype "bidirectional+no_connect"))
    (pad "B9" smd rect (at -2.45 -4.045 90) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(F3-Pad1)") (pinfunction "VBUS") (pintype "passive"))
    (pad "B12" smd roundrect (at -3.25 -4.045 90) (size 0.6 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0)
      (chamfer_ratio 0.5) (chamfer bottom_left)
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole oval (at -4.4 -3.13 90) (size 1.5 1.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 "unconnected-(J3-PadS1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "S1" thru_hole oval (at 4.4 -3.13 90) (size 1.5 1.5) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 "unconnected-(J3-PadS1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "S1" thru_hole circle (at 4.32 1.05 90) (size 1.2 1.2) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 "unconnected-(J3-PadS1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (pad "S1" thru_hole circle (at -4.32 1.05 90) (size 1.2 1.2) (drill 0.9) (layers *.Cu *.Mask)
      (net 34 "unconnected-(J3-PadS1)") (pinfunction "SHIELD") (pintype "passive+no_connect"))
    (model "${KIPRJMOD}/USBC.stp"
      (offset (xyz 0 0.5 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Capacitor_SMD:CP_Elec_6.3x4.9" (layer "F.Cu")
    (tedit 5BCA39CF)
    (at 141.715 76.222756)
    (descr "SMD capacitor, aluminum electrolytic, Panasonic C5, 6.3x4.9mm")
    (tags "capacitor electrolytic")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 -4.35) (layer "F.SilkS") hide)
    (fp_text value "100µF" (at 0 4.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8 0) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 138 "+VDC") (pintype "passive"))
    (pad "2" smd roundrect (at 2.8 0) (size 3.5 1.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.15625)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x4.9.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 158.215 98.722756)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C24" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.465 96.722756 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R30" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(C22-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122.455 87.962874 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R18" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "Net-(R18-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "RF_Module:ESP32-WROOM-32" (layer "F.Cu")
    (tedit 61D4B4ED)
    (at 139.215 104.727756 180)
    (descr "Single 2.4 GHz Wi-Fi and Bluetooth combo chip https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32_datasheet_en.pdf")
    (tags "Single 2.4 GHz Wi-Fi and Bluetooth combo  chip")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U6" (at -10.61 8.43 90) (layer "F.SilkS") hide)
    (fp_text value "ESP32-WROOM-32E" (at 0 11.5) (layer "F.Fab"))
    (fp_text user "5 mm" (at -11.2 -14.375) (layer "Cmts.User"))
    (fp_text user "KEEP-OUT ZONE" (at 0 -19) (layer "Cmts.User"))
    (fp_text user "Antenna" (at 0 -13) (layer "Cmts.User"))
    (fp_text user "5 mm" (at 11.8 -14.375) (layer "Cmts.User"))
    (fp_text user "5 mm" (at 7.8 -19.075 90) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -8.75 -8.25 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect (at -8.75 -6.98 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "3" smd rect (at -8.75 -5.71 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "RST") (pinfunction "EN") (pintype "input"))
    (pad "4" smd rect (at -8.75 -4.44 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "T-END") (pinfunction "SENSOR_VP") (pintype "input"))
    (pad "5" smd rect (at -8.75 -3.17 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "T-BED") (pinfunction "SENSOR_VN") (pintype "input"))
    (pad "6" smd rect (at -8.75 -1.9 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "X-MIN") (pinfunction "IO34") (pintype "input"))
    (pad "7" smd rect (at -8.75 -0.63 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "Y-MIN") (pinfunction "IO35") (pintype "input"))
    (pad "8" smd rect (at -8.75 0.64 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "Y-DIR") (pinfunction "IO32") (pintype "bidirectional"))
    (pad "9" smd rect (at -8.75 1.91 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "Y-STP") (pinfunction "IO33") (pintype "bidirectional"))
    (pad "10" smd rect (at -8.75 3.18 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "E-EN") (pinfunction "IO25") (pintype "bidirectional"))
    (pad "11" smd rect (at -8.75 4.45 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "X-DIR") (pinfunction "IO26") (pintype "bidirectional"))
    (pad "12" smd rect (at -8.75 5.72 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "X-STP") (pinfunction "IO27") (pintype "bidirectional"))
    (pad "13" smd rect (at -8.75 6.99 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "Z-STP") (pinfunction "IO14") (pintype "bidirectional"))
    (pad "14" smd rect (at -8.75 8.26 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 96 "Z-DIR") (pinfunction "IO12") (pintype "bidirectional"))
    (pad "15" smd rect (at -5.71 9.51 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "16" smd rect (at -4.44 9.51 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "FAN") (pinfunction "IO13") (pintype "bidirectional"))
    (pad "17" smd rect (at -3.17 9.51 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "unconnected-(U6-Pad17)") (pinfunction "SHD/SD2") (pintype "bidirectional"))
    (pad "18" smd rect (at -1.9 9.51 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "unconnected-(U6-Pad18)") (pinfunction "SWP/SD3") (pintype "bidirectional"))
    (pad "19" smd rect (at -0.63 9.51 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 133 "unconnected-(U6-Pad19)") (pinfunction "SCS/CMD") (pintype "bidirectional"))
    (pad "20" smd rect (at 0.64 9.51 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "unconnected-(U6-Pad20)") (pinfunction "SCK/CLK") (pintype "bidirectional"))
    (pad "21" smd rect (at 1.91 9.51 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 137 "unconnected-(U6-Pad21)") (pinfunction "SDO/SD0") (pintype "bidirectional"))
    (pad "22" smd rect (at 3.18 9.51 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "unconnected-(U6-Pad22)") (pinfunction "SDI/SD1") (pintype "bidirectional"))
    (pad "23" smd rect (at 4.45 9.51 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "Z-MIN") (pinfunction "IO15") (pintype "bidirectional"))
    (pad "24" smd rect (at 5.72 9.51 270) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "END") (pinfunction "IO2") (pintype "bidirectional"))
    (pad "25" smd rect (at 8.75 8.26 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "IO0") (pinfunction "IO0") (pintype "bidirectional"))
    (pad "26" smd rect (at 8.75 6.99 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "BED") (pinfunction "IO4") (pintype "bidirectional"))
    (pad "27" smd rect (at 8.75 5.72 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "E-STP") (pinfunction "IO16") (pintype "bidirectional"))
    (pad "28" smd rect (at 8.75 4.45 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "E-DIR") (pinfunction "IO17") (pintype "bidirectional"))
    (pad "29" smd rect (at 8.75 3.18 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "SS") (pinfunction "IO5") (pintype "bidirectional"))
    (pad "30" smd rect (at 8.75 1.91 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "SCK") (pinfunction "IO18") (pintype "bidirectional"))
    (pad "31" smd rect (at 8.75 0.64 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "MISO") (pinfunction "IO19") (pintype "bidirectional"))
    (pad "32" smd rect (at 8.75 -0.63 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "unconnected-(U6-Pad32)") (pinfunction "NC") (pintype "no_connect"))
    (pad "33" smd rect (at 8.75 -1.9 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "SDA") (pinfunction "IO21") (pintype "bidirectional"))
    (pad "34" smd rect (at 8.75 -3.17 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "TX") (pinfunction "RXD0/IO3") (pintype "bidirectional"))
    (pad "35" smd rect (at 8.75 -4.44 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "RX") (pinfunction "TXD0/IO1") (pintype "bidirectional"))
    (pad "36" smd rect (at 8.75 -5.71 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 41 "SCL") (pinfunction "IO22") (pintype "bidirectional"))
    (pad "37" smd rect (at 8.75 -6.98 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "MOSI") (pinfunction "IO23") (pintype "bidirectional"))
    (pad "38" smd rect (at 8.75 -8.25 180) (size 1.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "39" smd rect (at -0.68 -0.91 180) (size 4.2 4.2) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
      (connect_pads (clearance 0))
      (min_thickness 0.254)
      (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
      (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
      (polygon
        (pts
          (xy 153.215 114.697756)
          (xy 125.215 114.697756)
          (xy 125.215 125.477756)
          (xy 153.215 125.477756)
        )
      )
    )
    (model "${KICAD6_3DMODEL_DIR}/RF_Module.3dshapes/ESP32-WROOM-32.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 93.705 85.162874 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "220nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 153.155 76.972756 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "68mΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "Net-(R6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 114.055 85.662874)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C18" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "220nF" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C18-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.655 81.762874 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DIY:LED 0603 reverse mount" (layer "F.Cu")
    (tedit 0)
    (at 177.065 104.522756 180)
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D4" (at 0.15 -1.45 180 unlocked) (layer "F.SilkS") hide)
    (fp_text value "LED_Small" (at 0.2 1.85 180 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0 180) (size 1.3 1.3) (drill 1.3) (layers *.Mask "B.Cu"))
    (pad "1" smd rect (at -0.95 0 180) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 0.95 0 180) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(D4-Pad2)") (pinfunction "A") (pintype "passive"))
  )
  (footprint "DIY:microSD" (layer "F.Cu")
    (tedit 0)
    (at 113.965 111.972756)
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J2" (at 0 -11.3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Micro_SD_Holder" (at 0 -9.8 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -4.7 4.5) (size 1 1) (drill 1) (layers *.Mask))
    (pad "" np_thru_hole circle (at 3.3 4.5) (size 1 1) (drill 1) (layers *.Mask))
    (pad "1" smd rect (at 2.2 -6.5) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "unconnected-(J2-Pad1)") (pinfunction "DAT2") (pintype "bidirectional+no_connect"))
    (pad "2" smd rect (at 1.1 -6.5) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "SS") (pinfunction "DAT3/CD") (pintype "bidirectional"))
    (pad "3" smd rect (at 0 -6.5) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 42 "MOSI") (pinfunction "CMD") (pintype "input"))
    (pad "4" smd rect (at -1.1 -6.5) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+3.3V") (pinfunction "VDD") (pintype "power_in"))
    (pad "5" smd rect (at -2.2 -6.5) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "SCK") (pinfunction "CLK") (pintype "input"))
    (pad "6" smd rect (at -3.3 -6.5) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "7" smd rect (at -4.4 -6.5) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "MISO") (pinfunction "DAT0") (pintype "bidirectional"))
    (pad "8" smd rect (at -5.5 -6.5) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "unconnected-(J2-Pad8)") (pinfunction "DAT1") (pintype "bidirectional+no_connect"))
    (pad "9" smd rect (at 7.1 -5.3) (size 1.6 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "unconnected-(J2-Pad9)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "9" smd rect (at -7.8 4.3) (size 1.2 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "unconnected-(J2-Pad9)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "9" smd rect (at 8 4.1) (size 1.2 2.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "unconnected-(J2-Pad9)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "9" smd rect (at -7.8 -5.3) (size 1.2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "unconnected-(J2-Pad9)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "NC" smd rect (at -6.6 -6.5) (size 0.7 1.6) (layers "F.Cu" "F.Paste" "F.Mask"))
    (model "${KIPRJMOD}/microsd.stp"
      (offset (xyz -0.5 -1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.855 88.662874)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R20" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "100kΩ" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(R20-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DIY:resonator_3,2x1,3" (layer "F.Cu")
    (tedit 0)
    (at 171.965 116.472756 90)
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Y1" (at 0 -2.75 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "Resonator_12mhz" (at 0 3.25 90 unlocked) (layer "F.Fab"))
    (pad "1" smd rect (at -1.2 0 90) (size 0.4 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 43 "Net-(U7-Pad7)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 0 0 90) (size 0.4 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 1.2 0 270) (size 0.4 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "Net-(U7-Pad8)") (pinfunction "3") (pintype "passive"))
    (model "${KIPRJMOD}/resonator.stp"
      (offset (xyz 0 0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_1206_3216Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 178.055 109.512874 180)
    (descr "Fuse SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "fuse")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F3" (at 0 -1.82) (layer "F.SilkS") hide)
    (fp_text value "Polyfuse 500mA" (at 0 1.82) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 27 "Net-(F3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2)
      (net 26 "Net-(D6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 137.715 92.222756)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q2" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "S9014 or equivalent" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "Net-(Q2-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 141 "RTS") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "RST") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 151.465 110.472756)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C26" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "10µF" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.555 81.862874 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(C12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TerminalBlock:TerminalBlock_bornier-6_P5.08mm" (layer "F.Cu")
    (tedit 59FF03F5)
    (at 184.555 71.512874 -90)
    (descr "simple 6pin terminal block, pitch 5.08mm, revamped version of bornier6")
    (tags "terminal block bornier6")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 12.65 -4.55 90) (layer "F.SilkS") hide)
    (fp_text value "8x screw terminal, 5,08mm spacing. rated for >20A" (at 12.7 4.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 12.7 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 126 "VIN") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at 10.16 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 139 "BEDCONN") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 15.24 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 124 "BEDCONN-F") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at 20.32 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 138 "+VDC") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at 25.4 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 123 "ENDCONN") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 30.47 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 138 "+VDC") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 35.55 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 125 "Net-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-6_P5.08mm.wrl"
      (offset (xyz 12.69999981 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-8-5.08_1x08_P5.08mm_Horizontal.step"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 180 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 154.215 87.472756 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "20kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "Net-(R17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 92.965 78.722756 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "+VDC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.655 84.912874 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at -0.05 -1.5 90) (layer "F.SilkS") hide)
    (fp_text value "220nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_SMD:Potentiometer_Bourns_3314J_Vertical" (layer "F.Cu")
    (tedit 5A81E1D7)
    (at 157.465 83.722756 180)
    (descr "Potentiometer, vertical, Bourns 3314J, http://www.bourns.com/docs/Product-Datasheets/3314.pdf")
    (tags "Potentiometer vertical Bourns 3314J")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RV4" (at 0 -4.25) (layer "F.SilkS") hide)
    (fp_text value "Potentiometer_10kΩ" (at 0 4.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.7) (layer "F.Fab"))
    (pad "1" smd rect (at 1.15 -2 180) (size 1.3 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(R17-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 0 2 180) (size 2 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "Net-(RV4-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at -1.15 -2 180) (size 1.3 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3314J_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 117.715 77.742756 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "68mΩ" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(R8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 170.155 98.922756 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q4" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "PMV40UN2R or equivalent" (at 0 3.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "END") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "ENDCONN") (pinfunction "D") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "S") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 165.215 112.972756 90)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U7" (at 0 -5.9 90) (layer "F.SilkS") hide)
    (fp_text value "CH340G" (at 0 5.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -4.445 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.475 -3.175 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(R38-Pad2)") (pinfunction "TXD") (pintype "output"))
    (pad "3" smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "Net-(R41-Pad1)") (pinfunction "RXD") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "V3") (pintype "passive"))
    (pad "5" smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(R39-Pad1)") (pinfunction "UD+") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "Net-(R42-Pad2)") (pinfunction "UD-") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -2.475 3.175 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(U7-Pad7)") (pinfunction "XI") (pintype "input"))
    (pad "8" smd roundrect (at -2.475 4.445 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "Net-(U7-Pad8)") (pinfunction "XO") (pintype "output"))
    (pad "9" smd roundrect (at 2.475 4.445 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 45 "unconnected-(U7-Pad9)") (pinfunction "~{CTS}") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 3.175 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "unconnected-(U7-Pad10)") (pinfunction "~{DSR}") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "unconnected-(U7-Pad11)") (pinfunction "~{RI}") (pintype "input"))
    (pad "12" smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 101 "unconnected-(U7-Pad12)") (pinfunction "~{DCD}") (pintype "input"))
    (pad "13" smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "DTR") (pinfunction "~{DTR}") (pintype "output"))
    (pad "14" smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 141 "RTS") (pinfunction "~{RTS}") (pintype "output"))
    (pad "15" smd roundrect (at 2.475 -3.175 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "unconnected-(U7-Pad15)") (pinfunction "R232") (pintype "input"))
    (pad "16" smd roundrect (at 2.475 -4.445 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.755 86.262874 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "10kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(R12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 133.715 92.222756)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Q1" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "S9014 or equivalent" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(Q1-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "DTR") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "IO0") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 146.105 81.812874 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 0.05 -1.75) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "+VDC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.665 86.362874 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C19" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "220nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 93.655 81.862874 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "100nF" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 179.305 112.512874 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RV5" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "ESD varistor, optional" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "D+") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 120.055 87.262874)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "20kΩ" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(R15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_SMD:Potentiometer_Bourns_3314J_Vertical" (layer "F.Cu")
    (tedit 5A81E1D7)
    (at 121.255 83.162874 180)
    (descr "Potentiometer, vertical, Bourns 3314J, http://www.bourns.com/docs/Product-Datasheets/3314.pdf")
    (tags "Potentiometer vertical Bourns 3314J")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RV3" (at 0 -4.25) (layer "F.SilkS") hide)
    (fp_text value "Potentiometer_10kΩ" (at 15.58 -1.475) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.7) (layer "F.Fab"))
    (pad "1" smd rect (at 1.15 -2 180) (size 1.3 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "Net-(R15-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 0 2 180) (size 2 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "Net-(RV3-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at -1.15 -2 180) (size 1.3 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_SMD.3dshapes/Potentiometer_Bourns_3314J_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.765 87.112874)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "20kΩ" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(R13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 178.215 96.222756)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R28" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1kΩ" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "END") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(D2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm" (layer "F.Cu")
    (tedit 5DC5F6A4)
    (at 115.555 81.662874)
    (descr "QFN, 28 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=283), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0 -3.8) (layer "F.SilkS") hide)
    (fp_text value "A4988" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect (at 0 1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.12 1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.12 -1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 -1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.12 -1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.12 1.12) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0 0) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 1.12 0) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -1.12 0) (size 0.9 0.9) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect (at -2.45 -1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "Z-2B") (pinfunction "OUT2B") (pintype "power_out"))
    (pad "2" smd roundrect (at -2.45 -1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "E-EN") (pinfunction "EN") (pintype "input"))
    (pad "3" smd roundrect (at -2.45 -0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "4" smd roundrect (at -2.45 0) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(C12-Pad1)") (pinfunction "CP1") (pintype "input"))
    (pad "5" smd roundrect (at -2.45 0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(C12-Pad2)") (pinfunction "CP2") (pintype "input"))
    (pad "6" smd roundrect (at -2.45 1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(C11-Pad1)") (pinfunction "VCP") (pintype "input"))
    (pad "7" smd roundrect (at -2.45 1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "unconnected-(U4-Pad7)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "8" smd roundrect (at -1.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(C18-Pad1)") (pinfunction "VREG") (pintype "input"))
    (pad "9" smd roundrect (at -1 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "MS1") (pintype "input"))
    (pad "10" smd roundrect (at -0.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "MS2") (pintype "input"))
    (pad "11" smd roundrect (at 0 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "MS3") (pintype "input"))
    (pad "12" smd roundrect (at 0.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "Net-(R18-Pad2)") (pinfunction "RESET") (pintype "input"))
    (pad "13" smd roundrect (at 1 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(R12-Pad1)") (pinfunction "ROSC") (pintype "input"))
    (pad "14" smd roundrect (at 1.5 2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "Net-(R18-Pad2)") (pinfunction "SLEEP") (pintype "input"))
    (pad "15" smd roundrect (at 2.45 1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+3.3V") (pinfunction "VDD") (pintype "input"))
    (pad "16" smd roundrect (at 2.45 1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "Z-STP") (pinfunction "STEP") (pintype "input"))
    (pad "17" smd roundrect (at 2.45 0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "Net-(RV3-Pad2)") (pinfunction "VREF") (pintype "input"))
    (pad "18" smd roundrect (at 2.45 0) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (pad "19" smd roundrect (at 2.45 -0.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Z-DIR") (pinfunction "DIR") (pintype "input"))
    (pad "20" smd roundrect (at 2.45 -1) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "unconnected-(U4-Pad20)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "21" smd roundrect (at 2.45 -1.5) (size 0.8 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Z-1B") (pinfunction "OUT1B") (pintype "power_out"))
    (pad "22" smd roundrect (at 1.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "+VDC") (pinfunction "VBB1") (pintype "input"))
    (pad "23" smd roundrect (at 1 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "Net-(R8-Pad2)") (pinfunction "SENSE1") (pintype "input"))
    (pad "24" smd roundrect (at 0.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Z-1A") (pinfunction "OUT1A") (pintype "power_out"))
    (pad "25" smd roundrect (at 0 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "unconnected-(U4-Pad25)") (pinfunction "NC") (pintype "free+no_connect"))
    (pad "26" smd roundrect (at -0.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "Z-2A") (pinfunction "OUT2A") (pintype "power_out"))
    (pad "27" smd roundrect (at -1 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(R7-Pad1)") (pinfunction "SENSE2") (pintype "input"))
    (pad "28" smd roundrect (at -1.5 -2.45) (size 0.25 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "+VDC") (pinfunction "VBB2") (pintype "input"))
    (pad "29" smd rect (at 0 0) (size 3.35 3.35) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 171.965 112.222756)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R39" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "22Ω" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(R39-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "D+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 174.715 104.582638 -90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R36" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "FAN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 270) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(D4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 169.965 106.222756 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R37" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "1kΩ" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(D5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DIY:LED 0603 reverse mount" (layer "F.Cu")
    (tedit 0)
    (at 150.465 93.012874 -90)
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at 0.15 -1.45 -90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "LED_Small" (at 0.2 1.85 -90 unlocked) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0 270) (size 1.3 1.3) (drill 1.3) (layers *.Mask "B.Cu"))
    (pad "1" smd rect (at -0.95 0 270) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 0.95 0 270) (size 0.6 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 158.215 111.222756)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R38" (at 0 -1.43) (layer "F.SilkS") hide)
    (fp_text value "1kΩ" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "TX") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(R38-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 97.965 112.472756 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Y" (at 0 2.33) (layer "B.SilkS"))
    (fp_text value "1x3" (at 0 -7.41) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "+3.3V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 54 "Y-MIN") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 96.24 90.722756 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J9" (at 0 2.33) (layer "B.SilkS") hide)
    (fp_text value "1x2" (at 0 -4.87) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.27 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "T-END") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LOGO" (layer "B.Cu")
    (tedit 0)
    (at 138.915 100.942756 -177)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0 3) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0 3) (layer "B.SilkS") hide)
  )
  (footprint "LOGO" (layer "B.Cu")
    (tedit 0)
    (at 110.805 101.512874 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (footprint "Button_Switch_THT:SW_PUSH_6mm" (layer "B.Cu")
    (tedit 5A02FE31)
    (at 117.305 100.012874 90)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 3.25 2 90) (layer "B.SilkS") hide)
    (fp_text value "SW_MEC_5G" (at 3.75 -6.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 -2.25 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 6.5 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 "Net-(C22-Pad2)") (pinfunction "A") (pintype "passive"))
    (pad "1" thru_hole circle (at 0 0) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 28 "Net-(C22-Pad2)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 -4.5) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "B") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 -4.5) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 137.015 70.472756 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J5" (at 0 2.33 90) (layer "B.SilkS") hide)
    (fp_text value "1x4" (at 0 -9.95 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.81) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 105 "Y-1B") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 "Y-1A") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 "Y-2A") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 102 "Y-2B") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 127.215 112.222756)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J13" (at 0 2.33) (layer "B.SilkS") hide)
    (fp_text value "1x8" (at 0 -20.11) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -8.89 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "+3.3V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "SCL") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "SDA") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "MOSI") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "MISO") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "SCK") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "IO0") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DIY:mini fuse sep" (layer "B.Cu")
    (tedit 0)
    (at 173.965 80.472756 -90)
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "F2" (at 0 -0.05 90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "15A Mini fuse + Keystone 3557 fuse holders, or equivalent" (at 0 4 90 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 5.65 1.65 270) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 139 "BEDCONN") (pintype "passive"))
    (pad "1" thru_hole circle (at 5.65 -1.75 270) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 139 "BEDCONN") (pintype "passive"))
    (pad "2" thru_hole circle (at -5.75 -1.75 270) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 126 "VIN") (pintype "passive"))
    (pad "2" thru_hole circle (at -5.75 1.65 270) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 126 "VIN") (pintype "passive"))
    (model "${KIPRJMOD}/fuse.stp"
      (offset (xyz -0.1 0 -22))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 118.265 70.472756 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J6" (at 0 2.33 90) (layer "B.SilkS") hide)
    (fp_text value "1x4" (at 0 -9.95 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.81) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 "Z-1B") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 113 "Z-1A") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 "Z-2A") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 "Z-2B") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 151.215 99.722756 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J11" (at 0 2.33) (layer "B.SilkS") hide)
    (fp_text value "1x4" (at 0 -9.95) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.81 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "+3.3V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "RX") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "TX") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 101.265 70.472756 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J7" (at 0 2.33 90) (layer "B.SilkS") hide)
    (fp_text value "1x4" (at 0 -9.95 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.81) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 119 "E-1B") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 120 "E-1A") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 122 "E-2A") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 116 "E-2B") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 118.265 73.472756 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J8" (at 0 2.33 90) (layer "B.SilkS") hide)
    (fp_text value "1x4" (at 0 -9.95 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.81) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 "Z-1B") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 113 "Z-1A") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 "Z-2A") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 "Z-2B") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 94.24 112.447756 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "X" (at 0 2.33) (layer "B.SilkS"))
    (fp_text value "1x3" (at 0 -7.41) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "+3.3V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "X-MIN") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 101.715 112.472756 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Z" (at 0 2.33 180) (layer "B.SilkS"))
    (fp_text value "1x3" (at 0 -7.41) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J12-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J15-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "DIY:mini fuse sep" (layer "B.Cu")
    (tedit 0)
    (at 166.715 80.472756 -90)
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "F1" (at 0 -0.05 -90 unlocked) (layer "B.SilkS") hide)
    (fp_text value "15A Mini fuse + Keystone 3557 fuse holders, or equivalent" (at 0 4 90 unlocked) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 5.65 -1.75 270) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 138 "+VDC") (pintype "passive"))
    (pad "1" thru_hole circle (at 5.65 1.65 270) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 138 "+VDC") (pintype "passive"))
    (pad "2" thru_hole circle (at -5.75 1.65 270) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 126 "VIN") (pintype "passive"))
    (pad "2" thru_hole circle (at -5.75 -1.75 270) (size 3 3) (drill 1.65) (layers *.Cu *.Mask)
      (net 126 "VIN") (pintype "passive"))
    (model "${KIPRJMOD}/fuse.stp"
      (offset (xyz -0.1 0 -22))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 154.765 70.472756 90)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 0 2.33 90) (layer "B.SilkS") hide)
    (fp_text value "1x4" (at 0 -9.95 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.81) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 89 "X-1B") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 90 "X-1A") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 92 "X-2A") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 84 "X-2B") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 97.28 106.762874 -90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J12" (at 0 2.33 90) (layer "B.SilkS") hide)
    (fp_text value "1x3" (at 0 -7.41 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2.54) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "+3.3V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "Net-(J12-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 138 "+VDC") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 96.24 97 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "File: hammar.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J10" (at 0 2.33) (layer "B.SilkS") hide)
    (fp_text value "1x2" (at 0 -4.87) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.27 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "T-BED") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 188.555 120.762874) (end 91.055 65.762874) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "MISO" (at 125.305 99.444302) (layer "B.SilkS"))
  (gr_text "E" (at 97.465 73.5) (layer "B.SilkS"))
  (gr_text "S" (at 104.305 117.537874) (layer "B.SilkS"))
  (gr_text "+\n-" (at 179.715 94.372756) (layer "B.SilkS"))
  (gr_text "TX" (at 154.012143 104.762874) (layer "B.SilkS"))
  (gr_text "3,3V" (at 154.774047 99.762874) (layer "B.SilkS"))
  (gr_text "RX" (at 154.13119 107.352874) (layer "B.SilkS"))
  (gr_text "Hammar\nv1,1" (at 138.655476 87.25) (layer "B.SilkS"))
  (gr_text "Bed" (at 176.84 80.972756) (layer "B.SilkS"))
  (gr_text "Power" (at 171.715 108.472756) (layer "B.SilkS"))
  (gr_text "End" (at 176.84 97.5) (layer "B.SilkS"))
  (gr_text "Fan" (at 176.84 101.3) (layer "B.SilkS"))
  (gr_text "0" (at 125.305 94.442874) (layer "B.SilkS"))
  (gr_text "3,3V" (at 125.305 112.262874) (layer "B.SilkS"))
  (gr_text "RST" (at 119.915 96.762874) (layer "B.SilkS"))
  (gr_text "CERN OHL-P" (at 139.215 117.472756) (layer "B.SilkS"))
  (gr_text "Bed" (at 99.95 98.040118) (layer "B.SilkS"))
  (gr_text "SCK" (at 125.305 96.943588) (layer "B.SilkS"))
  (gr_text "Z voltage\n3,3V  VIN" (at 96.145 103.577992) (layer "B.SilkS"))
  (gr_text "SDA" (at 125.305 104.44573) (layer "B.SilkS"))
  (gr_text "+\n-" (at 179.715 84.222756) (layer "B.SilkS"))
  (gr_text "+\n-" (at 179.715 104.522756) (layer "B.SilkS"))
  (gr_text "Hotend" (at 101.75 91.762874) (layer "B.SilkS"))
  (gr_text "X" (at 150.965 73.5) (layer "B.SilkS"))
  (gr_text "Y" (at 133.215 73.5) (layer "B.SilkS"))
  (gr_text "SCL" (at 125.305 106.946444) (layer "B.SilkS"))
  (gr_text "VIN" (at 176.805 71.372756) (layer "B.SilkS"))
  (gr_text "Bed" (at 153.465 92.972756) (layer "B.SilkS"))
  (gr_text "-\n+" (at 179.715 74.072756) (layer "B.SilkS"))
  (gr_text "Z" (at 114.465 76.5) (layer "B.SilkS"))
  (gr_text "MOSI" (at 125.305 101.945016) (layer "B.SilkS"))
  (gr_text "VCC" (at 105.257381 112.472756) (layer "B.SilkS"))
  (zone (net 126) (net_name "VIN") (layers F&B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 163.555 73.312874)
        (xy 186.305 73.312874)
        (xy 186.305 78.262874)
        (xy 163.555 78.262874)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 182.305 69.262874)
        (xy 186.805 69.262874)
        (xy 186.805 73.012874)
        (xy 182.305 73.012874)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 142.465 108.222756)
        (xy 137.215 108.222756)
        (xy 137.215 102.972756)
        (xy 142.465 102.972756)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 157.555 83.012874)
        (xy 160.055 83.012874)
        (xy 160.055 87.262874)
        (xy 157.555 87.262874)
      )
    )
  )
  (zone (net 124) (net_name "BEDCONN-F") (layers F&B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 185.727636 89.907383)
        (xy 182.727632 89.972543)
        (xy 182.715 91.122756)
        (xy 168.715 91.122756)
        (xy 168.715 87.972756)
        (xy 178.215 87.972756)
        (xy 178.215 84.222756)
        (xy 185.715004 84.224978)
      )
    )
  )
  (zone (net 139) (net_name "BEDCONN") (layers F&B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 185.715 84.222756)
        (xy 178.215 84.222756)
        (xy 178.215 87.972756)
        (xy 170.215 87.972756)
        (xy 170.215 80.222756)
        (xy 185.715 80.222756)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 155.865 114.472756)
        (xy 155.865 121.472756)
        (xy 122.565 121.472756)
        (xy 122.565 114.222756)
      )
    )
  )
  (zone (net 138) (net_name "+VDC") (layers F&B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 184.555 78.262874)
        (xy 187.805 78.262874)
        (xy 187.805 105.262874)
        (xy 184.555 105.262874)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 165.965 90.972756)
        (xy 165.965 87.972756)
        (xy 168.715 87.972756)
        (xy 168.715 90.972756)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 160.165 80.422756)
        (xy 157.665 80.422756)
        (xy 157.665 75.922756)
        (xy 160.165 75.922756)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 92.055 66.762874)
        (xy 187.555 66.762874)
        (xy 187.555 119.762874)
        (xy 92.055 119.762874)
      )
    )
  )
  (zone (net 138) (net_name "+VDC") (layers F&B.Cu) (hatch edge 0.508)
    (priority 3)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 186.465 80.222756)
        (xy 170.215 80.222756)
        (xy 170.215 87.722756)
        (xy 163.465 87.722756)
        (xy 163.465 78.222756)
        (xy 186.465 78.222756)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 165.965 107.722756)
        (xy 165.965 104.722756)
        (xy 168.715 104.722756)
        (xy 168.715 107.722756)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160.505 91.362874)
        (xy 173.955 91.362874)
        (xy 173.955 103.062874)
        (xy 160.505 103.062874)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 96.005 80.012874)
        (xy 99.305 80.012874)
        (xy 99.305 83.312874)
        (xy 96.005 83.312874)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 149.955 79.962874)
        (xy 153.255 79.962874)
        (xy 153.255 83.262874)
        (xy 149.955 83.262874)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 113.905 80.012874)
        (xy 117.205 80.012874)
        (xy 117.205 83.312874)
        (xy 113.905 83.312874)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 161.065 91.562874)
        (xy 173.715 91.562874)
        (xy 173.715 96.472756)
        (xy 173.715001 102.722756)
        (xy 161.065001 102.812874)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 1))
    (polygon
      (pts
        (xy 132.005 79.962874)
        (xy 135.305 79.962874)
        (xy 135.305 83.262874)
        (xy 132.005 83.262874)
      )
    )
  )
)
